IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "3bd housA.ifc"
Time stamp: "2024-04-05T20:11:47+02:00"
Preprocessor: "IfcOpenShell v0.7.0-f7c03db75"
Originating system: "BlenderBIM 0.0.240403-7087452"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDING "Electrical"
        contains 4 elements
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "13 plate DW" | names: "ElectricAppliance"
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "4 plate ST" | names: "ElectricAppliance"
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "15kg WM" | names: "ElectricAppliance"
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "200lt FF" | names: "ElectricAppliance"
      IFCBUILDINGSTOREY "Furniture"
        contains 6 elements
          3 x IFCFURNITURE | type IFCFURNITURETYPE "King Size" | names: "Furniture"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "6 diner" | names: "Furniture"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "3 seater" | names: "Furniture"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "2 seater" | names: "Furniture"
      IFCBUILDINGSTOREY "Plumbing"
        contains 8 elements
          2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Shower" | names: "SanitaryTerminal"
          3 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Single basin" | names: "SanitaryTerminal"
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Sink" | names: "SanitaryTerminal"
          2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Toilet" | names: "SanitaryTerminal"
      IFCBUILDINGSTOREY "Roof"
        contains 36 elements
          16 x IFCBEAM | type IFCBEAMTYPE "Timber 38x114" | names: "Beam" | property sets: EPset_Parametric
          20 x IFCBEAM | type IFCBEAMTYPE "Timber 38x38x600" | names: "Beam" | material: profiles ("-test 240326") | property sets: EPset_Parametric
      IFCBUILDINGSTOREY "Wet works"
        contains 39 elements
          8 x IFCWALL | type IFCWALLTYPE "220mm load bearing" | names: "Wall" | material: layers ("Default" 250.) | property sets: EPset_Parametric
          15 x IFCWALL | type IFCWALLTYPE "110mm non-load bearing" | names: "Wall" | material: layers ("Unknown" 110.) | property sets: EPset_Parametric
          2 x IFCDOOR | type IFCDOORTYPE "Internal door LH" | names: "Door"
          2 x IFCDOOR | type IFCDOORTYPE "Internal door RH" | names: "Door"
          2 x IFCDOOR | type IFCDOORTYPE "External door RD" | names: "Door"
          1 x IFCCOVERING | type IFCCOVERINGTYPE "TYPEX" | CEILING | names: "Surface bed" | material: layers ("Unknown" 41.) | property sets: EPset_Parametric
          3 x IFCWINDOW | type IFCWINDOWTYPE "1790x1190 alu" | names: "Window"
          2 x IFCWINDOW | type IFCWINDOWTYPE "890x590 al" | names: "Window"
          3 x IFCWINDOW | type IFCWINDOWTYPE "1490x590 al" | TRIPLE_PANEL_VERTICAL | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "1490x590 al" | names: "Window"

Types
  IFCELECTRICAPPLIANCETYPE "13 plate DW" | DISHWASHER | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "4 plate ST" | ELECTRICCOOKER | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "15kg WM" | WASHINGMACHINE | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "200lt FF" | FRIDGE_FREEZER | 1 occurrence
  IFCFURNITURETYPE "King Size" | BED | 3 occurrences
  IFCFURNITURETYPE "6 diner" | TABLE | 1 occurrence | description "1x1.6m tabke with 1m movement space"
  IFCFURNITURETYPE "3 seater" | SOFA | 1 occurrence
  IFCFURNITURETYPE "2 seater" | SOFA | 1 occurrence
  IFCSANITARYTERMINALTYPE "Shower" | SHOWER | 2 occurrences
  IFCSANITARYTERMINALTYPE "Single basin" | WASHHANDBASIN | 3 occurrences
  IFCSANITARYTERMINALTYPE "Sink" | SINK | 1 occurrence
  IFCSANITARYTERMINALTYPE "Toilet" | TOILETPAN | 2 occurrences
  IFCBEAMTYPE "Timber 38x114" | BEAM | 16 occurrences
  IFCBEAMTYPE "Timber 38x38x600" | BEAM | 20 occurrences | material: profiles ("-test 240326")
  IFCWALLTYPE "220mm load bearing" | SOLIDWALL | 8 occurrences | material: layers ("Default" 250.) | property sets: EPset_Parametric
  IFCWALLTYPE "110mm non-load bearing" | SOLIDWALL | 15 occurrences | material: layers ("Unknown" 110.) | property sets: EPset_Parametric
  IFCDOORTYPE "Internal door LH" | DOOR | SINGLE_SWING_LEFT | 2 occurrences | property sets: BBIM_Door | description "RDF4"
  IFCDOORTYPE "Internal door RH" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | property sets: BBIM_Door | description "RDF4"
  IFCDOORTYPE "External door RD" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | property sets: BBIM_Door
  IFCCOVERINGTYPE "TYPEX" | CEILING | 1 occurrence | material: layers ("Unknown" 41.) | property sets: EPset_Parametric
  IFCWINDOWTYPE "1790x1190 alu" | WINDOW | TRIPLE_PANEL_LEFT | 3 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "890x590 al" | WINDOW | DOUBLE_PANEL_HORIZONTAL | 2 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "1490x590 al" | WINDOW | TRIPLE_PANEL_VERTICAL | 4 occurrences | property sets: BBIM_Window

Property sets
  EPset_Parametric | properties | on 36 objects (36 IFCBEAM)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 23 objects (23 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 1 object (1 IFCCOVERING)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS3" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1:20" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/20" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2100.0001430511475, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 115.00000208616257, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 110.00000685453415, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 2100.0001430511475, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 115.00000208616257, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 110.00000685453415, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 2000.0, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 220.0000137090683, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 100.00000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_LEFT", "overall_height": 1190.000057220459, "overall_width": 1790.000081062317, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 700.0000476837158, "transom_thickness": 50.00000074505806, "first_transom_offset": 650.0000357627869}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_HORIZONTAL", "overall_height": 890.00004529953, "overall_width": 600.0000238418579, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 50.00000074505806, "first_transom_offset": 500.0}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_VERTICAL", "overall_height": 600.0000238418579, "overall_width": 1490.0001287460327, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 500.0, "second_mullion_offset": 1000.0}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)