IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
File name: "0001"
Time stamp: "2021-12-28T23:05:49"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.50.27 - Exporter 21.1.50.27 - Alternate UI 21.1.50.27"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "paulius.spudys" of Organization (no name given)
  Owner history of Person "paulius.spudys" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1640725397 (2021-12-28T21:03:17Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 18 elements
          8 x IFCWALL | type IFCWALLTYPE "Basic Wall:Exterior - Brick on Mtl. Stud" | object type "Basic Wall:Exterior - Brick on Mtl. Stud" | names: "Basic Wall:Exterior - Brick on Mtl. Stud:346591", "Basic Wall:Exterior - Brick on Mtl. Stud:346614", "Basic Wall:Exterior - Brick on Mtl. Stud:346652" (+5 more) | material: layers "Basic Wall:Exterior - Brick on Mtl. Stud" ("Brick, Common" 90., "Air" 76., "Air Infiltration Barrier" 0., "Plywood, Sheathing" 19., "Metal Stud Layer" 152., "Vapour Retarder" 0., "Gypsum Wall Board" 13.) | property sets: Qto_WallBaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | DOOR | SINGLE_SWING_RIGHT | names: "M_Single-Flush:0915 x 2134mm:346907", "M_Single-Flush:0915 x 2134mm:346974" | material: constituents "MaterialConstituentSet" ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators, Qto_DoorBaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Interior - 135mm Partition (2-hr)" | object type "Basic Wall:Interior - 135mm Partition (2-hr)" | names: "Basic Wall:Interior - 135mm Partition (2-hr):347078", "Basic Wall:Interior - 135mm Partition (2-hr):347116" | material: layers "Basic Wall:Interior - 135mm Partition (2-hr)" ("Gypsum Wall Board" 15.5, "Gypsum Wall Board" 15.5, "Metal Stud Layer" 64., "Gypsum Wall Board" 15.5, "Gypsum Wall Board" 15.5, "Gypsum Wall Board" 9.5) | property sets: Qto_WallBaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWINDOW | type IFCWINDOWTYPE "M_Fixed:0406 x 0610mm" | object type "M_Fixed:0406 x 0610mm" | WINDOW | names: "M_Fixed:0406 x 0610mm:347127" | material: constituents "MaterialConstituentSet" ("Glass": "Glass", "Sash": "Sash") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon, Qto_WindowBaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0762 x 2134mm" | object type "M_Single-Flush:0762 x 2134mm" | DOOR | SINGLE_SWING_RIGHT | names: "M_Single-Flush:0762 x 2134mm:347178" | material: constituents "MaterialConstituentSet" ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators, Qto_DoorBaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWTYPE "M_Fixed:0406 x 0610mm" | object type "M_Fixed:0406 x 0610mm" | WINDOW | names: "M_Fixed:0406 x 0610mm:347350", "M_Fixed:0406 x 0610mm:347377" | material: constituents "MaterialConstituentSet" ("Glass": "Glass", "Sash": "Sash") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon, Qto_WindowBaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWTYPE "M_Fixed:0406 x 0610mm" | object type "M_Fixed:0406 x 0610mm" | WINDOW | names: "M_Fixed:0406 x 0610mm:347447" | material: constituents "MaterialConstituentSet" ("Glass": "Glass", "Sash": "Sash") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon, Qto_WindowBaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Concrete-Domestic 425mm" | object type "Floor:Concrete-Domestic 425mm" | FLOOR | names: "Floor:Concrete-Domestic 425mm:347525" | material: layers "Floor:Concrete-Domestic 425mm" ("Concrete, Sand/Cement Screed" 50., "Concrete, Cast In Situ" 175., "Damp-proofing" 0., "Rigid insulation" 50., "Site - Hardcore" 150.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities, Constraints, Dimensions
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:8mm Head" | elevation 3500.
        contains 1 element
          1 x IFCROOF | object type "Basic Roof:Generic - 400mm" | names: "Basic Roof:Generic - 400mm:347580" | parts: 4 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon, Constraints, Construction, Dimensions, Other

Types
  IFCWALLTYPE "Basic Wall:Exterior - Brick on Mtl. Stud" | 8 occurrences | material: layers "Basic Wall:Exterior - Brick on Mtl. Stud" ("Brick, Common" 90., "Air" 76., "Air Infiltration Barrier" 0., "Plywood, Sheathing" 19., "Metal Stud Layer" 152., "Vapour Retarder" 0., "Gypsum Wall Board" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORTYPE "M_Single-Flush:0915 x 2134mm" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:346907, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:Interior - 135mm Partition (2-hr)" | 2 occurrences | material: layers "Basic Wall:Interior - 135mm Partition (2-hr)" ("Gypsum Wall Board" 15.5, "Gypsum Wall Board" 15.5, "Metal Stud Layer" 64., "Gypsum Wall Board" 15.5, "Gypsum Wall Board" 15.5, "Gypsum Wall Board" 9.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWTYPE "M_Fixed:0406 x 0610mm" | WINDOW | 1 occurrence | material: materials ("Sash", "Glass", "Sash", "Sash") | property sets: M_Fixed:0406 x 0610mm:347127, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORTYPE "M_Single-Flush:0762 x 2134mm" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Panel", "Door - Frame") | property sets: M_Single-Flush:0762 x 2134mm:347178, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWTYPE "M_Fixed:0406 x 0610mm" | WINDOW | 2 occurrences | material: materials ("Sash", "Sash", "Sash", "Glass") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWTYPE "M_Fixed:0406 x 0610mm" | WINDOW | 1 occurrence | material: materials ("Sash", "Glass", "Sash", "Sash") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCSLABTYPE "Floor:Concrete-Domestic 425mm" | FLOOR | 1 occurrence | material: layers "Floor:Concrete-Domestic 425mm" ("Concrete, Sand/Cement Screed" 50., "Concrete, Cast In Situ" 175., "Damp-proofing" 0., "Rigid insulation" 50., "Site - Hardcore" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "3" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 2" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 3 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "23.30.20.17.11" (IFCTEXT)
    OmniClass Title = "Fixed Windows" (IFCTEXT)
    Type Mark = "10" (IFCTEXT)
    Type Name = "0406 x 0610mm" (IFCTEXT)
  Identity Data: 5 more contents on 0 objects not shown
  Other | properties | on 8 objects (8 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Exterior - Brick on Mtl. Stud" (IFCLABEL)
    Family and Type = "Basic Wall: Exterior - Brick on Mtl. Stud" (IFCLABEL)
    Type = "Basic Wall: Exterior - Brick on Mtl. Stud" (IFCLABEL)
    Type Id = "Basic Wall: Exterior - Brick on Mtl. Stud" (IFCLABEL)
  Other | properties | on 3 objects (3 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "M_Fixed: 0406 x 0610mm" (IFCLABEL)
    Family and Type = "M_Fixed: 0406 x 0610mm" (IFCLABEL)
    Head Height = 1525. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: Exterior - Brick on Mtl. Stud" (IFCLABEL)
    Type = "M_Fixed: 0406 x 0610mm" (IFCLABEL)
    Type Id = "M_Fixed: 0406 x 0610mm" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "M_Single-Flush: 0915 x 2134mm" (IFCLABEL)
    Family and Type = "M_Single-Flush: 0915 x 2134mm" (IFCLABEL)
    Head Height = 2134. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: Exterior - Brick on Mtl. Stud" (IFCLABEL)
    Type = "M_Single-Flush: 0915 x 2134mm" (IFCLABEL)
    Type Id = "M_Single-Flush: 0915 x 2134mm" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Interior - 135mm Partition (2-hr)" (IFCLABEL)
    Family and Type = "Basic Wall: Interior - 135mm Partition (2-hr)" (IFCLABEL)
    Type = "Basic Wall: Interior - 135mm Partition (2-hr)" (IFCLABEL)
    Type Id = "Basic Wall: Interior - 135mm Partition (2-hr)" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "M_Fixed: 0406 x 0610mm" (IFCLABEL)
    Family and Type = "M_Fixed: 0406 x 0610mm" (IFCLABEL)
    Head Height = 1525. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: Interior - 135mm Partition (2-hr)" (IFCLABEL)
    Type = "M_Fixed: 0406 x 0610mm" (IFCLABEL)
    Type Id = "M_Fixed: 0406 x 0610mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "M_Single-Flush: 0762 x 2134mm" (IFCLABEL)
    Family and Type = "M_Single-Flush: 0762 x 2134mm" (IFCLABEL)
    Head Height = 2134. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: Interior - 135mm Partition (2-hr)" (IFCLABEL)
    Type = "M_Single-Flush: 0762 x 2134mm" (IFCLABEL)
    Type Id = "M_Single-Flush: 0762 x 2134mm" (IFCLABEL)
  Other: 6 more contents on 2 objects not shown
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 3.09749999999999 [SQUARE_METRE]
    Height = 3500. [MILLI METRE]
    Length = 8850. [MILLI METRE]
    NetSideArea = 28.77473 [SQUARE_METRE]
    NetSideArea = 30975000. [SQUARE_METRE]
    NetVolume = 10.0711555 [CUBIC_METRE]
    NetVolume = 10841250000. [CUBIC_METRE]
    Width = 350. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 4.20000000000001 [SQUARE_METRE]
    Height = 3500. [MILLI METRE]
    Length = 12000. [MILLI METRE]
    NetSideArea = 42. [SQUARE_METRE]
    NetSideArea = 42000000. [SQUARE_METRE]
    NetVolume = 14.7 [CUBIC_METRE]
    NetVolume = 14700000000. [CUBIC_METRE]
    Width = 350. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.97500000000001 [SQUARE_METRE]
    Height = 3500. [MILLI METRE]
    Length = 8500. [MILLI METRE]
    NetSideArea = 29.75 [SQUARE_METRE]
    NetSideArea = 29750000. [SQUARE_METRE]
    NetVolume = 10.4125 [CUBIC_METRE]
    NetVolume = 10412500000. [CUBIC_METRE]
    Width = 350. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.065 [SQUARE_METRE]
    Height = 3500. [MILLI METRE]
    Length = 5900. [MILLI METRE]
    NetSideArea = 20.65 [SQUARE_METRE]
    NetSideArea = 20650000. [SQUARE_METRE]
    NetVolume = 7.2275 [CUBIC_METRE]
    NetVolume = 7227500000. [CUBIC_METRE]
    Width = 350. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.085 [SQUARE_METRE]
    Height = 3500. [MILLI METRE]
    Length = 3100. [MILLI METRE]
    NetSideArea = 10.60234 [SQUARE_METRE]
    NetSideArea = 10850000. [SQUARE_METRE]
    NetVolume = 3.710819 [CUBIC_METRE]
    NetVolume = 3797500000. [CUBIC_METRE]
    Width = 350. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.365 [SQUARE_METRE]
    Height = 3500. [MILLI METRE]
    Length = 3900. [MILLI METRE]
    NetSideArea = 11.69739 [SQUARE_METRE]
    NetSideArea = 13650000. [SQUARE_METRE]
    NetVolume = 4.0940865 [CUBIC_METRE]
    NetVolume = 4777500000. [CUBIC_METRE]
    Width = 350. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.085 [SQUARE_METRE]
    Height = 3500. [MILLI METRE]
    Length = 3100.00000000001 [MILLI METRE]
    NetSideArea = 10.85 [SQUARE_METRE]
    NetSideArea = 10850000. [SQUARE_METRE]
    NetVolume = 3.79750000000002 [CUBIC_METRE]
    NetVolume = 3797500000.00001 [CUBIC_METRE]
    Width = 350. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.647500000000004 [SQUARE_METRE]
    Height = 3500. [MILLI METRE]
    Length = 1850.00000000001 [MILLI METRE]
    NetSideArea = 6.22734000000003 [SQUARE_METRE]
    NetSideArea = 6475000.00000003 [SQUARE_METRE]
    NetVolume = 2.17956900000001 [CUBIC_METRE]
    NetVolume = 2266250000.00001 [CUBIC_METRE]
    Width = 350. [MILLI METRE]
  Qto_WallBaseQuantities: 2 more contents on 2 objects not shown
  Constraints | properties | on 10 objects (10 IFCWALL)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Cross-Section = "Vertical" (IFCIDENTIFIER)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 2" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3500. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 4 objects (4 IFCWINDOW)
    Level = "Level: Level 1" (IFCLABEL)
    Sill Height = 915.000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 3 objects (3 IFCDOOR)
    Level = "Level: Level 1" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: Level 1" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCROOF)
    Base Level = "Level: Level 2" (IFCLABEL)
    Base Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cutoff Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 3500. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 3 objects (3 IFCWINDOW)
    Area = 1.06240800000004 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0247528520000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCDOOR)
    Area = 3.18957899999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.119856109999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 28.77473 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 8500. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 10.0711555 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 42. (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 12000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 14.7 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 29.75 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 8500. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 10.4125 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 20.65 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 5900. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 7.2275 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 10.60234 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3100. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 3.710819 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 12 more contents on 9 objects not shown
  Phasing | properties | on 19 objects (10 IFCWALL, 4 IFCWINDOW, 3 IFCDOOR, 1 IFCROOF)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 10 objects (10 IFCWALL)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 1 object (1 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Pset_EnvironmentalImpactIndicators | properties | on 8 objects (8 IFCWALL) | on 1 type object
    Reference = "Exterior - Brick on Mtl. Stud" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 5 objects (4 IFCSLAB, 1 IFCROOF)
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 4 objects (4 IFCWINDOW) | on 3 type objects
    Reference = "0406 x 0610mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 2 objects (2 IFCDOOR) | on 1 type object
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 2 objects (2 IFCWALL) | on 1 type object
    Reference = "Interior - 135mm Partition (2-hr)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Reference = "0762 x 2134mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Concrete-Domestic 425mm" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 8 objects (8 IFCWALL) | on 1 type object
    Reference = "Exterior - Brick on Mtl. Stud" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALL) | on 1 type object
    Reference = "Interior - 135mm Partition (2-hr)" (IFCLABEL)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Exterior - Brick on Mtl. Stud" (IFCIDENTIFIER)
    ThermalTransmittance = 0.105419490008354 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - 135mm Partition (2-hr)" (IFCIDENTIFIER)
    ThermalTransmittance = 0.374531835205993 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Exterior - Brick on Mtl. Stud" (IFCIDENTIFIER)
    ThermalTransmittance = 0.105419490008354 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Interior - 135mm Partition (2-hr)" (IFCIDENTIFIER)
    ThermalTransmittance = 0.374531835205993 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0762 x 2134mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Qto_DoorBaseQuantities | quantities | on 2 objects (2 IFCDOOR)
    Area = 3.18957899999998 [SQUARE_METRE]
    Height = 2134. [MILLI METRE]
    Width = 915. [MILLI METRE]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 2.82436799999998 [SQUARE_METRE]
    Height = 2134. [MILLI METRE]
    Width = 762. [MILLI METRE]
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0406 x 0610mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW) | on 3 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0406 x 0610mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Qto_WindowBaseQuantities | quantities | on 3 objects (3 IFCWINDOW)
    Area = 1.06240800000004 [SQUARE_METRE]
    Height = 610. [MILLI METRE]
    Width = 406. [MILLI METRE]
  Qto_WindowBaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Area = 0.654000000000043 [SQUARE_METRE]
    Height = 610. [MILLI METRE]
    Width = 406. [MILLI METRE]
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB)
    Reference = "Generic - 400mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Concrete-Domestic 425mm" (IFCLABEL)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 33.0797337253075 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Concrete-Domestic 425mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.608392189447445 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Concrete-Domestic 425mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.608392189447445 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Qto_SlabBaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    GrossArea = 3.76193978301695 [SQUARE_METRE]
    GrossVolume = 1504.77591320679 [CUBIC_METRE]
    NetArea = 271.995485317924 [SQUARE_METRE]
    NetVolume = 50.4823528374025 [CUBIC_METRE]
    Perimeter = 29368.5983001197 [MILLI METRE]
    Width = 400.000000000002 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 81.7725 [SQUARE_METRE]
    GrossVolume = 34753.3125 [CUBIC_METRE]
    NetArea = 183.01 [SQUARE_METRE]
    NetVolume = 34.7533125 [CUBIC_METRE]
    Perimeter = 45800. [MILLI METRE]
    Width = 425. [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 2.1005152731672 [SQUARE_METRE]
    GrossVolume = 840.206109266883 [CUBIC_METRE]
    NetArea = 271.995485317924 [SQUARE_METRE]
    NetVolume = 50.4823528374025 [CUBIC_METRE]
    Perimeter = 22368.5983001197 [MILLI METRE]
    Width = 400.000000000003 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 2.10051527316719 [SQUARE_METRE]
    GrossVolume = 840.206109266882 [CUBIC_METRE]
    NetArea = 271.995485317924 [SQUARE_METRE]
    NetVolume = 50.4823528374025 [CUBIC_METRE]
    Perimeter = 22368.5983001197 [MILLI METRE]
    Width = 400.000000000002 [MILLI METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 6516.65515651579 (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 3 type objects
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Width = 135.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Default Thickness = 425. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "8mm Head" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Qto_OpeningElementBaseQuantities | quantities | on 2 objects (2 IFCOPENINGELEMENT)
    Depth = 350. [MILLI METRE]
    Height = 915. [MILLI METRE]
    Width = 2134. [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 2 objects (2 IFCOPENINGELEMENT)
    Depth = 350. [MILLI METRE]
    Height = 406. [MILLI METRE]
    Width = 609.999999999999 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 350. [MILLI METRE]
    Height = 405.999999999999 [MILLI METRE]
    Width = 609.999999999999 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 135.5 [MILLI METRE]
    Height = 762. [MILLI METRE]
    Width = 2134. [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 135.5 [MILLI METRE]
    Height = 406.000000000001 [MILLI METRE]
    Width = 609.999999999999 [MILLI METRE]
  Analytical Properties | properties | on 3 type objects
    Analytic Construction = "1/8 in Pilkington single glazing" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
    Heat Transfer Coefficient (U) = 3.6886 (IFCREAL)
    Solar Heat Gain Coefficient = 0.78 (IFCREAL)
    Thermal Resistance (R) = 0.271105568508377 (IFCREAL)
    Visual Light Transmittance = 0.9 (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Analytic Construction = "Metal" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.105419490008354 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 13.4114380379735 (IFCREAL)
    Thermal Resistance (R) = 9.48591194968553 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.374531835205993 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 6.14489216644915 (IFCREAL)
    Thermal Resistance (R) = 2.67 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.608392189447445 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Mass = 31.74385393152 (IFCREAL)
    Thermal Resistance (R) = 1.64367659109533 (IFCREAL)
  Graphics | properties | on 3 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Materials and Finishes | properties | on 3 type objects
    Frame Exterior Material = "Sash" (IFCLABEL)
    Frame Interior Material = "Sash" (IFCLABEL)
    Glass Pane Material = "Glass" (IFCLABEL)
    Sash = "Sash" (IFCLABEL)
  Materials and Finishes | properties | on 2 type objects
    Structural Material = "Metal Stud Layer" (IFCLABEL)
  Materials and Finishes | properties | on 2 type objects
    Door Material = "Door - Panel" (IFCLABEL)
    Frame Material = "Door - Frame" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Structural Material = "Concrete, Cast In Situ" (IFCLABEL)
  M_Single-Flush:0915 x 2134mm:346907 | predefined | on 2 type objects
  M_Fixed:0406 x 0610mm:347127 | predefined | on 1 type object
  M_Single-Flush:0762 x 2134mm:347178 | predefined | on 2 type objects
  M_Fixed:0406 x 0610mm:347350 | predefined | on 1 type object
  M_Fixed:0406 x 0610mm:347447 | predefined | on 1 type object