IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2023-05-12T11:58:18"
Preprocessor: "IfcOpenShell v0.7.0-476ab506d"
Originating system: "IfcOpenShell v0.7.0-476ab506d"
Application: "Tekla Structures" version "2021 Service Pack 12" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "WIJNEN\g.mijnsbergen" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "WIJNEN\g.mijnsbergen" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 12" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1682339209 (2023-04-24T12:26:49Z)
  Owner history of Person "Undefined" id "WIJNEN\g.mijnsbergen" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 12" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1682344800 (2023-04-24T14:00:00Z)
  6 x Owner history of Person "Undefined" id "WIJNEN\g.mijnsbergen" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 12" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | state READWRITE | change ADDED | created 1683023765 (2023-05-02T10:36:05Z) | last modified 1683023765 (2023-05-02T10:36:05Z) by Person "Undefined" id "WIJNEN\g.mijnsbergen" of Organization "Trimble Solutions Corporation" with "Tekla Structures" version "2021 Service Pack 12" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "WIJNEN\g.mijnsbergen" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 12" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | state READWRITE | change ADDED | created 1683885498 (2023-05-12T09:58:18Z) | last modified 1683885498 (2023-05-12T09:58:18Z) by Person "Undefined" id "WIJNEN\g.mijnsbergen" of Organization "Trimble Solutions Corporation" with "Tekla Structures" version "2021 Service Pack 12" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Project"
IFCELEMENTASSEMBLY "BORDES" | REINFORCEMENT_UNIT
  IFCSLAB "BORDES" | object type "1220*300" | FLOOR | description "1220*300"

Property sets
  ILS Ontwerp en Engineering | properties | on 1 object (1 IFCSLAB)
    3.3 Bouwlaag (no value)
    3.4 Entiteit (no value)
    3.5 Naamgeving element (no value)
    3.6 Codering - NL-SfB = "23.24" (IFCLABEL)
    4.3 Dragend (no value)
    4.4 Uitwendig (no value)
    4.5 A Brandwerendheid (no value)
    4.6 A Warmtedoorgangscoefficient (no value)
    4.6 B Luchtgeluidisolatie (no value)
    4.7 Materiaal (no value)
    4.8 B Aantrede (no value)
    4.8 B Afwerking/ behandeling (no value)
    4.8 B Fase (no value)
    4.8 B Kleur (no value)
    4.8 B Merk = "BO5" (IFCLABEL)
    4.8 B Optrede (no value)
    4.8 B Vlakheidsklasse (no value)
    4.8 B Weerstandsklasse (no value)
    4.8 C Brandwerendheid hoofddraagconstructie (no value)
    4.8 C Conservering (no value)
    4.8 C Kolomnummer (no value)
    4.8 C Liggernummer (no value)
    4.8 C Massa (no value)
    4.8 C Milieuklasse (no value)
    4.8 C Oppervlakteklasse (no value)
    4.8 C Overspanningsrichting (no value)
    4.8 C Paalnummer (no value)
    4.8 C Sterkteklasse (no value)
    4.8 C Wapeningshoeveelheid (no value)
    Q Breedte/Dikte (no value)
    Q Breedte/Dikte (no value)
    Q Hoogte (no value)
    Q Inhoud (no value)
    Q Lengte (no value)
    Q Oppervlakte = 3.23 (IFCAREAMEASURE) [SQUARE_METRE]
    Q Profiel (no value)
  ILS Ontwerp en Engineering | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    3.3 Bouwlaag = "16 zestiende verdieping" (IFCLABEL)
    3.4 Entiteit = "IfcSlab" (IFCLABEL)
    3.5 Naamgeving element = "BORDES" (IFCLABEL)
    3.6 Codering - NL-SfB = "23.24" (IFCLABEL)
    4.3 Dragend = "Ja" (IFCLABEL)
    4.4 Uitwendig = "Nee" (IFCLABEL)
    4.5 A Brandwerendheid = "-" (IFCLABEL)
    4.6 A Warmtedoorgangscoefficient = "-" (IFCLABEL)
    4.6 B Luchtgeluidisolatie (no value)
    4.7 Materiaal = "CONCRETE" (IFCLABEL)
    4.8 B Aantrede (no value)
    4.8 B Afwerking/ behandeling = "n.t.b." (IFCLABEL)
    4.8 B Fase = "Nieuwbouw" (IFCLABEL)
    4.8 B Kleur = "-" (IFCLABEL)
    4.8 B Merk = "BO5" (IFCLABEL)
    4.8 B Optrede (no value)
    4.8 B Vlakheidsklasse = "-" (IFCLABEL)
    4.8 B Weerstandsklasse = "-" (IFCLABEL)
    4.8 C Brandwerendheid hoofddraagconstructie = "-" (IFCLABEL)
    4.8 C Conservering = "-" (IFCLABEL)
    4.8 C Kolomnummer (no value)
    4.8 C Liggernummer (no value)
    4.8 C Massa = 2500. (IFCMASSMEASURE) [KILO GRAM]
    4.8 C Milieuklasse = "n.t.b." (IFCLABEL)
    4.8 C Oppervlakteklasse = "-" (IFCLABEL)
    4.8 C Overspanningsrichting = "-" (IFCLABEL)
    4.8 C Paalnummer (no value)
    4.8 C Sterkteklasse = "C45/55" (IFCLABEL)
    4.8 C Wapeningshoeveelheid = "-" (IFCLABEL)
    Q Breedte/Dikte = 1220. (IFCLENGTHMEASURE) [MILLI METRE]
    Q Breedte/Dikte = 1220. (IFCLENGTHMEASURE) [MILLI METRE]
    Q Hoogte = 320. (IFCLENGTHMEASURE) [MILLI METRE]
    Q Inhoud = 0.98 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Q Lengte = 2710. (IFCLENGTHMEASURE) [MILLI METRE]
    Q Oppervlakte = 3.28 (IFCAREAMEASURE) [SQUARE_METRE]
    Q Profiel = "1220*300" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCSLAB)
    Bottom elevation = "+47.700" (IFCLABEL)
    Class = "5" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+48.020" (IFCLABEL)
  Tekla Quantity | properties | on 1 object (1 IFCSLAB)
    Area per tons = 3.751 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.585 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 320. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 2710. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 9.15 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.976 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 2439.54 (IFCMASSMEASURE) [KILO GRAM]
    Width = 1220. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "BO5" (IFCIDENTIFIER)
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 0.5854 [SQUARE_METRE]
    NetVolume = 0.975817174892292 [CUBIC_METRE]
    NetWeight = 2439.54293723073 [KILO GRAM]
    Width = 1220. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCELEMENTASSEMBLY)
    Width = 1220. [MILLI METRE]
  ILS Ontwerp en Engineering_Bordes | properties | on 1 object (1 IFCSLAB)
    3.3 Bouwlaag = "16 zestiende verdieping" (IFCLABEL)
    3.4 Entiteit = "IfcSlab" (IFCLABEL)
    3.5 Naamgeving element = "BORDES" (IFCLABEL)
    3.6 Codering - NL-SfB = "23.24" (IFCLABEL)
    4.3 Dragend = "Ja" (IFCLABEL)
    4.4 Uitwendig = "Nee" (IFCLABEL)
    4.5 A Brandwerendheid = "-" (IFCLABEL)
    4.6 A Warmtedoorgangscoefficient = "-" (IFCLABEL)
    4.7 Materiaal = "CONCRETE" (IFCLABEL)
    4.8 B Afwerking/ behandeling = "n.t.b." (IFCLABEL)
    4.8 B Fase = "Nieuwbouw" (IFCLABEL)
    4.8 B Kleur = "-" (IFCLABEL)
    4.8 B Merk = "BO5" (IFCLABEL)
    4.8 B Vlakheidsklasse = "-" (IFCLABEL)
    4.8 B Weerstandsklasse = "-" (IFCLABEL)
    4.8 C Brandwerendheid hoofddraagconstructie = "-" (IFCLABEL)
    4.8 C Conservering = "-" (IFCLABEL)
    4.8 C Massa = 2500. (IFCREAL)
    4.8 C Milieuklasse = "n.t.b." (IFCLABEL)
    4.8 C Oppervlakteklasse = "-" (IFCLABEL)
    4.8 C Overspanningsrichting = "-" (IFCLABEL)
    4.8 C Sterkteklasse = "C45/55" (IFCLABEL)
    4.8 C Wapeningshoeveelheid = "-" (IFCLABEL)
    Q Breedte/Dikte = 1220. (IFCREAL)
    Q Hoogte = 320. (IFCREAL)
    Q Inhoud = 0.98 (IFCREAL)
    Q Lengte = 2710. (IFCREAL)
    Q Oppervlakte = 3.28 (IFCREAL)
    Q Profiel = "1220*300" (IFCLABEL)
  Tekla Assembly_Bordes | properties | on 1 object (1 IFCSLAB)
    Assembly/Cast unit Mark = "BO5" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+47.700" (IFCLABEL)
    Assembly/Cast unit position code = "2-3/C-D" (IFCLABEL)
    Assembly/Cast unit top elevation = "+48.020" (IFCLABEL)
    Assembly/Cast unit weight = 2439.5 (IFCREAL)
    Cast unit rebar weight = 0. (IFCREAL)
  BaseQuantities_Bordes | properties | on 1 object (1 IFCSLAB)
    Width = 1220. (IFCREAL)
  Tekla Assembly | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "BO5" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+47.700" (IFCLABEL)
    Assembly/Cast unit position code = "2-3/C-D" (IFCLABEL)
    Assembly/Cast unit top elevation = "+48.020" (IFCLABEL)
    Assembly/Cast unit weight = 2439.5 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Control number (no value)