IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2023-01-20T14:55:09"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.20.44 - Exporter 21.1.20.44 - Interface utilisateur alternative 21.1.20.44"
Application: "Autodesk Revit 2021 (FRA)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (FRA)"

People and organizations
  Person "arthur.bellemin" of Organization (no name given)
  Owner history of Person "arthur.bellemin" of Organization (no name given) | application "Autodesk Revit 2021 (FRA)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (FRA)" | change NOCHANGE | created 1674036031 (2023-01-18T10:00:31Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 48° 51′ 23.999633″ | longitude 2° 21′ 3.553905″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l'adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | object type "Niveau:Pointe 8 mm" | elevation 0.
        contains 13 elements
          1 x IFCSLAB | type IFCSLABTYPE "Sol:STR_19+1cm" | object type "Sol:STR_19+1cm" | FLOOR | names: "Sol:STR_19+1cm:140951" | material: layers "Sol:STR_19+1cm" ("Moquette" 10., "Béton - Ordinaire" 190.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Mur de base:Cloison 100" | object type "Mur de base:Cloison 100" | names: "Mur de base:Cloison 100:143942", "Mur de base:Cloison 100:143943", "Mur de base:Cloison 100:143944" (+1 more) | material: layers "Mur de base:Cloison 100" ("Cloison" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Fenetre:Fenetre" | object type "Fenetre:Fenetre" | names: "Fenetre:Fenetre:145290", "Fenetre:Fenetre:145333" | material: "Fenetre" | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Plafond composé:Normal" | object type "Plafond composé:Normal" | CEILING | names: "Plafond composé:Normal:147710" | material: layers "Plafond composé:Normal" ("Montant métallique" 45., "Plaque de mur de gypse" 12.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Simple avec alignement:93x210ht" | object type "Simple avec alignement:93x210ht" | names: "Simple avec alignement:93x210ht:147725" | material: materials ("Porte - Cadre", "Porte - Panneau") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Lightning_Ceiling-Mounted_Fasual_P66L_FR:P66L WW" | object type "Lightning_Ceiling-Mounted_Fasual_P66L_FR:P66L WW" | names: "Lightning_Ceiling-Mounted_Fasual_P66L_FR:P66L WW:149191", "Lightning_Ceiling-Mounted_Fasual_P66L_FR:P66L WW:149192", "Lightning_Ceiling-Mounted_Fasual_P66L_FR:P66L WW:149354" (+1 more) | material: materials ("FAS_Aluminum, Anodized Blue", "FAS_Polycarbonate, Clear", "FAS_Aluminium") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff

Types
  IFCSLABTYPE "Sol:STR_19+1cm" | FLOOR | 1 occurrence | material: layers "Sol:STR_19+1cm" ("Moquette" 10., "Béton - Ordinaire" 190.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Mur de base:Cloison 100" | STANDARD | 4 occurrences | material: layers "Mur de base:Cloison 100" ("Cloison" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWINDOWSTYLE "Fenetre:Fenetre" | 2 occurrences | material: "Fenetre" | property sets: Fenetre:Fenetre:145290, Pset_QuantityTakeOff, Pset_WindowCommon
  IFCCOVERINGTYPE "Plafond composé:Normal" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Simple avec alignement:93x210ht" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Porte - Cadre", "Porte - Panneau") | property sets: Simple avec alignement:93x210ht:147725, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "Lightning_Ceiling-Mounted_Fasual_P66L_FR:P66L WW" | 4 occurrences | material: materials ("FAS_Aluminium", "FAS_Aluminum, Anodized Blue") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff

Property sets
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Cloison 100" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCFLOWTERMINAL) | on 1 type object
    Reference = "P66L WW" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCWINDOW) | on 1 type object
    Reference = "Fenetre" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "STR_19+1cm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "Normal" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Reference = "93x210ht" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "25x25ht" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "STR_19+1cm" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "STR_19+1cm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "STR_19+1cm" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Cloison 100" (IFCLABEL)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Cloison 100" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Cloison 100" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "25x25ht" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fenetre" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Fenetre" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Plaque de mur de gypse;" (IFCTEXT)
    Reference = "Normal" (IFCIDENTIFIER)
    TotalThickness = 57. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    Reference = "Normal" (IFCIDENTIFIER)
    TotalThickness = 57. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "93x210ht" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWTERMINAL) | on 1 type object
    Reference = "P66L WW" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Fenetre:Fenetre:145290 | predefined | on 1 type object
  Simple avec alignement:93x210ht:147725 | predefined | on 2 type objects