IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "2018_01"
Time stamp: "2021-07-08T08:00:38"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20180328_1600(x64) - Exporter 19.0.1.1 - Alternativ-UI 19.0.1.1"
Application: "Autodesk Revit 2019 (DEU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (DEU)"

People and organizations
  Person "Darija" of Organization (no name given)
  Owner history of Person "Darija" of Organization (no name given) | application "Autodesk Revit 2019 (DEU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (DEU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "2018_01" | phase "Projekt Status"
  IFCSITE "Default" | latitude 48° 8′ 15.359802″ | longitude 11° 34′ 47.783432″ | elevation above sea level 519.
    IFCBUILDING | postal address: "Projektadresse", "Platzl 9", "80331", "München", "Deutschland"
      IFCBUILDINGSTOREY "EG- OK FFB" | long name "EG- OK FFB" | elevation 0.
        contains 5 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basiswand:STB 200" | object type "Basiswand:STB 200:1028196" | names: "Basiswand:STB 200:2305836", "Basiswand:STB 200:2305872", "Basiswand:STB 200:2305922" (+1 more) | material: layers "Basiswand:STB 200" ("Ortbeton - bewehrt Verputzt" 0.2) | property sets: Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "2000 x 1400" | object type "2000 x 1400" | names: "FE 2 tlg - 1 Nurglasecke-konfigurierbar:2000 x 1400:2306007" | material: materials ("Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70") | property sets: Pset_WindowCommon

Types
  IFCWALLTYPE "Basiswand:STB 200" | STANDARD | 4 occurrences | material: layers "Basiswand:STB 200" ("Ortbeton - bewehrt Verputzt" 0.2)
  IFCWINDOWSTYLE "2000 x 1400" | 1 occurrence | material: materials ("Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70") | property sets: FE 2 tlg - 1 Nurglasecke-konfigurierbar:2000 x 1400:2306007

Property sets
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2000 x 1400" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STB 200" (IFCIDENTIFIER)
    ThermalTransmittance = 5.23 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  FE 2 tlg - 1 Nurglasecke-konfigurierbar:2000 x 1400:2306007 | predefined | on 1 type object