IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "RiverRd.ifc"
Time stamp: "2023-05-08T15:15:00-04:00"
Preprocessor: "IfcOpenShell (HEAD detached at 476ab506d)-476ab506d"
Originating system: "BlenderBIM 0.0.230323"
Authorization: "Nobody"

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: square inch (conversion based)
  LENGTHUNIT: inch (conversion based)
  VOLUMEUNIT: cubic inch (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      contains 1 element
        1 x IFCBEAM | names: "Beam"
      IFCBUILDINGSTOREY "Roof"
        contains 32 elements
          3 x IFCMEMBER | type IFCMEMBERTYPE "2x4 wood member" | names: "Member" | material: layers "2x4 wood member" ("Default" 1.5) | property sets: EPset_Parametric
          3 x IFCMEMBER | type IFCMEMBERTYPE "2x12 wood rafter" | names: "Member" | material: layers "2x12 wood rafter" ("Default" 1.5) | property sets: EPset_Parametric
          20 x IFCMEMBER | type IFCMEMBERTYPE "2x6 wood member" | names: "Member" | material: layers ("Default" 1.5) | property sets: EPset_Parametric
          1 x IFCSLAB | type IFCSLABTYPE "8in concrete slab" | names: "Slab" | material: layers "8in concrete slab" ("Default" 8.) | property sets: EPset_Parametric
          4 x IFCELEMENTASSEMBLY | TRUSS | names: "QueenTruss" | parts: 33 IFCMEMBER
          1 x IFCELEMENTASSEMBLY | names: "Assembly" | parts: 6 IFCMEMBER
      IFCBUILDINGSTOREY "Basement"
        contains 22 elements
          5 x IFCWALL | type IFCWALLTYPE "10 in Concrete Wall" | names: "Wall" | material: layers "10 in concrete wall" ("Default" 10.) | property sets: EPset_Parametric
          1 x IFCWALL | type IFCWALLTYPE "12 in concrete wall" | names: "Wall" | material: layers "12 in concrete wall" ("Default" 12.) | property sets: EPset_Parametric
          1 x IFCPLATE | names: "Plate" | property sets: EPset_Parametric
          1 x IFCBEAM | type IFCBEAMTYPE "1.25in rim joist" | names: "Beam" | material: layers "1.25in rim joist" ("Default" 1.25) | property sets: EPset_Parametric
          4 x IFCBEAM | type IFCBEAMTYPE "IPE240" | names: "Beam" | material: profiles ("Unknown") | property sets: EPset_Parametric
          4 x IFCFOOTING | type IFCFOOTINGTYPE "18in footer" | names: "Footing" | material: layers "18in concrete footer" ("Default" 18.) | property sets: EPset_Parametric
          1 x IFCMEMBER | type IFCMEMBERTYPE "2x12 wood member plate" | names: "Member" | material: layers "2x12 wood member plate" ("Default" 1.5) | property sets: EPset_Parametric
          4 x IFCMEMBER | type IFCMEMBERTYPE "2x10 wood member plate" | names: "Member" | material: layers "2x10 wood member palte" ("Default" 1.5) | property sets: EPset_Parametric
          1 x IFCSLAB | type IFCSLABTYPE "8in concrete slab" | names: "Slab" | material: layers "8in concrete slab" ("Default" 8.) | property sets: EPset_Parametric
      IFCBUILDINGSTOREY "1st Floor"
        contains 66 elements
          4 x IFCWALL | type IFCWALLTYPE "6in studed wall" | names: "Wall" | material: layers "6in" ("Default" 6.) | property sets: EPset_Parametric
          28 x IFCWALL | type IFCWALLTYPE "4.5 in inter stud wall" | names: "Wall" | material: layers "4.5 wall" ("Default" 4.5) | property sets: EPset_Parametric
          1 x IFCSLAB | type IFCSLABTYPE "23/32 floor osb" | names: "Slab" | material: layers "osb floor" ("Default" 0.71875) | property sets: EPset_Parametric
          2 x IFCBEAM | type IFCBEAMTYPE "1.25in rim joist" | names: "Beam" | material: layers "1.25in rim joist" ("Default" 1.25) | property sets: EPset_Parametric
          28 x IFCBEAM | type IFCBEAMTYPE "FloorTruss 3.5 in top/bottom chords" | names: "Beam" | material: layers "FloorTruss 3.5 in top/bottom chords" ("Default" 3.5) | property sets: EPset_Parametric
          3 x IFCMEMBER | type IFCMEMBERTYPE "2x12 wood rafter" | names: "Member" | material: layers "2x12 wood rafter" ("Default" 1.5) | property sets: EPset_Parametric

Types
  IFCMEMBERTYPE "2x4 wood member" | 3 occurrences | material: layers "2x4 wood member" ("Default" 1.5)
  IFCMEMBERTYPE "2x12 wood rafter" | RAFTER | 6 occurrences | material: layers "2x12 wood rafter" ("Default" 1.5)
  IFCMEMBERTYPE "2x6 wood member" | 20 occurrences | material: layers ("Default" 1.5)
  IFCSLABTYPE "8in concrete slab" | BASESLAB | 2 occurrences | material: layers "8in concrete slab" ("Default" 8.)
  IFCWALLTYPE "10 in Concrete Wall" | SOLIDWALL | 5 occurrences | material: layers "10 in concrete wall" ("Default" 10.)
  IFCWALLTYPE "12 in concrete wall" | SOLIDWALL | 1 occurrence | material: layers "12 in concrete wall" ("Default" 12.)
  IFCBEAMTYPE "1.25in rim joist" | JOIST | 3 occurrences | material: layers "1.25in rim joist" ("Default" 1.25)
  IFCBEAMTYPE "IPE240" | 4 occurrences | material: profiles ("Unknown")
  IFCFOOTINGTYPE "18in footer" | STRIP_FOOTING | 4 occurrences | material: layers "18in concrete footer" ("Default" 18.)
  IFCMEMBERTYPE "2x12 wood member plate" | PLATE | 1 occurrence | material: layers "2x12 wood member plate" ("Default" 1.5)
  IFCMEMBERTYPE "2x10 wood member plate" | PLATE | 4 occurrences | material: layers "2x10 wood member palte" ("Default" 1.5)
  IFCWALLTYPE "6in studed wall" | ELEMENTEDWALL | 4 occurrences | material: layers "6in" ("Default" 6.)
  IFCWALLTYPE "4.5 in inter stud wall" | ELEMENTEDWALL | 28 occurrences | material: layers "4.5 wall" ("Default" 4.5)
  IFCSLABTYPE "23/32 floor osb" | FLOOR | 1 occurrence | material: layers "osb floor" ("Default" 0.71875)
  IFCBEAMTYPE "FloorTruss 3.5 in top/bottom chords" | JOIST | 28 occurrences | material: layers "FloorTruss 3.5 in top/bottom chords" ("Default" 3.5)

Property sets
  EPset_Parametric | properties | on 147 objects (74 IFCMEMBER, 38 IFCWALL, 31 IFCBEAM, 4 IFCFOOTING)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 4 objects (3 IFCSLAB, 1 IFCPLATE)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 4 objects (4 IFCBEAM)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)