IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
File name: "BBRI House.ifc"
Time stamp: "2022-11-24T15:12:37+01:00"
Author: "Hélène Dewint"
Organization: "WTCB-CSTC-BBRI"
Preprocessor: "IfcOpenShell v0.7.0-cdde5366"
Originating system: "BlenderBIM 0.0.221116"
Application: "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist"
Application: "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)"
Application: "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist"
Application: "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist"

People and organizations
  3 x Person (no name given) of Organization "Simplebim"
  Person "louis.casteleynRM9MV" of Organization (no name given)
  Owner history of Person (no name given) of Organization "Simplebim" | application "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist" | change ADDED | created 1668605572 (2022-11-16T13:32:52Z)
  Owner history of Person "louis.casteleynRM9MV" of Organization (no name given) | application "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)" | change NOCHANGE | created 1661852956 (2022-08-30T09:49:16Z)
  Owner history of Person (no name given) of Organization "Simplebim" | application "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist" | change ADDED | created 1668605058 (2022-11-16T13:24:18Z)
  Owner history of Person (no name given) of Organization "Simplebim" | application "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist" | change ADDED | created 1663754073 (2022-09-21T09:54:33Z)
  Owner history of Person (no name given) of Organization "Simplebim" | application "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist" | change ADDED | created 1663593884 (2022-09-19T13:24:44Z)

Units
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: SQUARE_METRE
  LENGTHUNIT: METRE
  MASSUNIT: KILO GRAM
  POWERUNIT: WATT
  PRESSUREUNIT: PASCAL
  FORCEUNIT: KILO NEWTON
  ELECTRICVOLTAGEUNIT: VOLT
  ELECTRICCURRENTUNIT: AMPERE
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  TIMEUNIT: SECOND
  VOLUMEUNIT: CUBIC_METRE
  LINEARVELOCITYUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  THERMALTRANSMITTANCEUNIT: derived
  SOUNDPRESSUREUNIT: derived

Spatial structure
IFCPROJECT "BBRI1" | long name "Buildwise House" | object type "Educational Project" | phase "Construction" | description "This is an IFC model for educational purposes"
  IFCSITE "Surface" | latitude 50° 41′ 21.976318″ | longitude 4° 31′ 28.124084″ | elevation above sea level 417.1
    IFCBUILDING | postal address: "Avenue Pierre Holoffe 1", "Limelette", "Wallonia", "Belgium"
      IFCBUILDINGSTOREY "-294 Caves - Kelder" | long name "-294 Caves" | elevation -2.93999999998093
        contains 31 elements
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 39cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 39cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 39cm" ("beton_generiek_blok" 3.9E-1) | property sets: ePset_ModelInfo, Pset_WallCommon, ePset_Simplebim, Qto_WallBaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 19cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 19cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 19cm" ("beton_generiek_blok" 1.9E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 83" | DOOR | SINGLE_SWING_LEFT | names: "Ouvrante simple - enkele draaideur:Standard 83 x 204" | material: "hout_generiek_profiel" | property sets: ePset_ModelInfo, IfcDoorPanelProperties, ePset_Simplebim, Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 83" | DOOR | names: "Ouvrante simple - enkele draaideur:Standard 83 x 204" | material: "hout_generiek_profiel" | property sets: ePset_ModelInfo, IfcDoorPanelProperties, ePset_Simplebim, Pset_DoorCommon
          1 x IFCFOOTING | type IFCFOOTINGTYPE "H 20 cm - L +20cm" | STRIP_FOOTING | names: "H 20 cm - L +20cm" | material: "beton_gewapend_ntb" | property sets: ePset_ModelInfo, Pset_FootingCommon, ePset_Simplebim
          4 x IFCFOOTING | STRIP_FOOTING | names: "H 20 cm - L +20cm" | property sets: ePset_ModelInfo, ePset_Simplebim
          1 x IFCSTAIR | type IFCSTAIRTYPE "Béton + bois" | names: "Stair" | parts: 1 IFCSTAIRFLIGHT | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_StairCommon
          1 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | CONTACTOR | names: "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SwitchingDeviceTypeCommon
          8 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond plafonnier:Hermétique" | names: "BS_63_FA_Luminaire rond plafonnier:Hermétique" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_LightFixtureTypeCommon
          2 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Unipolaire" | names: "BS_63_LD_FA_Interrupteur:Unipolaire" | property sets: ePset_ModelInfo, Pset_SwitchingDeviceTypeCommon, ePset_Simplebim
          3 x IFCOUTLET | POWEROUTLET | names: "BS_62_EF_FA_Prise:Double prise 2P+T apparent.001", "BS_62_EF_FA_Prise:Double prise 2P+T apparent", "BS_62_EF_FA_Prise:Double prise 2P+T apparent.002" | property sets: ePset_ModelInfo, ePset_Simplebim
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Dalle - draagvloer 25cm" | FLOOR | names: "Dalle - draagvloer 20cm" | material: layers "Floor:Dalle - draagvloer 25cm" ("beton_generiek_granulaat" 2.5E-1) | property sets: ePset_ModelInfo, Pset_SlabCommon, ePset_Simplebim
          1 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:19 x 20" | BEAM | names: "14 x 20" | material: profiles "19 x 20" ("19 x 20": "beton_generiek_granulaat", "19 x 20": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_BeamCommon
          1 x IFCSLAB | type IFCSLABTYPE "Pad:Sable de propreté - werkvloer 5cm" | USERDEFINED | names: "Sable de propreté - werkvloer 5cm" | material: layers "Pad:Sable de propreté - werkvloer 5cm" ("Sable - Zand" 5.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SlabCommon
        IFCSITE "Remblai - grondaanvulling:Remblai - Aarde"
      IFCBUILDINGSTOREY "-044 NI Rez-de-chaussée - IN Gelijkvloers" | long name "-044 NI Rez-de-chaussée" | elevation -4.39999999980858E-1
        contains 6 elements
          1 x IFCSLAB | type IFCSLABTYPE "Pad:Sable de propreté - werkvloer 5cm" | USERDEFINED | names: "Sable de propreté - werkvloer 5cm" | material: layers "Pad:Sable de propreté - werkvloer 5cm" ("Sable - Zand" 5.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SlabCommon
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 39cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 39cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 39cm" ("beton_generiek_blok" 3.9E-1) | property sets: ePset_ModelInfo, Pset_WallCommon, ePset_Simplebim, Qto_WallBaseQuantities
          1 x IFCSLAB | FLOOR | names: "7,5 x 16" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SlabCommon
      IFCBUILDINGSTOREY "-020 Site - Maaiveld" | long name "-020 Site" | elevation -2.E-1
        contains 22 elements
          5 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Briques de parement - gevelmetselwerk" | CLADDING | names: "Briques de parement - gevelmetselwerk" | material: layers "Basic Wall:Briques de parement - gevelmetselwerk" ("steenachtig_baksteen_generiek-pierreux_brique_génerique" 9.00000035762787E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Isolant - isolatie EPS 22cm" | INSULATION | names: "Isolant - isolatie EPS 22cm" | material: layers "Basic Wall:Isolant - isolatie EPS 22cm" ("isolatie_pur_schuim" 2.2E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          5 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Enduit - gevelbepleistering 2cm" | CLADDING | names: "Enduit - gevelbepleistering 2cm" | material: layers "Basic Wall:Enduit - gevelbepleistering 2cm" ("gips_stuc_bedekking" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon, ePset_LocationTool
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Lattage - latten 6cm" | CLADDING | names: "Lattage - latten 6cm" | material: layers "Basic Wall:Lattage - latten 6cm" ("hout_ntb_profiel" 6.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, ePset_LocationTool, Pset_CoveringCommon
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Bardage bois - houten gevelbekleding 2cm" | CLADDING | names: "Bardage bois - houten gevelbekleding 2cm" | material: layers "Basic Wall:Bardage bois - houten gevelbekleding 2cm" ("hout_ntb_ntb" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, ePset_LocationTool, Pset_CoveringCommon
          1 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire extérieur sur façade:Générique" | names: "BS_63_FA_Luminaire extérieur sur façade:Générique" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_LightFixtureTypeCommon
          4 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond en applique:Hermétique" | names: "BS_63_FA_Luminaire rond en applique:Hermétique" | property sets: ePset_ModelInfo, Pset_LightFixtureTypeCommon, ePset_Simplebim
      IFCBUILDINGSTOREY "000 Rez-de-Chaussée - Gelijksvloers" | long name "000 Rez-de-Chaussée" | elevation 1.91459258570865E-11
        contains 904 elements
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Parquet - parket 2cm" | FLOORING | names: "Parquet - parket 2cm" | material: layers "Floor:Parquet - parket 2cm" ("hout_generiek_plaat" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon, ePset_LocationTool
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Chape - dekvloer 8cm" | FLOORING | names: "Chape - dekvloer 8cm" | material: layers "Floor:Chape - dekvloer 8cm" ("cement_zandcement_ihw" 8.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon, ePset_LocationTool
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Isolation - isolatie PUR 14cm" | INSULATION | names: "Isolation - isolatie PUR 14cm" | material: layers "Floor:Isolation - isolatie PUR 14cm" ("isolatie_ntb_schuim" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon, ePset_LocationTool
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Chape de compression - druklaag 4cm" | FLOOR | names: "Chape de compression - druklaag 4cm" | material: layers "Floor:Chape de compression - druklaag 4cm" ("cement_zandcement_ihw" 4.E-2) | property sets: ePset_ModelInfo, Pset_SlabCommon, ePset_Simplebim
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Isolation - Isolatie PUR 14cm" | INSULATION | names: "Isolation - Isolatie PUR 14cm" | material: layers "Basic Wall:Isolation - Isolatie PUR 14cm" ("isolatie_pur_schuim" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          12 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 14cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 14cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 14cm" ("beton_generiek_blok" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          24 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" | STANDARD | names: "Bloc de béton cellulaire - cellenbeton blok 15cm" | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" ("beton_cellenbeton_blok" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          6 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 9cm" | STANDARD | names: "Bloc béton - beton metselwerk 9cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 9cm" ("beton_generiek_blok" 9.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 19cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 19cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 19cm" ("beton_generiek_blok" 1.9E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          2 x IFCDOOR | type IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 83" | DOOR | names: "Ouvrante simple - enkele draaideur:Standard 83 x 204" | material: "hout_generiek_profiel" | property sets: ePset_ModelInfo, IfcDoorPanelProperties, ePset_Simplebim, Pset_DoorCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Isolant en laine de bois - isolatie houtwol 23cm" | INSULATION | names: "Isolant en laine de bois - isolatie houtwol 23cm" | material: layers "Basic Roof:Isolant en laine de bois - isolatie houtwol 23cm" ("hout_houtvulling_vulling" 2.3E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Simple panneau" | names: "Simple panneau" | parts: 18 IFCMEMBER, 4 IFCDOOR, 4 IFCPLATE | property sets: ePset_ModelInfo, Pset_CurtainWallCommon, ePset_Simplebim
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Carrelage - tegels 2cm" | FLOORING | names: "Carrelage - tegels 2cm" | material: layers "Floor:Carrelage - tegels 2cm" ("steenachtig_ntb_tegel" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon, ePset_LocationTool
          1 x IFCDOOR | type IFCDOORTYPE "Porte sectionnelle - sectionaaldeur:L300 H220" | DOOR | names: "Porte sectionnelle - sectionaaldeur:L300 H220" | material: constituents "MaterialConstituentSet" ("Bois blanc - Witte hout": "hout_generiek_profiel", "Aluminium": "Aluminium") | property sets: ePset_ModelInfo, IfcDoorPanelProperties, ePset_Simplebim, Pset_DoorCommon
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 19cm" | STANDARD | names: "Bloc de béton cellulaire - cellenbeton blok 19cm" | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 19cm" ("beton_cellenbeton_blok" 1.9E-1) | property sets: ePset_ModelInfo, Pset_WallCommon, ePset_Simplebim, Qto_WallBaseQuantities
          9 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 9cm" | STANDARD | names: "Bloc de béton cellulaire - cellenbeton blok 9cm" | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 9cm" ("beton_cellenbeton_blok" 9.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          3 x IFCDOOR | type IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 73 x 204" | DOOR | names: "Ouvrante simple - enkele draaideur:Standard 73 x 20", "Ouvrante simple - enkele draaideur:Standard 73 x 204" | material: "hout_generiek_profiel" | property sets: ePset_ModelInfo, IfcDoorPanelProperties, Pset_DoorCommon, ePset_Simplebim
          10 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:14 x 20" | BEAM | names: "14 x 20" | material: profiles "14 x 20" ("14 x 20": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, Pset_BeamCommon, ePset_Simplebim
          2 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:19 x 20" | BEAM | names: "14 x 20" | material: profiles "19 x 20" ("19 x 20": "beton_generiek_granulaat", "19 x 20": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_BeamCommon
          3 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:9 x 20" | BEAM | names: "14 x 20" | material: profiles "9 x 20" ("9 x 20": "beton_generiek_granulaat", "9 x 20": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, Pset_BeamCommon, ePset_Simplebim
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Dalle - draagvloer 20cm" | FLOOR | names: "Dalle - draagvloer 20cm" | material: layers "Floor:Dalle - draagvloer 20cm" ("beton_generiek_granulaat" 2.E-1) | property sets: ePset_ModelInfo, ePset_LocationTool, Pset_SlabCommon, ePset_Simplebim
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Isolant en laine de bois - isolatie houtwol 23cm" | INSULATION | names: "Isolant en laine de bois - isolatie houtwol 23cm" | material: layers "Basic Wall:Isolant en laine de bois - isolatie houtwol 23cm" ("hout_houtvulling_vulling" 2.3E-1) | property sets: ePset_ModelInfo, ePset_LocationTool, ePset_Simplebim, Pset_CoveringCommon
          29 x IFCMEMBER | type IFCMEMBERTYPE "Colonne rectangulaire:8 x 23" | STUD | names: "8 x 23" | material: profiles "8 x 23" ("8 x 23": "hout_ntb_profiel", "8 x 23": "hout_ntb_profiel") | property sets: ePset_ModelInfo, Pset_MemberCommon, ePset_Simplebim, ePset_LocationTool
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Isolant en laine de bois - isolatie houtwol 3cm" | INSULATION | names: "Isolant en laine de bois - isolatie houtwol 3cm" | material: layers "Basic Wall:Isolant en laine de bois - isolatie houtwol 3cm" ("hout_houtvulling_vulling" 3.E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim, ePset_LocationTool
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:OSB 2cm" | CLADDING | names: "OSB 2cm" | material: layers "Basic Wall:OSB 2cm" ("hout_osb_plaat" 2.E-2) | property sets: ePset_ModelInfo, ePset_LocationTool, Pset_CoveringCommon, ePset_Simplebim
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Lattage - latten 6cm" | CLADDING | names: "Lattage - latten 6cm" | material: layers "Basic Wall:Lattage - latten 6cm" ("hout_ntb_profiel" 6.E-2) | property sets: ePset_ModelInfo, ePset_LocationTool, ePset_Simplebim, Pset_CoveringCommon
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Enduit - gevelbepleistering 2cm" | CLADDING | names: "Enduit - gevelbepleistering 2cm" | material: layers "Basic Wall:Enduit - gevelbepleistering 2cm" ("gips_stuc_bedekking" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          11 x IFCMEMBER | type IFCMEMBERTYPE "Rectangle - rechthoek:8 x 23 horiz" | PLATE | names: "8 x 23 horiz" | material: profiles "8 x 23 horiz" ("8 x 23 horiz": "hout_ntb_profiel", "8 x 23 horiz": "hout_ntb_profiel") | property sets: ePset_ModelInfo, ePset_LocationTool, ePset_Simplebim, Pset_MemberCommon
          1 x IFCSLAB | type IFCSLABTYPE "Pad:Sable de propreté - werkvloer 5cm" | USERDEFINED | names: "Sable de propreté - werkvloer 5cm" | material: layers "Pad:Sable de propreté - werkvloer 5cm" ("Sable - Zand" 5.E-2) | property sets: ePset_ModelInfo, Pset_SlabCommon, ePset_LocationTool, ePset_Simplebim
          5 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Plafond" | CEILING | names: "Plafond" | material: layers "Compound Ceiling:Plafond" ("gips_gipskarton_plaat" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon, ePset_LocationTool
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:OSB 2cm" | ROOFING | names: "OSB 2cm" | material: layers "Basic Roof:OSB 2cm" ("hout_osb_plaat" 2.E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim, ePset_LocationTool
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Etanchéité - vochtwerende folie 1cm" | ROOFING | names: "Etanchéité - vochtwerende folie 1cm" | material: layers "Basic Roof:Etanchéité - vochtwerende folie 1cm" ("kunststof_ntb_folie_vochtwerend" 1.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon, ePset_LocationTool
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Isolant en laine de bois - isolatie houtwol 3cm" | INSULATION | names: "Isolant en laine de bois - isolatie houtwol 3cm" | material: layers "Basic Roof:Isolant en laine de bois - isolatie houtwol 3cm" ("isolatie_nbt_plaat" 3.E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Lattage - latten 6cm" | ROOFING | names: "Lattage - latten 6cm" | material: layers "Basic Roof:Lattage - latten 6cm" ("hout_ntb_profiel" 6.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Ardoises - leien" | ROOFING | names: "Ardoises - leien" | material: layers "Basic Roof:Ardoises - leien" ("natuursteen_lei_pan" 2.E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          2 x IFCMEMBER | type IFCMEMBERTYPE "Rectangle - rechthoek:7 x 14 horiz" | PLATE | names: "7 x 14 horiz" | material: profiles "7 x 14 horiz" ("7 x 14 horiz": "hout_ntb_profiel", "7 x 14 horiz": "hout_ntb_profiel") | property sets: ePset_ModelInfo, Pset_MemberCommon, ePset_Simplebim
          1 x IFCMEMBER | type IFCMEMBERTYPE "Rectangle - rechthoek:10 x 30" | PURLIN | names: "10 x 30" | material: "hout_ntb_profiel" | property sets: ePset_ModelInfo, Pset_MemberCommon, ePset_Simplebim
          1 x IFCWINDOW | WINDOW | names: "Fenêtre double fixe + ouvrante (porte) - vast + draairaam (deur):L160 H230" | material: constituents "MaterialConstituentSet" ("Aluminium": "Aluminium", "Verre - Glas": "Verre - Glas", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre triple - fixe + ouvrante + fixe:L300 H230" | WINDOW | names: "Fenêtre triple - fixe + ouvrante + fixe:L300 H230" | material: constituents "MaterialConstituentSet" ("Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, Pset_WindowCommon, ePset_Simplebim
          3 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre simple fixe - enkele vastraam:L100 H230" | WINDOW | names: "Fenêtre simple fixe - enkele vastraam:L360 H230:1611951", "Fenêtre simple fixe - enkele vastraam:L360 H230", "Fenêtre simple fixe - enkele vastraam:L100 H230" | material: constituents "MaterialConstituentSet" ("Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, Pset_WindowCommon, ePset_Simplebim, ePset_LocationTool
          1 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre coulissante triple - drie schuifraam:L360 H238" | WINDOW | names: "Fenêtre coulissante triple - drie schuifraam:L360 H238" | material: constituents "MaterialConstituentSet" ("Aluminium": "Aluminium", "Verre - Glas": "Verre - Glas") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Hourdis - welfsel 16cm" | FLOOR | names: "Hourdis - welfsel 16cm" | material: layers "Floor:Hourdis - welfsel 16cm" ("Hourdis - Welfsel" 1.6E-1) | property sets: ePset_ModelInfo, Pset_SlabCommon, ePset_Simplebim
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Paroi légère - lichte muur 10cm" | CLADDING | names: "Paroi légère - lichte muur 10cm" | material: layers "Basic Wall:Paroi légère - lichte muur 10cm" ("gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2, "isolatie_glaswol_vulling" 5.E-2, "gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre simple ouvrante - enkele draairaam:L80 H125" | WINDOW | names: "Fenêtre simple ouvrante - enkele draairaam:L80 H125" | material: constituents "MaterialConstituentSet" ("Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, Pset_WindowCommon, ePset_Simplebim, ePset_LocationTool
          1 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre simple ouvrante - enkele draairaam:L80 H70" | WINDOW | names: "Fenêtre simple ouvrante - enkele draairaam:L80 H70" | material: constituents "MaterialConstituentSet" ("Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb", "Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium") | property sets: ePset_ModelInfo, Pset_WindowCommon, ePset_LocationTool, ePset_Simplebim
          1 x IFCELECTRICAPPLIANCE | ELECTRICCOOKER | names: "Taque électrique (4):60 x 60cm" | property sets: ePset_ModelInfo, ePset_LocationTool, Pset_ElectricApplianceTypeCommon, ePset_Simplebim
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "Evier grand 1 bac:110 x 53.5cm" | names: "Evier grand 1 bac:110 x 53.5cm" | property sets: ePset_ModelInfo, ePset_LocationTool, ePset_Simplebim
          1 x IFCDAMPER | FUMEHOODEXHAUST | names: "dampkap eiland" | material: "hout_generiek_profiel" | property sets: ePset_ModelInfo, Pset_DamperTypeCommon, ePset_LocationTool, ePset_Simplebim, Pset_BuildingElementProxyCommon
          4 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Blanc" | CLADDING | names: "Blanc" | material: layers "Basic Wall:Blanc" ("hout_generiek_profiel" 1.E-3) | property sets: ePset_ModelInfo, ePset_Simplebim, ePset_LocationTool, Pset_CoveringCommon
          1 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "HVAC_Heaters_Finimetal_Vonaris-VSV-M_FR:VSV-M 10" | names: "HVAC_Heaters_Finimetal_Vonaris-VSV-M_FR:VSV-M 10" | material: "Metal - Finimetal - R9016 Traffic White" | property sets: ePset_ModelInfo, ePset_Simplebim, ePset_LocationTool, Pset_SpaceHeaterTypeCommon
          1 x IFCSTAIR | type IFCSTAIRTYPE "Béton + bois" | names: "Stair" | parts: 1 IFCSTAIRFLIGHT | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_StairCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Paroi légère - lichte muur 7,5cm" | CLADDING | names: "Paroi légère - lichte muur 10cm" | material: layers "Basic Wall:Paroi légère - lichte muur 7,5cm" ("isolatie_glaswol_vulling" 5.E-2, "gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          1 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:BS_53_PI_Acier inox - Cheminée double paroi" | names: "BS_53_PI_Acier inox - Cheminée double paroi" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_PipeSegmentTypeCommon
          1 x IFCUNITARYEQUIPMENT | AIRHANDLER | names: "BS_57_ME_UN_CTA_Groupe de ventilation - double flux - domestique:Générique" | material: constituents "MaterialConstituentSet" ("2-V-Air repris": "2-V-Air repris", "2-V-Air refoulé": "2-V-Air refoulé", "2-V-Air pulsé": "2-V-Air pulsé", "2-Z-Equipement Hvac (multi-techniques)": "2-Z-Equipement Hvac (multi-techniques)") | property sets: ePset_ModelInfo, ePset_Simplebim
          70 x IFCDUCTSEGMENT | type IFCDUCTSEGMENTTYPE "Round Duct:BS_57_DU_Galva (Tés)" | names: "BS_57_DU_Galva (Tés)" | property sets: ePset_ModelInfo, Pset_DuctSegmentTypeCommon, ePset_Simplebim
          37 x IFCDUCTFITTING | type IFCDUCTFITTINGTYPE "BS_57_DUF_Coude circulaire:Galva" | USERDEFINED | names: "BS_57_DUF_Coude circulaire:Galva" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_DuctFittingTypeCommon
          12 x IFCDUCTSEGMENT | type IFCDUCTSEGMENTTYPE "Flex Duct Round:BS_57_FDU_Souple - Circulaire" | FLEXIBLESEGMENT | names: "BS_57_FDU_Souple - Circulaire" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_DuctSegmentTypeCommon
          13 x IFCDUCTFITTING | type IFCDUCTFITTINGTYPE "BS_57_DUF_Té circulaire:Galva" | USERDEFINED | names: "BS_57_DUF_Té circulaire:Galva" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_DuctFittingTypeCommon
          1 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "BS_57_AIR_UN_Grille circulaire LVS:D100" | names: "BS_57_AIR_UN_Grille circulaire LVS:D100" | property sets: ePset_ModelInfo, Pset_AirTerminalTypeCommon, ePset_Simplebim
          8 x IFCDUCTFITTING | type IFCDUCTFITTINGTYPE "BS_57_DUF_Transformation circulaire - Angle:Galva 45°" | USERDEFINED | names: "BS_57_DUF_Transformation circulaire - Angle:Galva 45°" | property sets: ePset_ModelInfo, Pset_DuctFittingTypeCommon, ePset_Simplebim
          28 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond plafonnier:Appareil standard" | names: "BS_63_FA_Luminaire rond plafonnier:Appareil standard" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_LightFixtureTypeCommon
          4 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Unipolaire" | names: "BS_63_LD_FA_Interrupteur:Unipolaire" | property sets: ePset_ModelInfo, Pset_SwitchingDeviceTypeCommon, ePset_Simplebim
          1 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond en applique:Hermétique" | names: "BS_63_FA_Luminaire rond en applique:Hermétique" | property sets: ePset_ModelInfo, Pset_LightFixtureTypeCommon, ePset_Simplebim
          24 x IFCOUTLET | POWEROUTLET | names: "BS_62_EF_FA_Prise:Double prise 2P+T verticale", "BS_62_EF_FA_Prise:Double prise 2P+T verticale.001", "BS_62_EF_FA_Prise:Double prise 2P+T verticale.002" (+21 more) | property sets: ePset_ModelInfo, ePset_Simplebim
          3 x IFCOUTLET | type IFCOUTLETTYPE "BS_64_DD_FA_Prise data:RJ45" | DATAOUTLET | names: "BS_64_DD_FA_Prise data:RJ45" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_OutletTypeCommon
          16 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | names: "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SwitchingDeviceTypeCommon
          2 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Inverseur unipolaire" | names: "BS_63_LD_FA_Interrupteur:Inverseur unipo", "BS_63_LD_FA_Interrupteur:Inverseur unipolaire" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SwitchingDeviceTypeCommon
          3 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Bipolaire" | names: "BS_63_LD_FA_Interrupteur:Bipolaire" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SwitchingDeviceTypeCommon
          1 x IFCBOILER | type IFCBOILERTYPE "BS_56_Chaudière mural:45 kW" | WATER | names: "BS_56_Chaudière mural:45 kW" | material: constituents "MaterialConstituentSet" ("Equipment": "Color RGB 127-118-121") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_BoilerTypeCommon
          1 x IFCSENSOR | MOVEMENTSENSOR | names: "BS_63_LD_FA_Détecteur de mouvement" | material: "Par défaut" | property sets: ePset_ModelInfo, ePset_Simplebim
          2 x IFCDUCTFITTING | type IFCDUCTFITTINGTYPE "BS_57_DUF_Raccord à 45 degrés circulaire:Standard" | USERDEFINED | names: "BS_57_DUF_Raccord à 45 degrés circulaire:Standard" | property sets: ePset_ModelInfo, Pset_DuctFittingTypeCommon, ePset_Simplebim
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "Evier grand 1 bac1:110 x 53.5cm 2" | names: "Evier grand 1 bac:110 x 53.5cm.001" | property sets: ePset_ModelInfo, ePset_Simplebim
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "Lavabo arrondi (petit)1:45 cm 2" | names: "Lavabo arrondi (petit)1:45 cm 2" | property sets: ePset_ModelInfo, ePset_Simplebim
          59 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:BS_52_PI_PVC" | names: "BS_52_PI_PVC" | property sets: ePset_ModelInfo, Pset_PipeSegmentTypeCommon, ePset_Simplebim
          12 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "BS_52_PIF_Té - Evacuation:PVC" | names: "BS_52_PIF_Té - Evacuation:PVC" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_PipeFittingTypeCommon
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "BS_74_PF_LE_Lave-main_2:360x250" | WASHHANDBASIN | names: "BS_74_PF_LE_Lave-main_2:360x250" | property sets: ePset_ModelInfo, Pset_SanitaryTerminalTypeCommon, ePset_Simplebim
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "BS_53_PF_Collecteur EF 4 départs:BS_53_PF_Collecteur EF 4 départs" | names: "BS_53_PF_Collecteur EF 4 départs" | property sets: ePset_ModelInfo, ePset_Simplebim
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "BS_53_PF_Collecteur ECS 2 départs:BS_53_PF_Collecteur ECS 2 départs" | names: "BS_53_PF_Collecteur ECS 2 départs" | property sets: ePset_ModelInfo, ePset_Simplebim
          195 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:BS_53_PI_PEX-Alu-PEX" | names: "BS_53_PI_PEX-Alu-PEX" | property sets: ePset_ModelInfo, Pset_PipeSegmentTypeCommon, ePset_Simplebim
          90 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "BS_53_PIF_Courbure - Adduction:PEX-Alu-PEX" | names: "BS_53_PIF_Courbure - Adduction:PEX-Alu-PEX" | property sets: ePset_ModelInfo, Pset_PipeFittingTypeCommon, ePset_Simplebim
          33 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "BS_52_PIF_Coude - Evacuation:PVC" | names: "BS_52_PIF_Coude - Evacuation:PVC" | property sets: ePset_ModelInfo, Pset_PipeFittingTypeCommon, ePset_Simplebim
          1 x IFCVALVE | type IFCVALVETYPE "Distribution manifold for heating systems_Caleffi_662 x5:5 outlets" | names: "Distribution manifold for heating systems_Caleffi_662 x5:5 outlets" | material: constituents "MaterialConstituentSet" ("Technopolymer - Caleffi - white": "Technopolymer - Caleffi - white", "Metal - Caleffi - Brass": "Metal - Caleffi - Brass", "Metal - Caleffi - Stainless Steel": "Metal - Caleffi - Stainless Steel") | property sets: ePset_ModelInfo, Pset_ValveTypeCommon, ePset_Simplebim
          70 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "BS_53_PIF_Coude - Adduction:PEX-Alu-PEX" | names: "BS_53_PIF_Coude - Adduction:PEX-Alu-PEX" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_PipeFittingTypeCommon
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "BS_52_PIF_Réduction - Evacuation:PVC" | names: "BS_52_PIF_Réduction - Evacuation:PVC" | property sets: ePset_ModelInfo, Pset_PipeFittingTypeCommon, ePset_Simplebim
          3 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "BS_53_PIF_Té - Adduction:PEX-Alu-PEX" | names: "BS_53_PIF_Té - Adduction:PEX-Alu-PEX" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_PipeFittingTypeCommon
          3 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "BS_53_PIF_Bouchon - Adduction:PEX-Alu-PEX" | names: "BS_53_PIF_Bouchon - Adduction:PEX-Alu-PEX" | property sets: ePset_ModelInfo, Pset_PipeFittingTypeCommon, ePset_Simplebim
          4 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "BS_53_PIF_Réduction - Adduction:PEX-Alu-PEX" | names: "BS_53_PIF_Réduction - Adduction:PEX-Alu-PEX" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_PipeFittingTypeCommon
          1 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Descente d'eau ronde - ronde afvoerpijp 8cm 2:Descente d'eau ronde - ronde afvoerpijp 8cm" | RIGIDSEGMENT | names: "Descente d'eau ronde - ronde afvoerpijp 8cm" | material: "metaal_zink_profiel" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_PipeSegmentTypeCommon
          4 x IFCPIPESEGMENT | RIGIDSEGMENT | names: "Descente d'eau ronde - ronde afvoerpijp 8cm.006", "Descente d'eau ronde - ronde afvoerpijp 8cm.005", "Descente d'eau ronde - ronde afvoerpijp 8cm.003" (+1 more) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_PipeSegmentTypeCommon
          1 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Descente d'eau ronde - ronde afvoerpijp 8cm 1:Descente d'eau ronde - ronde afvoerpijp 8cm" | RIGIDSEGMENT | names: "Descente d'eau ronde - ronde afvoerpijp 8cm" | material: "metaal_zink_profiel" | property sets: ePset_ModelInfo, ePset_Simplebim, ePset_LocationTool, Pset_PipeSegmentTypeCommon
          1 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Descente d'eau ronde - ronde afvoerpijp 8cm 3:Descente d'eau ronde - ronde afvoerpijp 8cm" | RIGIDSEGMENT | names: "Descente d'eau ronde - ronde afvoerpijp 8cm.001" | material: "metaal_zink_profiel" | property sets: ePset_ModelInfo, Pset_PipeSegmentTypeCommon, ePset_Simplebim
          1 x IFCMEMBER | names: "2 x 25" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_MemberCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Isolation laine de bois - Isolatie houtwol 23cm:Isolation laine de bois - Isolatie houtwol 23cm" | INSULATION | names: "Isolation laine de bois - Isolatie houtwol 23cm" | material: "hout_houtvulling_vulling" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon, ePset_LocationTool
          1 x IFCFLOWSEGMENT | names: "Gouttière demi-lune" | property sets: ePset_ModelInfo, ePset_Simplebim
          2 x IFCDOOR | type IFCDOORTYPE "Fenêtre double fixe + ouvrante (porte) - vast + draairaam (deur): L160 H230" | DOOR | names: "Fenêtre double fixe + ouvrante (porte) - vast + dr", "Fenêtre double fixe + ouvrante (porte) - vast + draairaam (deur): L160 H230" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORTYPE "Porte pleine (ouverture vers l'intérieur) - volle deur (binnen openend): L90 H230" | DOOR | names: "Porte pleine (ouverture vers l'intérieur) - volle de" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORTYPE "Porte (ouverture vers l'intérieur) - deur (binnen openend): L110 H230" | DOOR | names: "Porte (ouverture vers l'intérieur) - deur (binnen op" | property sets: ePset_ModelInfo, Pset_DoorCommon, ePset_Simplebim
      IFCBUILDINGSTOREY "250 FP Rez-de-chaussée - VP Gelijkvloers" | long name "250 FP Rez-de-chaussée" | elevation 2.50000000001905
        contains 5 elements
          2 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire - reprise:GPD-100" | names: "BS_57_AIR_FA_Bouche circulaire - reprise", "BS_57_AIR_FA_Bouche circulaire - reprise:GPD-100" | material: "Steel Sheet - Koolair" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_AirTerminalTypeCommon
          3 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire - pulsion:GPD-I-100" | names: "BS_57_AIR_FA_Bouche circulaire - pulsion:GPD", "BS_57_AIR_FA_Bouche circulaire - pulsion:GPD-I-100" | material: "Steel Sheet - Koolair" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_AirTerminalTypeCommon
      IFCBUILDINGSTOREY "280 NI Premier étage - IN Eerste verdieping" | long name "280 NI Premier étage" | elevation 2.79999999999978
        contains 40 elements
          1 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:19 x 30" | BEAM | names: "14 x 20" | material: profiles "19 x 30" ("19 x 30": "beton_generiek_granulaat", "19 x 30": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_BeamCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:14 x 20" | BEAM | names: "14 x 20" | material: profiles "14 x 20" ("14 x 20": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, Pset_BeamCommon, ePset_Simplebim
          10 x IFCMEMBER | type IFCMEMBERTYPE "Rectangle - rechthoek:8 x 23" | RAFTER | names: "8 x 23" | material: profiles "8 x 23" ("8 x 23": "hout_ntb_profiel") | property sets: ePset_ModelInfo, ePset_LocationTool, ePset_Simplebim, Pset_MemberCommon
          27 x IFCMEMBER | type IFCMEMBERTYPE "Colonne rectangulaire:8 x 23" | STUD | names: "8 x 23" | material: profiles "8 x 23" ("8 x 23": "hout_ntb_profiel", "8 x 23": "hout_ntb_profiel") | property sets: ePset_ModelInfo, Pset_MemberCommon, ePset_Simplebim, ePset_LocationTool
          1 x IFCSLAB | FLOOR | names: "7 x 20" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SlabCommon
      IFCBUILDINGSTOREY "310 Premier étage - Eerste verdieping" | long name "310 Premier étage" | elevation 3.1
        contains 154 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Parquet - parket 2cm" | FLOORING | names: "Parquet - parket 2cm" | material: layers "Floor:Parquet - parket 2cm" ("hout_generiek_plaat" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Chape - dekvloer 8cm" | FLOORING | names: "Chape - dekvloer 8cm" | material: layers "Floor:Chape - dekvloer 8cm" ("cement_zandcement_ihw" 8.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Chape de compression - druklaag 4cm" | FLOOR | names: "Chape de compression - druklaag 4cm" | material: layers "Floor:Chape de compression - druklaag 4cm" ("cement_zandcement_ihw" 4.E-2) | property sets: ePset_ModelInfo, Pset_SlabCommon, ePset_Simplebim
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Hourdis - welfsel 16cm" | FLOOR | names: "Hourdis - welfsel 16cm" | material: layers "Floor:Hourdis - welfsel 16cm" ("Hourdis - Welfsel" 1.6E-1) | property sets: ePset_ModelInfo, Pset_SlabCommon, ePset_Simplebim
          9 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 14cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 14cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 14cm" ("beton_generiek_blok" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          8 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Briques de parement - gevelmetselwerk" | CLADDING | names: "Briques de parement - gevelmetselwerk" | material: layers "Basic Wall:Briques de parement - gevelmetselwerk" ("steenachtig_baksteen_generiek-pierreux_brique_génerique" 9.00000035762787E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          4 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Isolation - Isolatie PUR 14cm" | INSULATION | names: "Isolation - Isolatie PUR 14cm" | material: layers "Basic Wall:Isolation - Isolatie PUR 14cm" ("isolatie_pur_schuim" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 19cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 19cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 19cm" ("beton_generiek_blok" 1.9E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          4 x IFCDOOR | type IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 83" | DOOR | names: "Ouvrante simple - enkele draaideur:Standard 83 x 204" | material: "hout_generiek_profiel" | property sets: ePset_ModelInfo, IfcDoorPanelProperties, ePset_Simplebim, Pset_DoorCommon
          8 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 9cm" | STANDARD | names: "Bloc béton - beton metselwerk 9cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 9cm" ("beton_generiek_blok" 9.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" | STANDARD | names: "Bloc de béton cellulaire - cellenbeton blok 15cm" | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" ("beton_cellenbeton_blok" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Isolant - isolatie PIR 14cm" | INSULATION | names: "Isolant - isolatie PIR 14cm" | material: layers "Basic Roof:Isolant - isolatie PIR 14cm" ("isolatie_nbt_plaat" 1.4E-1) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          1 x IFCDISCRETEACCESSORY | type IFCDISCRETEACCESSORYTYPE "Couvre-mur - muurafdekker 2:Couvre-mur - muurafdekker 2" | USERDEFINED | names: "Couvre-mur - muurafdekker 2" | property sets: ePset_ModelInfo, ePset_Simplebim
          3 x IFCMEMBER | type IFCMEMBERTYPE "Rectangle - rechthoek:8 x 23 horiz" | PLATE | names: "8 x 23 horiz" | material: profiles "8 x 23 horiz" ("8 x 23 horiz": "hout_ntb_profiel", "8 x 23 horiz": "hout_ntb_profiel") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_MemberCommon, ePset_LocationTool
          1 x IFCDISCRETEACCESSORY | type IFCDISCRETEACCESSORYTYPE "Couvre-mur - muurafdekker 1:Couvre-mur - muurafdekker 1" | USERDEFINED | names: "Couvre-mur - muurafdekker 1" | material: "natuursteen_hardsteen_ntb" | property sets: ePset_ModelInfo, ePset_Simplebim, ePset_LocationTool
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Carrelage - tegels 2cm" | FLOORING | names: "Carrelage - tegels 2cm" | material: layers "Basic Roof:Carrelage - tegels 2cm" ("steenachtig_ntb_tegel" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 26cm" | STANDARD | names: "Bloc de béton cellulaire - cellenbeton blok 26cm" | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 26cm" ("beton_cellenbeton_blok" 2.6E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          5 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Carrelage - tegels 2cm" | CLADDING | names: "Carrelage - tegels 2cm" | material: layers "Basic Wall:Carrelage - tegels 2cm" ("steenachtig_ntb_tegel" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Paroi légère - lichte muur 10cm" | CLADDING | names: "Paroi légère - lichte muur 10cm" | material: layers "Basic Wall:Paroi légère - lichte muur 10cm" ("gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2, "isolatie_glaswol_vulling" 5.E-2, "gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Carrelage - tegels 2cm" | FLOORING | names: "Carrelage - tegels 2cm" | material: layers "Floor:Carrelage - tegels 2cm" ("steenachtig_ntb_tegel" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          4 x IFCMEMBER | type IFCMEMBERTYPE "Rectangle - rechthoek:8 x 23" | RAFTER | names: "8 x 23" | material: profiles "8 x 23" ("8 x 23": "hout_ntb_profiel"); "hout_ntb_profiel" | property sets: ePset_ModelInfo, Pset_MemberCommon, ePset_Simplebim, ePset_LocationTool
          1 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre triple - fixe + ouvrante + fixe:L300 H130" | WINDOW | names: "Fenêtre triple - fixe + ouvrante + fixe:L300 H130" | material: constituents "MaterialConstituentSet" ("Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, Pset_WindowCommon, ePset_Simplebim
          4 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre double fixe + ouvrante - vast + draairaam:L160 H130" | WINDOW | names: "Fenêtre double fixe + ouvrante - vast + draairaam:L160 H130" | material: constituents "MaterialConstituentSet" ("Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre simple ouvrante - enkele draairaam:L100 H130" | WINDOW | names: "Fenêtre simple ouvrante - enkele draairaam:L100 H130" | material: constituents "MaterialConstituentSet" ("Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre double ouvrante - dubbele draairaam:L232 H197" | WINDOW | names: "Fenêtre double ouvrante - dubbele draairaam:L232 H197" | material: constituents "MaterialConstituentSet" ("Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WindowCommon
          8 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:14 x 20" | BEAM | names: "14 x 20" | material: profiles "14 x 20" ("14 x 20": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, Pset_BeamCommon, ePset_Simplebim
          2 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:19 x 20" | BEAM | names: "14 x 20" | material: profiles "19 x 20" ("19 x 20": "beton_generiek_granulaat", "19 x 20": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_BeamCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Chape de pente - hellingslaag 5cm" | ROOF | names: "Chape de pente - hellingslaag 5cm" | material: layers "Floor:Chape de pente - hellingslaag 5cm" ("cement_zandcement_ihw" 5.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SlabCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "CFP_ISD 2093:80 x 80" | WINDOW | names: "CFP_ISD 2093:80 x 80" | material: constituents "MaterialConstituentSet" ("Aluminium profiles / 4 mm toughened glass pane": "Aluminium profiles / 4 mm toughened glass pane", "73FQT + ISD 2093": "73FQT + ISD 2093", "PVC Color NCS S 0502-Y": "PVC Color NCS S 0502-Y") | property sets: ePset_ModelInfo, ePset_Simplebim, ePset_LocationTool, Pset_WindowCommon
          1 x IFCSTAIR | type IFCSTAIRTYPE "Béton + bois" | names: "Stair" | parts: 1 IFCSTAIRFLIGHT | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_StairCommon
          1 x IFCDOOR | type IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 73 x 204" | DOOR | SWING_FIXED_LEFT | names: "Ouvrante simple - enkele draaideur:Standard 73 x 204" | material: "hout_generiek_profiel" | property sets: ePset_ModelInfo, IfcDoorPanelProperties, Pset_DoorCommon, ePset_Simplebim
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Paroi légère - lichte muur 7,5cm" | CLADDING | names: "Paroi légère - lichte muur 10cm" | material: layers "Basic Wall:Paroi légère - lichte muur 7,5cm" ("isolatie_glaswol_vulling" 5.E-2, "gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          6 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Plafond" | CEILING | names: "Plafond" | material: layers "Compound Ceiling:Plafond" ("gips_gipskarton_plaat" 2.E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          10 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | names: "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SwitchingDeviceTypeCommon
          24 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond plafonnier:Appareil standard" | names: "BS_63_FA_Luminaire rond plafonnier:Appareil standard" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_LightFixtureTypeCommon
          14 x IFCOUTLET | POWEROUTLET | names: "BS_62_EF_FA_Prise:Prise 2P+T.008", "BS_62_EF_FA_Prise:Prise 2P+T.009", "BS_62_EF_FA_Prise:Prise 2P+T.010" (+11 more) | property sets: ePset_ModelInfo, ePset_Simplebim
          2 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Unipolaire" | names: "BS_63_LD_FA_Interrupteur:Unipolaire" | property sets: ePset_ModelInfo, Pset_SwitchingDeviceTypeCommon, ePset_Simplebim
          3 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Bipolaire" | names: "BS_63_LD_FA_Interrupteur:Bipolaire" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SwitchingDeviceTypeCommon
          3 x IFCOUTLET | type IFCOUTLETTYPE "BS_64_DD_FA_Prise data:RJ45" | DATAOUTLET | names: "BS_64_DD_FA_Prise data:RJ45" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_OutletTypeCommon
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "BS_74_PF_LE_Lave-main_2:360x250" | WASHHANDBASIN | names: "BS_74_PF_LE_Lave-main_2:360x250" | property sets: ePset_ModelInfo, Pset_SanitaryTerminalTypeCommon, ePset_Simplebim
          1 x IFCVALVE | type IFCVALVETYPE "Collecteur_2x6_CALEFFI:6 outlets" | names: "Collecteur_2x6_CALEFFI:6 outlets" | material: constituents "MaterialConstituentSet" ("Technopolymer - Caleffi - white": "Technopolymer - Caleffi - white", "Metal - Caleffi - Brass": "Metal - Caleffi - Brass", "Technopolymer - Caleffi - Black": "Technopolymer - Caleffi - Black", "Metal - Caleffi - Stainless Steel": "Metal - Caleffi - Stainless Steel") | property sets: ePset_ModelInfo, Pset_ValveTypeCommon, ePset_Simplebim
          6 x IFCSPACEHEATER | RADIATOR | names: "BS_56_ME_UN_Radiateur:700x900", "BS_56_ME_UN_Radiateur:700x900.001", "BS_56_ME_UN_Radiateur:700x900.002" (+3 more) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SpaceHeaterTypeCommon
          1 x IFCRAILING | BALUSTRADE | names: "Garde-corps à barreaux - leuning met spijlen" | material: constituents "MaterialConstituentSet" ("Aluminium": "Aluminium") | property sets: ePset_ModelInfo, ePset_Simplebim
      IFCBUILDINGSTOREY "540 FP Première étage - VP Eerste verdieping" | long name "540 FP Première étage" | elevation 5.39999999999992
        contains 7 elements
          3 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire - pulsion:GPD-I-100" | names: "BS_57_AIR_FA_Bouche circulaire - pulsion:GPD-I-100" | material: "Steel Sheet - Koolair" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_AirTerminalTypeCommon
          4 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire - reprise:GPD-100" | names: "BS_57_AIR_FA_Bouche circulaire - reprise", "BS_57_AIR_FA_Bouche circulaire - reprise:GPD-100" | material: "Steel Sheet - Koolair" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_AirTerminalTypeCommon
      IFCBUILDINGSTOREY "570 NI Deuxième étage - IN Tweede verdieping" | long name "570 NI Deuxième étage" | elevation 5.69999999999992
        contains 5 elements
          1 x IFCSLAB | FLOOR | names: "Slab Edge:7 x 20:1649032" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SlabCommon
          2 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "BS_57_AIR_UN_Grille circulaire LVS:D100" | names: "BS_57_AIR_UN_Grille circulaire LVS:D100" | property sets: ePset_ModelInfo, Pset_AirTerminalTypeCommon, ePset_Simplebim
          1 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire LVS pulsion:D100" | names: "BS_57_AIR_FA_Bouche circulaire LVS pulsion:D" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_AirTerminalTypeCommon
          1 x IFCAIRTERMINAL | type IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire LVS pulsion:D100" | GRILLE | names: "BS_57_AIR_FA_Bouche circulaire LVS pulsion:D100" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_AirTerminalTypeCommon
      IFCBUILDINGSTOREY "600 Deuxième étage - Tweede verdieping" | long name "600 Deuxième étage" | elevation 6.
        contains 37 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Hourdis - welfsel 16cm" | FLOOR | names: "Hourdis - welfsel 16cm" | material: layers "Floor:Hourdis - welfsel 16cm" ("Hourdis - Welfsel" 1.6E-1) | property sets: ePset_ModelInfo, Pset_SlabCommon, ePset_Simplebim
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 19cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 19cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 19cm" ("beton_generiek_blok" 1.9E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 14cm" | SOLIDWALL | names: "Bloc béton - beton metselwerk 14cm" | material: layers "Basic Wall:Bloc béton - beton metselwerk 14cm" ("beton_generiek_blok" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          7 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Briques de parement - gevelmetselwerk" | CLADDING | names: "Briques de parement - gevelmetselwerk" | material: layers "Basic Wall:Briques de parement - gevelmetselwerk" ("steenachtig_baksteen_generiek-pierreux_brique_génerique" 9.00000035762787E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          6 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Isolation - Isolatie PUR 14cm" | INSULATION | names: "Isolation - Isolatie PUR 14cm" | material: layers "Basic Wall:Isolation - Isolatie PUR 14cm" ("isolatie_pur_schuim" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCMEMBER | names: "2 x 25.001" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_MemberCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Chape de compression - druklaag 4cm" | FLOOR | names: "Chape de compression - druklaag 4cm" | material: layers "Floor:Chape de compression - druklaag 4cm" ("cement_zandcement_ihw" 4.E-2) | property sets: ePset_ModelInfo, Pset_SlabCommon, ePset_Simplebim
          1 x IFCDOOR | type IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 83" | DOOR | names: "Ouvrante simple - enkele draaideur:Standard 83 x 204" | material: "hout_generiek_profiel" | property sets: ePset_ModelInfo, IfcDoorPanelProperties, ePset_Simplebim, Pset_DoorCommon
          2 x IFCBEAM | type IFCBEAMTYPE "Rectangle - rechthoek:19 x 20" | BEAM | names: "14 x 20" | material: profiles "19 x 20" ("19 x 20": "beton_generiek_granulaat", "19 x 20": "beton_generiek_granulaat") | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_BeamCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Chape - dekvloer 8cm" | FLOORING | names: "Chape - dekvloer 8cm" | material: layers "Floor:Chape - dekvloer 8cm" ("cement_zandcement_ihw" 8.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:Parquet - parket 2cm" | FLOORING | names: "Parquet - parket 2cm" | material: layers "Floor:Parquet - parket 2cm" ("hout_generiek_plaat" 2.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" | STANDARD | names: "Bloc de béton cellulaire - cellenbeton blok 15cm" | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" ("beton_cellenbeton_blok" 1.4E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_WallCommon, Qto_WallBaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Isolant - isolatie PIR 14cm" | INSULATION | names: "Isolant - isolatie PIR 14cm" | material: layers "Basic Roof:Isolant - isolatie PIR 14cm" ("isolatie_nbt_plaat" 1.4E-1) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Etanchéité - vochtwerende folie 1cm" | ROOFING | names: "Etanchéité - vochtwerende folie 1cm" | material: layers "Basic Roof:Etanchéité - vochtwerende folie 1cm" ("kunststof_ntb_folie_vochtwerend" 1.E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          1 x IFCWINDOW | type IFCWINDOWTYPE "Fenêtre simple ouvrante - enkele draairaam:L100 H130" | WINDOW | names: "Fenêtre simple ouvrante - enkele draairaam:L100 H130" | material: constituents "MaterialConstituentSet" ("Verre - Glas": "Verre - Glas", "Aluminium": "Aluminium", "Pierre bleue - Blauwe hardsteen": "natuursteen_hardsteen_ntb") | property sets: ePset_ModelInfo, Pset_WindowCommon, ePset_Simplebim
          4 x IFCMEMBER | type IFCMEMBERTYPE "Rectangle - rechthoek:8 x 23" | RAFTER | names: "8 x 23" | material: profiles "8 x 23" ("8 x 23": "hout_ntb_profiel"); "hout_ntb_profiel" | property sets: ePset_ModelInfo, Pset_MemberCommon, ePset_Simplebim
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Chape de pente - hellingslaag 5cm" | ROOF | names: "Chape de pente - hellingslaag 5cm" | material: layers "Floor:Chape de pente - hellingslaag 5cm" ("cement_zandcement_ihw" 5.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SlabCommon
      IFCBUILDINGSTOREY "650 Gouttière - Dakgoot" | long name "650 Gouttière" | elevation 6.5
        contains 13 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Isolant en laine de bois - isolatie houtwol 23cm" | INSULATION | names: "Isolant en laine de bois - isolatie houtwol 23cm" | material: layers "Basic Roof:Isolant en laine de bois - isolatie houtwol 23cm" ("hout_houtvulling_vulling" 2.3E-1) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Isolant en laine de bois - isolatie houtwol 3cm" | INSULATION | names: "Isolant en laine de bois - isolatie houtwol 3cm" | material: layers "Basic Roof:Isolant en laine de bois - isolatie houtwol 3cm" ("isolatie_nbt_plaat" 3.E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Lattage - latten 6cm" | ROOFING | names: "Lattage - latten 6cm" | material: layers "Basic Roof:Lattage - latten 6cm" ("hout_ntb_profiel" 6.E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Roof:Ardoises - leien" | ROOFING | names: "Ardoises - leien" | material: layers "Basic Roof:Ardoises - leien" ("natuursteen_lei_pan" 2.E-2) | property sets: ePset_ModelInfo, Pset_CoveringCommon, ePset_Simplebim
          1 x IFCPIPESEGMENT | GUTTER | names: "Gouttière demi-lune" | property sets: ePset_ModelInfo, ePset_Simplebim
          2 x IFCMEMBER | type IFCMEMBERTYPE "Rectangle - rechthoek:7 x 14 horiz" | PLATE | names: "7 x 14 horiz" | material: "hout_ntb_profiel"; profiles "7 x 14 horiz" ("7 x 14 horiz": "hout_ntb_profiel", "7 x 14 horiz": "hout_ntb_profiel") | property sets: ePset_ModelInfo, Pset_MemberCommon, ePset_Simplebim
          1 x IFCDISCRETEACCESSORY | type IFCDISCRETEACCESSORYTYPE "Couvre-mur - muurafdekker 3:Couvre-mur - muurafdekker 3" | USERDEFINED | names: "Couvre-mur - muurafdekker 3" | material: "natuursteen_hardsteen_ntb" | property sets: ePset_ModelInfo, ePset_Simplebim
          1 x IFCWINDOW | type IFCWINDOWTYPE "Velux:SK 06 - 114 x 118" | WINDOW | names: "Velux:SK 06 - 114 x 118" | material: constituents "MaterialConstituentSet" ("Aluminium": "Aluminium", "Verre - Glas": "Verre - Glas") | property sets: ePset_ModelInfo, Pset_WindowCommon, ePset_Simplebim
          1 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | names: "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_SwitchingDeviceTypeCommon
          2 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond en applique:Appareil standard" | names: "BS_63_FA_Luminaire rond en applique:Appareil standard" | property sets: ePset_ModelInfo, Pset_LightFixtureTypeCommon, ePset_Simplebim
          1 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Unipolaire" | names: "BS_63_LD_FA_Interrupteur:Unipolaire" | property sets: ePset_ModelInfo, Pset_SwitchingDeviceTypeCommon, ePset_Simplebim
      IFCBUILDINGSTOREY "1004 Faîte - Nok" | long name "1004 Faîte" | elevation 10.04
        contains 5 elements
          4 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:Briques de parement - gevelmetselwerk" | CLADDING | names: "Briques de parement - gevelmetselwerk" | material: layers "Basic Wall:Briques de parement - gevelmetselwerk" ("steenachtig_baksteen_generiek-pierreux_brique_génerique" 9.00000035762787E-2) | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_CoveringCommon
          1 x IFCCHIMNEY | type IFCCHIMNEYTYPE "Rectangle générique:Rectangle générique" | USERDEFINED | names: "Rectangle générique" | material: "natuursteen_hardsteen_ntb" | property sets: ePset_ModelInfo, ePset_Simplebim, Pset_ChimneyCommon

Types
  IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 39cm" | SOLIDWALL | 8 occurrences | material: layers "Basic Wall:Bloc béton - beton metselwerk 39cm" ("beton_generiek_blok" 3.9E-1)
  IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 19cm" | SOLIDWALL | 8 occurrences | material: layers "Basic Wall:Bloc béton - beton metselwerk 19cm" ("beton_generiek_blok" 1.9E-1)
  IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 83" | DOOR | 9 occurrences | material: "hout_generiek_profiel" | property sets: IfcDoorPanelProperties
  IFCFOOTINGTYPE "H 20 cm - L +20cm" | STRIP_FOOTING | 1 occurrence | material: "beton_gewapend_ntb"
  IFCSTAIRTYPE "Béton + bois" | 3 occurrences
  IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" | CONTACTOR | 28 occurrences
  IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond plafonnier:Hermétique" | 8 occurrences
  IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Unipolaire" | 9 occurrences
  IFCSLABTYPE "Floor:Dalle - draagvloer 25cm" | FLOOR | 1 occurrence | material: layers "Floor:Dalle - draagvloer 25cm" ("beton_generiek_granulaat" 2.5E-1)
  IFCBEAMTYPE "Rectangle - rechthoek:19 x 20" | BEAM | 7 occurrences | material: profiles "19 x 20" ("19 x 20": "beton_generiek_granulaat", "19 x 20": "beton_generiek_granulaat")
  IFCSLABTYPE "Pad:Sable de propreté - werkvloer 5cm" | 3 occurrences | material: layers "Pad:Sable de propreté - werkvloer 5cm" ("Sable - Zand" 5.E-2)
  IFCCOVERINGTYPE "Basic Wall:Briques de parement - gevelmetselwerk" | CLADDING | 24 occurrences | material: layers "Basic Wall:Briques de parement - gevelmetselwerk" ("steenachtig_baksteen_generiek-pierreux_brique_génerique" 9.00000035762787E-2)
  IFCCOVERINGTYPE "Basic Wall:Isolant - isolatie EPS 22cm" | INSULATION | 3 occurrences | material: layers "Basic Wall:Isolant - isolatie EPS 22cm" ("isolatie_pur_schuim" 2.2E-1)
  IFCCOVERINGTYPE "Basic Wall:Enduit - gevelbepleistering 2cm" | CLADDING | 7 occurrences | material: layers "Basic Wall:Enduit - gevelbepleistering 2cm" ("gips_stuc_bedekking" 2.E-2)
  IFCCOVERINGTYPE "Basic Wall:Lattage - latten 6cm" | CLADDING | 5 occurrences | material: layers "Basic Wall:Lattage - latten 6cm" ("hout_ntb_profiel" 6.E-2)
  IFCCOVERINGTYPE "Basic Wall:Bardage bois - houten gevelbekleding 2cm" | CLADDING | 2 occurrences | material: layers "Basic Wall:Bardage bois - houten gevelbekleding 2cm" ("hout_ntb_ntb" 2.E-2)
  IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire extérieur sur façade:Générique" | 1 occurrence
  IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond en applique:Hermétique" | 5 occurrences
  IFCCOVERINGTYPE "Floor:Parquet - parket 2cm" | FLOORING | 4 occurrences | material: layers "Floor:Parquet - parket 2cm" ("hout_generiek_plaat" 2.E-2)
  IFCCOVERINGTYPE "Floor:Chape - dekvloer 8cm" | FLOORING | 4 occurrences | material: layers "Floor:Chape - dekvloer 8cm" ("cement_zandcement_ihw" 8.E-2)
  IFCCOVERINGTYPE "Floor:Isolation - isolatie PUR 14cm" | FLOORING | 2 occurrences | material: layers "Floor:Isolation - isolatie PUR 14cm" ("isolatie_ntb_schuim" 1.4E-1)
  IFCSLABTYPE "Floor:Chape de compression - druklaag 4cm" | FLOOR | 3 occurrences | material: layers "Floor:Chape de compression - druklaag 4cm" ("cement_zandcement_ihw" 4.E-2)
  IFCCOVERINGTYPE "Basic Wall:Isolation - Isolatie PUR 14cm" | INSULATION | 13 occurrences | material: layers "Basic Wall:Isolation - Isolatie PUR 14cm" ("isolatie_pur_schuim" 1.4E-1)
  IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 14cm" | SOLIDWALL | 24 occurrences | material: layers "Basic Wall:Bloc béton - beton metselwerk 14cm" ("beton_generiek_blok" 1.4E-1)
  IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" | STANDARD | 29 occurrences | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" ("beton_cellenbeton_blok" 1.4E-1)
  IFCWALLTYPE "Basic Wall:Bloc béton - beton metselwerk 9cm" | STANDARD | 14 occurrences | material: layers "Basic Wall:Bloc béton - beton metselwerk 9cm" ("beton_generiek_blok" 9.E-2)
  IFCCOVERINGTYPE "Basic Roof:Isolant en laine de bois - isolatie houtwol 23cm" | INSULATION | 2 occurrences
  IFCCURTAINWALLTYPE "Curtain Wall:Simple panneau" | 2 occurrences
  IFCCOVERINGTYPE "Floor:Carrelage - tegels 2cm" | FLOORING | 4 occurrences | material: layers "Floor:Carrelage - tegels 2cm" ("steenachtig_ntb_tegel" 2.E-2)
  IFCDOORTYPE "Porte sectionnelle - sectionaaldeur:L300 H220" | DOOR | 1 occurrence | material: constituents "MaterialConstituentSet" ("Bois blanc - Witte hout": "hout_generiek_profiel", "Aluminium": "Aluminium") | property sets: IfcDoorPanelProperties
  IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 19cm" | STANDARD | 4 occurrences | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 19cm" ("beton_cellenbeton_blok" 1.9E-1)
  IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 9cm" | STANDARD | 9 occurrences | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 9cm" ("beton_cellenbeton_blok" 9.E-2)
  IFCDOORTYPE "Ouvrante simple - enkele draaideur:Standard 73 x 204" | DOOR | SINGLE_SWING_LEFT | 4 occurrences | material: "hout_generiek_profiel" | property sets: IfcDoorPanelProperties
  IFCBEAMTYPE "Rectangle - rechthoek:14 x 20" | BEAM | 19 occurrences | material: profiles "14 x 20" ("14 x 20": "beton_generiek_granulaat")
  IFCBEAMTYPE "Rectangle - rechthoek:9 x 20" | BEAM | 3 occurrences | material: profiles "9 x 20" ("9 x 20": "beton_generiek_granulaat", "9 x 20": "beton_generiek_granulaat")
  IFCSLABTYPE "Floor:Dalle - draagvloer 20cm" | FLOOR | 1 occurrence | material: layers "Floor:Dalle - draagvloer 20cm" ("beton_generiek_granulaat" 2.E-1)
  IFCCOVERINGTYPE "Basic Wall:Isolant en laine de bois - isolatie houtwol 23cm" | INSULATION | 3 occurrences | material: layers "Basic Wall:Isolant en laine de bois - isolatie houtwol 23cm" ("hout_houtvulling_vulling" 2.3E-1)
  IFCMEMBERTYPE "Colonne rectangulaire:8 x 23" | STUD | 56 occurrences | material: profiles "8 x 23" ("8 x 23": "hout_ntb_profiel", "8 x 23": "hout_ntb_profiel")
  IFCCOVERINGTYPE "Basic Wall:Isolant en laine de bois - isolatie houtwol 3cm" | INSULATION | 3 occurrences | material: layers "Basic Wall:Isolant en laine de bois - isolatie houtwol 3cm" ("hout_houtvulling_vulling" 3.E-2)
  IFCCOVERINGTYPE "Basic Wall:OSB 2cm" | CLADDING | 3 occurrences | material: layers "Basic Wall:OSB 2cm" ("hout_osb_plaat" 2.E-2)
  IFCMEMBERTYPE "Rectangle - rechthoek:8 x 23 horiz" | PLATE | 14 occurrences | material: profiles "8 x 23 horiz" ("8 x 23 horiz": "hout_ntb_profiel", "8 x 23 horiz": "hout_ntb_profiel")
  IFCCOVERINGTYPE "Compound Ceiling:Plafond" | CEILING | 11 occurrences
  IFCCOVERINGTYPE "Basic Roof:OSB 2cm" | ROOFING | 1 occurrence
  IFCCOVERINGTYPE "Basic Roof:Etanchéité - vochtwerende folie 1cm" | ROOFING | 2 occurrences
  IFCCOVERINGTYPE "Basic Roof:Isolant en laine de bois - isolatie houtwol 3cm" | INSULATION | 2 occurrences
  IFCCOVERINGTYPE "Basic Roof:Lattage - latten 6cm" | ROOFING | 2 occurrences
  IFCCOVERINGTYPE "Basic Roof:Ardoises - leien" | ROOFING | 2 occurrences
  IFCMEMBERTYPE "Rectangle - rechthoek:7 x 14 horiz" | PLATE | 4 occurrences | material: profiles "7 x 14 horiz" ("7 x 14 horiz": "hout_ntb_profiel", "7 x 14 horiz": "hout_ntb_profiel")
  IFCMEMBERTYPE "Rectangle - rechthoek:10 x 30" | PURLIN | 1 occurrence | material: "hout_ntb_profiel"
  IFCWINDOWTYPE "Fenêtre triple - fixe + ouvrante + fixe:L300 H230" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Glass": "Verre - Glas", "Frame/Mullion": "Aluminium", "Sill/Head": "natuursteen_hardsteen_ntb")
  IFCWINDOWTYPE "Fenêtre simple fixe - enkele vastraam:L100 H230" | WINDOW | 3 occurrences | material: constituents "MaterialConstituentSet" ("Glass": "Verre - Glas", "Frame/Mullion": "Aluminium", "Sill/Head": "natuursteen_hardsteen_ntb")
  IFCWINDOWTYPE "Fenêtre coulissante triple - drie schuifraam:L360 H238" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Frame/Mullion": "Aluminium", "Glass": "Verre - Glas")
  IFCSLABTYPE "Floor:Hourdis - welfsel 16cm" | FLOOR | 3 occurrences | material: layers "Floor:Hourdis - welfsel 16cm" ("Hourdis - Welfsel" 1.6E-1)
  IFCCOVERINGTYPE "Basic Wall:Paroi légère - lichte muur 10cm" | CLADDING | 4 occurrences | material: layers "Basic Wall:Paroi légère - lichte muur 10cm" ("gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2, "isolatie_glaswol_vulling" 5.E-2, "gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2)
  IFCWINDOWTYPE "Fenêtre simple ouvrante - enkele draairaam:L80 H125" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Glass": "Verre - Glas", "Frame/Mullion": "Aluminium", "Sill/Head": "natuursteen_hardsteen_ntb")
  IFCWINDOWTYPE "Fenêtre simple ouvrante - enkele draairaam:L80 H70" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Sill/Head": "natuursteen_hardsteen_ntb", "Glass": "Verre - Glas", "Frame/Mullion": "Aluminium")
  IFCDISTRIBUTIONELEMENTTYPE "Evier grand 1 bac:110 x 53.5cm" | 1 occurrence
  IFCCOVERINGTYPE "Basic Wall:Blanc" | CLADDING | 4 occurrences | material: layers "Basic Wall:Blanc" ("hout_generiek_profiel" 1.E-3)
  IFCSPACEHEATERTYPE "HVAC_Heaters_Finimetal_Vonaris-VSV-M_FR:VSV-M 10" | 1 occurrence | material: "Metal - Finimetal - R9016 Traffic White"
  IFCCOVERINGTYPE "Basic Wall:Paroi légère - lichte muur 7,5cm" | CLADDING | 2 occurrences | material: layers "Basic Wall:Paroi légère - lichte muur 7,5cm" ("isolatie_glaswol_vulling" 5.E-2, "gips_gipskarton_plaat" 1.25E-2, "gips_gipskarton_plaat" 1.25E-2)
  IFCPIPESEGMENTTYPE "Pipe Types:BS_53_PI_Acier inox - Cheminée double paroi" | 1 occurrence
  IFCDUCTSEGMENTTYPE "Round Duct:BS_57_DU_Galva (Tés)" | 70 occurrences
  IFCDUCTFITTINGTYPE "BS_57_DUF_Coude circulaire:Galva" | 37 occurrences
  IFCDUCTSEGMENTTYPE "Flex Duct Round:BS_57_FDU_Souple - Circulaire" | FLEXIBLESEGMENT | 12 occurrences
  IFCDUCTFITTINGTYPE "BS_57_DUF_Té circulaire:Galva" | 13 occurrences
  IFCAIRTERMINALTYPE "BS_57_AIR_UN_Grille circulaire LVS:D100" | GRILLE | 3 occurrences
  IFCDUCTFITTINGTYPE "BS_57_DUF_Transformation circulaire - Angle:Galva 45°" | 8 occurrences
  IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond plafonnier:Appareil standard" | 52 occurrences
  IFCOUTLETTYPE "BS_64_DD_FA_Prise data:RJ45" | DATAOUTLET | 6 occurrences
  IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Inverseur unipolaire" | 2 occurrences
  IFCSWITCHINGDEVICETYPE "BS_63_LD_FA_Interrupteur:Bipolaire" | CONTACTOR | 6 occurrences
  IFCBOILERTYPE "BS_56_Chaudière mural:45 kW" | WATER | 1 occurrence | material: constituents "MaterialConstituentSet" ("Equipment": "Color RGB 127-118-121")
  IFCDUCTFITTINGTYPE "BS_57_DUF_Raccord à 45 degrés circulaire:Standard" | 2 occurrences
  IFCDISTRIBUTIONELEMENTTYPE "Evier grand 1 bac1:110 x 53.5cm 2" | 1 occurrence
  IFCDISTRIBUTIONELEMENTTYPE "Lavabo arrondi (petit)1:45 cm 2" | 1 occurrence
  IFCPIPESEGMENTTYPE "Pipe Types:BS_52_PI_PVC" | 59 occurrences
  IFCPIPEFITTINGTYPE "BS_52_PIF_Té - Evacuation:PVC" | 12 occurrences
  IFCSANITARYTERMINALTYPE "BS_74_PF_LE_Lave-main_2:360x250" | WASHHANDBASIN | 2 occurrences
  IFCDISTRIBUTIONELEMENTTYPE "BS_53_PF_Collecteur EF 4 départs:BS_53_PF_Collecteur EF 4 départs" | 1 occurrence
  IFCDISTRIBUTIONELEMENTTYPE "BS_53_PF_Collecteur ECS 2 départs:BS_53_PF_Collecteur ECS 2 départs" | 1 occurrence
  IFCPIPESEGMENTTYPE "Pipe Types:BS_53_PI_PEX-Alu-PEX" | 195 occurrences
  IFCPIPEFITTINGTYPE "BS_53_PIF_Courbure - Adduction:PEX-Alu-PEX" | 90 occurrences
  IFCPIPEFITTINGTYPE "BS_52_PIF_Coude - Evacuation:PVC" | 33 occurrences
  IFCVALVETYPE "Distribution manifold for heating systems_Caleffi_662 x5:5 outlets" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Handle": "Technopolymer - Caleffi - white", "Body": "Metal - Caleffi - Brass", "Metal - Caleffi - Stainless Steel": "Metal - Caleffi - Stainless Steel")
  IFCPIPEFITTINGTYPE "BS_53_PIF_Coude - Adduction:PEX-Alu-PEX" | 70 occurrences
  IFCPIPEFITTINGTYPE "BS_52_PIF_Réduction - Evacuation:PVC" | 2 occurrences
  IFCPIPEFITTINGTYPE "BS_53_PIF_Té - Adduction:PEX-Alu-PEX" | 3 occurrences
  IFCPIPEFITTINGTYPE "BS_53_PIF_Bouchon - Adduction:PEX-Alu-PEX" | 3 occurrences
  IFCPIPEFITTINGTYPE "BS_53_PIF_Réduction - Adduction:PEX-Alu-PEX" | 4 occurrences
  IFCPIPESEGMENTTYPE "Descente d'eau ronde - ronde afvoerpijp 8cm 2:Descente d'eau ronde - ronde afvoerpijp 8cm" | RIGIDSEGMENT | 1 occurrence | material: "metaal_zink_profiel"
  IFCPIPESEGMENTTYPE "Descente d'eau ronde - ronde afvoerpijp 8cm 1:Descente d'eau ronde - ronde afvoerpijp 8cm" | RIGIDSEGMENT | 1 occurrence | material: "metaal_zink_profiel"
  IFCPIPESEGMENTTYPE "Descente d'eau ronde - ronde afvoerpijp 8cm 3:Descente d'eau ronde - ronde afvoerpijp 8cm" | RIGIDSEGMENT | 1 occurrence | material: "metaal_zink_profiel"
  IFCCOVERINGTYPE "Isolation laine de bois - Isolatie houtwol 23cm:Isolation laine de bois - Isolatie houtwol 23cm" | INSULATION | 1 occurrence
  IFCDOORTYPE "Fenêtre double fixe + ouvrante (porte) - vast + draairaam (deur): L160 H230" | DOOR | SWING_FIXED_RIGHT | 2 occurrences
  IFCDOORTYPE "Porte pleine (ouverture vers l'intérieur) - volle deur (binnen openend): L90 H230" | DOOR | SWING_FIXED_LEFT | 1 occurrence
  IFCDOORTYPE "Porte (ouverture vers l'intérieur) - deur (binnen openend): L110 H230" | DOOR | SWING_FIXED_LEFT | 1 occurrence
  IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire - reprise:GPD-100" | GRILLE | 6 occurrences | material: "Steel Sheet - Koolair"
  IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire - pulsion:GPD-I-100" | GRILLE | 6 occurrences | material: "Steel Sheet - Koolair"
  IFCBEAMTYPE "Rectangle - rechthoek:19 x 30" | BEAM | 1 occurrence | material: profiles "19 x 30" ("19 x 30": "beton_generiek_granulaat", "19 x 30": "beton_generiek_granulaat")
  IFCMEMBERTYPE "Rectangle - rechthoek:8 x 23" | RAFTER | 18 occurrences | material: profiles "8 x 23" ("8 x 23": "hout_ntb_profiel")
  IFCCOVERINGTYPE "Basic Roof:Isolant - isolatie PIR 14cm" | INSULATION | 2 occurrences
  IFCDISCRETEACCESSORYTYPE "Couvre-mur - muurafdekker 2:Couvre-mur - muurafdekker 2" | 1 occurrence
  IFCDISCRETEACCESSORYTYPE "Couvre-mur - muurafdekker 1:Couvre-mur - muurafdekker 1" | 1 occurrence | material: "natuursteen_hardsteen_ntb"
  IFCCOVERINGTYPE "Basic Roof:Carrelage - tegels 2cm" | FLOORING | 1 occurrence
  IFCWALLTYPE "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 26cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 26cm" ("beton_cellenbeton_blok" 2.6E-1)
  IFCCOVERINGTYPE "Basic Wall:Carrelage - tegels 2cm" | CLADDING | 5 occurrences | material: layers "Basic Wall:Carrelage - tegels 2cm" ("steenachtig_ntb_tegel" 2.E-2)
  IFCWINDOWTYPE "Fenêtre triple - fixe + ouvrante + fixe:L300 H130" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Glass": "Verre - Glas", "Frame/Mullion": "Aluminium", "Sill/Head": "natuursteen_hardsteen_ntb")
  IFCWINDOWTYPE "Fenêtre double fixe + ouvrante - vast + draairaam:L160 H130" | WINDOW | 4 occurrences | material: constituents "MaterialConstituentSet" ("Glass": "Verre - Glas", "Frame/Mullion": "Aluminium", "Sill/Head": "natuursteen_hardsteen_ntb")
  IFCWINDOWTYPE "Fenêtre simple ouvrante - enkele draairaam:L100 H130" | WINDOW | 2 occurrences | material: constituents "MaterialConstituentSet" ("Glass": "Verre - Glas", "Frame/Mullion": "Aluminium", "Sill/Head": "natuursteen_hardsteen_ntb")
  IFCWINDOWTYPE "Fenêtre double ouvrante - dubbele draairaam:L232 H197" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Glass": "Verre - Glas", "Frame/Mullion": "Aluminium", "Sill/Head": "natuursteen_hardsteen_ntb")
  IFCSLABTYPE "Floor:Chape de pente - hellingslaag 5cm" | ROOF | 2 occurrences | material: layers "Floor:Chape de pente - hellingslaag 5cm" ("cement_zandcement_ihw" 5.E-2)
  IFCWINDOWTYPE "CFP_ISD 2093:80 x 80" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Frame/Mullion": "Aluminium profiles / 4 mm toughened glass pane", "Glass": "73FQT + ISD 2093", "Frame/Mullion": "PVC Color NCS S 0502-Y")
  IFCVALVETYPE "Collecteur_2x6_CALEFFI:6 outlets" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Handle": "Technopolymer - Caleffi - white", "Body": "Metal - Caleffi - Brass", "Body": "Technopolymer - Caleffi - white", "Body": "Technopolymer - Caleffi - Black", "Metal - Caleffi - Stainless Steel": "Metal - Caleffi - Stainless Steel")
  IFCAIRTERMINALTYPE "BS_57_AIR_FA_Bouche circulaire LVS pulsion:D100" | GRILLE | 2 occurrences
  IFCDISCRETEACCESSORYTYPE "Couvre-mur - muurafdekker 3:Couvre-mur - muurafdekker 3" | 1 occurrence | material: "natuursteen_hardsteen_ntb"
  IFCWINDOWTYPE "Velux:SK 06 - 114 x 118" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Frame/Mullion": "Aluminium", "Glass": "Verre - Glas")
  IFCLIGHTFIXTURETYPE "BS_63_FA_Luminaire rond en applique:Appareil standard" | 2 occurrences
  IFCCHIMNEYTYPE "Rectangle générique:Rectangle générique" | 1 occurrence | material: "natuursteen_hardsteen_ntb"

Property sets
  ePset_ModelInfo | properties | on 1394 objects (263 IFCPIPESEGMENT, 217 IFCPIPEFITTING, 121 IFCOPENINGELEMENT, 118 IFCCOVERING)
    ModelName = "BBRI House.ifc" (IFCLABEL)
    Timestamp = "2022-11-16T14:20:15+01:00" (IFCLABEL)
  ePset_ModelInfo | properties | on 1273 objects (263 IFCPIPESEGMENT, 217 IFCPIPEFITTING, 118 IFCCOVERING, 113 IFCMEMBER)
    ModelName = "BBRI House.blend.ifc" (IFCLABEL)
    Timestamp = "2022-11-16T14:20:15+01:00" (IFCLABEL)
  Pset_AirTerminalTypeCommon | properties | on 6 objects (6 IFCAIRTERMINAL)
    Reference = "BS_57_AIR_FA_Bouche circulaire - pulsion:GPD-I-100" (IFCIDENTIFIER)
  Pset_AirTerminalTypeCommon | properties | on 6 objects (6 IFCAIRTERMINAL)
    Reference = "BS_57_AIR_FA_Bouche circulaire - reprise:GPD-100" (IFCIDENTIFIER)
  Pset_AirTerminalTypeCommon | properties | on 3 objects (3 IFCAIRTERMINAL)
    Reference = "BS_57_AIR_UN_Grille circulaire LVS:D100" (IFCIDENTIFIER)
  Pset_AirTerminalTypeCommon | properties | on 2 objects (2 IFCAIRTERMINAL)
    Reference = "BS_57_AIR_FA_Bouche circulaire LVS pulsion:D100" (IFCIDENTIFIER)
  ePset_Simplebim | properties | on 1224 objects (263 IFCPIPESEGMENT, 217 IFCPIPEFITTING, 118 IFCCOVERING, 98 IFCWALL)
    Assembly Level = "Single" (IFCIDENTIFIER)
  ePset_Simplebim | properties | on 29 objects (18 IFCMEMBER, 4 IFCDOOR, 4 IFCPLATE, 3 IFCSTAIRFLIGHT)
    Assembly Level = "Leaf" (IFCIDENTIFIER)
  ePset_Simplebim | properties | on 5 objects (3 IFCSTAIR, 2 IFCCURTAINWALL)
    Assembly Level = "Topmost" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 19 objects (19 IFCBEAM)
    Reference = "Rectangle - rechthoek:14 x 20" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 7 objects (7 IFCBEAM)
    Reference = "Rectangle - rechthoek:19 x 20" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    Reference = "Rectangle - rechthoek:9 x 20" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    Reference = "Rectangle - rechthoek:19 x 30" (IFCIDENTIFIER)
  Pset_BoilerTypeCommon | properties | on 1 object (1 IFCBOILER)
    Reference = "BS_56_Chaudière mural:45 kW" (IFCIDENTIFIER)
  Pset_ChimneyCommon | properties | on 1 object (1 IFCCHIMNEY)
    Reference = "Rectangle générique:Rectangle générique" (IFCIDENTIFIER)
  ePset_LocationTool | properties | on 1 object (1 IFCCOVERING)
    Location 0 = "Based on Clipping Plane" (IFCIDENTIFIER)
    Parent Guid = "2wjauRddzFaQxoS8JDbPRP" (IFCIDENTIFIER)
    Splitting = "ORIGINAL" (IFCIDENTIFIER)
  ePset_LocationTool | properties | on 1 object (1 IFCCOVERING)
    Location 0 = "Based on Clipping Plane" (IFCIDENTIFIER)
    Parent Guid = "0Gp0yMwcb28utMMEVamGmp" (IFCIDENTIFIER)
    Splitting = "ORIGINAL" (IFCIDENTIFIER)
  ePset_LocationTool | properties | on 1 object (1 IFCCOVERING)
    Location 0 = "Based on Clipping Plane" (IFCIDENTIFIER)
    Parent Guid = "0MO7x7lpbA7O$XvIfeRjp6" (IFCIDENTIFIER)
    Splitting = "ORIGINAL" (IFCIDENTIFIER)
  ePset_LocationTool | properties | on 1 object (1 IFCCOVERING)
    Location 0 = "Based on Clipping Plane" (IFCIDENTIFIER)
    Parent Guid = "0Gp0yMwcb28utMMEVamHAq" (IFCIDENTIFIER)
    Splitting = "ORIGINAL" (IFCIDENTIFIER)
  ePset_LocationTool | properties | on 1 object (1 IFCCOVERING)
    Location 0 = "Based on Clipping Plane" (IFCIDENTIFIER)
    Parent Guid = "0Gp0yMwcb28utMMEVamGlD" (IFCIDENTIFIER)
    Splitting = "ORIGINAL" (IFCIDENTIFIER)
  ePset_LocationTool | properties | on 1 object (1 IFCCOVERING)
    Location 0 = "Based on Clipping Plane" (IFCIDENTIFIER)
    Parent Guid = "04etSB5mnCwP3c4mJjUW0Z" (IFCIDENTIFIER)
    Splitting = "ORIGINAL" (IFCIDENTIFIER)
  ePset_LocationTool | properties | on 1 object (1 IFCCOVERING)
    Location 0 = "Based on Clipping Plane" (IFCIDENTIFIER)
    Parent Guid = "0MO7x7lpbA7O$XvIfeRjpP" (IFCIDENTIFIER)
    Splitting = "ORIGINAL" (IFCIDENTIFIER)
  ePset_LocationTool | properties | on 1 object (1 IFCCOVERING)
    Location 0 = "Based on Clipping Plane" (IFCIDENTIFIER)
    Parent Guid = "0Gp0yMwcb28utMMEVamGww" (IFCIDENTIFIER)
    Splitting = "ORIGINAL" (IFCIDENTIFIER)
  ePset_LocationTool: 111 more contents on 111 objects not shown
  Pset_CoveringCommon | properties | on 24 objects (24 IFCCOVERING)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Basic Wall:Briques de parement - gevelmetselwerk" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_CoveringCommon | properties | on 13 objects (13 IFCCOVERING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:Isolation - Isolatie PUR 14cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_CoveringCommon | properties | on 10 objects (10 IFCCOVERING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Compound Ceiling:Plafond" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_CoveringCommon | properties | on 5 objects (5 IFCCOVERING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:Carrelage - tegels 2cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Basic Wall:Enduit - gevelbepleistering 2cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:Blanc" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:Paroi légère - lichte muur 10cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:OSB 2cm" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_CoveringCommon: 28 more contents on 51 objects not shown
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Curtain Wall:Simple panneau" (IFCIDENTIFIER)
  Pset_DamperTypeCommon | properties | on 1 object (1 IFCDAMPER)
    Status = "New" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCDAMPER)
    Reference = "dampkap eiland" (IFCIDENTIFIER)
  IfcDoorPanelProperties | properties | on 18 objects (18 IFCDOOR)
    PanelOperation = "NOTDEFINED" (IFCTEXT)
    PanelOperation = "NOTDEFINED" (IFCTEXT)
    PanelPosition = "NOTDEFINED" (IFCTEXT)
    PanelPosition = "NOTDEFINED" (IFCTEXT)
  IfcDoorPanelProperties | predefined | on 3 type objects
  Pset_DoorCommon | properties | on 9 objects (9 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Ouvrante simple - enkele draaideur:Standard 83" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Ouvrante simple - enkele draaideur:Standard 73 x 204" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Ouvrant - draaideur:Meneau - lijst 6cm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Porte (ouverture vers l'intérieur) - deur (binnen openend): L110 H230" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Fenêtre double fixe + ouvrante (porte) - vast + draairaam (deur): L160 H230" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Fenêtre double fixe + ouvrante (porte) - vast + draairaam (deur): L160 H230" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Porte sectionnelle - sectionaaldeur:L300 H220" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Porte pleine (ouverture vers l'intérieur) - volle deur (binnen openend): L90 H230" (IFCIDENTIFIER)
  Pset_DuctFittingTypeCommon | properties | on 37 objects (37 IFCDUCTFITTING)
    Reference = "BS_57_DUF_Coude circulaire:Galva" (IFCIDENTIFIER)
  Pset_DuctFittingTypeCommon | properties | on 13 objects (13 IFCDUCTFITTING)
    Reference = "BS_57_DUF_Té circulaire:Galva" (IFCIDENTIFIER)
  Pset_DuctFittingTypeCommon | properties | on 8 objects (8 IFCDUCTFITTING)
    Reference = "BS_57_DUF_Transformation circulaire - Angle:Galva 45°" (IFCIDENTIFIER)
  Pset_DuctFittingTypeCommon | properties | on 2 objects (2 IFCDUCTFITTING)
    Reference = "BS_57_DUF_Raccord à 45 degrés circulaire:Standard" (IFCIDENTIFIER)
  Pset_DuctSegmentTypeCommon | properties | on 70 objects (70 IFCDUCTSEGMENT)
    Reference = "Round Duct:BS_57_DU_Galva (Tés)" (IFCIDENTIFIER)
  Pset_DuctSegmentTypeCommon | properties | on 12 objects (12 IFCDUCTSEGMENT)
    Reference = "Flex Duct Round:BS_57_FDU_Souple - Circulaire" (IFCIDENTIFIER)
  Pset_ElectricApplianceTypeCommon | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Status = "New" (IFCLABEL)
  Pset_FootingCommon | properties | on 1 object (1 IFCFOOTING)
    Reference = "H 20 cm - L +20cm" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 52 objects (52 IFCLIGHTFIXTURE)
    Reference = "BS_63_FA_Luminaire rond plafonnier:Appareil standard" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 8 objects (8 IFCLIGHTFIXTURE)
    Reference = "BS_63_FA_Luminaire rond plafonnier:Hermétique" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 5 objects (5 IFCLIGHTFIXTURE)
    Reference = "BS_63_FA_Luminaire rond en applique:Hermétique" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 2 objects (2 IFCLIGHTFIXTURE)
    Reference = "BS_63_FA_Luminaire rond en applique:Appareil standard" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Reference = "BS_63_FA_Luminaire extérieur sur façade:Générique" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 52 objects (52 IFCMEMBER)
    Reference = "Colonne rectangulaire:8 x 23" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_MemberCommon | properties | on 18 objects (18 IFCMEMBER)
    Reference = "Rectangular Mullion:3 x 6" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_MemberCommon | properties | on 14 objects (14 IFCMEMBER)
    Reference = "Rectangle - rechthoek:8 x 23 horiz" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_MemberCommon | properties | on 11 objects (11 IFCMEMBER)
    Reference = "Rectangle - rechthoek:8 x 23" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_MemberCommon | properties | on 7 objects (7 IFCMEMBER)
    Reference = "Rectangle - rechthoek:8 x 23" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    Reference = "Rectangle - rechthoek:7 x 14 horiz" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    Reference = "Colonne rectangulaire:8 x 23" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    Status = "Existing" (IFCLABEL)
  Pset_MemberCommon: 1 more content on 1 objects not shown
  Pset_OutletTypeCommon | properties | on 6 objects (6 IFCOUTLET)
    Reference = "BS_64_DD_FA_Prise data:RJ45" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 90 objects (90 IFCPIPEFITTING)
    Reference = "BS_53_PIF_Courbure - Adduction:PEX-Alu-PEX" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 70 objects (70 IFCPIPEFITTING)
    Reference = "BS_53_PIF_Coude - Adduction:PEX-Alu-PEX" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 33 objects (33 IFCPIPEFITTING)
    Reference = "BS_52_PIF_Coude - Evacuation:PVC" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 12 objects (12 IFCPIPEFITTING)
    Reference = "BS_52_PIF_Té - Evacuation:PVC" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 4 objects (4 IFCPIPEFITTING)
    Reference = "BS_53_PIF_Réduction - Adduction:PEX-Alu-PEX" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 3 objects (3 IFCPIPEFITTING)
    Reference = "BS_53_PIF_Bouchon - Adduction:PEX-Alu-PEX" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 3 objects (3 IFCPIPEFITTING)
    Reference = "BS_53_PIF_Té - Adduction:PEX-Alu-PEX" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 2 objects (2 IFCPIPEFITTING)
    Reference = "BS_52_PIF_Réduction - Evacuation:PVC" (IFCIDENTIFIER)
  Pset_PipeSegmentTypeCommon | properties | on 195 objects (195 IFCPIPESEGMENT)
    Reference = "Pipe Types:BS_53_PI_PEX-Alu-PEX" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_PipeSegmentTypeCommon | properties | on 59 objects (59 IFCPIPESEGMENT)
    Reference = "Pipe Types:BS_52_PI_PVC" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_PipeSegmentTypeCommon | properties | on 4 objects (4 IFCPIPESEGMENT)
    Status = "Existing" (IFCLABEL)
  Pset_PipeSegmentTypeCommon | properties | on 1 object (1 IFCPIPESEGMENT)
    Reference = "Descente d'eau ronde - ronde afvoerpijp 8cm 3:Descente d'eau ronde - ronde afvoerpijp 8cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_PipeSegmentTypeCommon | properties | on 1 object (1 IFCPIPESEGMENT)
    Reference = "Descente d'eau ronde - ronde afvoerpijp 8cm 2:Descente d'eau ronde - ronde afvoerpijp 8cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_PipeSegmentTypeCommon | properties | on 1 object (1 IFCPIPESEGMENT)
    Reference = "Pipe Types:BS_53_PI_Acier inox - Cheminée double paroi" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_PipeSegmentTypeCommon | properties | on 1 object (1 IFCPIPESEGMENT)
    Reference = "Descente d'eau ronde - ronde afvoerpijp 8cm 1:Descente d'eau ronde - ronde afvoerpijp 8cm" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_PlateCommon | properties | on 4 objects (4 IFCPLATE)
    Reference = "Panneau système:Vitré" (IFCIDENTIFIER)
  Pset_SanitaryTerminalTypeCommon | properties | on 2 objects (2 IFCSANITARYTERMINAL)
    Reference = "BS_74_PF_LE_Lave-main_2:360x250" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    Reference = "Floor:Hourdis - welfsel 16cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    Reference = "Floor:Chape de compression - druklaag 4cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    Reference = "Floor:Chape de pente - hellingslaag 5cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    Reference = "Pad:Sable de propreté - werkvloer 5cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    Reference = "Floor:Dalle - draagvloer 25cm" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    Reference = "Pad:Sable de propreté - werkvloer 5cm" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    Reference = "Floor:Dalle - draagvloer 20cm" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_SpaceHeaterTypeCommon | properties | on 6 objects (6 IFCSPACEHEATER)
    Status = "Existing" (IFCLABEL)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACEHEATER)
    Reference = "HVAC_Heaters_Finimetal_Vonaris-VSV-M_FR:VSV-M 10" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_StairCommon | properties | on 3 objects (3 IFCSTAIR)
    Reference = "Béton + bois" (IFCIDENTIFIER)
  Pset_StairFlightCommon | properties | on 3 objects (3 IFCSTAIRFLIGHT)
    Reference = "Béton + bois" (IFCIDENTIFIER)
  Pset_SwitchingDeviceTypeCommon | properties | on 28 objects (28 IFCSWITCHINGDEVICE)
    Reference = "BS_63_LD_FA_Interrupteur:Deux directions unipolaire" (IFCIDENTIFIER)
  Pset_SwitchingDeviceTypeCommon | properties | on 9 objects (9 IFCSWITCHINGDEVICE)
    Reference = "BS_63_LD_FA_Interrupteur:Unipolaire" (IFCIDENTIFIER)
  Pset_SwitchingDeviceTypeCommon | properties | on 6 objects (6 IFCSWITCHINGDEVICE)
    Reference = "BS_63_LD_FA_Interrupteur:Bipolaire" (IFCIDENTIFIER)
  Pset_SwitchingDeviceTypeCommon | properties | on 2 objects (2 IFCSWITCHINGDEVICE)
    Reference = "BS_63_LD_FA_Interrupteur:Inverseur unipolaire" (IFCIDENTIFIER)
  Pset_ValveTypeCommon | properties | on 1 object (1 IFCVALVE)
    Reference = "Distribution manifold for heating systems_Caleffi_662 x5:5 outlets" (IFCIDENTIFIER)
  Pset_ValveTypeCommon | properties | on 1 object (1 IFCVALVE)
    Reference = "Collecteur_2x6_CALEFFI:6 outlets" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 29 objects (29 IFCWALL)
    Reference = "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 15cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 24 objects (24 IFCWALL)
    Reference = "Basic Wall:Bloc béton - beton metselwerk 14cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 14 objects (14 IFCWALL)
    Reference = "Basic Wall:Bloc béton - beton metselwerk 9cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 9 objects (9 IFCWALL)
    Reference = "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 9cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALL)
    Reference = "Basic Wall:Bloc béton - beton metselwerk 39cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALL)
    Reference = "Basic Wall:Bloc béton - beton metselwerk 19cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALL)
    Reference = "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 19cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    Reference = "Basic Wall:Bloc de béton cellulaire - cellenbeton blok 26cm" (IFCIDENTIFIER)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 8.5259999999999E-1 [SQUARE_METRE]
    GrossSideArea = 1.4616 [SQUARE_METRE]
    GrossVolume = 2.04624E-1 [CUBIC_METRE]
    Height = 2.4E-1 [METRE]
    Length = 6.09 [METRE]
    NetSideArea = 1.4616 [SQUARE_METRE]
    NetVolume = 2.04624000000001E-1 [CUBIC_METRE]
    Width = 1.4E-1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.34100000000001E-1 [SQUARE_METRE]
    GrossSideArea = 4.17200000000003 [SQUARE_METRE]
    GrossVolume = 3.75480000000003E-1 [CUBIC_METRE]
    Height = 2.8 [METRE]
    Length = 1.49000000000001 [METRE]
    NetSideArea = 4.17200000000003 [SQUARE_METRE]
    NetVolume = 3.75480000000003E-1 [CUBIC_METRE]
    Width = 9.E-2 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.40000000000001E-1 [SQUARE_METRE]
    GrossSideArea = 2.04999999999998E-1 [SQUARE_METRE]
    GrossVolume = 2.86999999999997E-2 [CUBIC_METRE]
    Height = 2.04999999999998E-1 [METRE]
    Length = 9.99999999999999E-1 [METRE]
    NetSideArea = 2.04999999999998E-1 [SQUARE_METRE]
    NetVolume = 2.86999999999996E-2 [CUBIC_METRE]
    Width = 1.4E-1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 3.69E-2 [SQUARE_METRE]
    GrossSideArea = 1.10699999999989 [SQUARE_METRE]
    GrossVolume = 9.96299999999904E-2 [CUBIC_METRE]
    Height = 2.69999999999974 [METRE]
    Length = 4.1E-1 [METRE]
    NetSideArea = 1.10699999999989 [SQUARE_METRE]
    NetVolume = 9.96299999999903E-2 [CUBIC_METRE]
    Width = 9.E-2 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.77200000000002E-1 [SQUARE_METRE]
    GrossSideArea = 4.75200000000003E-1 [SQUARE_METRE]
    GrossVolume = 6.65280000000004E-2 [CUBIC_METRE]
    Height = 2.4E-1 [METRE]
    Length = 1.98000000000001 [METRE]
    NetSideArea = 4.75200000000003E-1 [SQUARE_METRE]
    NetVolume = 6.65280000000005E-2 [CUBIC_METRE]
    Width = 1.4E-1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 3.23999999999998E-1 [SQUARE_METRE]
    GrossSideArea = 8.21699999999992 [SQUARE_METRE]
    GrossVolume = 7.39529999999992E-1 [CUBIC_METRE]
    Height = 2.8 [METRE]
    Length = 3.59999999999997 [METRE]
    NetSideArea = 7.96899999999993 [SQUARE_METRE]
    NetVolume = 7.17209999999993E-1 [CUBIC_METRE]
    Width = 9.E-2 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.2754 [SQUARE_METRE]
    GrossSideArea = 24.5969999999993 [SQUARE_METRE]
    GrossVolume = 3.4435799999999 [CUBIC_METRE]
    Height = 2.69999999999992 [METRE]
    Length = 9.11 [METRE]
    NetSideArea = 19.6769999999993 [SQUARE_METRE]
    NetVolume = 2.75477999999989 [CUBIC_METRE]
    Width = 1.4E-1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 5.7525 [SQUARE_METRE]
    GrossSideArea = 36.875000000001 [SQUARE_METRE]
    GrossVolume = 14.3812500000004 [CUBIC_METRE]
    Height = 2.50000000000007 [METRE]
    Length = 14.75 [METRE]
    NetSideArea = 36.875000000001 [SQUARE_METRE]
    NetVolume = 14.3812500000004 [CUBIC_METRE]
    Width = 3.9E-1 [METRE]
  Qto_WallBaseQuantities: 88 more contents on 88 objects not shown
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fenêtre double fixe + ouvrante - vast + draairaam:L160 H130" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fenêtre simple fixe - enkele vastraam:L100 H230" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fenêtre simple ouvrante - enkele draairaam:L100 H130 (19)" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fenêtre simple ouvrante - enkele draairaam:L80 H125" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fenêtre simple fixe - enkele vastraam:L100 H230 (6)" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Velux:SK 06 - 114 x 118" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fenêtre simple ouvrante - enkele draairaam:L80 H70" (IFCIDENTIFIER)
    Status = "New" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fenêtre triple - fixe + ouvrante + fixe:L300 H230" (IFCIDENTIFIER)
    Status = "Existing" (IFCLABEL)
  Pset_WindowCommon: 7 more contents on 7 objects not shown