IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition[DesignTransferView]"
File name: "00.SJCES - Main Building - 240907 - Window Test.ifc"
Time stamp: "2024-09-14T06:04:54-04:00"
Preprocessor: "IfcOpenShell 0.8.1-alpha240914"
Originating system: "Bonsai 0.8.1-alpha240914-c487643"
Authorization: "Nobody"

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  LENGTHUNIT: MILLI METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "000 - SITE"
    IFCBUILDING "001 - SJCES"
      contains 1 element
        1 x IFCANNOTATION | object type "ASBUILTAREA" | names: "Empty - Existing Building"
      IFCBUILDINGSTOREY "001 - TOP OF FIN. FLOOR"
        contains 20 elements
          5 x IFCWALL | type IFCWALLTYPE "Brick - 90mm" | names: "Wall" | material: layers ("Brick" 90.) | property sets: EPset_Parametric
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Foundation Wall Insulation - 75" | INSULATION | names: "BuildingElementPart.016", "BuildingElementPart.001" | material: layers ("Rigid Insulation" 75.) | property sets: EPset_Parametric, Pset_CoveringCommon
          6 x IFCWALL | type IFCWALLTYPE "Arc. Block- 90mm" | names: "Wall" | material: layers ("Architectural Masonry Block" 90.) | property sets: EPset_Parametric
          2 x IFCWALL | type IFCWALLTYPE "Conc. Block- 90mm" | names: "Wall" | material: layers ("Concrete Masonry Block" 90.) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "w1" | names: "Window"
          2 x IFCWALL | type IFCWALLTYPE "Conc. Block- 190mm" | names: "Wall" | material: layers ("Concrete Masonry Block" 190.) | property sets: EPset_Parametric, Pset_WallCommon
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Spray Foam Insulation - 100" | names: "Covering" | material: layers ("Spray Foam" 100.) | property sets: EPset_Parametric, Pset_CoveringCommon
      IFCBUILDINGSTOREY "003 - U/S NEW DECK"
      IFCBUILDINGSTOREY "002 - U/S OF EX. DECK"
      IFCBUILDINGSTOREY "-001 - TOP OF FOUNDATIONM FOOTING"
        contains 8 elements
          2 x IFCWALL | type IFCWALLTYPE "FDW- 400mm" | ELEMENTEDWALL | names: "Wall.042", "Wall.035" | material: layers ("Concrete" 400.) | property sets: EPset_Parametric, EPset_Status
          2 x IFCFOOTING | type IFCFOOTINGTYPE "SJCES - WF8" | names: "Footing" | material: layers ("Concrete" 800.) | property sets: EPset_Parametric, EPset_Status
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Foundation Wall Insulation - 50" | INSULATION | names: "VerticalRigidInsulation.001", "VerticalRigidInsulation", "BuildingElementPart.012" | material: layers ("Rigid Insulation" 50.) | property sets: EPset_Parametric, Pset_CoveringCommon
          1 x IFCOPENINGELEMENT | names: "Opening"

Types
  IFCWALLTYPE "Brick - 90mm" | ELEMENTEDWALL | 5 occurrences | material: layers ("Brick" 90.) | property sets: EPset_Parametric
  IFCCOVERINGTYPE "Foundation Wall Insulation - 75" | INSULATION | 2 occurrences | material: layers ("Rigid Insulation" 75.) | property sets: EPset_Parametric
  IFCWALLTYPE "Arc. Block- 90mm" | ELEMENTEDWALL | 6 occurrences | material: layers ("Architectural Masonry Block" 90.) | property sets: EPset_Parametric
  IFCWALLTYPE "Conc. Block- 90mm" | ELEMENTEDWALL | 2 occurrences | material: layers ("Concrete Masonry Block" 90.) | property sets: EPset_Parametric
  IFCWINDOWTYPE "w1" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCWALLTYPE "Conc. Block- 190mm" | ELEMENTEDWALL | 2 occurrences | material: layers ("Concrete Masonry Block" 190.) | property sets: EPset_Parametric
  IFCCOVERINGTYPE "Spray Foam Insulation - 100" | INSULATION | 2 occurrences | material: layers ("Spray Foam" 100.) | property sets: EPset_Parametric
  IFCWALLTYPE "FDW- 400mm" | ELEMENTEDWALL | 2 occurrences | material: layers ("Concrete" 400.) | property sets: EPset_Parametric
  IFCFOOTINGTYPE "SJCES - WF8" | STRIP_FOOTING | 2 occurrences | material: layers ("Concrete" 800.) | property sets: EPset_Parametric
  IFCCOVERINGTYPE "Foundation Wall Insulation - 50" | INSULATION | 3 occurrences | material: layers ("Rigid Insulation" 50.) | property sets: EPset_Parametric

Property sets
  EPset_Parametric | properties | on 16 objects (15 IFCWALL, 1 IFCCOVERING)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 15 objects (8 IFCCOVERING, 5 IFCWALL, 2 IFCFOOTING)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 9 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  EPset_Status | properties | on 4 objects (2 IFCFOOTING, 2 IFCWALL)
    Status in {"NEW"} (IFCLABEL)
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 5.59999990463257 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    IsExternal = TRUE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Flame 5 Smoke 135" (IFCLABEL)
    ThermalTransmittance = 5.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "https://www.insulfoam.com/rigid-foam-insulation-types/" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 5. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 5. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    Status in {"NEW"} (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 899.9999761581421, "overall_width": 600.0000238418579, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)