IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "merged.ifc"
Time stamp: "2023-04-21T12:01:51-05:00"
Preprocessor: "IfcOpenShell v0.7.0-476ab506d"
Originating system: "BlenderBIM 0.0.230330"
Authorization: "Nobody"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  4 x Person "ryan@openingdesign.com" of Organization (no name given)
  4 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1680878644 (2023-04-07T14:44:04Z)

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: square foot (conversion based)
  LENGTHUNIT: foot (conversion based)
  VOLUMEUNIT: cubic foot (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      contains 70 elements
        15 x IFCWALL | type IFCWALLTYPE "M358BØD_EX" | names: "Wall" | material: layers "existing" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Drawing
        18 x IFCWINDOW | type IFCWINDOWTYPE "Empty" | names: "Window" | material: profiles "existing" ("WINDOW") | property sets: EPset_Parametric, EPset_Drawing
        4 x IFCPLATE | type IFCPLATETYPE "Empty" | names: "Plate" | material: layers "existing" ("EXISTING STOREFRONT" 0.0416666679084301) | property sets: EPset_Parametric, EPset_Drawing
        1 x IFCDOOR | type IFCDOORTYPE "3070L-SF" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, EPset_Drawing, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "3070R-SF" | SINGLE_SWING_RIGHT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "21070R" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        2 x IFCDOOR | type IFCDOORTYPE "21070R" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Neufert Toilet with Cistern" | BATH | names: "Furniture.001"
        1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Generic Medium Sink" | BATH | names: "Furniture.002" | property sets: EPset_Drawing
        1 x IFCDOOR | type IFCDOORTYPE "3070L" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: EPset_Drawing, Pset_DoorCommon, Qto_DoorBaseQuantities
        2 x IFCDOOR | type IFCDOORTYPE "21070L" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "21070L" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "3070R" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "3070R" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCFURNITURE | BED | names: "Plane" | material: constituents "existing" () | property sets: EPset_Drawing
        2 x IFCFURNITURE | names: "Cube", "Plane" | property sets: Pset_FurnitureTypeCommon
        1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Neufert Medium Basin" | BATH | names: "Furniture"
        1 x IFCDOOR | type IFCDOORTYPE "3070L-SF" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        2 x IFCWALL | type IFCWALLTYPE "M6BØD" | names: "Wall" | material: layers "existing" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.5, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon
        1 x IFCSLAB | type IFCSLABTYPE "FLR150" | names: "Slab" | material: "SPACE" | property sets: EPset_Parametric, Qto_SlabBaseQuantities, EPset_Drawing
        5 x IFCWALL | type IFCWALLTYPE "M358BØD_DEMO" | names: "Wall" | material: layers "demolish" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, EPset_Drawing, Pset_WallCommon, Qto_WallBaseQuantities
        3 x IFCWALL | type IFCWALLTYPE "M358BØD" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Drawing
        3 x IFCWALL | type IFCWALLTYPE "EX" | names: "Wall" | material: layers "existing" ("Unknown" 0.416667014360428, "WINDOW" 0.416667014360428) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Drawing
        1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "ADA Grab Bars" | names: "SanitaryTerminal"
      IFCSPACE "110" | long name "STORAGE" | INTERNAL
      IFCSPACE "107" | long name "FITTING"
      IFCSPACE "105" | long name "STORAGE"
      IFCSPACE "102" | long name "CORRIDOR - BACK-OF-HOUSE"
      IFCSPACE "103" | long name "RESTROOM"
      IFCSPACE "108" | long name "FITTING"
      IFCSPACE "111" | long name "CORRIDOR" | INTERNAL
      IFCSPACE "101" | long name "REGISTER"
      IFCSPACE "104" | long name "STORAGE"
      IFCSPACE "106" | long name "DISPLAY AREA 2"
      IFCSPACE "109" | long name "STORAGE" | INTERNAL
      IFCSPACE "100" | long name "DISPLAY AREA 1" | INTERNAL
      IFCBUILDINGSTOREY "My Storey"
        contains 399 elements
          2 x IFCANNOTATION | type IFCTYPEPRODUCT "Material_Name_First_Item" | object type "TEXT_LEADER" | names: "Material_Name_First_Item"
          397 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "Continuous Angle1:Continuous Angle:1463390", "Continuous Angle2:Continuous Angle:1578039", "Continuous Angle3:Continuous Angle:1578050" (+394 more) | material: constituents "concrete" (); "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)"; "METAL RUNNER CHANNEL; FASTEN @ 24" O.C."; "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL"; "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL"; "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC" | property sets: EPset_Drawing

Types
  IFCWALLTYPE "M358BØD_EX" | STANDARD | 15 occurrences | material: layers "existing" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWINDOWTYPE "Empty" | WINDOW | 18 occurrences | material: profiles "existing" ("WINDOW")
  IFCPLATETYPE "Empty" | CURTAIN_PANEL | 4 occurrences | material: layers "existing" ("EXISTING STOREFRONT" 0.0416666679084301)
  IFCDOORTYPE "3070L-SF" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCDOORTYPE "3070R-SF" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCDOORTYPE "21070R" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCFURNITURETYPE "Neufert Toilet with Cistern" | 1 occurrence | property sets: EPset_Drawing
  IFCFURNITURETYPE "Generic Medium Sink" | 1 occurrence | property sets: EPset_Drawing
  IFCDOORTYPE "3070L" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing, OD_DoorType_Hackjob | description "WOOD FLUSH W/ HM FRAME"
  IFCDOORTYPE "21070L" | DOOR | SINGLE_SWING_LEFT | 3 occurrences | property sets: BBIM_Door
  IFCDOORTYPE "3070R" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing, OD_DoorType_Hackjob | description "WOOD FLUSH W/ HM FRAME"
  IFCFURNITURETYPE "Neufert Medium Basin" | 1 occurrence
  IFCWALLTYPE "M6BØD" | STANDARD | 2 occurrences | material: layers "existing" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.5, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon | description "5/8 GYP - 6 METAL(BATT) - 5/8 GYP"
  IFCSLABTYPE "FLR150" | 1 occurrence | material: layers ("Unknown" 0.656167979002625)
  IFCWALLTYPE "M358BØD_DEMO" | STANDARD | 5 occurrences | material: layers "demolish" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWALLTYPE "M358BØD" | STANDARD | 3 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWALLTYPE "EX" | 3 occurrences | material: layers "existing" ("Unknown" 0.416667014360428, "WINDOW" 0.416667014360428) | description "GENERIC EXTERIOR"
  IFCSANITARYTERMINALTYPE "ADA Grab Bars" | element type "GRAB_BARS" | USERDEFINED | 1 occurrence | property sets: EPset_Drawing
  IFCTYPEPRODUCT "Material_Name_First_Item" | 2 occurrences | property sets: EPset_Drawing

Property sets
  EPset_Parametric | properties | on 28 objects (28 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 18 objects (18 IFCWINDOW)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 5 objects (4 IFCPLATE, 1 IFCSLAB)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  Pset_DoorCommon | properties | on 9 objects (9 IFCDOOR)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    Status in {"NEW"} (IFCLABEL)
  Pset_WallCommon | properties | on 19 objects (19 IFCWALL)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_WallCommon | properties | on 5 objects (5 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    Status in {"NEW"} (IFCLABEL)
  Pset_WallCommon | properties | on 1 type object
    Status in {"EXISTING"} (IFCLABEL)
    ThermalTransmittance (no value)
  EPset_Drawing | properties | on 39 objects (10 IFCANNOTATION, 7 IFCWALL, 7 IFCWINDOW, 4 IFCPLATE) | on 9 type objects
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/96" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "material.Category" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/4" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    Exclude = ".IfcElement[r"Pset_.*Common"."Status"="NEW"]" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "r"Pset_.*Common"" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/96" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    Exclude = ".IfcElement[r"Pset_.*Common"."Status"="DEMOLISH"]" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    ImperialPrecision = "1/4" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "Pset_WallCommon.Status | Pset_DoorCommon.Status" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/48" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = TRUE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/96" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    Include = ".IfcElement[r"Pset_.*Common"."Status"="NEW"]" (IFCTEXT)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/48" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    Include = ".IfcElement[r"Pset_.*Common"."Status"="DEMOLISH"]" (IFCTEXT)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/48" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing: 1 more content on 1 objects not shown
  EPset_Annotation | properties | on 11 objects (11 IFCANNOTATION)
    Classes = "oblique" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 1 object (1 IFCFURNITURE)
    Status in {"NEW"} (IFCLABEL)
  Qto_DoorBaseQuantities | quantities | on 4 objects (4 IFCDOOR)
    Area = 2.614 [square foot (conversion based)]
    Height = 2.197 [foot (conversion based)]
    Perimeter = 6.375 [foot (conversion based)]
    Width = 0.991 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 3 objects (3 IFCDOOR)
    Area = 2.173 [square foot (conversion based)]
    Height = 2.134 [foot (conversion based)]
    Perimeter = 6.299 [foot (conversion based)]
    Width = 1.016 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 2 objects (2 IFCDOOR)
    Area = 2.729 [square foot (conversion based)]
    Height = 84. [foot (conversion based)]
    Perimeter = 6.477 [foot (conversion based)]
    Width = 36. [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 2.729 [square foot (conversion based)]
    Height = 2.197 [foot (conversion based)]
    Perimeter = 6.477 [foot (conversion based)]
    Width = 1.041 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 0. [square foot (conversion based)]
    Height = 0. [foot (conversion based)]
    Perimeter = 1.975 [foot (conversion based)]
    Width = 0.987 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.66 [foot (conversion based)]
    GrossArea = 130.89 [square foot (conversion based)]
    GrossVolume = 26.18 [cubic foot (conversion based)]
    NetArea = 130.89 [square foot (conversion based)]
    NetVolume = 26.18 [cubic foot (conversion based)]
    Perimeter = 48.87 [foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 2 objects (2 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 47.424 [square foot (conversion based)]
    GrossFloorArea = 47.424 [square foot (conversion based)]
    GrossPerimeter = 28.217 [foot (conversion based)]
    GrossVolume = 466.767 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 47.424 [square foot (conversion based)]
    NetFloorArea = 47.424 [square foot (conversion based)]
    NetVolume = 466.767 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 99.597 [square foot (conversion based)]
    GrossFloorArea = 99.597 [square foot (conversion based)]
    GrossPerimeter = 40.374 [foot (conversion based)]
    GrossVolume = 980.287 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 99.597 [square foot (conversion based)]
    NetFloorArea = 99.597 [square foot (conversion based)]
    NetVolume = 980.287 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 34.309 [square foot (conversion based)]
    GrossFloorArea = 34.309 [square foot (conversion based)]
    GrossPerimeter = 23.447 [foot (conversion based)]
    GrossVolume = 337.685 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 34.309 [square foot (conversion based)]
    NetFloorArea = 34.309 [square foot (conversion based)]
    NetVolume = 337.685 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 10.609 [square foot (conversion based)]
    GrossFloorArea = 10.609 [square foot (conversion based)]
    GrossPerimeter = 13.656 [foot (conversion based)]
    GrossVolume = 104.423 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 10.609 [square foot (conversion based)]
    NetFloorArea = 10.609 [square foot (conversion based)]
    NetVolume = 104.423 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 103.345 [square foot (conversion based)]
    GrossFloorArea = 103.345 [square foot (conversion based)]
    GrossPerimeter = 48.665 [foot (conversion based)]
    GrossVolume = 1017.179 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 103.345 [square foot (conversion based)]
    NetFloorArea = 103.345 [square foot (conversion based)]
    NetVolume = 1017.179 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 44.285 [square foot (conversion based)]
    GrossFloorArea = 44.285 [square foot (conversion based)]
    GrossPerimeter = 26.671 [foot (conversion based)]
    GrossVolume = 435.875 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 44.285 [square foot (conversion based)]
    NetFloorArea = 44.285 [square foot (conversion based)]
    NetVolume = 435.875 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 140.281 [square foot (conversion based)]
    GrossFloorArea = 140.281 [square foot (conversion based)]
    GrossPerimeter = 73.518 [foot (conversion based)]
    GrossVolume = 1380.721 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 140.281 [square foot (conversion based)]
    NetFloorArea = 140.281 [square foot (conversion based)]
    NetVolume = 1380.721 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 130.76 [square foot (conversion based)]
    GrossFloorArea = 130.76 [square foot (conversion based)]
    GrossPerimeter = 45.749 [foot (conversion based)]
    GrossVolume = 1287.006 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 130.76 [square foot (conversion based)]
    NetFloorArea = 130.76 [square foot (conversion based)]
    NetVolume = 1287.006 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities: 3 more contents on 3 objects not shown
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Height = 84. [foot (conversion based)]
    Width = 36. [foot (conversion based)]
  BBIM_Dimension | properties | on 1 object (1 IFCANNOTATION)
    ShowDescriptionOnly = TRUE (IFCBOOLEAN)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 7.0, "overall_width": 3.3333332538604736, "lining_properties": {"lining_depth": 0.3333333432674408, "lining_thickness": 0.1666666716337204, "lining_offset": 0.32999998331069946, "lining_to_panel_offset_x": 0.1666666716337204, "lining_to_panel_offset_y": 0.08202099800109863, "transom_thickness": 0.0, "threshold_thickness": 0.08202099800109863, "threshold_depth": 0.32808399200439453, "threshold_offset": 0.32999998331069946}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0, "overall_width": 3.3333332538604736, "lining_properties": {"lining_depth": 0.3333333432674408, "lining_thickness": 0.1666666716337204, "lining_offset": 0.3333333432674408, "lining_to_panel_offset_x": 0.1666666716337204, "lining_to_panel_offset_y": 0.08202099800109863, "transom_thickness": 0.0, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0625, "overall_width": 2.958329916000366, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 7.0625, "overall_width": 3.125, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 7.0625, "overall_width": 2.958329916000366, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0625, "overall_width": 3.125, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  OD_DoorType_Hackjob | properties | on 2 type objects
    DoorHeight = "7' - 0"" (IFCTEXT)
    DoorWidth = "3' - 0"" (IFCTEXT)
    TypeComments = "MATCH EXISTING (HEIGHT, MATERIAL/FINISH, HARDWARE)" (IFCTEXT)