IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[SteelFabricationView]"
File name: "nclous_IFCexport.ifc"
Time stamp: "2023-11-22T03:13:16"
Organization: "ACCDEF Fabrications"
Preprocessor: "IFC Toolkit 2.0.26.0"
Originating system: "Advance Steel 2023"
Application: "Advance Steel" version "2023" identifier "Autodesk.Advance Steel" by Organization "Autodesk"

People and organizations
  Person "C. Monkey" "C. Monkey" of Organization (no name given)
  Owner history of Person "C. Monkey" "C. Monkey" of Organization (no name given) | application "Advance Steel" version "2023" identifier "Autodesk.Advance Steel" by Organization "Autodesk" | state READWRITE | change ADDED | created 1700622796 (2023-11-22T03:13:16Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "SYSDEF / Graitec Demo"
  IFCSITE "SYSDEF / Graitec Demo"
    IFCBUILDING "Structure 1"
      IFCBUILDINGSTOREY "01 Concrete" | elevation 0.
        contains 4 elements
          4 x IFCELEMENTASSEMBLY | object type "Steel Assembly" | FACTORY | parts: 4 IFCPLATE | property sets: AISC_EM11_Pset_PieceIdentification, AISC_EM11_Pset_VersionInformation, AISC_EM11_Pset_SchedulingInformation, AISC_EM11_Pset_ToleranceForLayout, AISC_EM11_Pset_StatusInformation
      IFCBUILDINGSTOREY "02 Masonry" | elevation 0.
        contains 1 element
          1 x IFCELEMENTASSEMBLY | object type "Steel Assembly" | FACTORY | parts: 2 IFCFASTENER, 1 IFCDISCRETEACCESSORY, 1 IFCPLATE | property sets: AISC_EM11_Pset_PieceIdentification, AISC_EM11_Pset_VersionInformation, AISC_EM11_Pset_SchedulingInformation, AISC_EM11_Pset_ToleranceForLayout, AISC_EM11_Pset_StatusInformation
      IFCBUILDINGSTOREY "03 Billboard" | elevation 0.
        contains 71 elements
          66 x IFCELEMENTASSEMBLY | object type "Steel Assembly" | FACTORY | parts: 523 IFCFASTENER, 296 IFCDISCRETEACCESSORY, 42 IFCPLATE, 17 IFCBEAM, 7 IFCCOLUMN | property sets: AISC_EM11_Pset_PieceIdentification, AISC_EM11_Pset_VersionInformation, AISC_EM11_Pset_SchedulingInformation, AISC_EM11_Pset_ToleranceForLayout, AISC_EM11_Pset_StatusInformation
          3 x IFCDISCRETEACCESSORY | object type "Bar" | names: "Bar" | descriptions: "RMS12", "RMS16", "RMS20" | property sets: AISC_EM11_Pset_PieceIdentification, AISC_EM11_Pset_ToleranceForLayout, AISC_EM11_Pset_StatusInformation, AISC_EM11_Pset_VersionInformation, AISC_EM11_Pset_SurfaceTreatment
          2 x IFCDISCRETEACCESSORY | object type "Handrail_Post" | names: "Handrail_Post" | descriptions: "EA 65x65x6" | property sets: AISC_EM11_Pset_PieceIdentification, AISC_EM11_Pset_ToleranceForLayout, AISC_EM11_Pset_StatusInformation, AISC_EM11_Pset_VersionInformation, AISC_EM11_Pset_SurfaceTreatment
    IFCBUILDING "Structure 2"
      IFCBUILDINGSTOREY "Default Storey" | elevation 0.
        contains 105 elements
          1 x IFCMECHANICALFASTENER | object type "Anchor_Bolt" | property sets: AISC_EM11_Pset_Bolt, AISC_EM11_Pset_SurfaceTreatment
          87 x IFCMECHANICALFASTENER | object type "Bolt" | property sets: AISC_EM11_Pset_Bolt, AISC_EM11_Pset_SurfaceTreatment
          7 x IFCFASTENER | object type "Weld" | property sets: AISC_EM11_Pset_Weld
          10 x IFCGRID

Property sets
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "ANG-0301" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1075. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BRK-0304" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1199.998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BE-0307" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 923.997171572876 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BE-0409" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4074.00066974788 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BE-0409" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4073.97645078859 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BE-0224" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 7939.998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BE-0306" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8137.998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BE-0403" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 984.998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon: 3 more contents on 3 objects not shown
  AISC_EM11_Pset_PieceIdentification | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    BarCode = "" (IFCIDENTIFIER)
    IndicationMark = "" (IFCIDENTIFIER)
    MainPieceTag = FALSE (IFCBOOLEAN)
    PieceMark = "CL-0203" (IFCIDENTIFIER)
    PrelimMark = "2" (IFCIDENTIFIER)
  AISC_EM11_Pset_PieceIdentification | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    BarCode = "" (IFCIDENTIFIER)
    IndicationMark = "" (IFCIDENTIFIER)
    MainPieceTag = FALSE (IFCBOOLEAN)
    PieceMark = "CL-0202" (IFCIDENTIFIER)
    PrelimMark = "2" (IFCIDENTIFIER)
  AISC_EM11_Pset_PieceIdentification | properties | on 16 objects (16 IFCDISCRETEACCESSORY)
    BarCode = "" (IFCIDENTIFIER)
    IndicationMark = "" (IFCIDENTIFIER)
    MainPieceTag = FALSE (IFCBOOLEAN)
    PieceMark = "CL-0202" (IFCIDENTIFIER)
    PrelimMark = "7" (IFCIDENTIFIER)
  AISC_EM11_Pset_PieceIdentification | properties | on 10 objects (10 IFCDISCRETEACCESSORY)
    BarCode = "" (IFCIDENTIFIER)
    IndicationMark = "" (IFCIDENTIFIER)
    MainPieceTag = FALSE (IFCBOOLEAN)
    PieceMark = "CL-0304" (IFCIDENTIFIER)
    PrelimMark = "2" (IFCIDENTIFIER)
  AISC_EM11_Pset_PieceIdentification | properties | on 8 objects (8 IFCDISCRETEACCESSORY)
    BarCode = "" (IFCIDENTIFIER)
    IndicationMark = "" (IFCIDENTIFIER)
    MainPieceTag = FALSE (IFCBOOLEAN)
    PieceMark = "CL-0205" (IFCIDENTIFIER)
    PrelimMark = "7" (IFCIDENTIFIER)
  AISC_EM11_Pset_PieceIdentification | properties | on 4 objects (4 IFCDISCRETEACCESSORY)
    BarCode = "" (IFCIDENTIFIER)
    IndicationMark = "" (IFCIDENTIFIER)
    MainPieceTag = FALSE (IFCBOOLEAN)
    PieceMark = "CL-0306" (IFCIDENTIFIER)
    PrelimMark = "2" (IFCIDENTIFIER)
  AISC_EM11_Pset_PieceIdentification | properties | on 4 objects (4 IFCDISCRETEACCESSORY)
    BarCode = "" (IFCIDENTIFIER)
    IndicationMark = "" (IFCIDENTIFIER)
    MainPieceTag = FALSE (IFCBOOLEAN)
    PieceMark = "CL-0307" (IFCIDENTIFIER)
    PrelimMark = "2" (IFCIDENTIFIER)
  AISC_EM11_Pset_PieceIdentification | properties | on 2 objects (2 IFCDISCRETEACCESSORY)
    BarCode = "" (IFCIDENTIFIER)
    IndicationMark = "" (IFCIDENTIFIER)
    MainPieceTag = FALSE (IFCBOOLEAN)
    PieceMark = "CL-0411" (IFCIDENTIFIER)
    PrelimMark = "1" (IFCIDENTIFIER)
  AISC_EM11_Pset_PieceIdentification: 366 more contents on 368 objects not shown
  AISC_EM11_Pset_ToleranceForLayout | properties | on 444 objects (302 IFCDISCRETEACCESSORY, 71 IFCELEMENTASSEMBLY, 47 IFCPLATE, 17 IFCBEAM)
    LayoutTolerance = 0.001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  AISC_EM11_Pset_StatusInformation | properties | on 444 objects (302 IFCDISCRETEACCESSORY, 71 IFCELEMENTASSEMBLY, 47 IFCPLATE, 17 IFCBEAM)
    ChangeStatus in {"Default"} (IFCLABEL)
    Status in {"Default"} (IFCLABEL)
    StatusApproved = TRUE (IFCBOOLEAN)
  AISC_EM11_Pset_VersionInformation | properties | on 444 objects (302 IFCDISCRETEACCESSORY, 71 IFCELEMENTASSEMBLY, 47 IFCPLATE, 17 IFCBEAM)
    VersionNumber = "" (IFCIDENTIFIER)
  AISC_EM11_Pset_SurfaceTreatment | properties | on 327 objects (301 IFCDISCRETEACCESSORY, 11 IFCBEAM, 8 IFCPLATE, 7 IFCCOLUMN)
    SequentialOrder = ["Hot Dipped Galv"] (IFCIDENTIFIER)
  AISC_EM11_Pset_SurfaceTreatment | properties | on 87 objects (87 IFCMECHANICALFASTENER)
    SequentialOrder = ["Galvanised"] (IFCIDENTIFIER)
  AISC_EM11_Pset_SurfaceTreatment | properties | on 39 objects (33 IFCPLATE, 6 IFCBEAM)
    SequentialOrder = ["Powder Coated"] (IFCIDENTIFIER)
  AISC_EM11_Pset_SurfaceTreatment | properties | on 5 objects (5 IFCPLATE)
    SequentialOrder = ["None"] (IFCIDENTIFIER)
  AISC_EM11_Pset_SurfaceTreatment | properties | on 2 objects (1 IFCDISCRETEACCESSORY, 1 IFCPLATE)
    SequentialOrder = ["Painted"] (IFCIDENTIFIER)
  AISC_EM11_Pset_SurfaceTreatment | properties | on 1 object (1 IFCMECHANICALFASTENER)
    SequentialOrder = ["Hot Dip Galvanized"] (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "COL-0407" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "COL-0308" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "HR-0401" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "COL-0215" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "COL-0319" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "COL-0417" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_PlateCommon | properties | on 4 objects (4 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MSH-0301" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_PlateCommon | properties | on 4 objects (4 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MSH-0302" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_PlateCommon | properties | on 4 objects (4 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "PL-0403" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MSH-0303" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MSH-0305" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MSH-0306" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MSH-0307" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MSH-0308" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_PlateCommon: 23 more contents on 25 objects not shown
  AISC_EM11_Pset_Bolt | properties | on 46 objects (46 IFCMECHANICALFASTENER)
    BoltDiameter = 12. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltFieldAssembled = TRUE (IFCBOOLEAN)
    BoltGrade = ["8.8"] (IFCIDENTIFIER)
    BoltLength = 38. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltStandard = "BS 3692" (IFCIDENTIFIER)
    BoltType = "SET SCREW" (IFCIDENTIFIER)
  AISC_EM11_Pset_Bolt | properties | on 12 objects (12 IFCMECHANICALFASTENER)
    BoltDiameter = 20. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltFieldAssembled = TRUE (IFCBOOLEAN)
    BoltGrade = ["8.8"] (IFCIDENTIFIER)
    BoltLength = 60. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltStandard = "AS 4100" (IFCIDENTIFIER)
    BoltType = "AS 1252" (IFCIDENTIFIER)
  AISC_EM11_Pset_Bolt | properties | on 8 objects (8 IFCMECHANICALFASTENER)
    BoltDiameter = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltFieldAssembled = TRUE (IFCBOOLEAN)
    BoltGrade = ["8.8"] (IFCIDENTIFIER)
    BoltLength = 90. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltStandard = "AS 4100" (IFCIDENTIFIER)
    BoltType = "AS 1252" (IFCIDENTIFIER)
  AISC_EM11_Pset_Bolt | properties | on 7 objects (7 IFCMECHANICALFASTENER)
    BoltDiameter = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltFieldAssembled = TRUE (IFCBOOLEAN)
    BoltGrade = ["8.8"] (IFCIDENTIFIER)
    BoltLength = 45. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltStandard = "AS 4100" (IFCIDENTIFIER)
    BoltType = "AS 1252" (IFCIDENTIFIER)
  AISC_EM11_Pset_Bolt | properties | on 4 objects (4 IFCMECHANICALFASTENER)
    BoltDiameter = 12. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltFieldAssembled = TRUE (IFCBOOLEAN)
    BoltGrade = ["8.8"] (IFCIDENTIFIER)
    BoltLength = 90. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltStandard = "AS 4100" (IFCIDENTIFIER)
    BoltType = "AS 1252" (IFCIDENTIFIER)
  AISC_EM11_Pset_Bolt | properties | on 4 objects (4 IFCMECHANICALFASTENER)
    BoltDiameter = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltFieldAssembled = TRUE (IFCBOOLEAN)
    BoltGrade = ["8.8"] (IFCIDENTIFIER)
    BoltLength = 140. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltStandard = "AS 4100" (IFCIDENTIFIER)
    BoltType = "AS 1252" (IFCIDENTIFIER)
  AISC_EM11_Pset_Bolt | properties | on 2 objects (2 IFCMECHANICALFASTENER)
    BoltDiameter = 20. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltFieldAssembled = TRUE (IFCBOOLEAN)
    BoltGrade = ["8.8"] (IFCIDENTIFIER)
    BoltLength = 170. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltStandard = "AS 4100" (IFCIDENTIFIER)
    BoltType = "AS 1252" (IFCIDENTIFIER)
  AISC_EM11_Pset_Bolt | properties | on 2 objects (2 IFCMECHANICALFASTENER)
    BoltDiameter = 20. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltFieldAssembled = TRUE (IFCBOOLEAN)
    BoltGrade = ["8.8"] (IFCIDENTIFIER)
    BoltLength = 55. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BoltStandard = "AS 4100" (IFCIDENTIFIER)
    BoltType = "AS 1252" (IFCIDENTIFIER)
  AISC_EM11_Pset_Bolt: 3 more contents on 3 objects not shown
  AISC_EM11_Pset_Weld | properties | on 530 objects (530 IFCFASTENER)
    FieldWeld = FALSE (IFCBOOLEAN)
    ProcessName = "" (IFCLABEL)
    Type1 = "Fillet Weld" (IFCLABEL)
    WeldDescription = "Weld" (IFCLABEL)
    a = 0. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    l = 0. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    s = 6. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  AISC_EM11_Pset_Weld | properties | on 2 objects (2 IFCFASTENER)
    FieldWeld = FALSE (IFCBOOLEAN)
    ProcessName = "" (IFCLABEL)
    Type1 = "None" (IFCLABEL)
    WeldDescription = "Weld" (IFCLABEL)
    a = 0. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    l = 0. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    s = 6. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  AISC_EM11_Pset_SchedulingInformation | properties | on 71 objects (71 IFCELEMENTASSEMBLY)
    OnSiteBy (no value)
    PhaseSequenceID = "" (IFCIDENTIFIER)
    SequenceLevel = "" (IFCIDENTIFIER)