IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "Project Number"
Time stamp: "2022-10-18T08:02:35"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "jure.cesnik" of Organization (no name given)
  Owner history of Person "jure.cesnik" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1666072955 (2022-10-18T06:02:35Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.804504″ | longitude -71° 1′ 58.789672″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 4 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:413951", "Basic Wall:Generic - 200mm:413953", "Basic Wall:Generic - 200mm:413955" (+1 more) | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing

Types
  IFCWALLTYPE "Basic Wall:Generic - 200mm" | STANDARD | 4 occurrences | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading

Property sets
  BaseQuantities | quantities | on 3 objects (3 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 2.98 [SQUARE_METRE]
    Height = 2700. [MILLI METRE]
    Length = 14900. [MILLI METRE]
    NetSideArea = 40.23 [SQUARE_METRE]
    NetSideArea = 40230000. [SQUARE_METRE]
    NetVolume = 8.04599999999999 [CUBIC_METRE]
    NetVolume = 8046000000. [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 2.98 [SQUARE_METRE]
    Height = 2700. [MILLI METRE]
    Length = 14900. [MILLI METRE]
    NetSideArea = 40.23 [SQUARE_METRE]
    NetSideArea = 40230000. [SQUARE_METRE]
    NetVolume = 8.04599999999997 [CUBIC_METRE]
    NetVolume = 8046000000. [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  Constraints | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = -3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 1" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = TRUE (IFCBOOLEAN)
    Unconnected Height = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    Area = 40.23 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 14900. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 8.04599999999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 40.23 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 14900. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 8.04599999999997 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Comments = "" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Generic - 200mm" (IFCTEXT)
  Other | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Family and Type = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type Id = "Basic Wall: Generic - 200mm" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Walls" (IFCLABEL)
    Family Name = "Basic Wall" (IFCTEXT)
  Phasing | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Structural = TRUE (IFCBOOLEAN)
    Structural Usage = "Bearing" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Roughness = 914.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Generic - 200mm" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Generic - 200mm" (IFCLABEL)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Generic - 200mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic - 200mm" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Graphics | properties | on 1 type object
    Coarse Scale Fill Color = 0 (IFCINTEGER)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"