IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "2321-01-ODM-Z1-01-M3-A-0003_AscensionSHS.ifc"
Time stamp: "2023-06-13T08:31:37+00:00"
Preprocessor: "IfcOpenShell (HEAD detached at 8f41ae0c1)-8f41ae0c1"
Originating system: "BlenderBIM 0.0.230601"
Authorization: "Nobody"

Units
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: degree (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "FOUNDATION"
        contains 72 elements
          9 x IFCWALL | type IFCWALLTYPE "FND150_CRX" | names: "WAL200" | material: layers "WALL_FND_1LYR_CRX" ("Sandcrete" 150.) | property sets: EPset_Parametric
          1 x IFCWALL | type IFCWALLTYPE "FND150_CRX" | SOLIDWALL | names: "SLD150" | descriptions: "Masonry wall rendered and painted" | material: layers "WALL_FND_1LYR_CRX" ("Sandcrete" 150.) | property sets: EPset_Parametric
          10 x IFCFOOTING | type IFCFOOTINGTYPE "FTG450x150" | STRIP_FOOTING | names: "FLR150", "FLR150.002", "FLR150.003" (+6 more) | material: layers "WALL_FND_FTG_1LYR" ("Mass Concrete" 150.) | property sets: EPset_Parametric
          2 x IFCFOOTING | type IFCFOOTINGTYPE "FTG450x150" | names: "FTG450x150" | material: layers "WALL_FND_FTG_1LYR" ("Mass Concrete" 150.)
          22 x IFCCOLUMN | type IFCCOLUMNTYPE "C1" | names: "C1" | material: profiles "RC_COL_150x150" ("Square Column": "Mass Concrete") | property sets: EPset_Parametric
          2 x IFCSLAB | type IFCSLABTYPE "FLR150" | names: "FLR150" | material: layers ("Mass Concrete" 150.)
          2 x IFCSLAB | type IFCSLABTYPE "FLR_150" | names: "FLR_150" | material: layers "FTG_COL_2LYR" ("Mass Concrete" 150., "Light Concrete" 50.)
          3 x IFCSLAB | type IFCSLABTYPE "FLR_150" | names: "FLR250" | material: layers "FTG_COL_1LYR" ("Mass Concrete" 150.) | property sets: EPset_Parametric
          21 x IFCFOOTING | type IFCSLABTYPE "FLR_150" | PAD_FOOTING | names: "FLR250.001", "FLR250.002", "FLR250.003" (+18 more) | material: layers "FTG_COL_1LYR" ("Mass Concrete" 150.) | property sets: EPset_Parametric, Qto_FootingBaseQuantities
      IFCBUILDINGSTOREY "GROUND FLOOR"
        contains 76 elements
          11 x IFCWALL | type IFCWALLTYPE "WAL200" | names: "WAL200" | material: layers ("Sandcrete" 200.) | property sets: EPset_Parametric
          18 x IFCWALL | type IFCWALLTYPE "WAL100" | names: "WAL100" | material: layers ("Sandcrete" 100.) | property sets: EPset_Parametric
          1 x IFCSLAB | type IFCSLABTYPE "FLR150" | names: "FLR150" | material: layers ("Mass Concrete" 150.) | property sets: EPset_Parametric
          1 x IFCDOOR | type IFCDOORTYPE "DT01" | SINGLE_SWING_LEFT | names: "DT01" | property sets: BBIM_Door
          9 x IFCDOOR | type IFCDOORTYPE "DT01" | names: "DT02", "DT01"
          10 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | names: "Neufert Toilet with Cistern"
          10 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Shower 75x90" | names: "Neufert Shower 75x90"
          8 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Small Basin" | names: "Generic Small Sink", "Neufert Small Basin"
          2 x IFCDOOR | type IFCDOORTYPE "DT02" | names: "DT02"
          6 x IFCWINDOW | type IFCWINDOWTYPE "WT01" | names: "WT01"

Types
  IFCWALLTYPE "FND150_CRX" | SOLIDWALL | 10 occurrences | material: layers "WALL_FND_1LYR_CRX" ("Sandcrete" 150.) | property sets: EPset_Parametric | description "Wall for foundation with exterior paint"
  IFCFOOTINGTYPE "FTG450x150" | STRIP_FOOTING | 12 occurrences | material: layers "WALL_FND_FTG_1LYR" ("Mass Concrete" 150.) | property sets: EPset_Parametric
  IFCCOLUMNTYPE "C1" | 22 occurrences | material: profiles "RC_COL_150x150" ("Square Column": "Mass Concrete")
  IFCSLABTYPE "FLR150" | 3 occurrences | material: layers ("Mass Concrete" 150.)
  IFCSLABTYPE "FLR_150" | 2 occurrences | material: layers "FTG_COL_2LYR" ("Mass Concrete" 150., "Light Concrete" 50.)
  IFCSLABTYPE "FLR_150" | 24 occurrences | material: layers "FTG_COL_1LYR" ("Mass Concrete" 150.)
  IFCWALLTYPE "WAL200" | 11 occurrences | material: layers ("Sandcrete" 200.)
  IFCWALLTYPE "WAL100" | 18 occurrences | material: layers ("Sandcrete" 100.)
  IFCDOORTYPE "DT01" | 10 occurrences
  IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | 10 occurrences
  IFCSANITARYTERMINALTYPE "Neufert Shower 75x90" | 10 occurrences
  IFCSANITARYTERMINALTYPE "Neufert Small Basin" | 8 occurrences
  IFCDOORTYPE "DT02" | DOOR | SINGLE_SWING_LEFT | 2 occurrences | property sets: BBIM_Door
  IFCWINDOWTYPE "WT01" | 6 occurrences

Property sets
  EPset_Parametric | properties | on 39 objects (39 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 35 objects (31 IFCFOOTING, 4 IFCSLAB)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 21 objects (21 IFCCOLUMN)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS2" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS3" (IFCLABEL)
  BBIM_Door | properties | on 1 object (1 IFCDOOR)
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2100.0, "overall_width": 750.0, "lining_properties": {"lining_depth": 50.0, "lining_thickness": 50.0, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.0, "lining_to_panel_offset_y": 25.0, "transom_thickness": 0.0, "casing_thickness": 75.0, "casing_depth": 5.0, "threshold_thickness": 25.0, "threshold_depth": 100.0, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.0, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2100.0, "overall_width": 900.0, "lining_properties": {"lining_depth": 50.0, "lining_thickness": 50.0, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.0, "lining_to_panel_offset_y": 25.0, "transom_thickness": 0.0, "casing_thickness": 75.0, "casing_depth": 5.0, "threshold_thickness": 25.0, "threshold_depth": 100.0, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.0, "panel_width_ratio": 1.0}}" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1:100" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/100" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 0.36 [SQUARE_METRE]
    GrossSurfaceArea = 1.08 [SQUARE_METRE]
    GrossVolume = 0.054 [CUBIC_METRE]
    Height = 150. [MILLI METRE]
    Length = 600. [MILLI METRE]
    NetVolume = 0.054 [CUBIC_METRE]
    OuterSurfaceArea = 0.9 [SQUARE_METRE]
    Width = 600. [MILLI METRE]