IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2023-11-13T20:42:28"
Preprocessor: "IfcOpenShell v0.7.0-6c9e130ca"
Originating system: "IfcOpenShell v0.7.0-6c9e130ca"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 11 elements
          5 x IFCPLATE | type IFCPLATETYPE "t18" | SHEET | names: "Sheet 536×1000", "Sheet 500×1000", "Sheet 500×500" | material: layers ("Timber" 18.)
          1 x IFCBUILDINGELEMENTPART | type IFCBUILDINGELEMENTPARTTYPE "Insulation250" | INSULATION | names: "Insulation 250" | material: layers ("Rockwool" 250.)
          2 x IFCELEMENTASSEMBLY | type IFCELEMENTASSEMBLYTYPE "Sub-Assembly" | ACCESSORY_ASSEMBLY | names: "Sub-Assembly" | parts: 10 IFCPLATE, 2 IFCBUILDINGELEMENTPART
          1 x IFCSLAB | type IFCSLABTYPE "Concrete100" | BASESLAB | names: "Slab 100" | material: layers ("Concrete" 100.)
          2 x IFCELEMENTASSEMBLY | type IFCELEMENTASSEMBLYTYPE "Assembly" | ACCESSORY_ASSEMBLY | names: "Assembly" | parts: 4 IFCELEMENTASSEMBLY, 2 IFCSLAB
IFCELEMENTASSEMBLYTYPE "Sub-Assembly" | ACCESSORY_ASSEMBLY
  IFCPLATE "Sheet 536×1000" | SHEET
  IFCPLATE "Sheet 500×1000" | SHEET
  IFCPLATE "Sheet 500×1000" | SHEET
  IFCPLATE "Sheet 500×500" | SHEET
  IFCPLATE "Sheet 500×500" | SHEET
  IFCBUILDINGELEMENTPART "Insulation 250" | INSULATION
IFCELEMENTASSEMBLYTYPE "Assembly" | ACCESSORY_ASSEMBLY
  IFCELEMENTASSEMBLY "Sub-Assembly" | ACCESSORY_ASSEMBLY
    IFCPLATE "Sheet 536×1000" | SHEET
    IFCPLATE "Sheet 500×1000" | SHEET
    IFCPLATE "Sheet 500×1000" | SHEET
    IFCPLATE "Sheet 500×500" | SHEET
    IFCPLATE "Sheet 500×500" | SHEET
    IFCBUILDINGELEMENTPART "Insulation 250" | INSULATION
  IFCELEMENTASSEMBLY "Sub-Assembly" | ACCESSORY_ASSEMBLY
    IFCPLATE "Sheet 536×1000" | SHEET
    IFCPLATE "Sheet 500×1000" | SHEET
    IFCPLATE "Sheet 500×1000" | SHEET
    IFCPLATE "Sheet 500×500" | SHEET
    IFCPLATE "Sheet 500×500" | SHEET
    IFCBUILDINGELEMENTPART "Insulation 250" | INSULATION
  IFCSLAB "Slab 100" | BASESLAB

Types
  IFCPLATETYPE "t18" | SHEET | 5 occurrences | material: layers ("Timber" 18.) | property sets: EPset_Parametric
  IFCBUILDINGELEMENTPARTTYPE "Insulation250" | INSULATION | 1 occurrence | material: layers ("Rockwool" 250.) | property sets: EPset_Parametric
  IFCELEMENTASSEMBLYTYPE "Sub-Assembly" | ACCESSORY_ASSEMBLY | 2 occurrences
  IFCSLABTYPE "Concrete100" | BASESLAB | 1 occurrence | material: layers ("Concrete" 100.) | property sets: EPset_Parametric
  IFCELEMENTASSEMBLYTYPE "Assembly" | ACCESSORY_ASSEMBLY | 2 occurrences

Property sets
  EPset_Parametric | properties | on 3 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)