IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "baie dankie.ifc"
Time stamp: "2024-02-20T14:35:50+01:00"
Preprocessor: "IfcOpenShell v0.7.0-6c9e130ca"
Originating system: "BlenderBIM 0.0.231104-4e76f36"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCBUILDING "Empty"
    IFCBUILDINGSTOREY "Empty"
      contains 72 elements
        1 x IFCFURNITURE | type IFCFURNITURETYPE "2 seater" | names: "Furniture"
        1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Double Basin" | names: "Double Basin"
        1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Single basin" | SINK | names: "Single Basin"
        1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Sink" | names: "SanitaryTerminal"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "3 seater" | names: "Furniture"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "1 seat" | names: "Furniture"
        2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Toilet" | names: "SanitaryTerminal"
        2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Cistern" | names: "SanitaryTerminal"
        2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Shower" | names: "SanitaryTerminal"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "15kg WM" | names: "ElectricAppliance"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Micorwave" | names: "ElectricAppliance"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "13 plate DW" | names: "ElectricAppliance"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "200lt FF" | names: "ElectricAppliance"
        12 x IFCPLATE | type IFCPLATETYPE "18mm x600x1000 board" | names: "Plate" | material: layers ("Unknown" 18.) | property sets: EPset_Parametric
        1 x IFCSLAB | type IFCSLABTYPE "85mm floor slab" | names: "Slab" | material: layers ("Unknown" 85.) | property sets: EPset_Parametric
        2 x IFCFURNITURE | type IFCFURNITURETYPE "King Size.NHB" | names: "Furniture"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "6 diner" | names: "Furniture"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "4 plate ST" | names: "ElectricAppliance"
        8 x IFCWALL | type IFCWALLTYPE "110mm non-load bearing" | names: "Wall" | material: layers ("Unknown" 110.) | property sets: EPset_Parametric
        11 x IFCBEAM | type IFCBEAMTYPE "Lintol 110x75" | names: "Beam" | material: profiles ("Unknown") | property sets: EPset_Parametric
        1 x IFCWASTETERMINAL | type IFCWASTETERMINALTYPE "SepticTank" | names: "WasteTerminal" | material: profiles ("Unknown") | property sets: EPset_Parametric
        4 x IFCWALL | type IFCWALLTYPE "220mm load bearing" | names: "Wall" | material: profiles (); layers ("Default" 220.) | property sets: EPset_Parametric, Qto_WallBaseQuantities
        4 x IFCWINDOW | type IFCWINDOWTYPE "600x600" | WINDOW | names: "Window.014", "Window.012", "Window"
        1 x IFCDOOR | type IFCDOORTYPE "External door RD" | DOOR | names: "Door"
        2 x IFCWINDOW | type IFCWINDOWTYPE "1500x900" | WINDOW | TRIPLE_PANEL_HORIZONTAL | names: "Window"
        1 x IFCDOOR | type IFCDOORTYPE "Internal door RH" | names: "Door"
        3 x IFCWINDOW | type IFCWINDOWTYPE "1800x2100" | DOUBLE_PANEL_VERTICAL | names: "Window"
        1 x IFCWINDOW | type IFCWINDOWTYPE "600x1500" | DOUBLE_PANEL_VERTICAL | names: "Window"
        2 x IFCDOOR | type IFCDOORTYPE "Internal door LH" | names: "Door"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "King Size" | names: "Furniture"
IFCELEMENTASSEMBLY "Assembly"
  IFCROOF "Beam" | BARREL_ROOF
  IFCROOF "Beam.044" | BARREL_ROOF
  IFCROOF "Beam.027" | BARREL_ROOF
  IFCROOF "Beam.021" | BARREL_ROOF
  IFCROOF "Beam.007" | BARREL_ROOF
  IFCROOF "Beam.014" | BARREL_ROOF
  IFCROOF "Beam.019" | BARREL_ROOF
  IFCROOF "Beam.073" | BARREL_ROOF
  IFCROOF "Beam.084" | BARREL_ROOF
  IFCROOF "Beam.034" | BARREL_ROOF
  IFCROOF "Beam.024" | BARREL_ROOF
  IFCROOF "Beam.008" | BARREL_ROOF
  IFCROOF "Beam.042" | BARREL_ROOF
  IFCROOF "Beam.048" | BARREL_ROOF
  IFCROOF "Beam.055" | BARREL_ROOF
  IFCROOF "Beam.080" | BARREL_ROOF
  IFCROOF "Beam.022" | BARREL_ROOF
  IFCROOF "Beam.028" | BARREL_ROOF
  IFCROOF "Beam.006" | BARREL_ROOF
  IFCROOF "Beam.064" | BARREL_ROOF
  IFCROOF "Beam.046" | BARREL_ROOF
  IFCROOF "Beam.052" | BARREL_ROOF
  IFCROOF "Beam.012" | BARREL_ROOF
  IFCROOF "Beam.020" | BARREL_ROOF
  IFCROOF "Beam.026" | BARREL_ROOF
  IFCROOF "Beam.057" | BARREL_ROOF
  IFCROOF "Beam.063" | BARREL_ROOF
  IFCROOF "Beam.085" | BARREL_ROOF
  IFCROOF "Beam.069" | BARREL_ROOF
  IFCROOF "Beam.038" | BARREL_ROOF
  IFCROOF "Beam.017" | BARREL_ROOF
  IFCROOF "Beam.025" | BARREL_ROOF
  IFCROOF "Beam.056" | BARREL_ROOF
  IFCROOF "Beam.079" | BARREL_ROOF
  IFCROOF "Beam.083" | BARREL_ROOF
  IFCROOF "Beam.002" | BARREL_ROOF
  IFCROOF "Beam.036" | BARREL_ROOF
  IFCROOF "Beam.041" | BARREL_ROOF
  IFCROOF "Beam.047" | BARREL_ROOF
  IFCROOF "Beam.005" | BARREL_ROOF
  IFCROOF "Beam.077" | BARREL_ROOF
  IFCROOF "Beam.082" | BARREL_ROOF
  IFCROOF "Beam.030" | BARREL_ROOF
  IFCROOF "Beam.035" | BARREL_ROOF
  IFCROOF "Beam.061" | BARREL_ROOF
  IFCROOF "Beam.066" | BARREL_ROOF
  IFCROOF "Beam.004" | BARREL_ROOF
  IFCROOF "Beam.011" | BARREL_ROOF
  IFCROOF "Beam.018" | BARREL_ROOF
  IFCROOF "Beam.049" | BARREL_ROOF
  IFCROOF "Beam.053" | BARREL_ROOF
  IFCROOF "Beam.059" | BARREL_ROOF
  IFCROOF "Beam.065" | BARREL_ROOF
  IFCROOF "Beam.003" | BARREL_ROOF
  IFCROOF "Beam.010" | BARREL_ROOF
  IFCROOF "Beam.015" | BARREL_ROOF
  IFCROOF "Beam.068" | BARREL_ROOF
  IFCROOF "Beam.072" | BARREL_ROOF
  IFCROOF "Beam.078" | BARREL_ROOF
  IFCROOF "Beam.023" | BARREL_ROOF
  IFCROOF "Beam.033" | BARREL_ROOF
  IFCROOF "Beam.040" | BARREL_ROOF
  IFCROOF "Beam.067" | BARREL_ROOF
  IFCROOF "Beam.076" | BARREL_ROOF
  IFCROOF "Beam.001" | BARREL_ROOF
  IFCROOF "Beam.060" | BARREL_ROOF
  IFCROOF "Beam.050" | BARREL_ROOF
  IFCROOF "Beam.016" | BARREL_ROOF
  IFCROOF "Beam.032" | BARREL_ROOF
  IFCROOF "Beam.062" | BARREL_ROOF
  IFCROOF "Beam.031" | BARREL_ROOF
  IFCROOF "Beam.009" | BARREL_ROOF
  IFCROOF "Beam.039" | BARREL_ROOF
  IFCROOF "Beam.043" | BARREL_ROOF
  IFCROOF "Beam.071" | BARREL_ROOF
  IFCROOF "Beam.075" | BARREL_ROOF
  IFCROOF "Beam.081" | BARREL_ROOF
  IFCROOF "Beam.029" | BARREL_ROOF
  IFCROOF "Beam.054" | BARREL_ROOF
  IFCROOF "Beam.037" | BARREL_ROOF
  IFCROOF "Beam.087" | BARREL_ROOF
  IFCROOF "Beam.070" | BARREL_ROOF
  IFCROOF "Beam.074" | BARREL_ROOF
  IFCROOF "Beam.013" | BARREL_ROOF
  IFCROOF "Beam.045" | BARREL_ROOF
  IFCROOF "Beam.051" | BARREL_ROOF
  IFCROOF "Beam.058" | BARREL_ROOF
  IFCROOF "Beam.086" | BARREL_ROOF

Types
  IFCFURNITURETYPE "2 seater" | SOFA | 1 occurrence
  IFCSANITARYTERMINALTYPE "Double Basin" | WASHHANDBASIN | 1 occurrence
  IFCSANITARYTERMINALTYPE "Single basin" | WASHHANDBASIN | 1 occurrence
  IFCSANITARYTERMINALTYPE "Sink" | SINK | 1 occurrence
  IFCFURNITURETYPE "3 seater" | SOFA | 1 occurrence
  IFCFURNITURETYPE "1 seat" | SOFA | 1 occurrence
  IFCSANITARYTERMINALTYPE "Toilet" | TOILETPAN | 2 occurrences
  IFCSANITARYTERMINALTYPE "Cistern" | CISTERN | 2 occurrences
  IFCSANITARYTERMINALTYPE "Shower" | SHOWER | 2 occurrences
  IFCELECTRICAPPLIANCETYPE "15kg WM" | WASHINGMACHINE | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "Micorwave" | KITCHENMACHINE | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "13 plate DW" | DISHWASHER | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "200lt FF" | FRIDGE_FREEZER | 1 occurrence
  IFCPLATETYPE "18mm x600x1000 board" | SHEET | 12 occurrences | material: layers ("Unknown" 18.) | property sets: EPset_Parametric
  IFCSLABTYPE "85mm floor slab" | FLOOR | 1 occurrence | material: layers ("Unknown" 85.) | property sets: EPset_Parametric
  IFCFURNITURETYPE "King Size.NHB" | BED | 2 occurrences
  IFCFURNITURETYPE "6 diner" | TABLE | 1 occurrence | description "1x1.6m tabke with 1m movement space"
  IFCELECTRICAPPLIANCETYPE "4 plate ST" | ELECTRICCOOKER | 1 occurrence
  IFCWALLTYPE "110mm non-load bearing" | SOLIDWALL | 8 occurrences | material: layers ("Unknown" 110.) | property sets: EPset_Parametric
  IFCBEAMTYPE "Lintol 110x75" | LINTEL | 11 occurrences | material: profiles ("Unknown")
  IFCWASTETERMINALTYPE "SepticTank" | WASTEDISPOSALUNIT | 1 occurrence | material: profiles ("Unknown")
  IFCWALLTYPE "220mm load bearing" | SOLIDWALL | 4 occurrences | material: layers ("Default" 220.) | property sets: EPset_Parametric
  IFCWINDOWTYPE "600x600" | WINDOW | SINGLE_PANEL | 4 occurrences | property sets: BBIM_Window
  IFCDOORTYPE "External door RD" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | property sets: BBIM_Door
  IFCWINDOWTYPE "1500x900" | WINDOW | TRIPLE_PANEL_VERTICAL | 2 occurrences | property sets: BBIM_Window
  IFCDOORTYPE "Internal door RH" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | property sets: BBIM_Door | description "RDF4"
  IFCWINDOWTYPE "1800x2100" | WINDOW | DOUBLE_PANEL_HORIZONTAL | 3 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "600x1500" | WINDOW | DOUBLE_PANEL_VERTICAL | 1 occurrence | property sets: BBIM_Window
  IFCDOORTYPE "Internal door LH" | DOOR | SINGLE_SWING_LEFT | 2 occurrences | property sets: BBIM_Door | description "RDF4"
  IFCFURNITURETYPE "King Size" | BED | 1 occurrence

Property sets
  EPset_Parametric | properties | on 100 objects (88 IFCROOF, 11 IFCBEAM, 1 IFCWASTETERMINAL)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 13 objects (12 IFCPLATE, 1 IFCSLAB)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 12 objects (12 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.75 [SQUARE_METRE]
    GrossSideArea = 23.88 [SQUARE_METRE]
    GrossVolume = 5.25 [CUBIC_METRE]
    Height = 3000. [MILLI METRE]
    Length = 7960. [MILLI METRE]
    NetFootprintArea = 1.75 [SQUARE_METRE]
    NetSideArea = 23.88 [SQUARE_METRE]
    NetVolume = 5.25 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.03 [SQUARE_METRE]
    GrossSideArea = 14.06 [SQUARE_METRE]
    GrossVolume = 3.09 [CUBIC_METRE]
    Height = 3000. [MILLI METRE]
    Length = 4686.26 [MILLI METRE]
    NetFootprintArea = 1.03 [SQUARE_METRE]
    NetSideArea = 14.06 [SQUARE_METRE]
    NetVolume = 3.09 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 600.0000238418579, "overall_width": 600.0000238418579, "lining_properties": {"lining_depth": 250.0, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_HORIZONTAL", "overall_height": 1200.0000476837158, "overall_width": 900.0000357627869, "lining_properties": {"lining_depth": 250.0, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 50.00000074505806, "first_transom_offset": 300.00001192092896, "second_transom_offset": 600.0000238418579}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 2100.0001430511475, "overall_width": 1800.0000715255737, "lining_properties": {"lining_depth": 250.0, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 900.0000357627869}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 600.0000238418579, "overall_width": 1500.0001192092896, "lining_properties": {"lining_depth": 250.0, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 600.0000238418579}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 2000.0, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 220.0000137090683, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 100.00000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 2100.0001430511475, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 115.00000208616257, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 110.00000685453415, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2100.0001430511475, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 115.00000208616257, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 110.00000685453415, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)