IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2024-03-21T08:43:25"
Preprocessor: "IfcOpenShell v0.7.0-6c9e130ca"
Originating system: "IfcOpenShell v0.7.0-6c9e130ca"
Application: "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1709284765 (2024-03-01T09:19:25Z)
  Owner history of Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1708606800 (2024-02-22T13:00:00Z)
  Owner history of Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1709114400 (2024-02-28T10:00:00Z)
  2 x Owner history of Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | state READWRITE | change MODIFIED | created 1711007006 (2024-03-21T07:43:26Z) | last modified 1711007027 (2024-03-21T07:43:47Z) by Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" with "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1708678800 (2024-02-23T09:00:00Z)
  2 x Owner history of Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | state READWRITE | change MODIFIED | created 1711007006 (2024-03-21T07:43:26Z) | last modified 1711007026 (2024-03-21T07:43:46Z) by Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" with "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1706799600 (2024-02-01T15:00:00Z)
  Owner history of Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | state READWRITE | change MODIFIED | created 1711007007 (2024-03-21T07:43:27Z) | last modified 1711007026 (2024-03-21T07:43:46Z) by Person "Undefined" id "TEST" of Organization "Trimble Solutions Corporation" with "Tekla Structures" version "2021 Service Pack 6" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Plant T"
  IFCSITE "Undefined" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″
    IFCBUILDING "Undefined" | postal address (none given)
      IFCBUILDINGSTOREY "Undefined" | elevation 0.
        contains 1 element
          1 x IFCELEMENTASSEMBLY | REINFORCEMENT_UNIT | names: "KOLOM" | parts: 58 IFCELEMENTASSEMBLY, 18 IFCBEAM, 9 IFCSLAB, 2 IFCREINFORCINGBAR, 1 IFCCOLUMN | property sets: BaseQuantities, Default, Tekla Assembly

Property sets
  Default | properties | on 24 objects (24 IFCELEMENTASSEMBLY)
    ACN (no value)
    Afschuiving (no value)
    CAST_UNIT_POS (no value)
    CAST_UNIT_POS = "HTA1" (IFCLABEL)
    Druk (t) (no value)
    Height (no value)
    Length (no value)
    Material (no value)
    NAME (no value)
    Name (no value)
    Trek (t) (no value)
    comment (no value)
  Default | properties | on 24 objects (24 IFCDISCRETEACCESSORY)
    ACN (no value)
    Afschuiving (no value)
    CAST_UNIT_POS = "HTA1" (IFCLABEL)
    CAST_UNIT_POS = "HTA1" (IFCLABEL)
    Druk (t) (no value)
    Height (no value)
    Length (no value)
    Material = "S235JR" (IFCLABEL)
    NAME = "HTA 38/17 - 150mm" (IFCLABEL)
    Name (no value)
    Trek (t) (no value)
    comment (no value)
  Default | properties | on 18 objects (18 IFCBEAM)
    ACN (no value)
    Afschuiving (no value)
    CAST_UNIT_POS = "K19" (IFCLABEL)
    CAST_UNIT_POS = "K19" (IFCLABEL)
    Druk (t) (no value)
    Height (no value)
    Length (no value)
    Material = "S235JR" (IFCLABEL)
    NAME = "TSE Ø20/M24" (IFCLABEL)
    Name (no value)
    Trek (t) (no value)
    comment (no value)
  Default | properties | on 18 objects (18 IFCDISCRETEACCESSORY)
    ACN (no value)
    Afschuiving (no value)
    CAST_UNIT_POS = "BA1" (IFCLABEL)
    CAST_UNIT_POS = "BA1" (IFCLABEL)
    Druk (t) (no value)
    Height (no value)
    Length (no value)
    Material = "8.8" (IFCLABEL)
    NAME = "Boutanker M24" (IFCLABEL)
    Name (no value)
    Trek (t) (no value)
    comment (no value)
  Default | properties | on 18 objects (18 IFCELEMENTASSEMBLY)
    ACN (no value)
    Afschuiving (no value)
    CAST_UNIT_POS (no value)
    CAST_UNIT_POS = "BA1" (IFCLABEL)
    Druk (t) (no value)
    Height (no value)
    Length (no value)
    Material (no value)
    NAME (no value)
    Name (no value)
    Trek (t) (no value)
    comment (no value)
  Default | properties | on 9 objects (9 IFCSLAB)
    ACN (no value)
    Afschuiving (no value)
    CAST_UNIT_POS = "K19" (IFCLABEL)
    CAST_UNIT_POS = "K19" (IFCLABEL)
    Druk (t) (no value)
    Height (no value)
    Length (no value)
    Material = "C50/60" (IFCLABEL)
    NAME = "CONSOLE" (IFCLABEL)
    Name (no value)
    Trek (t) (no value)
    comment (no value)
  Default | properties | on 6 objects (6 IFCELEMENTASSEMBLY)
    ACN (no value)
    Afschuiving (no value)
    CAST_UNIT_POS (no value)
    CAST_UNIT_POS = "IB62" (IFCLABEL)
    Druk (t) (no value)
    Height (no value)
    Length (no value)
    Material (no value)
    NAME (no value)
    Name (no value)
    Trek (t) (no value)
    comment (no value)
  Default | properties | on 6 objects (6 IFCBEAM)
    ACN (no value)
    Afschuiving (no value)
    CAST_UNIT_POS = "IB62" (IFCLABEL)
    CAST_UNIT_POS = "IB62" (IFCLABEL)
    Druk (t) (no value)
    Height (no value)
    Length (no value)
    Material = "NEG_BETON" (IFCLABEL)
    NAME = "IB Ø80/88" (IFCLABEL)
    Name (no value)
    Trek (t) (no value)
    comment (no value)
  Default: 11 more contents on 24 objects not shown
  Tekla Assembly | properties | on 6 objects (6 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "IB62" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "-1.290" (IFCLABEL)
    Assembly/Cast unit position code = "22/J" (IFCLABEL)
    Assembly/Cast unit top elevation = "+0.394" (IFCLABEL)
    Assembly/Cast unit weight = -4.3 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "HTA1" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+14.745" (IFCLABEL)
    Assembly/Cast unit position code = "22/J" (IFCLABEL)
    Assembly/Cast unit top elevation = "+14.895" (IFCLABEL)
    Assembly/Cast unit weight = 0.3 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "LUS1004" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+4.060" (IFCLABEL)
    Assembly/Cast unit position code = "22/J" (IFCLABEL)
    Assembly/Cast unit top elevation = "+4.308" (IFCLABEL)
    Assembly/Cast unit weight = 1.6 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "BA1" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+16.490" (IFCLABEL)
    Assembly/Cast unit position code = "22/J" (IFCLABEL)
    Assembly/Cast unit top elevation = "+16.690" (IFCLABEL)
    Assembly/Cast unit weight = 0.7 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "LUS999" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+15.912" (IFCLABEL)
    Assembly/Cast unit position code = "22/J" (IFCLABEL)
    Assembly/Cast unit top elevation = "+16.160" (IFCLABEL)
    Assembly/Cast unit weight = 1.6 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "HTA1" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "-1.165" (IFCLABEL)
    Assembly/Cast unit position code = "22/J" (IFCLABEL)
    Assembly/Cast unit top elevation = "-1.015" (IFCLABEL)
    Assembly/Cast unit weight = 0.3 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "HTA1" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+23.499" (IFCLABEL)
    Assembly/Cast unit position code = "22/J" (IFCLABEL)
    Assembly/Cast unit top elevation = "+23.580" (IFCLABEL)
    Assembly/Cast unit weight = 0.3 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Control number (no value)
  Tekla Assembly | properties | on 2 objects (2 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "LUS1004" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "+3.560" (IFCLABEL)
    Assembly/Cast unit position code = "22/J" (IFCLABEL)
    Assembly/Cast unit top elevation = "+3.808" (IFCLABEL)
    Assembly/Cast unit weight = 1.6 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight (no value)
    Control number (no value)
  Tekla Assembly: 21 more contents on 39 objects not shown
  BaseQuantities | quantities | on 18 objects (18 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.000432 [SQUARE_METRE]
    GrossArea = 0.0237453301345886 [SQUARE_METRE]
    GrossVolume = 0.000100403533850234 [CUBIC_METRE]
    NetArea = 0.023745330134443 [SQUARE_METRE]
    NetVolume = 0.00010040353384955 [CUBIC_METRE]
  BaseQuantities | quantities | on 18 objects (18 IFCELEMENTASSEMBLY)
    Width = 41.569219381653 [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCELEMENTASSEMBLY)
    Width = 394. [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCELEMENTASSEMBLY)
    Width = 38.0000000000085 [MILLI METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCDISCRETEACCESSORY)
    CrossSectionArea = 0.00024 [SQUARE_METRE]
    GrossArea = 0.0292049511239422 [SQUARE_METRE]
    GrossVolume = 4.2607205763483E-05 [CUBIC_METRE]
    NetArea = 0.0292049511239422 [SQUARE_METRE]
    NetVolume = 4.2607205763483E-05 [CUBIC_METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCELEMENTASSEMBLY)
    Width = 38.0000000002812 [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCSLAB)
    NetArea = 0.126 [SQUARE_METRE]
    NetVolume = 0.0378 [CUBIC_METRE]
    NetWeight = 94.5 [KILO GRAM]
    Width = 420. [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCBEAM)
    Length = 624. [MILLI METRE]
    NetVolume = 0.000176493852584162 [CUBIC_METRE]
    NetWeight = 1.4119508206733 [KILO GRAM]
    OuterSurfaceArea = 0.0387727993122798 [SQUARE_METRE]
  BaseQuantities: 33 more contents on 65 objects not shown
  Tekla Quantity | properties | on 22 objects (22 IFCDISCRETEACCESSORY)
    Area per tons = 85.681 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 81. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.029 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0.34 (IFCMASSMEASURE) [KILO GRAM]
    Width = 38. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 18 objects (18 IFCDISCRETEACCESSORY)
    Area per tons = 29.562 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 36. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.024 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0.8 (IFCMASSMEASURE) [KILO GRAM]
    Width = 41.6 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 8 objects (8 IFCDISCRETEACCESSORY)
    Area per tons = 34.853 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 27.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1281. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.057 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 1.62 (IFCMASSMEASURE) [KILO GRAM]
    Width = 570.1 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 6 objects (6 IFCSLAB)
    Area per tons = 7.238 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.126 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.684 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.038 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 94.5 (IFCMASSMEASURE) [KILO GRAM]
    Width = 420. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 6 objects (6 IFCBEAM)
    Area per tons = 27.649 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 424. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.026 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0.96 (IFCMASSMEASURE) [KILO GRAM]
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 6 objects (6 IFCBEAM)
    Area per tons = 27.46 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 624. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.039 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 1.41 (IFCMASSMEASURE) [KILO GRAM]
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 6 objects (6 IFCBEAM)
    Area per tons = 27.537 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 524. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.033 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 1.19 (IFCMASSMEASURE) [KILO GRAM]
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 6 objects (6 IFCBEAM)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 88. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1728.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.476 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = -4.27 (IFCMASSMEASURE) [KILO GRAM]
    Width = 88. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity: 5 more contents on 8 objects not shown
  Pset_PlateCommon | properties | on 24 objects (24 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "HTA1" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 18 objects (18 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BA1" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 4 objects (4 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "LUS1004" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 4 objects (4 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "LUS999" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 1 object (1 IFCDISCRETEACCESSORY)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "AARD1" (IFCIDENTIFIER)
  Tekla Common | properties | on 6 objects (6 IFCBEAM)
    Bottom elevation = "-1.290" (IFCLABEL)
    Class = "102" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.394" (IFCLABEL)
  Tekla Common | properties | on 2 objects (2 IFCDISCRETEACCESSORY)
    Bottom elevation = "+4.060" (IFCLABEL)
    Class = "106" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+4.308" (IFCLABEL)
  Tekla Common | properties | on 2 objects (2 IFCBEAM)
    Bottom elevation = "+5.126" (IFCLABEL)
    Class = "9" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+5.550" (IFCLABEL)
  Tekla Common | properties | on 2 objects (2 IFCDISCRETEACCESSORY)
    Bottom elevation = "+16.490" (IFCLABEL)
    Class = "11" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+16.690" (IFCLABEL)
  Tekla Common | properties | on 2 objects (2 IFCBEAM)
    Bottom elevation = "+11.366" (IFCLABEL)
    Class = "9" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+11.990" (IFCLABEL)
  Tekla Common | properties | on 2 objects (2 IFCDISCRETEACCESSORY)
    Bottom elevation = "+15.912" (IFCLABEL)
    Class = "106" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+16.160" (IFCLABEL)
  Tekla Common | properties | on 2 objects (2 IFCBEAM)
    Bottom elevation = "+5.706" (IFCLABEL)
    Class = "9" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+6.230" (IFCLABEL)
  Tekla Common | properties | on 2 objects (2 IFCDISCRETEACCESSORY)
    Bottom elevation = "-1.165" (IFCLABEL)
    Class = "102" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "-1.015" (IFCLABEL)
  Tekla Common: 39 more contents on 66 objects not shown
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "cons3" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "cons2" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "TSE1" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "TSE6" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "TSE4" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "IB62" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "SZ1" (IFCIDENTIFIER)
  Tekla Reinforcement | properties | on 2 objects (2 IFCREINFORCINGBAR)
    Cast unit mark = "K19" (IFCLABEL)
    Center-to-center distance = "" (IFCLABEL)
    Grade = "BE500" (IFCLABEL)
    Length = 1080. (IFCLENGTHMEASURE) [MILLI METRE]
    Name = "TSE Ø20/M24" (IFCLABEL)
    Phase = 1 (IFCINTEGER)
    Rebar Mark = "W1" (IFCIDENTIFIER)
    Shape = "1" (IFCIDENTIFIER)
    Size = "20" (IFCIDENTIFIER)
    TD = 1080. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Number = 1 (IFCINTEGER)
    Total Weight = 2.7 (IFCMASSMEASURE) [KILO GRAM]
    Weight = 2.71 (IFCMASSMEASURE) [KILO GRAM]
    a = 1080. (IFCLENGTHMEASURE) [MILLI METRE]
    b (no value)
    c (no value)
    d (no value)
    e (no value)
    f (no value)
    g (no value)
    h1 (no value)
    h2 (no value)
    i (no value)
    j (no value)
    k1 (no value)
    k2 (no value)
    o (no value)
    r (no value)
    s (no value)
    t (no value)
    u (no value)
    v (no value)
    x (no value)
    y (no value)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Beton_K-118" (IFCIDENTIFIER)