IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "Restaurant_Livingston - simplified.ifc"
Time stamp: "2023-06-03T16:58:08+02:00"
Preprocessor: "IfcOpenShell v0.7.0-8f41ae0c1"
Originating system: "BlenderBIM 0.0.230602"
Authorization: "Nobody"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  61 x Person "ryan@openingdesign.com" of Organization (no name given)
  53 x Organization "Autodesk Revit 2020 (ENU)"
  4 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1680878644 (2023-04-07T14:44:04Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1661457979 (2022-08-25T20:06:19Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1682123705 (2023-04-22T00:35:05Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1633996150 (2021-10-11T23:49:10Z)
  37 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1682305051 (2023-04-24T02:57:31Z)
  17 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1681941947 (2023-04-19T22:05:47Z)

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: square foot (conversion based)
  LENGTHUNIT: foot (conversion based)
  VOLUMEUNIT: cubic foot (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      contains 1 element
        1 x IFCWALL | ELEMENTEDWALL | names: "G-No_Name_001"
      IFCBUILDINGSTOREY "My Storey"
        contains 784 elements
          390 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "Continuous Angle1:Continuous Angle:1463390", "Continuous Angle2:Continuous Angle:1578039", "Continuous Angle3:Continuous Angle:1578050" (+387 more) | material: "ACOUSTICAL SEALANT"; constituents "concrete" (); "TOP METAL STUD TRACK (FASTENER 24" O.C.)"; "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)"; "METAL RUNNER CHANNEL; FASTEN @ 24" O.C."; "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: EPset_Drawing, BBIM_Array, Pset_BuildingElementProxyCommon
          1 x IFCDOOR | type IFCDOORTYPE "3070P" | names: "Door" | material: constituents "existing" ("DOOR & FRAME") | property sets: Pset_DoorCommon
          1 x IFCSLAB | type IFCSLABTYPE "FLR150" | names: "Slab" | material: layers "Floor_LayerSetName" ("GENERIC_FLOOR" 0.656167984008789) | property sets: EPset_Parametric, Qto_SlabBaseQuantities, EPset_Drawing, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORTYPE "30"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          1 x IFCDOOR | type IFCDOORTYPE "34"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          1 x IFCDOOR | type IFCDOORTYPE "34"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          2 x IFCDOOR | type IFCDOORTYPE "36"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: OD_Options, Pset_DoorCommon
          5 x IFCDOOR | type IFCDOORTYPE "36"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          1 x IFCDOOR | type IFCDOORTYPE "32"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          1 x IFCDOOR | type IFCDOORTYPE "30"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          4 x IFCWALL | type IFCWALLTYPE "W1" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "30"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: EPset_Drawing
          1 x IFCDOOR | type IFCDOORTYPE "34"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          2 x IFCDOOR | type IFCDOORTYPE "32"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: OD_Options, Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORTYPE "34"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          2 x IFCDOOR | type IFCDOORTYPE "36"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: OD_Options, Pset_DoorCommon
          3 x IFCDOOR | type IFCDOORTYPE "36"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          1 x IFCDOOR | type IFCDOORTYPE "21070R" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "21070L" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
          2 x IFCDOOR | type IFCDOORTYPE "21070R" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "21070L" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORTYPE "3070L-SF" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, EPset_Drawing, Qto_DoorBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "3070L-SF" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "3070R-SF" | SINGLE_SWING_RIGHT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "3070R" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "36"84"R" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "34"84"L" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
          18 x IFCFURNITURE | names: "Cube", "Plane.001", "Plane" (+15 more) | material: "CASEWORK" | property sets: Pset_FurnitureTypeCommon, EPset_Drawing
          1 x IFCFURNITURE | BED | names: "Plane" | material: constituents "existing" () | property sets: EPset_Drawing, Pset_FurnitureTypeCommon
          3 x IFCPLATE | type IFCPLATETYPE "Empty" | names: "Plate" | material: layers "existing" ("EXISTING STOREFRONT" 0.0416666679084301) | property sets: EPset_Parametric, EPset_Drawing, Pset_PlateCommon
          1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Neufert Medium Basin" | BATH | names: "Furniture" | property sets: Pset_SanitaryTerminalTypeCommon
          1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Neufert Toilet with Cistern" | BATH | names: "Furniture.001" | property sets: Pset_SanitaryTerminalTypeCommon
          1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Generic Medium Sink" | BATH | names: "Furniture.002" | property sets: EPset_Drawing, Pset_SanitaryTerminalTypeCommon
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "ADA Grab Bars" | names: "SanitaryTerminal" | property sets: Pset_SanitaryTerminalTypeCommon
          32 x IFCWALL | type IFCWALLTYPE "M358BØD" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Drawing
          5 x IFCWALL | type IFCWALLTYPE "M358BØD_DEMO" | names: "Wall" | material: layers "demolish" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, EPset_Drawing, Pset_WallCommon, Qto_WallBaseQuantities
          5 x IFCWALL | type IFCWALLTYPE "M6BØD" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.5, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "W2" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "EX" | names: "Wall" | material: layers "existing" ("Unknown" 0.416667014360428, "WINDOW" 0.416667014360428) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Drawing
          1 x IFCWINDOW | type IFCPLATETYPE "Empty" | LIGHTDOME | names: "Plate" | material: layers "existing" ("EXISTING STOREFRONT" 0.0416666679084301) | property sets: EPset_Parametric, EPset_Drawing, Pset_WindowCommon
          18 x IFCWINDOW | type IFCWINDOWTYPE "Empty" | names: "Window" | material: profiles "existing" ("WINDOW") | property sets: EPset_Parametric, EPset_Drawing, Pset_WindowCommon
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "GENERIC" | names: "Column" | material: layers "poche" ("Unknown" 0.328083989501312) | property sets: EPset_Parametric
          4 x IFCCOVERING | CEILING | names: "G-No_Name_008", "G-No_Name_049", "G-No_Name_092" (+1 more)
          1 x IFCCURTAINWALL | names: "G-No_Name_051" | property sets: EPset_Drawing
          4 x IFCELECTRICAPPLIANCE | names: "Airpot base", "Beer Taps", "G-No_Name_022" (+1 more)
          2 x IFCELECTRICAPPLIANCE | REFRIGERATOR | names: "Refrigerator+-+True+TUC-27-LP", "G-No_Name_039"
          10 x IFCFURNITURE | type IFCFURNITURETYPE "Booth" | SOFA | names: "Booth1"
          1 x IFCFURNITURE | SOFA | names: "Booth1#1"
          24 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Retail Dining Chair" | CHAIR | names: "seat"
          1 x IFCFURNITURE | SHELF | names: "Shelf"
          8 x IFCFURNITURE | type IFCFURNITURETYPE "Chair_02" | CHAIR | names: "STOOL28-26"
          6 x IFCFURNITURE | type IFCFURNITURETYPE "Table_booth_01" | TABLE | names: "Table-booth1"
          3 x IFCFURNITURE | type IFCFURNITURETYPE "Table_01" | TABLE | names: "Table-booth1#1"
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Table_03" | TABLE | names: "Table-booth1#2"
          2 x IFCFURNITURE | TABLE | names: "Table-booth1#3", "Table-booth1#4"
          4 x IFCFURNITURE | type IFCFURNITURETYPE "Table_02" | TABLE | names: "Table-booth1#3"
          33 x IFCLIGHTFIXTURE | POINTSOURCE | names: "Component#11", "LightFixture" | property sets: BBIM_Array
          2 x IFCSANITARYTERMINAL | SINK | names: "G-No_Name_014", "G-No_Name_045"
          2 x IFCVALVE | FAUCET | names: "G-No_Name_030", "G-No_Name_046"
          6 x IFCWALL | type IFCWALLTYPE "EX-EXT" | names: "Wall" | material: layers "poche" ("GENERIC POCHE" 0.625) | property sets: EPset_Parametric
          5 x IFCWALL | type IFCWALLTYPE "GENERIC 6"" | names: "Wall" | material: layers "poche" ("GENERIC POCHE" 0.5) | property sets: EPset_Parametric
          3 x IFCWINDOW | WINDOW | names: "G-No_Name_052", "G-No_Name_053", "G-No_Name_054"
          11 x IFCWALL | ELEMENTEDWALL | names: "G-No_Name_001", "A-Door_curve_", "A-Fixt_curve_" (+8 more) | property sets: Pset_DoorCommon, Pset_SanitaryTerminalTypeCommon, EPset_Drawing, Pset_FurnitureTypeCommon, Pset_StairCommon, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "GENERIC 5"" | names: "Wall" | material: layers "poche" ("GENERIC POCHE" 0.416666656732559) | property sets: EPset_Parametric, OD_Options
          8 x IFCBEAM | type IFCBEAMTYPE "Curb" | names: "Beam" | material: profiles ("COMPOSITE DECKING") | property sets: EPset_Parametric, OD_Options, Pset_BeamCommon, EPset_Drawing
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Core_Fill_8in" | names: "BuildingElementProxy" | property sets: BBIM_Array
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "8inCMU" | names: "BuildingElementProxy" | property sets: BBIM_Array
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Horz Ladder Reinforcing" | names: "BuildingElementProxy" | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)"
          11 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Morter_8inCMU" | names: "BuildingElementProxy" | property sets: BBIM_Array
          16 x IFCBUILDINGELEMENTPROXY | names: "Cube", "Trace" | property sets: OD_Options, Pset_BuildingElementProxyCommon, EPset_Drawing
          2 x IFCBUILDINGELEMENTPROXY | type IFCGEOGRAPHICELEMENTTYPE "car" | COMPLEX | names: "GeographicElement" | property sets: Pset_BuildingElementProxyCommon, OD_Options
          1 x IFCDOOR | DOOR | names: "A-Door_curve_" | property sets: Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORTYPE "30"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          1 x IFCDOOR | type IFCDOORTYPE "24"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: OD_Options
          2 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Neufert Washing Machine" | names: "ElectricAppliance" | property sets: OD_Options, Pset_ElectricApplianceTypeCommon
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Retail 8-Seater Rectangular Table" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Retail 6-Seater Circular Table" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
          1 x IFCFURNITURE | object type "BENCH" | USERDEFINED | names: "Plane" | material: "COMPOSITE DECKING - DIAGONAL" | property sets: OD_Options, Pset_FurnitureTypeCommon
          1 x IFCGEOGRAPHICELEMENT | TERRAIN | names: "Cube" | property sets: EPset_Drawing
          1 x IFCRAILING | GUARDRAIL | names: "Vert" | property sets: OD_Options, Pset_RailingCommon
          3 x IFCSANITARYTERMINAL | names: "A-Fixt_curve_", "A-DETL_curve_" | property sets: Pset_SanitaryTerminalTypeCommon, EPset_Drawing
          2 x IFCSANITARYTERMINAL | BATH | names: "Cube" | property sets: OD_Options, Pset_SanitaryTerminalTypeCommon
          2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | names: "SanitaryTerminal" | property sets: OD_Options, Pset_SanitaryTerminalTypeCommon
          2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Sink 124x44" | names: "SanitaryTerminal" | property sets: EPset_Drawing, OD_Options, Pset_SanitaryTerminalTypeCommon
          2 x IFCSLAB | BASESLAB | names: "Cube" | property sets: OD_Options, Pset_SlabCommon
          5 x IFCSLAB | type IFCSLABTYPE "ASPHALT DRIVE WAY" | names: "Slab" | material: layers "10Fill" ("ASPHALT DRIVEWAY" 0.984251976013184) | property sets: EPset_Parametric, EPset_Drawing, OD_Options, Pset_SlabCommon
          7 x IFCSLAB | type IFCSLABTYPE "COMPOSITE DECK - HORZ." | names: "Slab" | material: layers "HorzLines6in48scale" ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric, OD_Options, EPset_Drawing, Pset_SlabCommon
          9 x IFCSLAB | type IFCSLABTYPE "COMPOSITE DECK - VERT." | names: "Slab" | material: layers "VertLines6in48scale" ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric, OD_Options, Pset_SlabCommon, EPset_Drawing
          2 x IFCSLAB | type IFCSLABTYPE "CONCRETE SLAB" | names: "Slab" | material: layers "concrete" ("CONCRETE SLAB" 0.5) | property sets: EPset_Parametric, OD_Options, Pset_SlabCommon, EPset_Drawing
          2 x IFCSTAIR | names: "A-Stairs_curve_" | property sets: Pset_StairCommon
          10 x IFCWALL | type IFCWALLTYPE "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, OD_Options, EPset_Drawing
          1 x IFCWALL | type IFCWALLTYPE "GENERIC 7"" | names: "Wall" | material: layers "poche" ("GENERIC POCHE" 0.583333313465118) | property sets: EPset_Parametric, OD_Options
          1 x IFCDOOR | type IFCDOORTYPE "48"84"D" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM")
          4 x IFCDOOR | type IFCDOORTYPE "S36"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM", "INSULATED GLAZING", "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING")
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "C1" | names: "Column" | material: profiles "poche" ("Unknown") | property sets: EPset_Parametric
          1 x IFCSLAB | type IFCSLABTYPE "Canopy" | names: "Slab" | material: layers "concrete" ("Unknown" 1.) | property sets: EPset_Parametric

Types
  IFCDOORTYPE "3070P" | 1 occurrence | property sets: EPset_Drawing
  IFCSLABTYPE "FLR150" | 1 occurrence | material: layers "Floor_LayerSetName" ("GENERIC_FLOOR" 0.656167984008789)
  IFCDOORTYPE "30"80"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "34"80"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:34" x 80":154791, Door-Single-Panel:34" x 80":154791:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "34"84"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:34" x 84":154865, Door-Single-Panel:34" x 84":154865:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "36"80"R" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:36" x 80":154902, Door-Single-Panel:36" x 80":154902:1, Pset_DoorCommon
  IFCDOORTYPE "36"84"R" | DOOR | SINGLE_SWING_RIGHT | 6 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Pset_DoorCommon
  IFCDOORTYPE "32"84"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:32" x 84":154765, Door-Single-Panel:32" x 84":154765:1, Pset_DoorCommon
  IFCDOORTYPE "30"84"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon
  IFCWALLTYPE "W1" | STANDARD | 4 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCDOORTYPE "30"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "34"80"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:34" x 80":154791, Door-Single-Panel:34" x 80":154791:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "32"84"L" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:32" x 84":154765, Door-Single-Panel:32" x 84":154765:1, Pset_DoorCommon
  IFCDOORTYPE "34"84"L" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:34" x 84":154865, Door-Single-Panel:34" x 84":154865:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "36"80"L" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:36" x 80":154902, Door-Single-Panel:36" x 80":154902:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "36"84"L" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Pset_DoorCommon
  IFCDOORTYPE "21070R" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCDOORTYPE "21070L" | DOOR | SINGLE_SWING_LEFT | 2 occurrences | property sets: BBIM_Door
  IFCDOORTYPE "3070L-SF" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCDOORTYPE "3070R-SF" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCDOORTYPE "3070R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing, OD_DoorType_Hackjob | description "WOOD FLUSH W/ HM FRAME"
  IFCPLATETYPE "Empty" | CURTAIN_PANEL | 4 occurrences | material: layers "existing" ("EXISTING STOREFRONT" 0.0416666679084301)
  IFCFURNITURETYPE "Neufert Medium Basin" | 1 occurrence | property sets: EPset_Drawing
  IFCFURNITURETYPE "Neufert Toilet with Cistern" | 1 occurrence | property sets: EPset_Drawing
  IFCFURNITURETYPE "Generic Medium Sink" | 1 occurrence | property sets: EPset_Drawing
  IFCSANITARYTERMINALTYPE "ADA Grab Bars" | element type "GRAB_BARS" | USERDEFINED | 1 occurrence | property sets: EPset_Drawing
  IFCWALLTYPE "M358BØD" | STANDARD | 32 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWALLTYPE "M358BØD_DEMO" | STANDARD | 5 occurrences | material: layers "demolish" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWALLTYPE "M6BØD" | STANDARD | 5 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.5, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon | description "5/8 GYP - 6 METAL(BATT) - 5/8 GYP"
  IFCWALLTYPE "W2" | STANDARD | 1 occurrence | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWALLTYPE "EX" | 3 occurrences | material: layers "existing" ("Unknown" 0.416667014360428, "WINDOW" 0.416667014360428) | description "GENERIC EXTERIOR"
  IFCWINDOWTYPE "Empty" | WINDOW | 18 occurrences | material: profiles "existing" ("WINDOW")
  IFCCOLUMNTYPE "GENERIC" | COLUMN | 4 occurrences | material: layers "poche" ("Unknown" 0.328083989501312) | property sets: EPset_Parametric
  IFCFURNITURETYPE "Booth" | SOFA | 10 occurrences
  IFCFURNITURETYPE "Neufert Retail Dining Chair" | 24 occurrences
  IFCFURNITURETYPE "Chair_02" | CHAIR | 8 occurrences
  IFCFURNITURETYPE "Table_booth_01" | TABLE | 6 occurrences
  IFCFURNITURETYPE "Table_01" | TABLE | 3 occurrences
  IFCFURNITURETYPE "Table_03" | TABLE | 2 occurrences
  IFCFURNITURETYPE "Table_02" | TABLE | 4 occurrences
  IFCWALLTYPE "EX-EXT" | STANDARD | 6 occurrences | material: layers "poche" ("GENERIC POCHE" 0.625) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "GENERIC 6"" | STANDARD | 5 occurrences | material: layers "poche" ("GENERIC POCHE" 0.5) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "GENERIC 5"" | STANDARD | 2 occurrences | material: layers "poche" ("GENERIC POCHE" 0.416666656732559) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCBEAMTYPE "Curb" | BEAM | 8 occurrences | material: profiles ("COMPOSITE DECKING")
  IFCBUILDINGELEMENTPROXYTYPE "Core_Fill_8in" | COMPLEX | 10 occurrences | property sets: EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "8inCMU" | COMPLEX | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Horz Ladder Reinforcing" | COMPLEX | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Morter_8inCMU" | COMPLEX | 11 occurrences
  IFCGEOGRAPHICELEMENTTYPE "car" | 2 occurrences
  IFCDOORTYPE "30"80"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "24"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon, EPset_Drawing
  IFCELECTRICAPPLIANCETYPE "Neufert Washing Machine" | 2 occurrences
  IFCFURNITURETYPE "Neufert Retail 8-Seater Rectangular Table" | 1 occurrence | property sets: EPset_Drawing
  IFCFURNITURETYPE "Neufert Retail 6-Seater Circular Table" | 1 occurrence
  IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | 2 occurrences
  IFCSANITARYTERMINALTYPE "Neufert Sink 124x44" | 2 occurrences
  IFCSLABTYPE "ASPHALT DRIVE WAY" | 5 occurrences | material: layers "10Fill" ("ASPHALT DRIVEWAY" 0.984251976013184)
  IFCSLABTYPE "COMPOSITE DECK - HORZ." | FLOOR | 7 occurrences | material: layers "HorzLines6in48scale" ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric
  IFCSLABTYPE "COMPOSITE DECK - VERT." | FLOOR | 9 occurrences | material: layers "VertLines6in48scale" ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric
  IFCSLABTYPE "CONCRETE SLAB" | FLOOR | 2 occurrences | material: layers "concrete" ("CONCRETE SLAB" 0.5) | property sets: EPset_Parametric
  IFCWALLTYPE "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | STANDARD | 10 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "GENERIC 7"" | STANDARD | 1 occurrence | material: layers "poche" ("GENERIC POCHE" 0.583333313465118) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCDOORTYPE "48"84"D" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "S36"80"L" | DOOR | SINGLE_SWING_RIGHT | 4 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "SOLID CORE DOOR", "Trim": "WOOD DOOR TRIM", "INSULATED GLAZING", "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING") | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Pset_DoorCommon
  IFCCOLUMNTYPE "C1" | 3 occurrences | material: profiles "poche" ("Unknown")
  IFCSLABTYPE "Canopy" | FLOOR | 1 occurrence | material: layers "concrete" ("Unknown" 1.) | property sets: EPset_Parametric

Property sets
  EPset_Parametric | properties | on 74 objects (74 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 34 objects (26 IFCSLAB, 4 IFCCOLUMN, 3 IFCPLATE, 1 IFCWINDOW)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 29 objects (18 IFCWINDOW, 8 IFCBEAM, 3 IFCCOLUMN)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 5 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  Pset_DoorCommon | properties | on 10 objects (10 IFCDOOR)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    Status in {"NEW"} (IFCLABEL)
  Pset_DoorCommon | properties | on 3 objects (2 IFCDOOR, 1 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_DoorCommon | properties | on 15 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 2.1946486495 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 2.19464874267578 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 22 objects (22 IFCWALL)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    Status in {"NEW"} (IFCLABEL)
  Pset_WallCommon | properties | on 4 type objects
    IsExternal = TRUE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
  Pset_WallCommon | properties | on 1 type object
    Status in {"EXISTING"} (IFCLABEL)
    ThermalTransmittance (no value)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 20.4724407196045 (IFCTHERMALTRANSMITTANCEMEASURE)
  EPset_Drawing | properties | on 60 objects (11 IFCANNOTATION, 11 IFCWALL, 8 IFCBUILDINGELEMENTPROXY, 8 IFCWINDOW) | on 20 type objects
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
  EPset_Drawing | properties | on 3 objects (3 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "material.Category" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/4" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    Exclude = "" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/96" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "MODEL_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    Exclude = "" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    ImperialPrecision = "1/4" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCTEXT)
    Metadata = "r"Pset_.*Common", material, material.Category, IfcElement" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCTEXT)
    Scale = "1/48" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCTEXT)
    Symbols = "drawings\assets\symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    Exclude = ".IfcElement[r"Pset_.*Common"."Status"="DEMOLISH"]" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    ImperialPrecision = "1/4" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "r"Pset_.*Common", material, material.Category, IfcElement" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/48" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = TRUE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/96" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    Exclude = "" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCTEXT)
    Scale = "1/96" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings\assets\default.css" (IFCTEXT)
    Symbols = "drawings\assets\symbols.svg" (IFCTEXT)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/96" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing: 13 more contents on 12 objects not shown
  EPset_Annotation | properties | on 20 objects (20 IFCANNOTATION)
    Classes = "oblique" (IFCLABEL)
  EPset_Annotation | properties | on 3 objects (3 IFCANNOTATION)
    Classes = "fill-bg" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 5 objects (5 IFCFURNITURE)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 4 objects (4 IFCFURNITURE)
    Status in {"NEW"} (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 1 object (1 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Qto_DoorBaseQuantities | quantities | on 4 objects (4 IFCDOOR)
    Area = 2.614 [square foot (conversion based)]
    Height = 2.197 [foot (conversion based)]
    Perimeter = 6.375 [foot (conversion based)]
    Width = 0.991 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 3 objects (3 IFCDOOR)
    Area = 2.173 [square foot (conversion based)]
    Height = 2.134 [foot (conversion based)]
    Perimeter = 6.299 [foot (conversion based)]
    Width = 1.016 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 2.729 [square foot (conversion based)]
    Height = 2.197 [foot (conversion based)]
    Perimeter = 6.477 [foot (conversion based)]
    Width = 1.041 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 0. [square foot (conversion based)]
    Height = 0. [foot (conversion based)]
    Perimeter = 1.975 [foot (conversion based)]
    Width = 0.987 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 2.729 [square foot (conversion based)]
    Height = 84. [foot (conversion based)]
    Perimeter = 6.477 [foot (conversion based)]
    Width = 36. [foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Height = 84. [foot (conversion based)]
    Width = 36. [foot (conversion based)]
  BBIM_Dimension | properties | on 2 objects (2 IFCANNOTATION)
    ShowDescriptionOnly = TRUE (IFCBOOLEAN)
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.656 [foot (conversion based)]
    GrossArea = 1408.847 [square foot (conversion based)]
    GrossVolume = 924.44 [cubic foot (conversion based)]
    Length = 53.742 [foot (conversion based)]
    NetArea = 1408.847 [square foot (conversion based)]
    NetVolume = 924.44 [cubic foot (conversion based)]
    Perimeter = 160.338 [foot (conversion based)]
    Width = 26.427 [foot (conversion based)]
  Pset_WindowCommon | properties | on 14 objects (14 IFCWINDOW)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_PlateCommon | properties | on 3 objects (3 IFCPLATE)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_SanitaryTerminalTypeCommon | properties | on 6 objects (6 IFCSANITARYTERMINAL)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_SanitaryTerminalTypeCommon | properties | on 6 objects (6 IFCSANITARYTERMINAL)
    Status in {"NEW"} (IFCLABEL)
  Pset_SanitaryTerminalTypeCommon | properties | on 1 object (1 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_SlabCommon | properties | on 14 objects (14 IFCSLAB)
    Status in {"NEW"} (IFCLABEL)
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    Status in {"NEW"} (IFCTEXT)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    Status in {"EXISTING"} (IFCLABEL)
  BBIM_reference_image_0 | properties | on 1 object (1 IFCBUILDING)
    Position X = "24.34749412536621" (IFCLABEL)
    Position Y = "-17.135032653808594" (IFCLABEL)
    Position Z = "0.0" (IFCLABEL)
    Rotation X = "0.0" (IFCLABEL)
    Rotation Y = "-0.0" (IFCLABEL)
    Rotation Z = "-3.1415929794311523" (IFCLABEL)
    Scale X = "-21.253463745117188" (IFCLABEL)
    Scale Y = "-21.253463745117188" (IFCLABEL)
    Scale Z = "-21.253463745117188" (IFCLABEL)
    image = "D:\Repositórios\OpeningDesign\mineral_point_residence\Existing Conditions and Code Research\Existing Conditions\aerial_2017.jpg" (IFCLABEL)
  Pset_StairCommon | properties | on 1 object (1 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    Status in {"NEW"} (IFCLABEL)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    Status in {"EXISTING"} (IFCLABEL)
  OD_Options | properties | on 26 objects (7 IFCBUILDINGELEMENTPROXY, 6 IFCSLAB, 4 IFCWALL, 3 IFCSANITARYTERMINAL)
    OD_Option_1 = "" (IFCTEXT)
    OD_Option_2 = "N" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 23 objects (6 IFCBEAM, 6 IFCWALL, 4 IFCSLAB, 3 IFCSANITARYTERMINAL)
    OD_Option_1 = "N" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
    OD_Options_2 = "" (IFCTEXT)
  OD_Options | properties | on 14 objects (10 IFCBUILDINGELEMENTPROXY, 1 IFCDOOR, 1 IFCRAILING, 1 IFCSLAB)
    OD_Option_1 = "N" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 3 objects (2 IFCSLAB, 1 IFCBUILDINGELEMENTPROXY)
    OD_Option_2 = "N" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 2 objects (2 IFCWALL)
    OD_Option_1 = "D" (IFCTEXT)
  OD_Options | properties | on 1 object (1 IFCSLAB)
    OD_Option_1 = "N" (IFCTEXT)
    OD_Option_2 = "" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 1 object (1 IFCWALL)
    OD_Option_2 = "D" (IFCTEXT)
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    Status in {"NEW"} (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Status in {"NEW"} (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Status in {"NEW"} (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_ElectricApplianceTypeCommon | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    Status in {"NEW"} (IFCLABEL)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Status in {"NEW"} (IFCLABEL)
  BBIM_Array | properties | on 31 objects (31 IFCLIGHTFIXTURE)
    Data (no value)
    Parent = "3k7OoTF0X0Z9B4dAAKUrCg" (IFCLABEL)
  BBIM_Array | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "3iGRJZfy51iAd8K3LgiYDq" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "0zDYnHKt9D9xBQ0J7EbG8P" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "0QwQTUhPr6EAqfEjNat8se" (IFCLABEL)
  BBIM_Array | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "3QecqJiErB$9TeAgOjclzW" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Data = "[{"children": ["3syCb0d5zDaf1UuAsd_Fxo", "17OoJfbx1FQP_yhRVQqSYn", "3B9HHI1M56hgq$o59XcyAn", "11ASd3UDv9SAGo77xAa5iX", "2jpLr8LAD8MwpGy$UTclFu", "07VBrshCz3hRkEb_0Pb6kF", "2NjRZ17Sf7ZwBsVLJPcW$i", "02lIXz8VDCShBckuHCsAP0", "3jtKSi5qb5mOXZ7jPH28B7", "3FI_7o4Dz1keW3geVnqXHX"], "count": 11, "x": 0.0, "y": 0.0, "z": 0.6666666865348816, "use_local_space": true, "sync_children": false, "method": "OFFSET"}]" (IFCLABEL)
    Parent = "3iGRJZfy51iAd8K3LgiYDq" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Data = "[{"children": ["0Hu5OZfpXCjuqdz_xm5p6$", "04KRMMDiLFIgW7HB4S4vIL", "05a_Wn$f928BFxplue91xZ", "30b0rmoPbFDugJMwVmEMGA", "1sUMWnnaTFLu73DtV$Vg5E", "10Tedwphz2Xw6DSFVkA1zb", "0XSgQoVYLCIACcxDoGGY44", "3KSgklMnr3QOnLfDhxaRy9", "3HF$OKLd1E$fWQN2MAZkGf"], "count": 10, "x": 0.0, "y": 0.0, "z": 0.6666666865348816, "use_local_space": true, "sync_children": false, "method": "OFFSET"}]" (IFCLABEL)
    Parent = "0zDYnHKt9D9xBQ0J7EbG8P" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Data = "[{"children": ["0BUZvVwhLFcOcAqiojq8XJ", "2dC8Tk5z59oAn9EQGs3qxr", "3JyzZ3SZ51EQennn87_bZW", "1piov1eK9CPAWWpE35mYlv", "1NusYV31DBN8_z5_ldWhch", "2Ul6tH$JDBjuajb8WfB8xm", "1$pb4RBKTDtP_eEP_TkpAP", "2NKikJo1T31egFEKkEgv$3", "0d1KDqYRrCE9_7zIFzbh7M"], "count": 10, "x": 0.0, "y": 0.0, "z": 0.6666666865348816, "use_local_space": true, "sync_children": false, "method": "OFFSET"}]" (IFCLABEL)
    Parent = "0QwQTUhPr6EAqfEjNat8se" (IFCLABEL)
  BBIM_Array: 2 more contents on 2 objects not shown
  Door-Single-Panel:30" x 80":154643 | predefined | on 2 type objects
  Door-Single-Panel:30" x 80":154643:1 | predefined | on 2 type objects
  Door-Single-Panel:34" x 80":154791 | predefined | on 2 type objects
  Door-Single-Panel:34" x 80":154791:1 | predefined | on 2 type objects
  Door-Single-Panel:34" x 84":154865 | predefined | on 2 type objects
  Door-Single-Panel:34" x 84":154865:1 | predefined | on 2 type objects
  Door-Single-Panel:36" x 80":154902 | predefined | on 2 type objects
  Door-Single-Panel:36" x 80":154902:1 | predefined | on 2 type objects
  Door-Single-Panel:36" x 84":154924 | predefined | on 3 type objects
  Door-Single-Panel:36" x 84":154924:1 | predefined | on 3 type objects
  Door-Single-Panel:32" x 84":154765 | predefined | on 2 type objects
  Door-Single-Panel:32" x 84":154765:1 | predefined | on 2 type objects
  Door-Single-Panel:30" x 84":154723 | predefined | on 4 type objects
  Door-Single-Panel:30" x 84":154723:1 | predefined | on 4 type objects
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0625, "overall_width": 2.958329916000366, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 7.0625, "overall_width": 2.958329916000366, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 7.0, "overall_width": 3.3333332538604736, "lining_properties": {"lining_depth": 0.3333333432674408, "lining_thickness": 0.1666666716337204, "lining_offset": 0.32999998331069946, "lining_to_panel_offset_x": 0.1666666716337204, "lining_to_panel_offset_y": 0.08202099800109863, "transom_thickness": 0.0, "threshold_thickness": 0.08202099800109863, "threshold_depth": 0.32808399200439453, "threshold_offset": 0.32999998331069946}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0, "overall_width": 3.3333332538604736, "lining_properties": {"lining_depth": 0.3333333432674408, "lining_thickness": 0.1666666716337204, "lining_offset": 0.3333333432674408, "lining_to_panel_offset_x": 0.1666666716337204, "lining_to_panel_offset_y": 0.08202099800109863, "transom_thickness": 0.0, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0625, "overall_width": 3.125, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  OD_DoorType_Hackjob | properties | on 1 type object
    DoorHeight = "7' - 0"" (IFCTEXT)
    DoorWidth = "3' - 0"" (IFCTEXT)
    TypeComments = "MATCH EXISTING (HEIGHT, MATERIAL/FINISH, HARDWARE)" (IFCTEXT)
  Pset_ElementShading | properties | on 5 type objects
    Roughness = 1. (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_ProductRequirements | properties | on 5 type objects
    Category = "Walls" (IFCLABEL)