IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition []"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and Archicad 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: On]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [IFC Model position: Survey Point and Project Origin]"
Description: "Option [Curtain Wall export mode: Container Element]"
Description: "Option [Railing export mode: Container Element]"
File name: "P:\Projects\Auckland\2024\24069 - Penny Homes R&D - 29 Manson St\CAD\_Plot\IFC & DWGs\House 1 BC.ifc"
Time stamp: "2024-06-14T11:23:12"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "DDS_IFC v3.0"
Originating system: "IFC file generated by Graphisoft Archicad 26.0.0 NZE FULL Windows version (IFC add-on version: 7004 NZE FULL)."
Authorization: "The authorising person"
Application: "Archicad" version "26.0.0" identifier "IFC add-on version: 7004 NZE FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Undefined" of Organization "Undefined"
  Owner history of Person "Undefined" of Organization "Undefined" | application "Archicad" version "26.0.0" identifier "IFC add-on version: 7004 NZE FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change NOCHANGE | created 1718320989 (2024-06-13T23:23:09Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: SQUAREDEGREE (conversion based)
  CURRENCY: USD
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "29 Manson Street, Gate Pa, Tauranga" | phase "Concept Design" | description "Residential Development for Penny Homes"
  IFCSITE "Site" | latitude -36° 50′ 0″ | longitude 174° 46′ 0″ | elevation above sea level 30450. | postal address: "29 Manson Street", "Gate Pa", "Tauranga", "New Zealand"
    IFCBUILDING "Building" | postal address: "29 Manson Street", "Gate Pa", "Tauranga", "New Zealand"
      IFCBUILDINGSTOREY "1. Ground Floor" | elevation -17290.
        contains 63 elements
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "INT 10Pb/Stud 90/10Pb 110" | names: "Wall - 005", "Wall - 006", "Wall - 004" | parts: 36 IFCBUILDINGELEMENTPART | property sets: AC_Pset_RenovationAndPhasing, ArchiCADQuantities, ArchiCADProperties
          9 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "CI Tools Door" | names: "ID05", "ID07", "ID04" (+3 more) | property sets: ArchiCADProperties, AC_Pset_CI_Tools_Door, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_CI_Tools_Door
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hot Water System #1550" | names: "OB - 0003" | property sets: ArchiCADProperties, AC_Pset_Hot_Water_System_#1550, AC_Equantity_Hot_Water_System_#1550, ArchiCADQuantities, AC_Pset_RenovationAndPhasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Concrete - Structural 250" | names: "Conc Slab-315mm" | material: "Concrete - Structural" | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, ArchiCADQuantities
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "CI Tools Wall Covering" | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, AC_Pset_CI_Tools_Wall_Covering, ArchiCADQuantities, AC_Equantity_CI_Tools_Wall_Covering
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "INT 10Pb/Stud 45/10Pb 65" | names: "Wall - 004" | parts: 6 IFCBUILDINGELEMENTPART | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, ArchiCADQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Dryer #1548" | names: "Dryer-01" | property sets: AC_Pset_Dryer_#1548, ArchiCADProperties, AC_Pset_RenovationAndPhasing, AC_Equantity_Dryer_#1548, ArchiCADQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Dining Table Rectangle 24" | names: "FURN-01" | property sets: ArchiCADProperties, AC_Pset_Dining_Table_Rectangle_24, ArchiCADQuantities, AC_Equantity_Dining_Table_Rectangle_24, AC_Pset_RenovationAndPhasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Laundry Tub #1546" | names: "TUB-01" | property sets: ArchiCADProperties, AC_Pset_Laundry_Tub_#1546, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Laundry_Tub_#1546
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Sofa 26" | names: "FURN-01" | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, AC_Pset_Sofa_26, ArchiCADQuantities, AC_Equantity_Sofa_26
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Coffee Table 02 26" | names: "FURN-01" | property sets: AC_Pset_Coffee_Table_02_26, ArchiCADProperties, ArchiCADQuantities, AC_Pset_RenovationAndPhasing, AC_Equantity_Coffee_Table_02_26
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hood 26" | names: "OB - 0013" | property sets: ArchiCADProperties, AC_Pset_Hood_26, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Hood_26
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Oven Standard #1015" | names: "OB - 0001" | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, AC_Pset_Oven_Standard_#1015, AC_Equantity_Oven_Standard_#1015, ArchiCADQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Standing Cabinet Block 26" | names: "OB - 0001" | property sets: AC_Pset_Standing_Cabinet_Block_26, ArchiCADProperties, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Standing_Cabinet_Block_26
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cabinet Base Double Door 24" | names: "Object - 001" | property sets: AC_Pset_Cabinet_Base_Double_Door_24, ArchiCADProperties, ArchiCADQuantities, AC_Pset_RenovationAndPhasing, AC_Equantity_Cabinet_Base_Double_Door_24
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Refrigerator 26" | names: "OB - 0001" | property sets: AC_Pset_Refrigerator_26, ArchiCADProperties, AC_Pset_RenovationAndPhasing, AC_Equantity_Refrigerator_26, ArchiCADQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cabinet Base Corner S 24" | names: "Object - 001" | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, AC_Equantity_Cabinet_Base_Corner_S_24, ArchiCADQuantities, AC_Pset_Cabinet_Base_Corner_S_24
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "CAL FL Finish: Carpet 12" | names: "Conc Slab-311mm" | parts: 6 IFCBUILDINGELEMENTPART | property sets: ArchiCADQuantities, AC_Pset_RenovationAndPhasing, ArchiCADProperties
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "FLOOR - 100CONC/250EPS 401" | names: "Conc Slab-310mm" | parts: 3 IFCBUILDINGELEMENTPART | property sets: AC_Pset_RenovationAndPhasing, ArchiCADProperties, ArchiCADQuantities
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "EXT Wall - 10Pb/Stud 90 Insul/7 Ply 107" | names: "Wall - 007", "Wall - 008", "Wall - 009" (+1 more) | parts: 12 IFCBUILDINGELEMENTPART | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, ArchiCADQuantities
          8 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "CI Tools Window" | names: "W1.03", "W1.01", "W1.02" (+5 more) | property sets: ArchiCADProperties, AC_Pset_CI_Tools_Window, AC_Pset_RenovationAndPhasing, AC_Equantity_CI_Tools_Window, ArchiCADQuantities
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Bed 01 26" | names: "FURN-01" | property sets: ArchiCADProperties, AC_Pset_Bed_01_26, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Bed_01_26
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Bed Layout 26" | names: "FURN-01" | property sets: AC_Pset_Bed_Layout_26, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, ArchiCADProperties, AC_Equantity_Bed_Layout_26
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Basin Cabinet 21" | names: "WHB-01" | property sets: ArchiCADProperties, AC_Pset_Basin_Cabinet_21, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Basin_Cabinet_21
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WC 26" | names: "WC01" | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, AC_Pset_WC_26, ArchiCADQuantities, AC_Equantity_WC_26
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Shower Cabin 26" | names: "Shower Waste-01" | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Shower_Cabin_26, AC_Pset_Shower_Cabin_26
      IFCBUILDINGSTOREY "1. Roof" | elevation -14830.
        contains 6 elements
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "CI Tools Roof Covering" | property sets: ArchiCADProperties, AC_Pset_RenovationAndPhasing, AC_Pset_CI_Tools_Roof_Covering, AC_Equantity_CI_Tools_Roof_Covering, ArchiCADQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Roof 45 Purlins/ BP 46" | names: "Roof - 39" | parts: 2 IFCBUILDINGELEMENTPART | property sets: AC_Pset_RenovationAndPhasing, ArchiCADProperties, ArchiCADQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "CEILING Insul 420/35Batten/13Pb 348" | names: "Conc Slab-310mm" | parts: 2 IFCBUILDINGELEMENTPART | property sets: AC_Pset_RenovationAndPhasing, ArchiCADProperties, ArchiCADQuantities

Types
  IFCBUILDINGELEMENTPROXYTYPE "INT 10Pb/Stud 90/10Pb 110" | 12 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "CI Tools Door" | 9 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hot Water System #1550" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Concrete - Structural 250" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "CI Tools Wall Covering" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "INT 10Pb/Stud 45/10Pb 65" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Dryer #1548" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Dining Table Rectangle 24" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Laundry Tub #1546" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Sofa 26" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Coffee Table 02 26" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Hood 26" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Oven Standard #1015" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Standing Cabinet Block 26" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Cabinet Base Double Door 24" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Refrigerator 26" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Cabinet Base Corner S 24" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "CAL FL Finish: Carpet 12" | 3 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "FLOOR - 100CONC/250EPS 401" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "EXT Wall - 10Pb/Stud 90 Insul/7 Ply 107" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "CI Tools Window" | 8 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Bed 01 26" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Bed Layout 26" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Basin Cabinet 21" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "WC 26" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Shower Cabin 26" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "CI Tools Roof Covering" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Roof 45 Purlins/ BP 46" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "CEILING Insul 420/35Batten/13Pb 348" | 1 occurrence

Property sets
  ArchiCADProperties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Acoustic Rating = "" (IFCLABEL)
    Archicad IFC ID = "2xfvSAxlDF18q87XG0HRNE" (IFCLABEL)
    Building Material / Composite / Profile / Fill = "Background Fill" (IFCLABEL)
    Building Materials (All) = "" (IFCLABEL)
    Colliding Zones = "KDL" (IFCLABEL)
    Egress Dimensions = "850.0×1,995.0" (IFCLABEL)
    Element ID = "ID05" (IFCLABEL)
    Element Type = "Door" (IFCLABEL)
    External IFC ID = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Home Story Name = "1. Ground Floor" (IFCLABEL)
    Home Story Number = "-3" (IFCLABEL)
    Hotlink Master ID = "" (IFCLABEL)
    Hotlink and Element ID = "ID05" (IFCLABEL)
    Layer = "A30 Wall INT" (IFCLABEL)
    Leaf Dimensions = "920.0×1,980.0" (IFCLABEL)
    Library Part Name = "CI Tools Door" (IFCLABEL)
    Linked Changes = "" (IFCLABEL)
    Locked = TRUE (IFCBOOLEAN)
    Marker Text = "" (IFCLABEL)
    Nominal W x H Size = "990.0×2,040.0" (IFCLABEL)
    Nominal W x H x T Size = "990.0×2,040.0×110.0" (IFCLABEL)
    Opening Library Part Name = "CI Tools Door" (IFCLABEL)
    Opening Side Fill Index = "Background Fill" (IFCLABEL)
    Orientation = "R" (IFCLABEL)
    Parent ID = "Wall - 006" (IFCLABEL)
    Position = "Undefined" (IFCLABEL)
    Property Object Name = "" (IFCLABEL)
    Related Zone Name = "" (IFCLABEL)
    Related Zone Number = "" (IFCLABEL)
    Renovation Status = "Existing" (IFCLABEL)
    Reveal Dimensions = "990.0×2,040.0" (IFCLABEL)
    Show On Renovation Filter = "All Relevant Filters" (IFCLABEL)
    Structural Function = "Undefined" (IFCLABEL)
    Surfaces (All) = "Paint - Titanium White" (IFCLABEL)
    Unique ID = "BBA7970A-EEF3-4F04-8D08-1E140045B5CE" (IFCLABEL)
    Unit Dimensions = "990.0×2,040.0" (IFCLABEL)
    Wall Structure = "INT 10Pb/Stud 90/10Pb" (IFCLABEL)
    Wallhole Dimensions = "1,010.0×2,050.0" (IFCLABEL)
  ArchiCADProperties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Archicad IFC ID = "3eeTHZF2j1h8q$OpoaTtM$" (IFCLABEL)
    Building Material / Composite / Profile / Fill = "Background Fill (2)" (IFCLABEL)
    Building Materials (All) = "" (IFCLABEL)
    Colliding Zones = "ST" (IFCLABEL)
    Element ID = "OB - 0003" (IFCLABEL)
    Element Type = "Object" (IFCLABEL)
    External IFC ID = "" (IFCLABEL)
    Fill Type = "Background Fill (2)" (IFCLABEL)
    Home Story Name = "1. Ground Floor" (IFCLABEL)
    Home Story Number = "-3" (IFCLABEL)
    Hotlink Master ID = "" (IFCLABEL)
    Hotlink and Element ID = "OB - 0003" (IFCLABEL)
    Layer = "A57 Furniture" (IFCLABEL)
    Library Part Name = "Hot Water System #1550" (IFCLABEL)
    Linked Changes = "" (IFCLABEL)
    Locked = TRUE (IFCBOOLEAN)
    Parent ID = "OB - 0003" (IFCLABEL)
    Position = "Undefined" (IFCLABEL)
    Property Object Name = "" (IFCLABEL)
    Related Zone Name = "" (IFCLABEL)
    Related Zone Number = "" (IFCLABEL)
    Renovation Status = "Existing" (IFCLABEL)
    Rotation Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Show On Renovation Filter = "All Relevant Filters" (IFCLABEL)
    Structural Function = "Undefined" (IFCLABEL)
    Surface = "GENERAL" (IFCLABEL)
    Surfaces (All) = "Paint - Light Gray" (IFCLABEL)
    Unique ID = "E8A1D463-3C2B-41AC-8D3F-633CA47775BF" (IFCLABEL)
  ArchiCADProperties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Archicad IFC ID = "1IYv4v0BX3kgQtOvUCH_xZ" (IFCLABEL)
    Bottom Surface = "Concrete - 02" (IFCLABEL)
    Building Material / Composite / Profile / Fill = "Concrete - Structural" (IFCLABEL)
    Building Material = "Concrete - Structural" (IFCLABEL)
    Building Materials (All) = "Concrete - Structural" (IFCLABEL)
    Colliding Zones = "ST" (IFCLABEL)
    Cover Fill = "Carpet" (IFCLABEL)
    Edge Surface = "Carpet - 03" (IFCLABEL)
    Element ID = "Conc Slab-315mm" (IFCLABEL)
    Element Type = "Slab" (IFCLABEL)
    External IFC ID = "" (IFCLABEL)
    Home Story Name = "1. Ground Floor" (IFCLABEL)
    Home Story Number = "-3" (IFCLABEL)
    Hotlink Master ID = "" (IFCLABEL)
    Hotlink and Element ID = "Conc Slab-315mm" (IFCLABEL)
    ID of Connected Openings = "" (IFCLABEL)
    Layer = "A30 Floor" (IFCLABEL)
    Linked Changes = "" (IFCLABEL)
    Locked = TRUE (IFCBOOLEAN)
    Number of Openings = 0 (IFCINTEGER)
    Parent ID = "Conc Slab-315mm" (IFCLABEL)
    Position = "Undefined" (IFCLABEL)
    Property Object Name = "" (IFCLABEL)
    Reference Plane Location = "Bottom" (IFCLABEL)
    Related Zone Name = "" (IFCLABEL)
    Related Zone Number = "" (IFCLABEL)
    Renovation Status = "Existing" (IFCLABEL)
    Show On Renovation Filter = "All Relevant Filters" (IFCLABEL)
    Structural Function = "Undefined" (IFCLABEL)
    Structure Type = "Basic" (IFCLABEL)
    Surfaces (All) = "Concrete - 02; Paint - Glossy White; Carpet - 03" (IFCLABEL)
    Top Surface = "Paint - Glossy White" (IFCLABEL)
    Unique ID = "528B9139-00B8-43BA-A6B7-63978C47EEE3" (IFCLABEL)
  ArchiCADProperties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Acoustic Rating = "" (IFCLABEL)
    Archicad IFC ID = "0vvEKagMyjDsKdVUAWnBSJ" (IFCLABEL)
    Building Material / Composite / Profile / Fill = "Background Fill" (IFCLABEL)
    Building Materials (All) = "" (IFCLABEL)
    Colliding Zones = "BEDROOM 2" (IFCLABEL)
    Egress Dimensions = "765.0×1,995.0" (IFCLABEL)
    Element ID = "ID07" (IFCLABEL)
    Element Type = "Door" (IFCLABEL)
    External IFC ID = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Home Story Name = "1. Ground Floor" (IFCLABEL)
    Home Story Number = "-3" (IFCLABEL)
    Hotlink Master ID = "" (IFCLABEL)
    Hotlink and Element ID = "ID07" (IFCLABEL)
    Layer = "A30 Wall INT" (IFCLABEL)
    Leaf Dimensions = "810.0×1,980.0" (IFCLABEL)
    Library Part Name = "CI Tools Door" (IFCLABEL)
    Linked Changes = "" (IFCLABEL)
    Locked = TRUE (IFCBOOLEAN)
    Marker Text = "" (IFCLABEL)
    Nominal W x H Size = "880.0×2,040.0" (IFCLABEL)
    Nominal W x H x T Size = "880.0×2,040.0×110.0" (IFCLABEL)
    Opening Library Part Name = "CI Tools Door" (IFCLABEL)
    Opening Side Fill Index = "Background Fill" (IFCLABEL)
    Orientation = "L" (IFCLABEL)
    Parent ID = "Wall - 004" (IFCLABEL)
    Position = "Undefined" (IFCLABEL)
    Property Object Name = "" (IFCLABEL)
    Related Zone Name = "" (IFCLABEL)
    Related Zone Number = "" (IFCLABEL)
    Renovation Status = "Existing" (IFCLABEL)
    Reveal Dimensions = "880.0×2,040.0" (IFCLABEL)
    Show On Renovation Filter = "All Relevant Filters" (IFCLABEL)
    Structural Function = "Undefined" (IFCLABEL)
    Surfaces (All) = "Paint - Titanium White" (IFCLABEL)
    Unique ID = "39E4E524-A96F-2D37-6527-7DE2A0C4B713" (IFCLABEL)
    Unit Dimensions = "880.0×2,040.0" (IFCLABEL)
    Wall Structure = "INT 10Pb/Stud 90/10Pb" (IFCLABEL)
    Wallhole Dimensions = "900.0×2,050.0" (IFCLABEL)
  ArchiCADProperties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Archicad IFC ID = "0DZAwcj9i4mB97Inlk96WJ" (IFCLABEL)
    Building Material / Composite / Profile / Fill = "Foreground Fill" (IFCLABEL)
    Building Materials (All) = "" (IFCLABEL)
    Colliding Zones = "" (IFCLABEL)
    Element ID = "" (IFCLABEL)
    Element Type = "Wall Covering" (IFCLABEL)
    External IFC ID = "" (IFCLABEL)
    Fill Type = "Foreground Fill" (IFCLABEL)
    Home Story Name = "1. Ground Floor" (IFCLABEL)
    Home Story Number = "-3" (IFCLABEL)
    Hotlink Master ID = "" (IFCLABEL)
    Hotlink and Element ID = "" (IFCLABEL)
    Layer = "A42 Wall Cladding" (IFCLABEL)
    Library Part Name = "CI Tools Wall Covering" (IFCLABEL)
    Linked Changes = "" (IFCLABEL)
    Locked = TRUE (IFCBOOLEAN)
    Parent ID = "" (IFCLABEL)
    Property Object Name = "" (IFCLABEL)
    Related Zone Name = "" (IFCLABEL)
    Related Zone Number = "" (IFCLABEL)
    Renovation Status = "Existing" (IFCLABEL)
    Rotation Angle = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Show On Renovation Filter = "All Relevant Filters" (IFCLABEL)
    Surface = "Stone - Marble Carrara White" (IFCLABEL)
    Surfaces (All) = "Stone - Marble Carrara White; Okarito Double" (IFCLABEL)
    Unique ID = "0D8CAEA6-B49B-04C0-B247-4B1BEE246813" (IFCLABEL)
  ArchiCADProperties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Acoustic Rating = "" (IFCLABEL)
    Archicad IFC ID = "1aQnyYY5KaMxWWt_5OjrjU" (IFCLABEL)
    Building Material / Composite / Profile / Fill = "Background Fill" (IFCLABEL)
    Building Materials (All) = "" (IFCLABEL)
    Colliding Zones = "BATH" (IFCLABEL)
    Egress Dimensions = "765.0×1,995.0" (IFCLABEL)
    Element ID = "ID05" (IFCLABEL)
    Element Type = "Door" (IFCLABEL)
    External IFC ID = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Home Story Name = "1. Ground Floor" (IFCLABEL)
    Home Story Number = "-3" (IFCLABEL)
    Hotlink Master ID = "" (IFCLABEL)
    Hotlink and Element ID = "ID05" (IFCLABEL)
    Layer = "A30 Wall INT" (IFCLABEL)
    Leaf Dimensions = "810.0×1,980.0" (IFCLABEL)
    Library Part Name = "CI Tools Door" (IFCLABEL)
    Linked Changes = "" (IFCLABEL)
    Locked = TRUE (IFCBOOLEAN)
    Marker Text = "" (IFCLABEL)
    Nominal W x H Size = "880.0×2,040.0" (IFCLABEL)
    Nominal W x H x T Size = "880.0×2,040.0×110.0" (IFCLABEL)
    Opening Library Part Name = "CI Tools Door" (IFCLABEL)
    Opening Side Fill Index = "Background Fill" (IFCLABEL)
    Orientation = "L" (IFCLABEL)
    Parent ID = "Wall - 004" (IFCLABEL)
    Position = "Undefined" (IFCLABEL)
    Property Object Name = "" (IFCLABEL)
    Related Zone Name = "" (IFCLABEL)
    Related Zone Number = "" (IFCLABEL)
    Renovation Status = "Existing" (IFCLABEL)
    Reveal Dimensions = "880.0×2,040.0" (IFCLABEL)
    Show On Renovation Filter = "All Relevant Filters" (IFCLABEL)
    Structural Function = "Undefined" (IFCLABEL)
    Surfaces (All) = "Paint - Titanium White" (IFCLABEL)
    Unique ID = "646B1F22-8855-245B-B820-DFE158B75B5E" (IFCLABEL)
    Unit Dimensions = "880.0×2,040.0" (IFCLABEL)
    Wall Structure = "INT 10Pb/Stud 90/10Pb" (IFCLABEL)
    Wallhole Dimensions = "900.0×2,050.0" (IFCLABEL)
  ArchiCADProperties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Acoustic Rating = "" (IFCLABEL)
    Archicad IFC ID = "3DH7Eda3joqYeWr8mJQjqA" (IFCLABEL)
    Building Material / Composite / Profile / Fill = "Background Fill" (IFCLABEL)
    Building Materials (All) = "" (IFCLABEL)
    Colliding Zones = "BEDROOM 1; ST" (IFCLABEL)
    Egress Dimensions = "950.0×1,995.0" (IFCLABEL)
    Element ID = "ID04" (IFCLABEL)
    Element Type = "Door" (IFCLABEL)
    External IFC ID = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Home Story Name = "1. Ground Floor" (IFCLABEL)
    Home Story Number = "-3" (IFCLABEL)
    Hotlink Master ID = "" (IFCLABEL)
    Hotlink and Element ID = "ID04" (IFCLABEL)
    Layer = "A30 Wall INT" (IFCLABEL)
    Leaf Dimensions = "1,020.0×1,980.0" (IFCLABEL)
    Library Part Name = "CI Tools Door" (IFCLABEL)
    Linked Changes = "" (IFCLABEL)
    Locked = TRUE (IFCBOOLEAN)
    Marker Text = "" (IFCLABEL)
    Nominal W x H Size = "1,090.0×2,040.0" (IFCLABEL)
    Nominal W x H x T Size = "1,090.0×2,040.0×65.0" (IFCLABEL)
    Opening Library Part Name = "CI Tools Door" (IFCLABEL)
    Opening Side Fill Index = "Background Fill" (IFCLABEL)
    Orientation = "R" (IFCLABEL)
    Parent ID = "Wall - 004" (IFCLABEL)
    Position = "Undefined" (IFCLABEL)
    Property Object Name = "" (IFCLABEL)
    Related Zone Name = "" (IFCLABEL)
    Related Zone Number = "" (IFCLABEL)
    Renovation Status = "Existing" (IFCLABEL)
    Reveal Dimensions = "1,090.0×2,040.0" (IFCLABEL)
    Show On Renovation Filter = "All Relevant Filters" (IFCLABEL)
    Structural Function = "Undefined" (IFCLABEL)
    Surfaces (All) = "Paint - Titanium White" (IFCLABEL)
    Unique ID = "CD4473A7-903B-72D2-2A20-D48C136ADD0A" (IFCLABEL)
    Unit Dimensions = "1,090.0×2,040.0" (IFCLABEL)
    Wall Structure = "INT 10Pb/Stud 45/10Pb" (IFCLABEL)
    Wallhole Dimensions = "1,110.0×2,050.0" (IFCLABEL)
  ArchiCADProperties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Acoustic Rating = "" (IFCLABEL)
    Archicad IFC ID = "3Dd3SmGKb4wu8jDBGdlj9w" (IFCLABEL)
    Building Material / Composite / Profile / Fill = "Background Fill" (IFCLABEL)
    Building Materials (All) = "" (IFCLABEL)
    Colliding Zones = "ST" (IFCLABEL)
    Egress Dimensions = "850.0×1,995.0" (IFCLABEL)
    Element ID = "ID04" (IFCLABEL)
    Element Type = "Door" (IFCLABEL)
    External IFC ID = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Home Story Name = "1. Ground Floor" (IFCLABEL)
    Home Story Number = "-3" (IFCLABEL)
    Hotlink Master ID = "" (IFCLABEL)
    Hotlink and Element ID = "ID04" (IFCLABEL)
    Layer = "A30 Wall INT" (IFCLABEL)
    Leaf Dimensions = "920.0×1,980.0" (IFCLABEL)
    Library Part Name = "CI Tools Door" (IFCLABEL)
    Linked Changes = "" (IFCLABEL)
    Locked = TRUE (IFCBOOLEAN)
    Marker Text = "" (IFCLABEL)
    Nominal W x H Size = "990.0×2,040.0" (IFCLABEL)
    Nominal W x H x T Size = "990.0×2,040.0×110.0" (IFCLABEL)
    Opening Library Part Name = "CI Tools Door" (IFCLABEL)
    Opening Side Fill Index = "Background Fill" (IFCLABEL)
    Orientation = "R" (IFCLABEL)
    Parent ID = "Wall - 005" (IFCLABEL)
    Position = "Undefined" (IFCLABEL)
    Property Object Name = "" (IFCLABEL)
    Related Zone Name = "" (IFCLABEL)
    Related Zone Number = "" (IFCLABEL)
    Renovation Status = "Existing" (IFCLABEL)
    Reveal Dimensions = "990.0×2,040.0" (IFCLABEL)
    Show On Renovation Filter = "All Relevant Filters" (IFCLABEL)
    Structural Function = "Undefined" (IFCLABEL)
    Surfaces (All) = "Paint - Titanium White" (IFCLABEL)
    Unique ID = "CD9C3730-4149-44EB-822D-34B427BED27A" (IFCLABEL)
    Unit Dimensions = "990.0×2,040.0" (IFCLABEL)
    Wall Structure = "INT 10Pb/Stud 90/10Pb" (IFCLABEL)
    Wallhole Dimensions = "1,010.0×2,050.0" (IFCLABEL)
  ArchiCADProperties: 61 more contents on 61 objects not shown
  AC_Pset_CI_Tools_Door | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle = "Lever" (IFCLABEL)
    (OLD) Exterior Handle Plate = "None" (IFCLABEL)
    (OLD) Exterior Handle Plate Position = 0 (IFCINTEGER)
    (OLD) Interior Handle = "Lever" (IFCLABEL)
    (OLD) Interior Handle Plate = "None" (IFCLABEL)
    (OLD) Interior Handle Plate Position = 0 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Acousitc Rating = "" (IFCLABEL)
    Apply Current Settings = FALSE (IFCBOOLEAN)
    Cavity Closure = "turn in" (IFCLABEL)
    Cavity Closure Exterior = "regular" (IFCLABEL)
    Cavity Closure Interior = "regular" (IFCLABEL)
    Cavity Closure Left = TRUE (IFCBOOLEAN)
    Cavity Closure Right = TRUE (IFCBOOLEAN)
    Cavity Closure Skins Turn In = 0 (IFCINTEGER)
    Cavity Closure Skins Turn Out = 0 (IFCINTEGER)
    Cost = 0. (IFCREAL)
    Door Leaf Mount Exterior = FALSE (IFCBOOLEAN)
    Door Leaf Mount Interior = FALSE (IFCBOOLEAN)
    Door Leaf Number Left = 1 (IFCINTEGER)
    Door Leaf Number Right = 1 (IFCINTEGER)
    Door Mounting to match Graphisoft Doors = TRUE (IFCBOOLEAN)
    Door Type Left = "Standard" (IFCLABEL)
    Door Type Right = "Standard" (IFCLABEL)
    Door belongs to the Zone into which it opens = TRUE (IFCBOOLEAN)
    Door height editing = 0 (IFCINTEGER)
    Elevation = "" (IFCLABEL)
    Exterior Handle Type = 0 (IFCINTEGER)
    Exterior Plate Option = 1 (IFCINTEGER)
    Exterior Plate Type = 0 (IFCINTEGER)
    Exterior Reveal Link Dimensions = TRUE (IFCBOOLEAN)
    Exterior Trim = "None" (IFCLABEL)
    Exterior Trim Bricks = FALSE (IFCBOOLEAN)
    Exterior Trim Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Exterior Trim Section Fill = "Background Fill" (IFCLABEL)
    Exterior Trim Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Exterior Trim Section Line Type = 1 (IFCINTEGER)
    Exterior Trim Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Exterior Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim View Pen = "Openings - General" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Frame Mitre Left = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Mitre Right = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Pen = "Openings - General" (IFCLABEL)
    Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame Section Fill = "Background Fill" (IFCLABEL)
    Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame Section Line Type = 1 (IFCINTEGER)
    Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Frame Surface = "Paint - Titanium White" (IFCLABEL)
    Frame Type Head = "Frame" (IFCLABEL)
    Frame Type Head Cut = FALSE (IFCBOOLEAN)
    Frame Type Left = "Frame" (IFCLABEL)
    Frame Type Right = "Frame" (IFCLABEL)
    Frame Under Leaf (frame_under_leaf) = FALSE (IFCBOOLEAN)
    Frame Under Leaf (frame_under_leaf_input) = 0 (IFCINTEGER)
    Frame View Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame View Fill = "Background Fill" (IFCLABEL)
    Frame View Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame View Line Type = 1 (IFCINTEGER)
    Frame View Pen = "Openings - General" (IFCLABEL)
    Glass Pen = "Openings - General" (IFCLABEL)
    Glass Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Glass Section Fill = "Background Fill" (IFCLABEL)
    Glass Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Glass Section Line Type = 1 (IFCINTEGER)
    Glass Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Glass Surface (gs_glass_mat) = "Glass - Clear Fast" (IFCLABEL)
    Glass View Pen = "Openings - General" (IFCLABEL)
    Glazing = "" (IFCLABEL)
    Glazing Bars Full Sash = FALSE (IFCBOOLEAN)
    Glazing Bars View Pen = "Openings - General" (IFCLABEL)
    Glazing Setout = 4 (IFCINTEGER)
    Group Type = "Others" (IFCLABEL)
    Handle Place Right Leaf = TRUE (IFCBOOLEAN)
    Handle Place Secondary Leaf = FALSE (IFCBOOLEAN)
    Handle View Pen = "Openings - General" (IFCLABEL)
    Hardware Keyside Rm. No = "" (IFCLABEL)
    Hardware Pen = "Openings - General" (IFCLABEL)
    Hardware Set = "" (IFCLABEL)
    Hardware Surface = "Metal - Stainless Steel" (IFCLABEL)
    Head Moulding = "None" (IFCLABEL)
    Head Moulding Bricks = FALSE (IFCBOOLEAN)
    Head Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding Position = "No Return" (IFCLABEL)
    Head Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Head Moulding Section Fill = "Background Fill" (IFCLABEL)
    Head Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Head Moulding Section Line Type = 1 (IFCINTEGER)
    Head Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Head Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding View Pen = "Openings - General" (IFCLABEL)
    Header Detail = "" (IFCLABEL)
    Heat Transfer Rate = "" (IFCLABEL)
    Hinges = "" (IFCLABEL)
    Hole Has Wall's Side Surface = FALSE (IFCBOOLEAN)
    Hole Surface's Split is Curved = FALSE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    IFC Operation (ifc_optype) = 2 (IFCINTEGER)
    IFC Operation (ifc_optypestr) = "Double Door Single Swing" (IFCLABEL)
    Inner Frame Bottom/Top Widths Differ = FALSE (IFCBOOLEAN)
    Inner Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame Section Fill = "Background Fill" (IFCLABEL)
    Inner Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame Section Line Type = 1 (IFCINTEGER)
    Inner Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Inner Frame View Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame View Fill = "Background Fill" (IFCLABEL)
    Inner Frame View Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame View Line Type = 1 (IFCINTEGER)
    Inner Frame View Pen = "Openings - General" (IFCLABEL)
    Interior Handle Type = 0 (IFCINTEGER)
    Interior Plate Option = 1 (IFCINTEGER)
    Interior Plate Type = 0 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Jamb Detail = "" (IFCLABEL)
    Jamb Moulding = "X" (IFCLABEL)
    Jamb Moulding Bricks = FALSE (IFCBOOLEAN)
    Jamb Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Jamb Moulding Section Fill = "Background Fill" (IFCLABEL)
    Jamb Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Jamb Moulding Section Line Type = 1 (IFCINTEGER)
    Jamb Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Jamb Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding View Pen = "Openings - General" (IFCLABEL)
    Kick Plate Exterior = FALSE (IFCBOOLEAN)
    Kick Plate Interior = FALSE (IFCBOOLEAN)
    Kick Plate Surface = "Metal - Stainless Steel" (IFCLABEL)
    Kick Plate View Pen = "Openings - General" (IFCLABEL)
    Leaf Glazing Bars Surface = "Paint - Titanium White" (IFCLABEL)
    Leaf Panel View Pen = "Openings - General" (IFCLABEL)
    Leaf Pen = "Openings - General" (IFCLABEL)
    Leaf Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Leaf Section Fill = "Background Fill" (IFCLABEL)
    Leaf Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Leaf Section Line Type = 1 (IFCINTEGER)
    Leaf Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Leaf Surface = "Paint - Titanium White" (IFCLABEL)
    Leaf View Pen = "Openings - General" (IFCLABEL)
    Link Pens = FALSE (IFCBOOLEAN)
    Lintel Type = "Double 140 x 45mm timber lintel" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lockset = "" (IFCLABEL)
    Louvres View Pen = "Openings - General" (IFCLABEL)
    Main Frame Flange = FALSE (IFCBOOLEAN)
    Manufacturer = "" (IFCLABEL)
    Mullion/Transom Widths Different to Frame = FALSE (IFCBOOLEAN)
    Nominal Size = 16 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Opening Angle in 2D = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Opening Angle in 3D = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Operation Type = "" (IFCLABEL)
    Overlight Glazing Bars = 2 (IFCINTEGER)
    Overlight Layout = 9 (IFCINTEGER)
    Overlight Panel = "F" (IFCLABEL)
    Pivot Line Style = 0 (IFCINTEGER)
    Production Year = "" (IFCLABEL)
    Resolution 3D = "Detailed" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shape Head = "Flat" (IFCLABEL)
    Showing 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Sidelight Double Hung Sash Ratio = 0.5 (IFCREAL)
    Sidelight Glazing Bars = 2 (IFCINTEGER)
    Sidelight Glazing Bars Top = 0 (IFCINTEGER)
    Sidelight Layout Left = 1 (IFCINTEGER)
    Sidelight Layout Right = 1 (IFCINTEGER)
    Sidelight Louvre Angle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sidelight Panel Type = "Bevelled 2" (IFCLABEL)
    Sill Bricks = FALSE (IFCBOOLEAN)
    Sill Detail = "" (IFCLABEL)
    Sill Fall Angle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sill Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Sill Place Under Leaves = FALSE (IFCBOOLEAN)
    Sill Surface = "Paint - Titanium White" (IFCLABEL)
    Sill Type = "None" (IFCLABEL)
    Size Constraint = 1 (IFCINTEGER)
    Symbol Pen = "2D Elements - General" (IFCLABEL)
    Threshold Type = 2 (IFCINTEGER)
    Timber SIll Type = 0 (IFCINTEGER)
    Total Glass Area = 0. (IFCREAL)
    Total Glass Perimeter = 0. (IFCREAL)
    Trim Pen = "Openings - General" (IFCLABEL)
    Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Use New Handles = TRUE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    User Defined 6 = "" (IFCLABEL)
    User Defined 7 = "" (IFCLABEL)
    User Defined 8 = "" (IFCLABEL)
    User Defined 9 = "" (IFCLABEL)
    Version Number = 26 (IFCINTEGER)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
  AC_Pset_CI_Tools_Door | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle = "Lever" (IFCLABEL)
    (OLD) Exterior Handle Plate = "None" (IFCLABEL)
    (OLD) Exterior Handle Plate Position = 0 (IFCINTEGER)
    (OLD) Interior Handle = "Lever" (IFCLABEL)
    (OLD) Interior Handle Plate = "None" (IFCLABEL)
    (OLD) Interior Handle Plate Position = 0 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Acousitc Rating = "" (IFCLABEL)
    Apply Current Settings = FALSE (IFCBOOLEAN)
    Cavity Closure = "turn in" (IFCLABEL)
    Cavity Closure Exterior = "regular" (IFCLABEL)
    Cavity Closure Interior = "regular" (IFCLABEL)
    Cavity Closure Left = TRUE (IFCBOOLEAN)
    Cavity Closure Right = TRUE (IFCBOOLEAN)
    Cavity Closure Skins Turn In = 0 (IFCINTEGER)
    Cavity Closure Skins Turn Out = 0 (IFCINTEGER)
    Cost = 0. (IFCREAL)
    Door Leaf Mount Exterior = FALSE (IFCBOOLEAN)
    Door Leaf Mount Interior = FALSE (IFCBOOLEAN)
    Door Leaf Number Left = 1 (IFCINTEGER)
    Door Leaf Number Right = 0 (IFCINTEGER)
    Door Mounting to match Graphisoft Doors = TRUE (IFCBOOLEAN)
    Door Type Left = "Standard" (IFCLABEL)
    Door Type Right = "Standard" (IFCLABEL)
    Door belongs to the Zone into which it opens = TRUE (IFCBOOLEAN)
    Door height editing = 0 (IFCINTEGER)
    Elevation = "" (IFCLABEL)
    Exterior Handle Type = 0 (IFCINTEGER)
    Exterior Plate Option = 1 (IFCINTEGER)
    Exterior Plate Type = 0 (IFCINTEGER)
    Exterior Reveal Link Dimensions = TRUE (IFCBOOLEAN)
    Exterior Trim = "None" (IFCLABEL)
    Exterior Trim Bricks = FALSE (IFCBOOLEAN)
    Exterior Trim Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Exterior Trim Section Fill = "Background Fill" (IFCLABEL)
    Exterior Trim Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Exterior Trim Section Line Type = 1 (IFCINTEGER)
    Exterior Trim Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Exterior Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim View Pen = "Openings - General" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Frame Mitre Left = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Mitre Right = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Pen = "Openings - General" (IFCLABEL)
    Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame Section Fill = "Background Fill" (IFCLABEL)
    Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame Section Line Type = 1 (IFCINTEGER)
    Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Frame Surface = "Paint - Titanium White" (IFCLABEL)
    Frame Type Head = "Frame" (IFCLABEL)
    Frame Type Head Cut = FALSE (IFCBOOLEAN)
    Frame Type Left = "Frame" (IFCLABEL)
    Frame Type Right = "Frame" (IFCLABEL)
    Frame Under Leaf (frame_under_leaf) = FALSE (IFCBOOLEAN)
    Frame Under Leaf (frame_under_leaf_input) = 0 (IFCINTEGER)
    Frame View Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame View Fill = "Background Fill" (IFCLABEL)
    Frame View Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame View Line Type = 1 (IFCINTEGER)
    Frame View Pen = "Openings - General" (IFCLABEL)
    Glass Pen = "Openings - General" (IFCLABEL)
    Glass Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Glass Section Fill = "Background Fill" (IFCLABEL)
    Glass Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Glass Section Line Type = 1 (IFCINTEGER)
    Glass Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Glass Surface (gs_glass_mat) = "Glass - Clear Fast" (IFCLABEL)
    Glass View Pen = "Openings - General" (IFCLABEL)
    Glazing = "" (IFCLABEL)
    Glazing Bars Full Sash = FALSE (IFCBOOLEAN)
    Glazing Bars View Pen = "Openings - General" (IFCLABEL)
    Glazing Setout = 4 (IFCINTEGER)
    Group Type = "Others" (IFCLABEL)
    Handle Place Right Leaf = TRUE (IFCBOOLEAN)
    Handle Place Secondary Leaf = FALSE (IFCBOOLEAN)
    Handle View Pen = "Openings - General" (IFCLABEL)
    Hardware Keyside Rm. No = "" (IFCLABEL)
    Hardware Pen = "Openings - General" (IFCLABEL)
    Hardware Set = "" (IFCLABEL)
    Hardware Surface = "Metal - Stainless Steel" (IFCLABEL)
    Head Moulding = "None" (IFCLABEL)
    Head Moulding Bricks = FALSE (IFCBOOLEAN)
    Head Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding Position = "No Return" (IFCLABEL)
    Head Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Head Moulding Section Fill = "Background Fill" (IFCLABEL)
    Head Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Head Moulding Section Line Type = 1 (IFCINTEGER)
    Head Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Head Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding View Pen = "Openings - General" (IFCLABEL)
    Header Detail = "" (IFCLABEL)
    Heat Transfer Rate = "" (IFCLABEL)
    Hinges = "" (IFCLABEL)
    Hole Has Wall's Side Surface = FALSE (IFCBOOLEAN)
    Hole Surface's Split is Curved = FALSE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    IFC Operation (ifc_optype) = 1 (IFCINTEGER)
    IFC Operation (ifc_optypestr) = "Single Door Single Swing" (IFCLABEL)
    Inner Frame Bottom/Top Widths Differ = FALSE (IFCBOOLEAN)
    Inner Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame Section Fill = "Background Fill" (IFCLABEL)
    Inner Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame Section Line Type = 1 (IFCINTEGER)
    Inner Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Inner Frame View Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame View Fill = "Background Fill" (IFCLABEL)
    Inner Frame View Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame View Line Type = 1 (IFCINTEGER)
    Inner Frame View Pen = "Openings - General" (IFCLABEL)
    Interior Handle Type = 0 (IFCINTEGER)
    Interior Plate Option = 1 (IFCINTEGER)
    Interior Plate Type = 0 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Jamb Detail = "" (IFCLABEL)
    Jamb Moulding = "X" (IFCLABEL)
    Jamb Moulding Bricks = FALSE (IFCBOOLEAN)
    Jamb Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Jamb Moulding Section Fill = "Background Fill" (IFCLABEL)
    Jamb Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Jamb Moulding Section Line Type = 1 (IFCINTEGER)
    Jamb Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Jamb Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding View Pen = "Openings - General" (IFCLABEL)
    Kick Plate Exterior = FALSE (IFCBOOLEAN)
    Kick Plate Interior = FALSE (IFCBOOLEAN)
    Kick Plate Surface = "Metal - Stainless Steel" (IFCLABEL)
    Kick Plate View Pen = "Openings - General" (IFCLABEL)
    Leaf Glazing Bars Surface = "Paint - Titanium White" (IFCLABEL)
    Leaf Panel View Pen = "Openings - General" (IFCLABEL)
    Leaf Pen = "Openings - General" (IFCLABEL)
    Leaf Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Leaf Section Fill = "Background Fill" (IFCLABEL)
    Leaf Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Leaf Section Line Type = 1 (IFCINTEGER)
    Leaf Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Leaf Surface = "Paint - Titanium White" (IFCLABEL)
    Leaf View Pen = "Openings - General" (IFCLABEL)
    Link Pens = FALSE (IFCBOOLEAN)
    Lintel Type = "Double 140 x 45mm timber lintel" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lockset = "" (IFCLABEL)
    Louvres View Pen = "Openings - General" (IFCLABEL)
    Main Frame Flange = FALSE (IFCBOOLEAN)
    Manufacturer = "" (IFCLABEL)
    Mullion/Transom Widths Different to Frame = FALSE (IFCBOOLEAN)
    Nominal Size = 16 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Opening Angle in 2D = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Opening Angle in 3D = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Operation Type = "" (IFCLABEL)
    Overlight Glazing Bars = 2 (IFCINTEGER)
    Overlight Layout = 9 (IFCINTEGER)
    Overlight Panel = "F" (IFCLABEL)
    Pivot Line Style = 0 (IFCINTEGER)
    Production Year = "" (IFCLABEL)
    Resolution 3D = "Detailed" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shape Head = "Flat" (IFCLABEL)
    Showing 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Sidelight Double Hung Sash Ratio = 0.5 (IFCREAL)
    Sidelight Glazing Bars = 2 (IFCINTEGER)
    Sidelight Glazing Bars Top = 0 (IFCINTEGER)
    Sidelight Layout Left = 1 (IFCINTEGER)
    Sidelight Layout Right = 1 (IFCINTEGER)
    Sidelight Louvre Angle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sidelight Panel Type = "Bevelled 2" (IFCLABEL)
    Sill Bricks = FALSE (IFCBOOLEAN)
    Sill Detail = "" (IFCLABEL)
    Sill Fall Angle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sill Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Sill Place Under Leaves = FALSE (IFCBOOLEAN)
    Sill Surface = "Paint - Titanium White" (IFCLABEL)
    Sill Type = "None" (IFCLABEL)
    Size Constraint = 1 (IFCINTEGER)
    Symbol Pen = "2D Elements - General" (IFCLABEL)
    Threshold Type = 2 (IFCINTEGER)
    Timber SIll Type = 0 (IFCINTEGER)
    Total Glass Area = 0. (IFCREAL)
    Total Glass Perimeter = 0. (IFCREAL)
    Trim Pen = "Openings - General" (IFCLABEL)
    Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Use New Handles = TRUE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    User Defined 6 = "" (IFCLABEL)
    User Defined 7 = "" (IFCLABEL)
    User Defined 8 = "" (IFCLABEL)
    User Defined 9 = "" (IFCLABEL)
    Version Number = 26 (IFCINTEGER)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
  AC_Pset_CI_Tools_Door | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle = "None" (IFCLABEL)
    (OLD) Exterior Handle Plate = "None" (IFCLABEL)
    (OLD) Exterior Handle Plate Position = 0 (IFCINTEGER)
    (OLD) Interior Handle = "Rod" (IFCLABEL)
    (OLD) Interior Handle Plate = "None" (IFCLABEL)
    (OLD) Interior Handle Plate Position = 0 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Acousitc Rating = "" (IFCLABEL)
    Apply Current Settings = FALSE (IFCBOOLEAN)
    Cavity Closure = "turn in" (IFCLABEL)
    Cavity Closure Exterior = "regular" (IFCLABEL)
    Cavity Closure Interior = "regular" (IFCLABEL)
    Cavity Closure Left = TRUE (IFCBOOLEAN)
    Cavity Closure Right = TRUE (IFCBOOLEAN)
    Cavity Closure Skins Turn In = 0 (IFCINTEGER)
    Cavity Closure Skins Turn Out = 0 (IFCINTEGER)
    Cost = 0. (IFCREAL)
    Door Leaf Mount Exterior = TRUE (IFCBOOLEAN)
    Door Leaf Mount Interior = FALSE (IFCBOOLEAN)
    Door Leaf Number Left = 1 (IFCINTEGER)
    Door Leaf Number Right = 0 (IFCINTEGER)
    Door Mounting to match Graphisoft Doors = TRUE (IFCBOOLEAN)
    Door Type Left = "Surface Slider" (IFCLABEL)
    Door Type Right = "Surface Slider" (IFCLABEL)
    Door belongs to the Zone into which it opens = TRUE (IFCBOOLEAN)
    Door height editing = 0 (IFCINTEGER)
    Elevation = "" (IFCLABEL)
    Exterior Handle Type = 0 (IFCINTEGER)
    Exterior Plate Option = 1 (IFCINTEGER)
    Exterior Plate Type = 0 (IFCINTEGER)
    Exterior Reveal Link Dimensions = TRUE (IFCBOOLEAN)
    Exterior Trim = "None" (IFCLABEL)
    Exterior Trim Bricks = FALSE (IFCBOOLEAN)
    Exterior Trim Mortar Surface = "Paint - Dark Gray" (IFCLABEL)
    Exterior Trim Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Exterior Trim Section Fill = "Background Fill" (IFCLABEL)
    Exterior Trim Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Exterior Trim Section Line Type = 1 (IFCINTEGER)
    Exterior Trim Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Exterior Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim View Pen = "Openings - General" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Frame Mitre Left = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Mitre Right = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Pen = "Openings - General" (IFCLABEL)
    Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame Section Fill = "Background Fill" (IFCLABEL)
    Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame Section Line Type = 1 (IFCINTEGER)
    Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Frame Surface = "Paint - Titanium White" (IFCLABEL)
    Frame Type Head = "Frame" (IFCLABEL)
    Frame Type Head Cut = FALSE (IFCBOOLEAN)
    Frame Type Left = "Frame" (IFCLABEL)
    Frame Type Right = "Frame" (IFCLABEL)
    Frame Under Leaf (frame_under_leaf) = FALSE (IFCBOOLEAN)
    Frame Under Leaf (frame_under_leaf_input) = 0 (IFCINTEGER)
    Frame View Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame View Fill = "Background Fill" (IFCLABEL)
    Frame View Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame View Line Type = 1 (IFCINTEGER)
    Frame View Pen = "Openings - General" (IFCLABEL)
    Glass Pen = "2D Elements - General" (IFCLABEL)
    Glass Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Glass Section Fill = "Background Fill" (IFCLABEL)
    Glass Section Fill Pen = "General - General" (IFCLABEL)
    Glass Section Line Type = 1 (IFCINTEGER)
    Glass Section Pen = "General - General" (IFCLABEL)
    Glass Surface (gs_glass_mat) = "Glass - Clear Fast" (IFCLABEL)
    Glass View Pen = "General - General" (IFCLABEL)
    Glazing = "" (IFCLABEL)
    Glazing Bars Full Sash = FALSE (IFCBOOLEAN)
    Glazing Bars View Pen = "Openings - General" (IFCLABEL)
    Glazing Setout = 4 (IFCINTEGER)
    Group Type = "Others" (IFCLABEL)
    Handle Place Right Leaf = TRUE (IFCBOOLEAN)
    Handle Place Secondary Leaf = FALSE (IFCBOOLEAN)
    Handle View Pen = "2D Elements - General" (IFCLABEL)
    Hardware Keyside Rm. No = "" (IFCLABEL)
    Hardware Pen = "2D Elements - General" (IFCLABEL)
    Hardware Set = "" (IFCLABEL)
    Hardware Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Head Moulding = "None" (IFCLABEL)
    Head Moulding Bricks = FALSE (IFCBOOLEAN)
    Head Moulding Mortar Surface = "Paint - Dark Gray" (IFCLABEL)
    Head Moulding Position = "No Return" (IFCLABEL)
    Head Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Head Moulding Section Fill = "Background Fill" (IFCLABEL)
    Head Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Head Moulding Section Line Type = 1 (IFCINTEGER)
    Head Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Head Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding View Pen = "2D Elements - General" (IFCLABEL)
    Header Detail = "" (IFCLABEL)
    Heat Transfer Rate = "" (IFCLABEL)
    Hinges = "" (IFCLABEL)
    Hole Has Wall's Side Surface = FALSE (IFCBOOLEAN)
    Hole Surface's Split is Curved = FALSE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    IFC Operation (ifc_optype) = 6 (IFCINTEGER)
    IFC Operation (ifc_optypestr) = "Single Door Sliding" (IFCLABEL)
    Inner Frame Bottom/Top Widths Differ = TRUE (IFCBOOLEAN)
    Inner Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame Section Fill = "Background Fill" (IFCLABEL)
    Inner Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame Section Line Type = 1 (IFCINTEGER)
    Inner Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Inner Frame View Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame View Fill = "Background Fill" (IFCLABEL)
    Inner Frame View Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame View Line Type = 1 (IFCINTEGER)
    Inner Frame View Pen = "Openings - General" (IFCLABEL)
    Interior Handle Type = -2 (IFCINTEGER)
    Interior Plate Option = 1 (IFCINTEGER)
    Interior Plate Type = 0 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Jamb Detail = "" (IFCLABEL)
    Jamb Moulding = "X" (IFCLABEL)
    Jamb Moulding Bricks = FALSE (IFCBOOLEAN)
    Jamb Moulding Mortar Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Jamb Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Jamb Moulding Section Fill = "Background Fill" (IFCLABEL)
    Jamb Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Jamb Moulding Section Line Type = 1 (IFCINTEGER)
    Jamb Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Jamb Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding View Pen = "2D Elements - General" (IFCLABEL)
    Kick Plate Exterior = FALSE (IFCBOOLEAN)
    Kick Plate Interior = FALSE (IFCBOOLEAN)
    Kick Plate Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Kick Plate View Pen = "2D Elements - General" (IFCLABEL)
    Leaf Glazing Bars Surface = "Paint - Titanium White" (IFCLABEL)
    Leaf Panel View Pen = "Openings - General" (IFCLABEL)
    Leaf Pen = "Openings - General" (IFCLABEL)
    Leaf Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Leaf Section Fill = "Background Fill" (IFCLABEL)
    Leaf Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Leaf Section Line Type = 1 (IFCINTEGER)
    Leaf Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Leaf Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Leaf View Pen = "Openings - General" (IFCLABEL)
    Link Pens = FALSE (IFCBOOLEAN)
    Lintel Type = "Double 140 x 45mm timber lintel" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lockset = "" (IFCLABEL)
    Louvres View Pen = "Openings - General" (IFCLABEL)
    Main Frame Flange = FALSE (IFCBOOLEAN)
    Manufacturer = "" (IFCLABEL)
    Mullion/Transom Widths Different to Frame = TRUE (IFCBOOLEAN)
    Nominal Size = 16 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Opening Angle in 2D = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Opening Angle in 3D = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Operation Type = "" (IFCLABEL)
    Overlight Glazing Bars = 2 (IFCINTEGER)
    Overlight Layout = 9 (IFCINTEGER)
    Overlight Panel = "F" (IFCLABEL)
    Pivot Line Style = 0 (IFCINTEGER)
    Production Year = "" (IFCLABEL)
    Resolution 3D = "Detailed" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shape Head = "Flat" (IFCLABEL)
    Showing 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Sidelight Double Hung Sash Ratio = 0.5 (IFCREAL)
    Sidelight Glazing Bars = 2 (IFCINTEGER)
    Sidelight Glazing Bars Top = 0 (IFCINTEGER)
    Sidelight Layout Left = 2 (IFCINTEGER)
    Sidelight Layout Right = 4 (IFCINTEGER)
    Sidelight Louvre Angle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sidelight Panel Type = "Bevelled 2" (IFCLABEL)
    Sill Bricks = FALSE (IFCBOOLEAN)
    Sill Detail = "" (IFCLABEL)
    Sill Fall Angle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sill Mortar Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Sill Place Under Leaves = FALSE (IFCBOOLEAN)
    Sill Surface = "Paint - Titanium White" (IFCLABEL)
    Sill Type = "None" (IFCLABEL)
    Size Constraint = 1 (IFCINTEGER)
    Symbol Pen = "2D Elements - General" (IFCLABEL)
    Threshold Type = 2 (IFCINTEGER)
    Timber SIll Type = 0 (IFCINTEGER)
    Total Glass Area = 0. (IFCREAL)
    Total Glass Perimeter = 6.780000000000001 (IFCREAL)
    Trim Pen = "Openings - General" (IFCLABEL)
    Trim Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Use New Handles = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    User Defined 6 = "" (IFCLABEL)
    User Defined 7 = "" (IFCLABEL)
    User Defined 8 = "" (IFCLABEL)
    User Defined 9 = "" (IFCLABEL)
    Version Number = 26 (IFCINTEGER)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
  AC_Pset_CI_Tools_Door | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle = "None" (IFCLABEL)
    (OLD) Exterior Handle Plate = "None" (IFCLABEL)
    (OLD) Exterior Handle Plate Position = 0 (IFCINTEGER)
    (OLD) Interior Handle = "Rod" (IFCLABEL)
    (OLD) Interior Handle Plate = "None" (IFCLABEL)
    (OLD) Interior Handle Plate Position = 0 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Acousitc Rating = "" (IFCLABEL)
    Apply Current Settings = FALSE (IFCBOOLEAN)
    Cavity Closure = "turn in" (IFCLABEL)
    Cavity Closure Exterior = "regular" (IFCLABEL)
    Cavity Closure Interior = "regular" (IFCLABEL)
    Cavity Closure Left = TRUE (IFCBOOLEAN)
    Cavity Closure Right = TRUE (IFCBOOLEAN)
    Cavity Closure Skins Turn In = 0 (IFCINTEGER)
    Cavity Closure Skins Turn Out = 0 (IFCINTEGER)
    Cost = 0. (IFCREAL)
    Door Leaf Mount Exterior = TRUE (IFCBOOLEAN)
    Door Leaf Mount Interior = FALSE (IFCBOOLEAN)
    Door Leaf Number Left = 1 (IFCINTEGER)
    Door Leaf Number Right = 0 (IFCINTEGER)
    Door Mounting to match Graphisoft Doors = TRUE (IFCBOOLEAN)
    Door Type Left = "Standard" (IFCLABEL)
    Door Type Right = "Standard" (IFCLABEL)
    Door belongs to the Zone into which it opens = TRUE (IFCBOOLEAN)
    Door height editing = 0 (IFCINTEGER)
    Elevation = "" (IFCLABEL)
    Exterior Handle Type = 0 (IFCINTEGER)
    Exterior Plate Option = 1 (IFCINTEGER)
    Exterior Plate Type = 0 (IFCINTEGER)
    Exterior Reveal Link Dimensions = TRUE (IFCBOOLEAN)
    Exterior Trim = "None" (IFCLABEL)
    Exterior Trim Bricks = FALSE (IFCBOOLEAN)
    Exterior Trim Mortar Surface = "Paint - Dark Gray" (IFCLABEL)
    Exterior Trim Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Exterior Trim Section Fill = "Background Fill" (IFCLABEL)
    Exterior Trim Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Exterior Trim Section Line Type = 1 (IFCINTEGER)
    Exterior Trim Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Exterior Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim View Pen = "Openings - General" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Frame Mitre Left = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Mitre Right = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Pen = "Openings - General" (IFCLABEL)
    Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame Section Fill = "Background Fill" (IFCLABEL)
    Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame Section Line Type = 1 (IFCINTEGER)
    Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Frame Surface = "Paint - Titanium White" (IFCLABEL)
    Frame Type Head = "Frame" (IFCLABEL)
    Frame Type Head Cut = FALSE (IFCBOOLEAN)
    Frame Type Left = "Frame" (IFCLABEL)
    Frame Type Right = "Frame" (IFCLABEL)
    Frame Under Leaf (frame_under_leaf) = FALSE (IFCBOOLEAN)
    Frame Under Leaf (frame_under_leaf_input) = 0 (IFCINTEGER)
    Frame View Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame View Fill = "Background Fill" (IFCLABEL)
    Frame View Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame View Line Type = 1 (IFCINTEGER)
    Frame View Pen = "Openings - General" (IFCLABEL)
    Glass Pen = "2D Elements - General" (IFCLABEL)
    Glass Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Glass Section Fill = "Background Fill" (IFCLABEL)
    Glass Section Fill Pen = "General - General" (IFCLABEL)
    Glass Section Line Type = 1 (IFCINTEGER)
    Glass Section Pen = "General - General" (IFCLABEL)
    Glass Surface (gs_glass_mat) = "Glass - Clear Fast" (IFCLABEL)
    Glass View Pen = "General - General" (IFCLABEL)
    Glazing = "" (IFCLABEL)
    Glazing Bars Full Sash = FALSE (IFCBOOLEAN)
    Glazing Bars View Pen = "Openings - General" (IFCLABEL)
    Glazing Setout = 4 (IFCINTEGER)
    Group Type = "Others" (IFCLABEL)
    Handle Place Right Leaf = TRUE (IFCBOOLEAN)
    Handle Place Secondary Leaf = FALSE (IFCBOOLEAN)
    Handle View Pen = "2D Elements - General" (IFCLABEL)
    Hardware Keyside Rm. No = "" (IFCLABEL)
    Hardware Pen = "2D Elements - General" (IFCLABEL)
    Hardware Set = "" (IFCLABEL)
    Hardware Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Head Moulding = "None" (IFCLABEL)
    Head Moulding Bricks = FALSE (IFCBOOLEAN)
    Head Moulding Mortar Surface = "Paint - Dark Gray" (IFCLABEL)
    Head Moulding Position = "No Return" (IFCLABEL)
    Head Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Head Moulding Section Fill = "Background Fill" (IFCLABEL)
    Head Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Head Moulding Section Line Type = 1 (IFCINTEGER)
    Head Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Head Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding View Pen = "2D Elements - General" (IFCLABEL)
    Header Detail = "" (IFCLABEL)
    Heat Transfer Rate = "" (IFCLABEL)
    Hinges = "" (IFCLABEL)
    Hole Has Wall's Side Surface = FALSE (IFCBOOLEAN)
    Hole Surface's Split is Curved = FALSE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    IFC Operation (ifc_optype) = 1 (IFCINTEGER)
    IFC Operation (ifc_optypestr) = "Single Door Single Swing" (IFCLABEL)
    Inner Frame Bottom/Top Widths Differ = TRUE (IFCBOOLEAN)
    Inner Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame Section Fill = "Background Fill" (IFCLABEL)
    Inner Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame Section Line Type = 1 (IFCINTEGER)
    Inner Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Inner Frame View Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame View Fill = "Background Fill" (IFCLABEL)
    Inner Frame View Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame View Line Type = 1 (IFCINTEGER)
    Inner Frame View Pen = "Openings - General" (IFCLABEL)
    Interior Handle Type = -2 (IFCINTEGER)
    Interior Plate Option = 1 (IFCINTEGER)
    Interior Plate Type = 0 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Jamb Detail = "" (IFCLABEL)
    Jamb Moulding = "X" (IFCLABEL)
    Jamb Moulding Bricks = FALSE (IFCBOOLEAN)
    Jamb Moulding Mortar Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Jamb Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Jamb Moulding Section Fill = "Background Fill" (IFCLABEL)
    Jamb Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Jamb Moulding Section Line Type = 1 (IFCINTEGER)
    Jamb Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Jamb Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding View Pen = "2D Elements - General" (IFCLABEL)
    Kick Plate Exterior = FALSE (IFCBOOLEAN)
    Kick Plate Interior = FALSE (IFCBOOLEAN)
    Kick Plate Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Kick Plate View Pen = "2D Elements - General" (IFCLABEL)
    Leaf Glazing Bars Surface = "Paint - Lead Oxide Yellow" (IFCLABEL)
    Leaf Panel View Pen = "Openings - General" (IFCLABEL)
    Leaf Pen = "Openings - General" (IFCLABEL)
    Leaf Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Leaf Section Fill = "Background Fill" (IFCLABEL)
    Leaf Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Leaf Section Line Type = 1 (IFCINTEGER)
    Leaf Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Leaf Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Leaf View Pen = "Openings - General" (IFCLABEL)
    Link Pens = FALSE (IFCBOOLEAN)
    Lintel Type = "Double 140 x 45mm timber lintel" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lockset = "" (IFCLABEL)
    Louvres View Pen = "Openings - General" (IFCLABEL)
    Main Frame Flange = FALSE (IFCBOOLEAN)
    Manufacturer = "" (IFCLABEL)
    Mullion/Transom Widths Different to Frame = TRUE (IFCBOOLEAN)
    Nominal Size = 16 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Opening Angle in 2D = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Opening Angle in 3D = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Operation Type = "" (IFCLABEL)
    Overlight Glazing Bars = 2 (IFCINTEGER)
    Overlight Layout = 9 (IFCINTEGER)
    Overlight Panel = "F" (IFCLABEL)
    Pivot Line Style = 0 (IFCINTEGER)
    Production Year = "" (IFCLABEL)
    Resolution 3D = "Detailed" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shape Head = "Flat" (IFCLABEL)
    Showing 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Sidelight Double Hung Sash Ratio = 0.5 (IFCREAL)
    Sidelight Glazing Bars = 2 (IFCINTEGER)
    Sidelight Glazing Bars Top = 0 (IFCINTEGER)
    Sidelight Layout Left = 2 (IFCINTEGER)
    Sidelight Layout Right = 4 (IFCINTEGER)
    Sidelight Louvre Angle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sidelight Panel Type = "Bevelled 2" (IFCLABEL)
    Sill Bricks = FALSE (IFCBOOLEAN)
    Sill Detail = "" (IFCLABEL)
    Sill Fall Angle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sill Mortar Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Sill Place Under Leaves = FALSE (IFCBOOLEAN)
    Sill Surface = "Paint - Titanium White" (IFCLABEL)
    Sill Type = "None" (IFCLABEL)
    Size Constraint = 1 (IFCINTEGER)
    Symbol Pen = "2D Elements - General" (IFCLABEL)
    Threshold Type = 2 (IFCINTEGER)
    Timber SIll Type = 0 (IFCINTEGER)
    Total Glass Area = 0. (IFCREAL)
    Total Glass Perimeter = 0. (IFCREAL)
    Trim Pen = "Openings - General" (IFCLABEL)
    Trim Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Use New Handles = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    User Defined 6 = "" (IFCLABEL)
    User Defined 7 = "" (IFCLABEL)
    User Defined 8 = "" (IFCLABEL)
    User Defined 9 = "" (IFCLABEL)
    Version Number = 26 (IFCINTEGER)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
  AC_Pset_RenovationAndPhasing | properties | on 58 objects (58 IFCBUILDINGELEMENTPROXY)
    Renovation Status = "Existing" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    Renovation Status = "New" (IFCLABEL)
  ArchiCADQuantities | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Bottom Elevation To First Reference Level = -16290.00000000001 [MILLI METRE]
    Bottom Elevation To Home Story = 999.9999999999858 [MILLI METRE]
    Bottom Elevation To Project Zero = -16290.00000000001 [MILLI METRE]
    Bottom Elevation To Sea Level = 14159.99999999999 [MILLI METRE]
    Bottom Elevation To Second Reference Level = -16290.00000000001 [MILLI METRE]
    Bottom Surface Area (Net) = 2.1367272 [SQUARE_METRE]
    Elevation to 1st Reference Level = -16290.00000000001 [MILLI METRE]
    Elevation to 2nd Reference Level = -16290.00000000001 [MILLI METRE]
    Elevation to Linked/Home Story = 999.9999999999858 [MILLI METRE]
    Elevation to Project Zero = -16290.00000000001 [MILLI METRE]
    Elevation to Sea Level = 14159.99999999999 [MILLI METRE]
    Frame Thickness = 50. [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Home Offset = 999.9999999999858 [MILLI METRE]
    Nominal W/D Opening Height on the Reveal Side = 1200. [MILLI METRE]
    Nominal W/D Opening Height on the Side Opposite to the Reveal Side = 1200. [MILLI METRE]
    Nominal W/D Opening Surface Area on the Reveal Side = 0.642 [SQUARE_METRE]
    Nominal W/D Opening Surface Area on the Side Opposite to the Reveal Side = 0.642 [SQUARE_METRE]
    Nominal W/D Opening Width on the Reveal Side = 535. [MILLI METRE]
    Nominal W/D Opening Width on the Side Opposite to the Reveal Side = 535. [MILLI METRE]
    Sill/Header Value = 2199.999999999989 [MILLI METRE]
    Surface Area = 2.1367272 [SQUARE_METRE]
    Top Elevation To First Reference Level = -15090.00000000001 [MILLI METRE]
    Top Elevation To Home Story = 2199.999999999985 [MILLI METRE]
    Top Elevation To Project Zero = -15090.00000000001 [MILLI METRE]
    Top Elevation To Sea Level = 15359.99999999999 [MILLI METRE]
    Top Elevation To Second Reference Level = -15090.00000000001 [MILLI METRE]
    Volume (Net) = 0.02272790399999999 [CUBIC_METRE]
    W/D Head Height on the Reveal Side = 2199.999999999989 [MILLI METRE]
    W/D Head Height on the Side Opposite to the Reveal Side = 2199.999999999989 [MILLI METRE]
    W/D Nominal Head Height = 2199.999999999989 [MILLI METRE]
    W/D Nominal Sill Height = 999.9999999999886 [MILLI METRE]
    W/D Opening Height on the Reveal Side = 1199.999999999999 [MILLI METRE]
    W/D Opening Height on the Side Opposite to the Reveal Side = 1199.999999999999 [MILLI METRE]
    W/D Opening Nominal Surface Area = 0.642 [SQUARE_METRE]
    W/D Opening Nominal Volume = 0.06869400000000001 [CUBIC_METRE]
    W/D Opening Opening Volume = 0.0686940000000001 [CUBIC_METRE]
    W/D Opening Surface Area = 2.1367272 [SQUARE_METRE]
    W/D Opening Surface Area on the Reveal Side = 0.6419999999999998 [SQUARE_METRE]
    W/D Opening Surface Area on the Side Opposite to the Reveal Side = 0.6419999999999998 [SQUARE_METRE]
    W/D Opening Width on the Reveal Side = 535.0000000000001 [MILLI METRE]
    W/D Opening Width on the Side Opposite to the Reveal Side = 535.0000000000001 [MILLI METRE]
    W/D Sill Height on the Reveal Side = 999.9999999999886 [MILLI METRE]
    W/D Sill Height on the Side Opposite to the Reveal Side = 999.9999999999886 [MILLI METRE]
    Wall Thickness = 107. [MILLI METRE]
    Width = 535. [MILLI METRE]
  ArchiCADQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Elevation To First Reference Level = -17290. [MILLI METRE]
    Bottom Elevation To Home Story = -3.552713678800501E-12 [MILLI METRE]
    Bottom Elevation To Project Zero = -17290. [MILLI METRE]
    Bottom Elevation To Sea Level = 13160. [MILLI METRE]
    Bottom Elevation To Second Reference Level = -17290. [MILLI METRE]
    Bottom Surface Area (Net) = 5.634613142827989 [SQUARE_METRE]
    Elevation to 1st Reference Level = -17290. [MILLI METRE]
    Elevation to 2nd Reference Level = -17290. [MILLI METRE]
    Elevation to Linked/Home Story = -3.552713678800501E-12 [MILLI METRE]
    Elevation to Project Zero = -17290. [MILLI METRE]
    Elevation to Sea Level = 13160. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Height = 2040. [MILLI METRE]
    Home Offset = -3.552713678800501E-12 [MILLI METRE]
    Nominal W/D Opening Height on the Reveal Side = 2040. [MILLI METRE]
    Nominal W/D Opening Height on the Side Opposite to the Reveal Side = 2040. [MILLI METRE]
    Nominal W/D Opening Surface Area on the Reveal Side = 2.0196 [SQUARE_METRE]
    Nominal W/D Opening Surface Area on the Side Opposite to the Reveal Side = 2.0196 [SQUARE_METRE]
    Nominal W/D Opening Width on the Reveal Side = 990. [MILLI METRE]
    Nominal W/D Opening Width on the Side Opposite to the Reveal Side = 990. [MILLI METRE]
    Sill/Header Value = 0. [MILLI METRE]
    Surface Area = 5.634613142827989 [SQUARE_METRE]
    Top Elevation To First Reference Level = -15250. [MILLI METRE]
    Top Elevation To Home Story = 2039.999999999996 [MILLI METRE]
    Top Elevation To Project Zero = -15250. [MILLI METRE]
    Top Elevation To Sea Level = 15200. [MILLI METRE]
    Top Elevation To Second Reference Level = -15250. [MILLI METRE]
    Volume (Net) = 0.08649808000000003 [CUBIC_METRE]
    W/D Head Height on the Reveal Side = 2040. [MILLI METRE]
    W/D Head Height on the Side Opposite to the Reveal Side = 2040. [MILLI METRE]
    W/D Nominal Head Height = 2040. [MILLI METRE]
    W/D Nominal Sill Height = 0. [MILLI METRE]
    W/D Opening Height on the Reveal Side = 2039.999999999999 [MILLI METRE]
    W/D Opening Height on the Side Opposite to the Reveal Side = 2039.999999999999 [MILLI METRE]
    W/D Opening Nominal Surface Area = 2.0196 [SQUARE_METRE]
    W/D Opening Nominal Volume = 0.222156 [CUBIC_METRE]
    W/D Opening Opening Volume = 0.2221560000000008 [CUBIC_METRE]
    W/D Opening Surface Area = 5.634613142827989 [SQUARE_METRE]
    W/D Opening Surface Area on the Reveal Side = 2.019599999999999 [SQUARE_METRE]
    W/D Opening Surface Area on the Side Opposite to the Reveal Side = 2.019599999999999 [SQUARE_METRE]
    W/D Opening Width on the Reveal Side = 990. [MILLI METRE]
    W/D Opening Width on the Side Opposite to the Reveal Side = 990. [MILLI METRE]
    W/D Sill Height on the Reveal Side = 0. [MILLI METRE]
    W/D Sill Height on the Side Opposite to the Reveal Side = 0. [MILLI METRE]
    Wall Thickness = 110. [MILLI METRE]
    Width = 990. [MILLI METRE]
  ArchiCADQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.488 [SQUARE_METRE]
    Bottom Elevation To First Reference Level = -17040. [MILLI METRE]
    Bottom Elevation To Home Story = 250. [MILLI METRE]
    Bottom Elevation To Project Zero = -17040. [MILLI METRE]
    Bottom Elevation To Sea Level = 13410. [MILLI METRE]
    Bottom Elevation To Second Reference Level = -17040. [MILLI METRE]
    Bottom Surface Area (Net) = 2.556098968828126 [SQUARE_METRE]
    Elevation to 1st Reference Level = -17040. [MILLI METRE]
    Elevation to 2nd Reference Level = -17040. [MILLI METRE]
    Elevation to Linked/Home Story = 250. [MILLI METRE]
    Elevation to Project Zero = -17040. [MILLI METRE]
    Elevation to Sea Level = 13410. [MILLI METRE]
    Height = 1335. [MILLI METRE]
    Home Offset = 250. [MILLI METRE]
    Length (A) = 488. [MILLI METRE]
    Surface Area = 2.556098968828126 [SQUARE_METRE]
    Survey Coordinate X = 370494292.0867943 [MILLI METRE]
    Survey Coordinate Y = 804285788.2577338 [MILLI METRE]
    Survey Coordinate Z = 13410. [MILLI METRE]
    Top Elevation To First Reference Level = -15676. [MILLI METRE]
    Top Elevation To Home Story = 1614.000000000001 [MILLI METRE]
    Top Elevation To Project Zero = -15676. [MILLI METRE]
    Top Elevation To Sea Level = 14774. [MILLI METRE]
    Top Elevation To Second Reference Level = -15676. [MILLI METRE]
    Top Surface Area (Net) = 0.488 [SQUARE_METRE]
    Volume (Net) = 0.2485024954143461 [CUBIC_METRE]
    Width = 1000. [MILLI METRE]
  ArchiCADQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.3025000000000005 [SQUARE_METRE]
    Bottom Elevation To First Reference Level = -17289.99999999999 [MILLI METRE]
    Bottom Elevation To Home Story = 7.105427357601002E-12 [MILLI METRE]
    Bottom Elevation To Project Zero = -17289.99999999999 [MILLI METRE]
    Bottom Elevation To Sea Level = 13160.00000000001 [MILLI METRE]
    Bottom Elevation To Second Reference Level = -17289.99999999999 [MILLI METRE]
    Bottom Surface Area (Conditional) = 0.3025000000000005 [SQUARE_METRE]
    Bottom Surface Area (Gross) = 0.3025000000000005 [SQUARE_METRE]
    Bottom Surface Area (Net) = 0.3025000000000005 [SQUARE_METRE]
    Edge Surface Area (Gross) = 0.5500000000000005 [SQUARE_METRE]
    Edge Surface Area (Net) = 0.5500000000000005 [SQUARE_METRE]
    Elevation Bottom = -17289.99999999999 [MILLI METRE]
    Elevation Top = -17039.99999999999 [MILLI METRE]
    Elevation to 1st Reference Level = -17289.99999999999 [MILLI METRE]
    Elevation to 2nd Reference Level = -17289.99999999999 [MILLI METRE]
    Elevation to Linked/Home Story = 7.105427357601002E-12 [MILLI METRE]
    Elevation to Project Zero = -17289.99999999999 [MILLI METRE]
    Elevation to Sea Level = 13160.00000000001 [MILLI METRE]
    Floor Plan Holes Perimeter = 0. [MILLI METRE]
    Floor Plan Perimeter = 2200.000000000002 [MILLI METRE]
    Height = 250. [MILLI METRE]
    Holes Surface Area = 0. [SQUARE_METRE]
    Home Offset = 7.105427357601002E-12 [MILLI METRE]
    Surface Area = 0.3025000000000005 [SQUARE_METRE]
    Surface Area of the Slab Bottom (Gross) = 0.3025000000000005 [SQUARE_METRE]
    Surface Area of the Slab Bottom (Gross, with holes) = 0.3025000000000005 [SQUARE_METRE]
    Surface Area of the Slab Edges (Gross) = 0.5500000000000005 [SQUARE_METRE]
    Surface Area of the Slab Edges (Gross, with holes) = 0.5500000000000005 [SQUARE_METRE]
    Surface Area of the Slab Top (Conditional) = 0.3025000000000005 [SQUARE_METRE]
    Surface Area of the Slab Top (Gross) = 0.3025000000000005 [SQUARE_METRE]
    Surface Area of the Slab Top (Gross, with holes) = 0.3025000000000005 [SQUARE_METRE]
    Thickness = 250. [MILLI METRE]
    Top Elevation To First Reference Level = -17039.99999999999 [MILLI METRE]
    Top Elevation To Home Story = 250.0000000000071 [MILLI METRE]
    Top Elevation To Project Zero = -17039.99999999999 [MILLI METRE]
    Top Elevation To Sea Level = 13410.00000000001 [MILLI METRE]
    Top Elevation To Second Reference Level = -17039.99999999999 [MILLI METRE]
    Top Surface Area (Conditional) = 0.3025000000000005 [SQUARE_METRE]
    Top Surface Area (Gross) = 0.3025000000000005 [SQUARE_METRE]
    Top Surface Area (Net) = 0.3025000000000005 [SQUARE_METRE]
    Volume (Conditional) = 0.07562500000000014 [CUBIC_METRE]
    Volume (Gross) = 0.07562500000000014 [CUBIC_METRE]
    Volume (Net) = 0.07562500000000014 [CUBIC_METRE]
  ArchiCADQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Elevation To First Reference Level = -17290. [MILLI METRE]
    Bottom Elevation To Home Story = -3.552713678800501E-12 [MILLI METRE]
    Bottom Elevation To Project Zero = -17290. [MILLI METRE]
    Bottom Elevation To Sea Level = 13160. [MILLI METRE]
    Bottom Elevation To Second Reference Level = -17290. [MILLI METRE]
    Bottom Surface Area (Net) = 5.021056571413995 [SQUARE_METRE]
    Elevation to 1st Reference Level = -17290. [MILLI METRE]
    Elevation to 2nd Reference Level = -17290. [MILLI METRE]
    Elevation to Linked/Home Story = -3.552713678800501E-12 [MILLI METRE]
    Elevation to Project Zero = -17290. [MILLI METRE]
    Elevation to Sea Level = 13160. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Height = 2040. [MILLI METRE]
    Home Offset = -3.552713678800501E-12 [MILLI METRE]
    Nominal W/D Opening Height on the Reveal Side = 2040. [MILLI METRE]
    Nominal W/D Opening Height on the Side Opposite to the Reveal Side = 2040. [MILLI METRE]
    Nominal W/D Opening Surface Area on the Reveal Side = 1.7952 [SQUARE_METRE]
    Nominal W/D Opening Surface Area on the Side Opposite to the Reveal Side = 1.7952 [SQUARE_METRE]
    Nominal W/D Opening Width on the Reveal Side = 880.0000000000001 [MILLI METRE]
    Nominal W/D Opening Width on the Side Opposite to the Reveal Side = 880.0000000000001 [MILLI METRE]
    Sill/Header Value = 0. [MILLI METRE]
    Surface Area = 5.021056571413995 [SQUARE_METRE]
    Top Elevation To First Reference Level = -15250. [MILLI METRE]
    Top Elevation To Home Story = 2039.999999999996 [MILLI METRE]
    Top Elevation To Project Zero = -15250. [MILLI METRE]
    Top Elevation To Sea Level = 15200. [MILLI METRE]
    Top Elevation To Second Reference Level = -15250. [MILLI METRE]
    Volume (Net) = 0.07837854000000005 [CUBIC_METRE]
    W/D Head Height on the Reveal Side = 2040. [MILLI METRE]
    W/D Head Height on the Side Opposite to the Reveal Side = 2040. [MILLI METRE]
    W/D Nominal Head Height = 2040. [MILLI METRE]
    W/D Nominal Sill Height = 0. [MILLI METRE]
    W/D Opening Height on the Reveal Side = 2039.999999999999 [MILLI METRE]
    W/D Opening Height on the Side Opposite to the Reveal Side = 2039.999999999999 [MILLI METRE]
    W/D Opening Nominal Surface Area = 1.7952 [SQUARE_METRE]
    W/D Opening Nominal Volume = 0.197472 [CUBIC_METRE]
    W/D Opening Opening Volume = 0.1974720000000006 [CUBIC_METRE]
    W/D Opening Surface Area = 5.021056571413995 [SQUARE_METRE]
    W/D Opening Surface Area on the Reveal Side = 1.795199999999997 [SQUARE_METRE]
    W/D Opening Surface Area on the Side Opposite to the Reveal Side = 1.795199999999997 [SQUARE_METRE]
    W/D Opening Width on the Reveal Side = 879.999999999999 [MILLI METRE]
    W/D Opening Width on the Side Opposite to the Reveal Side = 879.999999999999 [MILLI METRE]
    W/D Sill Height on the Reveal Side = 0. [MILLI METRE]
    W/D Sill Height on the Side Opposite to the Reveal Side = 0. [MILLI METRE]
    Wall Thickness = 110. [MILLI METRE]
    Width = 880.0000000000001 [MILLI METRE]
  ArchiCADQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0. [SQUARE_METRE]
    Bottom Elevation To First Reference Level = -17339.99999999999 [MILLI METRE]
    Bottom Elevation To Home Story = -49.99999999999361 [MILLI METRE]
    Bottom Elevation To Project Zero = -17339.99999999999 [MILLI METRE]
    Bottom Elevation To Sea Level = 13110.00000000001 [MILLI METRE]
    Bottom Elevation To Second Reference Level = -17339.99999999999 [MILLI METRE]
    Bottom Surface Area (Net) = 35.92907544452959 [SQUARE_METRE]
    Elevation to 1st Reference Level = -17289.99999999999 [MILLI METRE]
    Elevation to 2nd Reference Level = -17289.99999999999 [MILLI METRE]
    Elevation to Linked/Home Story = 7.105427357601002E-12 [MILLI METRE]
    Elevation to Project Zero = -17289.99999999999 [MILLI METRE]
    Elevation to Sea Level = 13160.00000000001 [MILLI METRE]
    Height = 2400.000000000001 [MILLI METRE]
    Home Offset = 7.105427357601002E-12 [MILLI METRE]
    Length (A) = 0. [MILLI METRE]
    Surface Area = 35.92907544452959 [SQUARE_METRE]
    Survey Coordinate X = 370494081.8362165 [MILLI METRE]
    Survey Coordinate Y = 804293168.9859614 [MILLI METRE]
    Survey Coordinate Z = 13160.00000000001 [MILLI METRE]
    Top Elevation To First Reference Level = -14889.99999999999 [MILLI METRE]
    Top Elevation To Home Story = 2400.000000000009 [MILLI METRE]
    Top Elevation To Project Zero = -14889.99999999999 [MILLI METRE]
    Top Elevation To Sea Level = 15560.00000000001 [MILLI METRE]
    Top Elevation To Second Reference Level = -14889.99999999999 [MILLI METRE]
    Top Surface Area (Net) = 0. [SQUARE_METRE]
    Volume (Net) = 0.1550287624989933 [CUBIC_METRE]
    Width = 0. [MILLI METRE]
  ArchiCADQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Elevation To First Reference Level = -17290. [MILLI METRE]
    Bottom Elevation To Home Story = -3.552713678800501E-12 [MILLI METRE]
    Bottom Elevation To Project Zero = -17290. [MILLI METRE]
    Bottom Elevation To Sea Level = 13160. [MILLI METRE]
    Bottom Elevation To Second Reference Level = -17290. [MILLI METRE]
    Bottom Surface Area (Net) = 5.021056571413995 [SQUARE_METRE]
    Elevation to 1st Reference Level = -17290. [MILLI METRE]
    Elevation to 2nd Reference Level = -17290. [MILLI METRE]
    Elevation to Linked/Home Story = -3.552713678800501E-12 [MILLI METRE]
    Elevation to Project Zero = -17290. [MILLI METRE]
    Elevation to Sea Level = 13160. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Height = 2040. [MILLI METRE]
    Home Offset = -3.552713678800501E-12 [MILLI METRE]
    Nominal W/D Opening Height on the Reveal Side = 2040. [MILLI METRE]
    Nominal W/D Opening Height on the Side Opposite to the Reveal Side = 2040. [MILLI METRE]
    Nominal W/D Opening Surface Area on the Reveal Side = 1.7952 [SQUARE_METRE]
    Nominal W/D Opening Surface Area on the Side Opposite to the Reveal Side = 1.7952 [SQUARE_METRE]
    Nominal W/D Opening Width on the Reveal Side = 880.0000000000001 [MILLI METRE]
    Nominal W/D Opening Width on the Side Opposite to the Reveal Side = 880.0000000000001 [MILLI METRE]
    Sill/Header Value = 0. [MILLI METRE]
    Surface Area = 5.021056571413995 [SQUARE_METRE]
    Top Elevation To First Reference Level = -15250. [MILLI METRE]
    Top Elevation To Home Story = 2039.999999999996 [MILLI METRE]
    Top Elevation To Project Zero = -15250. [MILLI METRE]
    Top Elevation To Sea Level = 15200. [MILLI METRE]
    Top Elevation To Second Reference Level = -15250. [MILLI METRE]
    Volume (Net) = 0.07837854000000005 [CUBIC_METRE]
    W/D Head Height on the Reveal Side = 2040. [MILLI METRE]
    W/D Head Height on the Side Opposite to the Reveal Side = 2040. [MILLI METRE]
    W/D Nominal Head Height = 2040. [MILLI METRE]
    W/D Nominal Sill Height = 0. [MILLI METRE]
    W/D Opening Height on the Reveal Side = 2039.999999999999 [MILLI METRE]
    W/D Opening Height on the Side Opposite to the Reveal Side = 2039.999999999999 [MILLI METRE]
    W/D Opening Nominal Surface Area = 1.7952 [SQUARE_METRE]
    W/D Opening Nominal Volume = 0.197472 [CUBIC_METRE]
    W/D Opening Opening Volume = 0.1974720000000003 [CUBIC_METRE]
    W/D Opening Surface Area = 5.021056571413995 [SQUARE_METRE]
    W/D Opening Surface Area on the Reveal Side = 1.795199999999999 [SQUARE_METRE]
    W/D Opening Surface Area on the Side Opposite to the Reveal Side = 1.795199999999999 [SQUARE_METRE]
    W/D Opening Width on the Reveal Side = 879.9999999999999 [MILLI METRE]
    W/D Opening Width on the Side Opposite to the Reveal Side = 879.9999999999999 [MILLI METRE]
    W/D Sill Height on the Reveal Side = 0. [MILLI METRE]
    W/D Sill Height on the Side Opposite to the Reveal Side = 0. [MILLI METRE]
    Wall Thickness = 110. [MILLI METRE]
    Width = 880.0000000000001 [MILLI METRE]
  ArchiCADQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Elevation To First Reference Level = -17290. [MILLI METRE]
    Bottom Elevation To Home Story = -3.552713678800501E-12 [MILLI METRE]
    Bottom Elevation To Project Zero = -17290. [MILLI METRE]
    Bottom Elevation To Sea Level = 13160. [MILLI METRE]
    Bottom Elevation To Second Reference Level = -17290. [MILLI METRE]
    Bottom Surface Area (Net) = 5.60846314282799 [SQUARE_METRE]
    Elevation to 1st Reference Level = -17290. [MILLI METRE]
    Elevation to 2nd Reference Level = -17290. [MILLI METRE]
    Elevation to Linked/Home Story = -3.552713678800501E-12 [MILLI METRE]
    Elevation to Project Zero = -17290. [MILLI METRE]
    Elevation to Sea Level = 13160. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Height = 2040. [MILLI METRE]
    Home Offset = -3.552713678800501E-12 [MILLI METRE]
    Nominal W/D Opening Height on the Reveal Side = 2040. [MILLI METRE]
    Nominal W/D Opening Height on the Side Opposite to the Reveal Side = 2040. [MILLI METRE]
    Nominal W/D Opening Surface Area on the Reveal Side = 2.2236 [SQUARE_METRE]
    Nominal W/D Opening Surface Area on the Side Opposite to the Reveal Side = 2.2236 [SQUARE_METRE]
    Nominal W/D Opening Width on the Reveal Side = 1090. [MILLI METRE]
    Nominal W/D Opening Width on the Side Opposite to the Reveal Side = 1090. [MILLI METRE]
    Sill/Header Value = 0. [MILLI METRE]
    Surface Area = 5.60846314282799 [SQUARE_METRE]
    Top Elevation To First Reference Level = -15250. [MILLI METRE]
    Top Elevation To Home Story = 2039.999999999996 [MILLI METRE]
    Top Elevation To Project Zero = -15250. [MILLI METRE]
    Top Elevation To Sea Level = 15200. [MILLI METRE]
    Top Elevation To Second Reference Level = -15250. [MILLI METRE]
    Volume (Net) = 0.08585057999999998 [CUBIC_METRE]
    W/D Head Height on the Reveal Side = 2040. [MILLI METRE]
    W/D Head Height on the Side Opposite to the Reveal Side = 2040. [MILLI METRE]
    W/D Nominal Head Height = 2040. [MILLI METRE]
    W/D Nominal Sill Height = 0. [MILLI METRE]
    W/D Opening Height on the Reveal Side = 2039.999999999999 [MILLI METRE]
    W/D Opening Height on the Side Opposite to the Reveal Side = 2039.999999999999 [MILLI METRE]
    W/D Opening Nominal Surface Area = 2.2236 [SQUARE_METRE]
    W/D Opening Nominal Volume = 0.144534 [CUBIC_METRE]
    W/D Opening Opening Volume = 0.1445340000000014 [CUBIC_METRE]
    W/D Opening Surface Area = 5.60846314282799 [SQUARE_METRE]
    W/D Opening Surface Area on the Reveal Side = 2.223599999999999 [SQUARE_METRE]
    W/D Opening Surface Area on the Side Opposite to the Reveal Side = 2.223599999999999 [SQUARE_METRE]
    W/D Opening Width on the Reveal Side = 1090. [MILLI METRE]
    W/D Opening Width on the Side Opposite to the Reveal Side = 1090. [MILLI METRE]
    W/D Sill Height on the Reveal Side = 0. [MILLI METRE]
    W/D Sill Height on the Side Opposite to the Reveal Side = 0. [MILLI METRE]
    Wall Thickness = 65. [MILLI METRE]
    Width = 1090. [MILLI METRE]
  ArchiCADQuantities: 60 more contents on 60 objects not shown
  AC_Equantity_CI_Tools_Door | quantities | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle Length = 160. [MILLI METRE]
    (OLD) Exterior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Exterior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Exterior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Exterior Handle Projection = 45. [MILLI METRE]
    (OLD) Exterior Handle Thickness = 19. [MILLI METRE]
    (OLD) Exterior Handle Width = 15. [MILLI METRE]
    (OLD) Interior Handle Length = 160. [MILLI METRE]
    (OLD) Interior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Interior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Interior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Interior Handle Projection = 45. [MILLI METRE]
    (OLD) Interior Handle Thickness = 19. [MILLI METRE]
    (OLD) Interior Handle Width = 16. [MILLI METRE]
    2D Symbol Detail Level = 0. [MILLI METRE]
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    ??? (extendFrameL) = 0. [MILLI METRE]
    ??? (extendFrameR) = 0. [MILLI METRE]
    ??? (extendOpeningL) = 10. [MILLI METRE]
    ??? (extendOpeningR) = 10. [MILLI METRE]
    Allow space for mitred ends = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Height = 76. [MILLI METRE]
    Brick Length = 230. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Brick Mortar Thickness = 10. [MILLI METRE]
    Camera Distance Fully Open = 1000. [MILLI METRE]
    Camera Distance Fully Shut = 3000. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset from Frame = 0. [MILLI METRE]
    Door Leaf Pivot Offset Left = 0. [MILLI METRE]
    Door Leaf Pivot Offset Right = 0. [MILLI METRE]
    Door Leaf Thickness = 35. [MILLI METRE]
    Door Leaf Width Left = 810. [MILLI METRE]
    Door Leaf Width Right = 810. [MILLI METRE]
    Door Stop Max Width = 90. [MILLI METRE]
    Door Stop Thickness = 10. [MILLI METRE]
    Egress Height = 1995. [MILLI METRE]
    Egress Width = 765. [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 80. [MILLI METRE]
    Exterior Trim Extend Below Threshold = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 18. [MILLI METRE]
    Exterior Trim Width = 80. [MILLI METRE]
    Fixed Glass Position = 12. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Width = 50. [MILLI METRE]
    Framed Glass Position = 12. [MILLI METRE]
    Glass Pane Spacing = 16. [MILLI METRE]
    Glass Thickness = 6. [MILLI METRE]
    Head Gap Height = 5. [MILLI METRE]
    Head Moulding Brick Width = 80. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 40. [MILLI METRE]
    Head Moulding Width = 80. [MILLI METRE]
    Inner Frame Backset = 10. [MILLI METRE]
    Inner Frame Depth = 35. [MILLI METRE]
    Inner Frame Head Width = 70. [MILLI METRE]
    Inner Frame Sill Width = 100. [MILLI METRE]
    Inner Frame Width = 25. [MILLI METRE]
    Interior Reveal Thickness = 18. [MILLI METRE]
    Interior Sill Extension = 80. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 10. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 20. [MILLI METRE]
    Interior Trim Width = 65. [MILLI METRE]
    Jamb Moulding Brick Width = 80. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Leaf Height (max) = 1980. [MILLI METRE]
    Leaf Height = 1980. [MILLI METRE]
    Leaf Overlap Head Frame = 0. [MILLI METRE]
    Leaf Overlap Left = 0. [MILLI METRE]
    Leaf Overlap Left Jamb = 0. [MILLI METRE]
    Leaf Overlap Right = 0. [MILLI METRE]
    Leaf Overlap Right Jamb = 0. [MILLI METRE]
    Leaf Width = 810. [MILLI METRE]
    Lintel Depth = 140. [MILLI METRE]
    Lintel Extension Left = 45. [MILLI METRE]
    Lintel Extension Right = 45. [MILLI METRE]
    Lintel Offset Back from Frame = 0. [MILLI METRE]
    Lintel Thickness = 90. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset) = 10. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset_2) = 10. [MILLI METRE]
    Main Frame Depth (FD) = 0. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 130. [MILLI METRE]
    Main Frame Flange Thickness = 5. [MILLI METRE]
    Main Frame Flange Width = 20. [MILLI METRE]
    Main Frame Width = 35. [MILLI METRE]
    Mullion Width = 35. [MILLI METRE]
    Mullion/Transom Depth = 10. [MILLI METRE]
    Opening Oversize Base = 0. [MILLI METRE]
    Opening Oversize Left = 0. [MILLI METRE]
    Opening Oversize Right = 0. [MILLI METRE]
    Opening Oversize Top = 0. [MILLI METRE]
    Overlight Glazing Bar Spacing Horz = 150. [MILLI METRE]
    Overlight Glazing Bar Spacing Vert = 150. [MILLI METRE]
    Overlight Rail Width Bottom = 0. [MILLI METRE]
    Overlight Rail Width Dividers = 35. [MILLI METRE]
    Overlight Rail Width Stiles = 0. [MILLI METRE]
    Overlight Rail Width Top = 0. [MILLI METRE]
    Overlite Height = 0. [MILLI METRE]
    Pivot Lne Dash Length = 50. [MILLI METRE]
    Reveal Height = 2040. [MILLI METRE]
    Reveal Width = 880.0000000000001 [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 440. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 0. [MILLI METRE]
    Sidelight Glazing Bar Spacing Horz = 300. [MILLI METRE]
    Sidelight Glazing Bar Spacing Vert = 400. [MILLI METRE]
    Sidelight Glazing Bar Thickness = 10. [MILLI METRE]
    Sidelight Glazing Bar Width = 20. [MILLI METRE]
    Sidelight Louvre Width = 60. [MILLI METRE]
    Sidelight Rail Height Eye Level = 1600. [MILLI METRE]
    Sidelight Rail Height Handle = 800. [MILLI METRE]
    Sidelight Rail Height Head = 2000. [MILLI METRE]
    Sidelight Rail Width Bottom = 0. [MILLI METRE]
    Sidelight Rail Width Eye Height = 35. [MILLI METRE]
    Sidelight Rail Width Handle Height = 35. [MILLI METRE]
    Sidelight Rail Width Head Height = 35. [MILLI METRE]
    Sidelight Rail Width Stiles = 0. [MILLI METRE]
    Sidelight Rail Width Top = 0. [MILLI METRE]
    Sidelite Sill Height Left = 0. [MILLI METRE]
    Sidelite Sill Height Right = 0. [MILLI METRE]
    Sidelite Width Left = 0. [MILLI METRE]
    Sidelite Width Right = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extend Left = 20. [MILLI METRE]
    Sill Extend Right = 20. [MILLI METRE]
    Sill Height = 0. [MILLI METRE]
    Sill Height to Current Story = 0. [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 60. [MILLI METRE]
    Threshold Height (max) = 20. [MILLI METRE]
    Threshold Thickness = 20. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 35. [MILLI METRE]
    Unit Height = 2040. [MILLI METRE]
    Unit Width = 880.0000000000001 [MILLI METRE]
    Wall Hole Height = 2050. [MILLI METRE]
    Wall Hole Width = 900.0000000000001 [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_CI_Tools_Door | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle Length = 160. [MILLI METRE]
    (OLD) Exterior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Exterior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Exterior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Exterior Handle Projection = 45. [MILLI METRE]
    (OLD) Exterior Handle Thickness = 19. [MILLI METRE]
    (OLD) Exterior Handle Width = 15. [MILLI METRE]
    (OLD) Interior Handle Length = 160. [MILLI METRE]
    (OLD) Interior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Interior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Interior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Interior Handle Projection = 45. [MILLI METRE]
    (OLD) Interior Handle Thickness = 19. [MILLI METRE]
    (OLD) Interior Handle Width = 16. [MILLI METRE]
    2D Symbol Detail Level = 0. [MILLI METRE]
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    ??? (extendFrameL) = 0. [MILLI METRE]
    ??? (extendFrameR) = 0. [MILLI METRE]
    ??? (extendOpeningL) = 10. [MILLI METRE]
    ??? (extendOpeningR) = 10. [MILLI METRE]
    Allow space for mitred ends = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Height = 76. [MILLI METRE]
    Brick Length = 230. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Brick Mortar Thickness = 10. [MILLI METRE]
    Camera Distance Fully Open = 1000. [MILLI METRE]
    Camera Distance Fully Shut = 3000. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset from Frame = 0. [MILLI METRE]
    Door Leaf Pivot Offset Left = 0. [MILLI METRE]
    Door Leaf Pivot Offset Right = 0. [MILLI METRE]
    Door Leaf Thickness = 35. [MILLI METRE]
    Door Leaf Width Left = 459.9999999999999 [MILLI METRE]
    Door Leaf Width Right = 459.9999999999999 [MILLI METRE]
    Door Stop Max Width = 90. [MILLI METRE]
    Door Stop Thickness = 10. [MILLI METRE]
    Egress Height = 1995. [MILLI METRE]
    Egress Width = 849.9999999999999 [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 80. [MILLI METRE]
    Exterior Trim Extend Below Threshold = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 18. [MILLI METRE]
    Exterior Trim Width = 80. [MILLI METRE]
    Fixed Glass Position = 12. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Width = 50. [MILLI METRE]
    Framed Glass Position = 12. [MILLI METRE]
    Glass Pane Spacing = 16. [MILLI METRE]
    Glass Thickness = 6. [MILLI METRE]
    Head Gap Height = 5. [MILLI METRE]
    Head Moulding Brick Width = 80. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 40. [MILLI METRE]
    Head Moulding Width = 80. [MILLI METRE]
    Inner Frame Backset = 10. [MILLI METRE]
    Inner Frame Depth = 35. [MILLI METRE]
    Inner Frame Head Width = 70. [MILLI METRE]
    Inner Frame Sill Width = 100. [MILLI METRE]
    Inner Frame Width = 25. [MILLI METRE]
    Interior Reveal Thickness = 18. [MILLI METRE]
    Interior Sill Extension = 80. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 10. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 20. [MILLI METRE]
    Interior Trim Width = 65. [MILLI METRE]
    Jamb Moulding Brick Width = 80. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Leaf Height (max) = 1980. [MILLI METRE]
    Leaf Height = 1980. [MILLI METRE]
    Leaf Overlap Head Frame = 0. [MILLI METRE]
    Leaf Overlap Left = 0. [MILLI METRE]
    Leaf Overlap Left Jamb = 0. [MILLI METRE]
    Leaf Overlap Right = 0. [MILLI METRE]
    Leaf Overlap Right Jamb = 0. [MILLI METRE]
    Leaf Width = 919.9999999999999 [MILLI METRE]
    Lintel Depth = 140. [MILLI METRE]
    Lintel Extension Left = 45. [MILLI METRE]
    Lintel Extension Right = 45. [MILLI METRE]
    Lintel Offset Back from Frame = 0. [MILLI METRE]
    Lintel Thickness = 90. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset) = 10. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset_2) = 10. [MILLI METRE]
    Main Frame Depth (FD) = 0. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 130. [MILLI METRE]
    Main Frame Flange Thickness = 5. [MILLI METRE]
    Main Frame Flange Width = 20. [MILLI METRE]
    Main Frame Width = 35. [MILLI METRE]
    Mullion Width = 35. [MILLI METRE]
    Mullion/Transom Depth = 10. [MILLI METRE]
    Opening Oversize Base = 0. [MILLI METRE]
    Opening Oversize Left = 0. [MILLI METRE]
    Opening Oversize Right = 0. [MILLI METRE]
    Opening Oversize Top = 0. [MILLI METRE]
    Overlight Glazing Bar Spacing Horz = 150. [MILLI METRE]
    Overlight Glazing Bar Spacing Vert = 150. [MILLI METRE]
    Overlight Rail Width Bottom = 0. [MILLI METRE]
    Overlight Rail Width Dividers = 35. [MILLI METRE]
    Overlight Rail Width Stiles = 0. [MILLI METRE]
    Overlight Rail Width Top = 0. [MILLI METRE]
    Overlite Height = 0. [MILLI METRE]
    Pivot Lne Dash Length = 50. [MILLI METRE]
    Reveal Height = 2040. [MILLI METRE]
    Reveal Width = 990. [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 440. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 0. [MILLI METRE]
    Sidelight Glazing Bar Spacing Horz = 300. [MILLI METRE]
    Sidelight Glazing Bar Spacing Vert = 400. [MILLI METRE]
    Sidelight Glazing Bar Thickness = 10. [MILLI METRE]
    Sidelight Glazing Bar Width = 20. [MILLI METRE]
    Sidelight Louvre Width = 60. [MILLI METRE]
    Sidelight Rail Height Eye Level = 1600. [MILLI METRE]
    Sidelight Rail Height Handle = 800. [MILLI METRE]
    Sidelight Rail Height Head = 2000. [MILLI METRE]
    Sidelight Rail Width Bottom = 0. [MILLI METRE]
    Sidelight Rail Width Eye Height = 35. [MILLI METRE]
    Sidelight Rail Width Handle Height = 35. [MILLI METRE]
    Sidelight Rail Width Head Height = 35. [MILLI METRE]
    Sidelight Rail Width Stiles = 0. [MILLI METRE]
    Sidelight Rail Width Top = 0. [MILLI METRE]
    Sidelite Sill Height Left = 0. [MILLI METRE]
    Sidelite Sill Height Right = 0. [MILLI METRE]
    Sidelite Width Left = 0. [MILLI METRE]
    Sidelite Width Right = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extend Left = 20. [MILLI METRE]
    Sill Extend Right = 20. [MILLI METRE]
    Sill Height = 0. [MILLI METRE]
    Sill Height to Current Story = 0. [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 60. [MILLI METRE]
    Threshold Height (max) = 20. [MILLI METRE]
    Threshold Thickness = 20. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 35. [MILLI METRE]
    Unit Height = 2040. [MILLI METRE]
    Unit Width = 990. [MILLI METRE]
    Wall Hole Height = 2050. [MILLI METRE]
    Wall Hole Width = 1010. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_CI_Tools_Door | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle Length = 160. [MILLI METRE]
    (OLD) Exterior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Exterior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Exterior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Exterior Handle Projection = 45. [MILLI METRE]
    (OLD) Exterior Handle Thickness = 19. [MILLI METRE]
    (OLD) Exterior Handle Width = 15. [MILLI METRE]
    (OLD) Interior Handle Length = 160. [MILLI METRE]
    (OLD) Interior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Interior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Interior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Interior Handle Projection = 45. [MILLI METRE]
    (OLD) Interior Handle Thickness = 19. [MILLI METRE]
    (OLD) Interior Handle Width = 16. [MILLI METRE]
    2D Symbol Detail Level = 0. [MILLI METRE]
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    ??? (extendFrameL) = 0. [MILLI METRE]
    ??? (extendFrameR) = 0. [MILLI METRE]
    ??? (extendOpeningL) = 10. [MILLI METRE]
    ??? (extendOpeningR) = 10. [MILLI METRE]
    Allow space for mitred ends = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Height = 76. [MILLI METRE]
    Brick Length = 230. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Brick Mortar Thickness = 10. [MILLI METRE]
    Camera Distance Fully Open = 1000. [MILLI METRE]
    Camera Distance Fully Shut = 3000. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset from Frame = 0. [MILLI METRE]
    Door Leaf Pivot Offset Left = 0. [MILLI METRE]
    Door Leaf Pivot Offset Right = 0. [MILLI METRE]
    Door Leaf Thickness = 35. [MILLI METRE]
    Door Leaf Width Left = 510. [MILLI METRE]
    Door Leaf Width Right = 510. [MILLI METRE]
    Door Stop Max Width = 90. [MILLI METRE]
    Door Stop Thickness = 10. [MILLI METRE]
    Egress Height = 1995. [MILLI METRE]
    Egress Width = 950. [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 80. [MILLI METRE]
    Exterior Trim Extend Below Threshold = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 18. [MILLI METRE]
    Exterior Trim Width = 80. [MILLI METRE]
    Fixed Glass Position = 12. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Width = 50. [MILLI METRE]
    Framed Glass Position = 12. [MILLI METRE]
    Glass Pane Spacing = 16. [MILLI METRE]
    Glass Thickness = 6. [MILLI METRE]
    Head Gap Height = 5. [MILLI METRE]
    Head Moulding Brick Width = 80. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 40. [MILLI METRE]
    Head Moulding Width = 80. [MILLI METRE]
    Inner Frame Backset = 10. [MILLI METRE]
    Inner Frame Depth = 35. [MILLI METRE]
    Inner Frame Head Width = 70. [MILLI METRE]
    Inner Frame Sill Width = 100. [MILLI METRE]
    Inner Frame Width = 25. [MILLI METRE]
    Interior Reveal Thickness = 18. [MILLI METRE]
    Interior Sill Extension = 80. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 10. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 20. [MILLI METRE]
    Interior Trim Width = 65. [MILLI METRE]
    Jamb Moulding Brick Width = 80. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Leaf Height (max) = 1980. [MILLI METRE]
    Leaf Height = 1980. [MILLI METRE]
    Leaf Overlap Head Frame = 0. [MILLI METRE]
    Leaf Overlap Left = 0. [MILLI METRE]
    Leaf Overlap Left Jamb = 0. [MILLI METRE]
    Leaf Overlap Right = 0. [MILLI METRE]
    Leaf Overlap Right Jamb = 0. [MILLI METRE]
    Leaf Width = 1020. [MILLI METRE]
    Lintel Depth = 140. [MILLI METRE]
    Lintel Extension Left = 45. [MILLI METRE]
    Lintel Extension Right = 45. [MILLI METRE]
    Lintel Offset Back from Frame = 0. [MILLI METRE]
    Lintel Thickness = 90. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset) = 10. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset_2) = 10. [MILLI METRE]
    Main Frame Depth (FD) = 0. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 84.99999999999999 [MILLI METRE]
    Main Frame Flange Thickness = 5. [MILLI METRE]
    Main Frame Flange Width = 20. [MILLI METRE]
    Main Frame Width = 35. [MILLI METRE]
    Mullion Width = 35. [MILLI METRE]
    Mullion/Transom Depth = 10. [MILLI METRE]
    Opening Oversize Base = 0. [MILLI METRE]
    Opening Oversize Left = 0. [MILLI METRE]
    Opening Oversize Right = 0. [MILLI METRE]
    Opening Oversize Top = 0. [MILLI METRE]
    Overlight Glazing Bar Spacing Horz = 150. [MILLI METRE]
    Overlight Glazing Bar Spacing Vert = 150. [MILLI METRE]
    Overlight Rail Width Bottom = 0. [MILLI METRE]
    Overlight Rail Width Dividers = 35. [MILLI METRE]
    Overlight Rail Width Stiles = 0. [MILLI METRE]
    Overlight Rail Width Top = 0. [MILLI METRE]
    Overlite Height = 0. [MILLI METRE]
    Pivot Lne Dash Length = 50. [MILLI METRE]
    Reveal Height = 2040. [MILLI METRE]
    Reveal Width = 1090. [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 440. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 0. [MILLI METRE]
    Sidelight Glazing Bar Spacing Horz = 300. [MILLI METRE]
    Sidelight Glazing Bar Spacing Vert = 400. [MILLI METRE]
    Sidelight Glazing Bar Thickness = 10. [MILLI METRE]
    Sidelight Glazing Bar Width = 20. [MILLI METRE]
    Sidelight Louvre Width = 60. [MILLI METRE]
    Sidelight Rail Height Eye Level = 1600. [MILLI METRE]
    Sidelight Rail Height Handle = 800. [MILLI METRE]
    Sidelight Rail Height Head = 2000. [MILLI METRE]
    Sidelight Rail Width Bottom = 0. [MILLI METRE]
    Sidelight Rail Width Eye Height = 35. [MILLI METRE]
    Sidelight Rail Width Handle Height = 35. [MILLI METRE]
    Sidelight Rail Width Head Height = 35. [MILLI METRE]
    Sidelight Rail Width Stiles = 0. [MILLI METRE]
    Sidelight Rail Width Top = 0. [MILLI METRE]
    Sidelite Sill Height Left = 0. [MILLI METRE]
    Sidelite Sill Height Right = 0. [MILLI METRE]
    Sidelite Width Left = 0. [MILLI METRE]
    Sidelite Width Right = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extend Left = 20. [MILLI METRE]
    Sill Extend Right = 20. [MILLI METRE]
    Sill Height = 0. [MILLI METRE]
    Sill Height to Current Story = 0. [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 60. [MILLI METRE]
    Threshold Height (max) = 20. [MILLI METRE]
    Threshold Thickness = 20. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 35. [MILLI METRE]
    Unit Height = 2040. [MILLI METRE]
    Unit Width = 1090. [MILLI METRE]
    Wall Hole Height = 2050. [MILLI METRE]
    Wall Hole Width = 1110. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_CI_Tools_Door | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle Length = 160. [MILLI METRE]
    (OLD) Exterior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Exterior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Exterior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Exterior Handle Projection = 45. [MILLI METRE]
    (OLD) Exterior Handle Thickness = 19. [MILLI METRE]
    (OLD) Exterior Handle Width = 15. [MILLI METRE]
    (OLD) Interior Handle Length = 160. [MILLI METRE]
    (OLD) Interior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Interior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Interior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Interior Handle Projection = 45. [MILLI METRE]
    (OLD) Interior Handle Thickness = 19. [MILLI METRE]
    (OLD) Interior Handle Width = 16. [MILLI METRE]
    2D Symbol Detail Level = 0. [MILLI METRE]
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    ??? (extendFrameL) = 0. [MILLI METRE]
    ??? (extendFrameR) = 0. [MILLI METRE]
    ??? (extendOpeningL) = 10. [MILLI METRE]
    ??? (extendOpeningR) = 10. [MILLI METRE]
    Allow space for mitred ends = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Height = 76. [MILLI METRE]
    Brick Length = 230. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Brick Mortar Thickness = 10. [MILLI METRE]
    Camera Distance Fully Open = 1000. [MILLI METRE]
    Camera Distance Fully Shut = 3000. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset from Frame = 0. [MILLI METRE]
    Door Leaf Pivot Offset Left = 0. [MILLI METRE]
    Door Leaf Pivot Offset Right = 0. [MILLI METRE]
    Door Leaf Thickness = 35. [MILLI METRE]
    Door Leaf Width Left = 510. [MILLI METRE]
    Door Leaf Width Right = 510. [MILLI METRE]
    Door Stop Max Width = 90. [MILLI METRE]
    Door Stop Thickness = 10. [MILLI METRE]
    Egress Height = 1995. [MILLI METRE]
    Egress Width = 950. [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 80. [MILLI METRE]
    Exterior Trim Extend Below Threshold = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 18. [MILLI METRE]
    Exterior Trim Width = 80. [MILLI METRE]
    Fixed Glass Position = 12. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Width = 50. [MILLI METRE]
    Framed Glass Position = 12. [MILLI METRE]
    Glass Pane Spacing = 16. [MILLI METRE]
    Glass Thickness = 6. [MILLI METRE]
    Head Gap Height = 5. [MILLI METRE]
    Head Moulding Brick Width = 80. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 40. [MILLI METRE]
    Head Moulding Width = 80. [MILLI METRE]
    Inner Frame Backset = 10. [MILLI METRE]
    Inner Frame Depth = 35. [MILLI METRE]
    Inner Frame Head Width = 70. [MILLI METRE]
    Inner Frame Sill Width = 100. [MILLI METRE]
    Inner Frame Width = 25. [MILLI METRE]
    Interior Reveal Thickness = 18. [MILLI METRE]
    Interior Sill Extension = 80. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 10. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 20. [MILLI METRE]
    Interior Trim Width = 65. [MILLI METRE]
    Jamb Moulding Brick Width = 80. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Leaf Height (max) = 1980. [MILLI METRE]
    Leaf Height = 1980. [MILLI METRE]
    Leaf Overlap Head Frame = 0. [MILLI METRE]
    Leaf Overlap Left = 0. [MILLI METRE]
    Leaf Overlap Left Jamb = 0. [MILLI METRE]
    Leaf Overlap Right = 0. [MILLI METRE]
    Leaf Overlap Right Jamb = 0. [MILLI METRE]
    Leaf Width = 1020. [MILLI METRE]
    Lintel Depth = 140. [MILLI METRE]
    Lintel Extension Left = 45. [MILLI METRE]
    Lintel Extension Right = 45. [MILLI METRE]
    Lintel Offset Back from Frame = 0. [MILLI METRE]
    Lintel Thickness = 90. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset) = 10. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset_2) = 10. [MILLI METRE]
    Main Frame Depth (FD) = 0. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 130. [MILLI METRE]
    Main Frame Flange Thickness = 5. [MILLI METRE]
    Main Frame Flange Width = 20. [MILLI METRE]
    Main Frame Width = 35. [MILLI METRE]
    Mullion Width = 35. [MILLI METRE]
    Mullion/Transom Depth = 10. [MILLI METRE]
    Opening Oversize Base = 0. [MILLI METRE]
    Opening Oversize Left = 0. [MILLI METRE]
    Opening Oversize Right = 0. [MILLI METRE]
    Opening Oversize Top = 0. [MILLI METRE]
    Overlight Glazing Bar Spacing Horz = 150. [MILLI METRE]
    Overlight Glazing Bar Spacing Vert = 150. [MILLI METRE]
    Overlight Rail Width Bottom = 0. [MILLI METRE]
    Overlight Rail Width Dividers = 35. [MILLI METRE]
    Overlight Rail Width Stiles = 0. [MILLI METRE]
    Overlight Rail Width Top = 0. [MILLI METRE]
    Overlite Height = 0. [MILLI METRE]
    Pivot Lne Dash Length = 50. [MILLI METRE]
    Reveal Height = 2040. [MILLI METRE]
    Reveal Width = 1090. [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 440. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 0. [MILLI METRE]
    Sidelight Glazing Bar Spacing Horz = 300. [MILLI METRE]
    Sidelight Glazing Bar Spacing Vert = 400. [MILLI METRE]
    Sidelight Glazing Bar Thickness = 10. [MILLI METRE]
    Sidelight Glazing Bar Width = 20. [MILLI METRE]
    Sidelight Louvre Width = 60. [MILLI METRE]
    Sidelight Rail Height Eye Level = 1600. [MILLI METRE]
    Sidelight Rail Height Handle = 800. [MILLI METRE]
    Sidelight Rail Height Head = 2000. [MILLI METRE]
    Sidelight Rail Width Bottom = 0. [MILLI METRE]
    Sidelight Rail Width Eye Height = 35. [MILLI METRE]
    Sidelight Rail Width Handle Height = 35. [MILLI METRE]
    Sidelight Rail Width Head Height = 35. [MILLI METRE]
    Sidelight Rail Width Stiles = 0. [MILLI METRE]
    Sidelight Rail Width Top = 0. [MILLI METRE]
    Sidelite Sill Height Left = 0. [MILLI METRE]
    Sidelite Sill Height Right = 0. [MILLI METRE]
    Sidelite Width Left = 0. [MILLI METRE]
    Sidelite Width Right = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extend Left = 20. [MILLI METRE]
    Sill Extend Right = 20. [MILLI METRE]
    Sill Height = 0. [MILLI METRE]
    Sill Height to Current Story = 0. [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 60. [MILLI METRE]
    Threshold Height (max) = 20. [MILLI METRE]
    Threshold Thickness = 20. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 35. [MILLI METRE]
    Unit Height = 2040. [MILLI METRE]
    Unit Width = 1090. [MILLI METRE]
    Wall Hole Height = 2050. [MILLI METRE]
    Wall Hole Width = 1110. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_CI_Tools_Door | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle Length = 160. [MILLI METRE]
    (OLD) Exterior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Exterior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Exterior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Exterior Handle Projection = 45. [MILLI METRE]
    (OLD) Exterior Handle Thickness = 19. [MILLI METRE]
    (OLD) Exterior Handle Width = 15. [MILLI METRE]
    (OLD) Interior Handle Length = 160. [MILLI METRE]
    (OLD) Interior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Interior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Interior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Interior Handle Projection = 45. [MILLI METRE]
    (OLD) Interior Handle Thickness = 19. [MILLI METRE]
    (OLD) Interior Handle Width = 16. [MILLI METRE]
    2D Symbol Detail Level = 0. [MILLI METRE]
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    ??? (extendFrameL) = 0. [MILLI METRE]
    ??? (extendFrameR) = 0. [MILLI METRE]
    ??? (extendOpeningL) = 10. [MILLI METRE]
    ??? (extendOpeningR) = 10. [MILLI METRE]
    Allow space for mitred ends = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Height = 76. [MILLI METRE]
    Brick Length = 230. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Brick Mortar Thickness = 10. [MILLI METRE]
    Camera Distance Fully Open = 1000. [MILLI METRE]
    Camera Distance Fully Shut = 3000. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset from Frame = 0. [MILLI METRE]
    Door Leaf Pivot Offset Left = 0. [MILLI METRE]
    Door Leaf Pivot Offset Right = 0. [MILLI METRE]
    Door Leaf Thickness = 35. [MILLI METRE]
    Door Leaf Width Left = 860. [MILLI METRE]
    Door Leaf Width Right = 860. [MILLI METRE]
    Door Stop Max Width = 90. [MILLI METRE]
    Door Stop Thickness = 10. [MILLI METRE]
    Egress Height = 2170. [MILLI METRE]
    Egress Width = 850. [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 80. [MILLI METRE]
    Exterior Trim Extend Below Threshold = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 140. [MILLI METRE]
    Exterior Trim Width = 40. [MILLI METRE]
    Fixed Glass Position = 12. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Width = 50. [MILLI METRE]
    Framed Glass Position = 12. [MILLI METRE]
    Glass Pane Spacing = 16. [MILLI METRE]
    Glass Thickness = 6. [MILLI METRE]
    Head Gap Height = 0. [MILLI METRE]
    Head Moulding Brick Width = 80. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 140. [MILLI METRE]
    Head Moulding Width = 45. [MILLI METRE]
    Inner Frame Backset = 10. [MILLI METRE]
    Inner Frame Depth = 100. [MILLI METRE]
    Inner Frame Head Width = 45. [MILLI METRE]
    Inner Frame Sill Width = 45. [MILLI METRE]
    Inner Frame Width = 45. [MILLI METRE]
    Interior Reveal Thickness = 18. [MILLI METRE]
    Interior Sill Extension = 80. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 10. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 20. [MILLI METRE]
    Interior Trim Width = 65. [MILLI METRE]
    Jamb Moulding Brick Width = 80. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Leaf Height (max) = 2180. [MILLI METRE]
    Leaf Height = 2180. [MILLI METRE]
    Leaf Overlap Head Frame = 0. [MILLI METRE]
    Leaf Overlap Left = 80. [MILLI METRE]
    Leaf Overlap Left Jamb = 0. [MILLI METRE]
    Leaf Overlap Right = 80. [MILLI METRE]
    Leaf Overlap Right Jamb = 0. [MILLI METRE]
    Leaf Width = 860. [MILLI METRE]
    Lintel Depth = 140. [MILLI METRE]
    Lintel Extension Left = 45. [MILLI METRE]
    Lintel Extension Right = 45. [MILLI METRE]
    Lintel Offset Back from Frame = 0. [MILLI METRE]
    Lintel Thickness = 90. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset) = 0. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset_2) = 0. [MILLI METRE]
    Main Frame Depth (FD) = 100. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 100. [MILLI METRE]
    Main Frame Flange Thickness = 105. [MILLI METRE]
    Main Frame Flange Width = 15. [MILLI METRE]
    Main Frame Width = 45. [MILLI METRE]
    Mullion Width = 35. [MILLI METRE]
    Mullion/Transom Depth = 10. [MILLI METRE]
    Opening Oversize Base = 0. [MILLI METRE]
    Opening Oversize Left = 0. [MILLI METRE]
    Opening Oversize Right = 0. [MILLI METRE]
    Opening Oversize Top = 0. [MILLI METRE]
    Overlight Glazing Bar Spacing Horz = 150. [MILLI METRE]
    Overlight Glazing Bar Spacing Vert = 150. [MILLI METRE]
    Overlight Rail Width Bottom = 0. [MILLI METRE]
    Overlight Rail Width Dividers = 35. [MILLI METRE]
    Overlight Rail Width Stiles = 0. [MILLI METRE]
    Overlight Rail Width Top = 0. [MILLI METRE]
    Overlite Height = 0. [MILLI METRE]
    Pivot Lne Dash Length = 50. [MILLI METRE]
    Reveal Height = 2225. [MILLI METRE]
    Reveal Width = 1735. [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 440. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 10. [MILLI METRE]
    Sidelight Glazing Bar Spacing Horz = 300. [MILLI METRE]
    Sidelight Glazing Bar Spacing Vert = 400. [MILLI METRE]
    Sidelight Glazing Bar Thickness = 10. [MILLI METRE]
    Sidelight Glazing Bar Width = 20. [MILLI METRE]
    Sidelight Louvre Width = 60. [MILLI METRE]
    Sidelight Rail Height Eye Level = 1430. [MILLI METRE]
    Sidelight Rail Height Handle = 800. [MILLI METRE]
    Sidelight Rail Height Head = 2000. [MILLI METRE]
    Sidelight Rail Width Bottom = 0. [MILLI METRE]
    Sidelight Rail Width Eye Height = 35. [MILLI METRE]
    Sidelight Rail Width Handle Height = 35. [MILLI METRE]
    Sidelight Rail Width Head Height = 35. [MILLI METRE]
    Sidelight Rail Width Stiles = 0. [MILLI METRE]
    Sidelight Rail Width Top = 0. [MILLI METRE]
    Sidelite Sill Height Left = 0. [MILLI METRE]
    Sidelite Sill Height Right = 0. [MILLI METRE]
    Sidelite Width Left = 795. [MILLI METRE]
    Sidelite Width Right = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extend Left = 20. [MILLI METRE]
    Sill Extend Right = 20. [MILLI METRE]
    Sill Height = -25.00000000001146 [MILLI METRE]
    Sill Height to Current Story = 10905. [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 60. [MILLI METRE]
    Threshold Height (max) = 0. [MILLI METRE]
    Threshold Thickness = 0. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 35. [MILLI METRE]
    Unit Height = 2225. [MILLI METRE]
    Unit Width = 1735. [MILLI METRE]
    Wall Hole Height = 2245. [MILLI METRE]
    Wall Hole Width = 1755. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_CI_Tools_Door | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    (OLD) Exterior Handle Length = 160. [MILLI METRE]
    (OLD) Exterior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Exterior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Exterior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Exterior Handle Projection = 45. [MILLI METRE]
    (OLD) Exterior Handle Thickness = 19. [MILLI METRE]
    (OLD) Exterior Handle Width = 15. [MILLI METRE]
    (OLD) Interior Handle Length = 160. [MILLI METRE]
    (OLD) Interior Handle Plate Length = 200. [MILLI METRE]
    (OLD) Interior Handle Plate Thickness = 0. [MILLI METRE]
    (OLD) Interior Handle Plate Width = 60. [MILLI METRE]
    (OLD) Interior Handle Projection = 45. [MILLI METRE]
    (OLD) Interior Handle Thickness = 19. [MILLI METRE]
    (OLD) Interior Handle Width = 16. [MILLI METRE]
    2D Symbol Detail Level = 0. [MILLI METRE]
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    ??? (extendFrameL) = 0. [MILLI METRE]
    ??? (extendFrameR) = 0. [MILLI METRE]
    ??? (extendOpeningL) = 10. [MILLI METRE]
    ??? (extendOpeningR) = 10. [MILLI METRE]
    Allow space for mitred ends = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Height = 76. [MILLI METRE]
    Brick Length = 230. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Brick Mortar Thickness = 10. [MILLI METRE]
    Camera Distance Fully Open = 1000. [MILLI METRE]
    Camera Distance Fully Shut = 3000. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset from Frame = 0. [MILLI METRE]
    Door Leaf Pivot Offset Left = 0. [MILLI METRE]
    Door Leaf Pivot Offset Right = 0. [MILLI METRE]
    Door Leaf Thickness = 35. [MILLI METRE]
    Door Leaf Width Left = 910. [MILLI METRE]
    Door Leaf Width Right = 910. [MILLI METRE]
    Door Stop Max Width = 90. [MILLI METRE]
    Door Stop Thickness = 10. [MILLI METRE]
    Egress Height = 2165. [MILLI METRE]
    Egress Width = 865. [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 80. [MILLI METRE]
    Exterior Trim Extend Below Threshold = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 140. [MILLI METRE]
    Exterior Trim Width = 40. [MILLI METRE]
    Fixed Glass Position = 12. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Width = 50. [MILLI METRE]
    Framed Glass Position = 12. [MILLI METRE]
    Glass Pane Spacing = 16. [MILLI METRE]
    Glass Thickness = 6. [MILLI METRE]
    Head Gap Height = 0. [MILLI METRE]
    Head Moulding Brick Width = 80. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 140. [MILLI METRE]
    Head Moulding Width = 45. [MILLI METRE]
    Inner Frame Backset = 10. [MILLI METRE]
    Inner Frame Depth = 100. [MILLI METRE]
    Inner Frame Head Width = 45. [MILLI METRE]
    Inner Frame Sill Width = 45. [MILLI METRE]
    Inner Frame Width = 45. [MILLI METRE]
    Interior Reveal Thickness = 18. [MILLI METRE]
    Interior Sill Extension = 80. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 10. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 20. [MILLI METRE]
    Interior Trim Width = 65. [MILLI METRE]
    Jamb Moulding Brick Width = 80. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Leaf Height (max) = 2175. [MILLI METRE]
    Leaf Height = 2175. [MILLI METRE]
    Leaf Overlap Head Frame = 0. [MILLI METRE]
    Leaf Overlap Left = 0. [MILLI METRE]
    Leaf Overlap Left Jamb = 0. [MILLI METRE]
    Leaf Overlap Right = 0. [MILLI METRE]
    Leaf Overlap Right Jamb = 0. [MILLI METRE]
    Leaf Width = 910. [MILLI METRE]
    Lintel Depth = 140. [MILLI METRE]
    Lintel Extension Left = 45. [MILLI METRE]
    Lintel Extension Right = 45. [MILLI METRE]
    Lintel Offset Back from Frame = 0. [MILLI METRE]
    Lintel Thickness = 90. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset) = 0. [MILLI METRE]
    Main Frame Backset from Wall Surface (frame_backset_2) = 0. [MILLI METRE]
    Main Frame Depth (FD) = 100. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 100. [MILLI METRE]
    Main Frame Flange Thickness = 105. [MILLI METRE]
    Main Frame Flange Width = 15. [MILLI METRE]
    Main Frame Width = 50. [MILLI METRE]
    Mullion Width = 50. [MILLI METRE]
    Mullion/Transom Depth = 0. [MILLI METRE]
    Opening Oversize Base = 0. [MILLI METRE]
    Opening Oversize Left = 0. [MILLI METRE]
    Opening Oversize Right = 0. [MILLI METRE]
    Opening Oversize Top = 0. [MILLI METRE]
    Overlight Glazing Bar Spacing Horz = 150. [MILLI METRE]
    Overlight Glazing Bar Spacing Vert = 150. [MILLI METRE]
    Overlight Rail Width Bottom = 0. [MILLI METRE]
    Overlight Rail Width Dividers = 35. [MILLI METRE]
    Overlight Rail Width Stiles = 0. [MILLI METRE]
    Overlight Rail Width Top = 0. [MILLI METRE]
    Overlite Height = 0. [MILLI METRE]
    Pivot Lne Dash Length = 50. [MILLI METRE]
    Reveal Height = 2225. [MILLI METRE]
    Reveal Width = 1010. [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 440. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 10. [MILLI METRE]
    Sidelight Glazing Bar Spacing Horz = 300. [MILLI METRE]
    Sidelight Glazing Bar Spacing Vert = 400. [MILLI METRE]
    Sidelight Glazing Bar Thickness = 10. [MILLI METRE]
    Sidelight Glazing Bar Width = 20. [MILLI METRE]
    Sidelight Louvre Width = 60. [MILLI METRE]
    Sidelight Rail Height Eye Level = 1430. [MILLI METRE]
    Sidelight Rail Height Handle = 800. [MILLI METRE]
    Sidelight Rail Height Head = 2000. [MILLI METRE]
    Sidelight Rail Width Bottom = 0. [MILLI METRE]
    Sidelight Rail Width Eye Height = 35. [MILLI METRE]
    Sidelight Rail Width Handle Height = 35. [MILLI METRE]
    Sidelight Rail Width Head Height = 35. [MILLI METRE]
    Sidelight Rail Width Stiles = 0. [MILLI METRE]
    Sidelight Rail Width Top = 0. [MILLI METRE]
    Sidelite Sill Height Left = 0. [MILLI METRE]
    Sidelite Sill Height Right = 0. [MILLI METRE]
    Sidelite Width Left = 0. [MILLI METRE]
    Sidelite Width Right = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extend Left = 20. [MILLI METRE]
    Sill Extend Right = 20. [MILLI METRE]
    Sill Height = -24.99999999999947 [MILLI METRE]
    Sill Height to Current Story = 10905. [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 60. [MILLI METRE]
    Threshold Height (max) = 0. [MILLI METRE]
    Threshold Thickness = 0. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 50. [MILLI METRE]
    Unit Height = 2225. [MILLI METRE]
    Unit Width = 1010. [MILLI METRE]
    Wall Hole Height = 2244.999999999999 [MILLI METRE]
    Wall Hole Width = 1030. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Pset_Hot_Water_System_#1550 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Accessories = "" (IFCLABEL)
    Contour Pen = "General - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Background Fill (2)" (IFCLABEL)
    Group Type (FM_Type) = "Others" (IFCLABEL)
    Group Type (iFMType) = 25 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Line Type = 1 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Menu Page Control = 1 (IFCINTEGER)
    Menu Part Control = 1 (IFCINTEGER)
    Menu Property Control = 3 (IFCINTEGER)
    Menu Subpart Control = 1 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Version Number = 1 (IFCINTEGER)
    Zone Name = "" (IFCLABEL)
    Zone Number = "" (IFCLABEL)
  AC_Equantity_Hot_Water_System_#1550 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 488. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height = 1335. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Pset_CI_Tools_Wall_Covering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Accessories = "" (IFCLABEL)
    Archi-FM Type = "Others" (IFCLABEL)
    Cladding Materials = TRUE (IFCBOOLEAN)
    Cladding Setout = 0 (IFCINTEGER)
    Cladding above Head Height = 0. (IFCREAL)
    Cladding above Head Height Preset = "" (IFCLABEL)
    Cladding above Openings = 0. (IFCREAL)
    Cladding above Openings Preset = "" (IFCLABEL)
    Cladding below Openings = 0. (IFCREAL)
    Cladding below Openings Preset = "" (IFCLABEL)
    Cladding below Sill Height = 0. (IFCREAL)
    Cladding below Sill Height Preset = "" (IFCLABEL)
    Claddings = TRUE (IFCBOOLEAN)
    Cost = 0. (IFCREAL)
    Custom Note 1 = "" (IFCLABEL)
    Custom Note 2 = "" (IFCLABEL)
    Custom Note 3 = "" (IFCLABEL)
    Custom Note 4 = "" (IFCLABEL)
    Custom Note 5 = "" (IFCLABEL)
    Group Type = 25 (IFCINTEGER)
    Ignore Openings in Plan View = FALSE (IFCBOOLEAN)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lock Cladding Origin = FALSE (IFCBOOLEAN)
    Main Cladding = 16.07130000000008 (IFCREAL)
    Main Cladding Preset = "Shiplap Smooth" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Note = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Unit = "kg" (IFCLABEL)
    Username = "" (IFCLABEL)
    Weight = 0. (IFCREAL)
  AC_Pset_CI_Tools_Wall_Covering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Accessories = "" (IFCLABEL)
    Archi-FM Type = "Others" (IFCLABEL)
    Cladding Materials = TRUE (IFCBOOLEAN)
    Cladding Setout = 0 (IFCINTEGER)
    Cladding above Head Height = 0. (IFCREAL)
    Cladding above Head Height Preset = "" (IFCLABEL)
    Cladding above Openings = 0. (IFCREAL)
    Cladding above Openings Preset = "" (IFCLABEL)
    Cladding below Openings = 0. (IFCREAL)
    Cladding below Openings Preset = "" (IFCLABEL)
    Cladding below Sill Height = 0. (IFCREAL)
    Cladding below Sill Height Preset = "" (IFCLABEL)
    Claddings = TRUE (IFCBOOLEAN)
    Cost = 0. (IFCREAL)
    Custom Note 1 = "" (IFCLABEL)
    Custom Note 2 = "" (IFCLABEL)
    Custom Note 3 = "" (IFCLABEL)
    Custom Note 4 = "" (IFCLABEL)
    Custom Note 5 = "" (IFCLABEL)
    Group Type = 25 (IFCINTEGER)
    Ignore Openings in Plan View = FALSE (IFCBOOLEAN)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lock Cladding Origin = FALSE (IFCBOOLEAN)
    Main Cladding = 19.43830000000003 (IFCREAL)
    Main Cladding Preset = "Shiplap Smooth" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Note = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Unit = "kg" (IFCLABEL)
    Username = "" (IFCLABEL)
    Weight = 0. (IFCREAL)
  AC_Pset_CI_Tools_Wall_Covering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Accessories = "" (IFCLABEL)
    Archi-FM Type = "Others" (IFCLABEL)
    Cladding Materials = TRUE (IFCBOOLEAN)
    Cladding Setout = 0 (IFCINTEGER)
    Cladding above Head Height = 0. (IFCREAL)
    Cladding above Head Height Preset = "" (IFCLABEL)
    Cladding above Openings = 0. (IFCREAL)
    Cladding above Openings Preset = "" (IFCLABEL)
    Cladding below Openings = 0. (IFCREAL)
    Cladding below Openings Preset = "" (IFCLABEL)
    Cladding below Sill Height = 0. (IFCREAL)
    Cladding below Sill Height Preset = "" (IFCLABEL)
    Claddings = TRUE (IFCBOOLEAN)
    Cost = 0. (IFCREAL)
    Custom Note 1 = "" (IFCLABEL)
    Custom Note 2 = "" (IFCLABEL)
    Custom Note 3 = "" (IFCLABEL)
    Custom Note 4 = "" (IFCLABEL)
    Custom Note 5 = "" (IFCLABEL)
    Group Type = 25 (IFCINTEGER)
    Ignore Openings in Plan View = FALSE (IFCBOOLEAN)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lock Cladding Origin = FALSE (IFCBOOLEAN)
    Main Cladding = 15.67029999999997 (IFCREAL)
    Main Cladding Preset = "Shiplap Smooth" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Note = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Unit = "kg" (IFCLABEL)
    Username = "" (IFCLABEL)
    Weight = 0. (IFCREAL)
  AC_Pset_CI_Tools_Wall_Covering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Accessories = "" (IFCLABEL)
    Archi-FM Type = "Others" (IFCLABEL)
    Cladding Materials = TRUE (IFCBOOLEAN)
    Cladding Setout = 0 (IFCINTEGER)
    Cladding above Head Height = 0. (IFCREAL)
    Cladding above Head Height Preset = "" (IFCLABEL)
    Cladding above Openings = 0. (IFCREAL)
    Cladding above Openings Preset = "" (IFCLABEL)
    Cladding below Openings = 0. (IFCREAL)
    Cladding below Openings Preset = "" (IFCLABEL)
    Cladding below Sill Height = 0. (IFCREAL)
    Cladding below Sill Height Preset = "" (IFCLABEL)
    Claddings = TRUE (IFCBOOLEAN)
    Cost = 0. (IFCREAL)
    Custom Note 1 = "" (IFCLABEL)
    Custom Note 2 = "" (IFCLABEL)
    Custom Note 3 = "" (IFCLABEL)
    Custom Note 4 = "" (IFCLABEL)
    Custom Note 5 = "" (IFCLABEL)
    Group Type = 25 (IFCINTEGER)
    Ignore Openings in Plan View = FALSE (IFCBOOLEAN)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lock Cladding Origin = FALSE (IFCBOOLEAN)
    Main Cladding = 11.42829999999994 (IFCREAL)
    Main Cladding Preset = "Shiplap Smooth" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Note = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Unit = "kg" (IFCLABEL)
    Username = "" (IFCLABEL)
    Weight = 0. (IFCREAL)
  AC_Equantity_CI_Tools_Wall_Covering | quantities | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Bottom Level = -50. [MILLI METRE]
    Head Height = 2200. [MILLI METRE]
    Sill Height = 900. [MILLI METRE]
    Top Level = 2400.000000000001 [MILLI METRE]
  AC_Pset_Dryer_#1548 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    3D Detail Level = "" (IFCLABEL)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Area = 0. (IFCREAL)
    Assembly Date = "" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Cabinet Surface = "Paint - Titanium White" (IFCLABEL)
    Collection of Specifications ID = "" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Control Area Surface = "Paint - Pale Jade" (IFCLABEL)
    Control Layout = 1 (IFCINTEGER)
    Control Panel Surface = "Paint - Titanium White" (IFCLABEL)
    Control Surface = "Paint - Titanium White" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Custom Text = "dr" (IFCLABEL)
    Dimensions W/D/H = "" (IFCLABEL)
    Door Surface = "Glass - Clear Fast" (IFCLABEL)
    Drum Surface = "Metal - Stainless Steel" (IFCLABEL)
    Edit Property = 1 (IFCINTEGER)
    Fill Background Pen = "Objects - Fill Backgrounds" (IFCLABEL)
    Fill Pen = "Objects - Cut Fills" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Group Type (FM_Type) = "HVAC Equipment" (IFCLABEL)
    Group Type (iFMType) = 12 (IFCINTEGER)
    ID Number = "" (IFCLABEL)
    IFC Predefined Type = 0 (IFCINTEGER)
    IFC Subtype = 0 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Label Content = "None" (IFCLABEL)
    Label Font = "Arial Western" (IFCLABEL)
    Label Orientation = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Label Pen = "Annotation Text - general" (IFCLABEL)
    Label Rotates with Object = FALSE (IFCBOOLEAN)
    Label Text Height = 2. (IFCREAL)
    Line Type = 1 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 0 (IFCINTEGER)
    ONORM Description = "" (IFCLABEL)
    ONORM Manufacturer = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Onorm Base Height = "" (IFCLABEL)
    Onorm Number = "" (IFCLABEL)
    Page = 5 (IFCINTEGER)
    Part = 1 (IFCINTEGER)
    Product ID = "" (IFCLABEL)
    Product Name (FM_ProductName) = "" (IFCLABEL)
    Product Name (gs_onorm_product) = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    SubPart = 0 (IFCINTEGER)
    To Zone Number = "" (IFCLABEL)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Version = 4 (IFCINTEGER)
    Version Number = 0 (IFCINTEGER)
    Volume = 0. (IFCREAL)
    Wall Mounted = 0 (IFCINTEGER)
    Zone Name = "" (IFCLABEL)
    Zone Number = "" (IFCLABEL)
  AC_Equantity_Dryer_#1548 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Control Panel Thickness = 25. [MILLI METRE]
    Control Panel Width = 120. [MILLI METRE]
    Toe Space Depth = 40. [MILLI METRE]
    Toe Space Height = 120. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    X Dimension = 650. [MILLI METRE]
    Y Dimension = 700. [MILLI METRE]
    Z Dimension = 900. [MILLI METRE]
  AC_Pset_Dining_Table_Rectangle_24 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 2 (IFCINTEGER)
    3D Detail Level = 3 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Backrest = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Chair Frame = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Chair Type = 1 (IFCINTEGER)
    Chair Type on the Bottom = "Chairs" (IFCLABEL)
    Chair Type on the Left = "Chair" (IFCLABEL)
    Chair on the Bottom (bChairBottom) = TRUE (IFCBOOLEAN)
    Chair on the Bottom (iBottomSideType) = 1 (IFCINTEGER)
    Chair on the Left (bChairLeft) = FALSE (IFCBOOLEAN)
    Chair on the Left (iLeftSideType) = 1 (IFCINTEGER)
    Chair on the Right = FALSE (IFCBOOLEAN)
    Chair on the Top = TRUE (IFCBOOLEAN)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Group Type (FM_Type) = "Furniture" (IFCLABEL)
    Group Type (iFMType) = 16 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Chairs X Direction = 2 (IFCINTEGER)
    Number of Chairs Y Direction = 1 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Resolution = 16 (IFCINTEGER)
    Seat = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Sizing (SizingType) = "by Chair and Distance" (IFCLABEL)
    Sizing (iSizingType) = 1 (IFCINTEGER)
    Symbol Type (gs_SymbolType) = "Rectangle with Backrest 1" (IFCLABEL)
    Symbol Type (gs_SymbolType_m) = 4 (IFCINTEGER)
    Symbol Type Enable Mask = 4083 (IFCINTEGER)
    Table Leg = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Tabletop = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Uniform Surfaces = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Equantity_Dining_Table_Rectangle_24 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Additional Side Space for Wheelchair = 300. [MILLI METRE]
    Additional Table Width = 200. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Chair Depth = 470. [MILLI METRE]
    Chair Height = 850. [MILLI METRE]
    Chair Width = 400. [MILLI METRE]
    Chair-Table Distance = -230.6911487816787 [MILLI METRE]
    Depth for Wheelchair = 869.9999999999999 [MILLI METRE]
    Depth per Chair = 539.3088512183213 [MILLI METRE]
    Dimension 1 = 1199.999999999999 [MILLI METRE]
    Dimension 2 = 1378.617702436643 [MILLI METRE]
    Distance behind Chair = 300. [MILLI METRE]
    Distance behind Wheelchair = 300. [MILLI METRE]
    Distance next to Wheelchair = 300. [MILLI METRE]
    Height = 850. [MILLI METRE]
    Leg Width = 40. [MILLI METRE]
    Min. Chair-Chair Distance = 200. [MILLI METRE]
    Real Chair Distance Horizontal = 199.9999999999996 [MILLI METRE]
    Real Chair Distance Vertical = 500.0000000000003 [MILLI METRE]
    Seat Height = 400. [MILLI METRE]
    Table Half Length = 599.9999999999997 [MILLI METRE]
    Table Half Width = 450.0000000000002 [MILLI METRE]
    Table Height = 750. [MILLI METRE]
    Table Length = 1199.999999999999 [MILLI METRE]
    Table Width = 900.0000000000003 [MILLI METRE]
    Table Width for Chairs = 800. [MILLI METRE]
    Tabletop Overhang X = 100. [MILLI METRE]
    Tabletop Overhang Y = 100. [MILLI METRE]
    Tabletop Thickness = 40. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Wheelchair Depth = 570. [MILLI METRE]
    Wheelchair Height = 850. [MILLI METRE]
    Wheelchair Width = 500. [MILLI METRE]
    Width for Wheelchair = 1100. [MILLI METRE]
    Width per Chair = 599.9999999999997 [MILLI METRE]
  AC_Pset_Laundry_Tub_#1546 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    3D Detail Level = "" (IFCLABEL)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Area = 0. (IFCREAL)
    Assembly Date = "" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Collection of Specifications ID = "" (IFCLABEL)
    Content = "None" (IFCLABEL)
    Contour Pen = "Fills - color 7" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Dimensions W/D/H = "" (IFCLABEL)
    Edit Property = 3 (IFCINTEGER)
    Fill Background Pen = "General- backgrounds" (IFCLABEL)
    Fill Pen = "Gypsum - Cut Lines" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Font = "Arial Western" (IFCLABEL)
    Full Text = "T" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Group Type (FM_Type) = "HVAC Equipment" (IFCLABEL)
    Group Type (iFMType) = 12 (IFCINTEGER)
    ID Number = "" (IFCLABEL)
    IFC Predefined Type = 0 (IFCINTEGER)
    IFC Subtype = 0 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Label Orientation = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Label Pen = "Annotation Text - header" (IFCLABEL)
    Line Type = 1 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 0 (IFCINTEGER)
    ONORM Description = "" (IFCLABEL)
    ONORM Manufacturer = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Onorm Base Height = "" (IFCLABEL)
    Onorm Number = "" (IFCLABEL)
    Page = 5 (IFCINTEGER)
    Part = 1 (IFCINTEGER)
    Product ID = "" (IFCLABEL)
    Product Name (FM_ProductName) = "" (IFCLABEL)
    Product Name (gs_onorm_product) = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Rotate with Object = FALSE (IFCBOOLEAN)
    Serial Number = "" (IFCLABEL)
    Short Text = "tub" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    SubPart = 2 (IFCINTEGER)
    Surface (cabinetMat) = "Paint - Titanium White" (IFCLABEL)
    Surface (tubMat) = "Metal - Stainless Steel" (IFCLABEL)
    Text Height = 1.5 (IFCREAL)
    To Zone Number = "" (IFCLABEL)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Version = 4 (IFCINTEGER)
    Version Number = 0 (IFCINTEGER)
    Volume = 0. (IFCREAL)
    Zone Name = "" (IFCLABEL)
    Zone Number = "" (IFCLABEL)
  AC_Equantity_Laundry_Tub_#1546 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Back Radius = 50. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Bottom Panel Width = 120. [MILLI METRE]
    Dimension 1 = 350. [MILLI METRE]
    Dimension 2 = 700. [MILLI METRE]
    Door Thickness = 25. [MILLI METRE]
    Front Radius = 50. [MILLI METRE]
    Handle Length = 80. [MILLI METRE]
    Handle Width = 30. [MILLI METRE]
    Height = 900. [MILLI METRE]
    Inset from Tub = 5. [MILLI METRE]
    Space at Back = 120. [MILLI METRE]
    Space at Front = 50. [MILLI METRE]
    Space at Sides = 50. [MILLI METRE]
    Thickness = 45. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Top Panel Width = 160. [MILLI METRE]
    Tub Depth = 180. [MILLI METRE]
    Upstand = 60. [MILLI METRE]
  AC_Pset_Sofa_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 6 (IFCINTEGER)
    3D Detail Level = 4 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Cushion = "Textile - 01" (IFCLABEL)
    Extra Hotspot Editing = TRUE (IFCBOOLEAN)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Foreground Fill" (IFCLABEL)
    Frame = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Group Type (FM_Type) = "Furniture" (IFCLABEL)
    Group Type (iFMType) = 16 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Leg (bLeg) = TRUE (IFCBOOLEAN)
    Leg (gs_leg_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Leg Style (gs_leg_type) = "Type 5" (IFCLABEL)
    Leg Style (iLegType) = 5 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    No. of Seats = 1 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Resolution = 12 (IFCINTEGER)
    Seating = "Paint - Sand Beige" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Seats in 2D = TRUE (IFCBOOLEAN)
    Side = "Wood - Walnut Horizontal" (IFCLABEL)
    Sofa = "Textile - 01" (IFCLABEL)
    Style (iStyle) = 1 (IFCINTEGER)
    Style (stStyle) = "Style 1" (IFCLABEL)
    Symbol Type = 4 (IFCINTEGER)
    Trimming = "Plastic - Laminate" (IFCLABEL)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Pset_Sofa_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 6 (IFCINTEGER)
    3D Detail Level = 4 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Cushion = "Textile - 01" (IFCLABEL)
    Extra Hotspot Editing = TRUE (IFCBOOLEAN)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Foreground Fill" (IFCLABEL)
    Frame = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Group Type (FM_Type) = "Furniture" (IFCLABEL)
    Group Type (iFMType) = 16 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Leg (bLeg) = TRUE (IFCBOOLEAN)
    Leg (gs_leg_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Leg Style (gs_leg_type) = "Type 5" (IFCLABEL)
    Leg Style (iLegType) = 5 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    No. of Seats = 3 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Resolution = 12 (IFCINTEGER)
    Seating = "Paint - Sand Beige" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Seats in 2D = TRUE (IFCBOOLEAN)
    Side = "Wood - Walnut Horizontal" (IFCLABEL)
    Sofa = "Textile - 01" (IFCLABEL)
    Style (iStyle) = 1 (IFCINTEGER)
    Style (stStyle) = "Style 1" (IFCLABEL)
    Symbol Type = 4 (IFCINTEGER)
    Trimming = "Plastic - Laminate" (IFCLABEL)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Equantity_Sofa_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Arm Height = 600. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 800. [MILLI METRE]
    Dimension 2 = 800. [MILLI METRE]
    Height = 800. [MILLI METRE]
    Leg Height = 80. [MILLI METRE]
    Minimal Space Behind = 200. [MILLI METRE]
    Minimal Space in Front = 250. [MILLI METRE]
    Minimal Space on Sides = 200. [MILLI METRE]
    Seat Height = 450. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Equantity_Sofa_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Arm Height = 600. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 2100. [MILLI METRE]
    Dimension 2 = 900. [MILLI METRE]
    Height = 800. [MILLI METRE]
    Leg Height = 80. [MILLI METRE]
    Minimal Space Behind = 200. [MILLI METRE]
    Minimal Space in Front = 250. [MILLI METRE]
    Minimal Space on Sides = 200. [MILLI METRE]
    Seat Height = 450. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Pset_Coffee_Table_02_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    3D Detail Level = 3 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Foreground Fill" (IFCLABEL)
    Glass = "Glass - Blue" (IFCLABEL)
    Glass in Tabletop = TRUE (IFCBOOLEAN)
    Group Type (FM_Type) = "Furniture" (IFCLABEL)
    Group Type (iFMType) = 16 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Leg = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Shelf (gs_shelv) = TRUE (IFCBOOLEAN)
    Shelf (gs_shelv_mat) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Tabletop = "Wood - Pine Grained Horizontal" (IFCLABEL)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Equantity_Coffee_Table_02_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Height = 450. [MILLI METRE]
    Leg Size = 40. [MILLI METRE]
    Minimal Space Behind = 600. [MILLI METRE]
    Minimal Space in Front = 600. [MILLI METRE]
    Minimal Space on Sides = 600. [MILLI METRE]
    Shelf Position = 250. [MILLI METRE]
    Shelf Thickness = 20. [MILLI METRE]
    Tabletop Overhang X = 40. [MILLI METRE]
    Tabletop Overhang Y = 40. [MILLI METRE]
    Tabletop Thickness = 40. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Pset_Hood_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 3 (IFCINTEGER)
    3D Detail Level = 3 (IFCINTEGER)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Base Height = "" (IFCLABEL)
    Additional Description = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Additional Manufacturer = "" (IFCLABEL)
    Additional Number = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Appliance = "Metal - Nickel" (IFCLABEL)
    Area = 0. (IFCREAL)
    Assembly Date = "" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Collection of Specifications ID = "" (IFCLABEL)
    Connection = "Metal - Stainless Steel" (IFCLABEL)
    Connection Status = TRUE (IFCBOOLEAN)
    Connection Type = "" (IFCLABEL)
    Contour Pen = "General - General" (IFCLABEL)
    Control Knobs = "Metal - Zinc" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Dimensions W/D/H = "" (IFCLABEL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Window Background" (IFCLABEL)
    Fill Type = "Background Fill (2)" (IFCLABEL)
    Filter Trim = "Metal - Stainless Steel" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Glass = "Glass - Blue" (IFCLABEL)
    Grease Filter = "Metal - Zinc" (IFCLABEL)
    Group Type (FM_Type) = "HVAC Equipment" (IFCLABEL)
    Group Type (iFMType) = 12 (IFCINTEGER)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Lamp = "Glass - Lamp" (IFCLABEL)
    Location = "" (IFCLABEL)
    MEP System = "Undefined" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    Nominal Diameter = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 1 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Overhead Line Type = 4 (IFCINTEGER)
    Product ID = "" (IFCLABEL)
    Product Name (FM_ProductName) = "" (IFCLABEL)
    Product Name (gs_onorm_product) = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Resolution = 18 (IFCINTEGER)
    Serial Number = "" (IFCLABEL)
    Set Program = FALSE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Shape Type = "Rectangle" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Story Sensitive = TRUE (IFCBOOLEAN)
    Symbol Line Type = 1 (IFCINTEGER)
    System Surface = "Paint - Cadmium Yellow" (IFCLABEL)
    To Zone Number = "" (IFCLABEL)
    Tool Type = 1 (IFCINTEGER)
    Type (type) = "Hood 6" (IFCLABEL)
    Type (type_m) = 6 (IFCINTEGER)
    Use System Surface = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Volume = 0. (IFCREAL)
    Wall Mounted = TRUE (IFCBOOLEAN)
  AC_Equantity_Hood_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 0. [MILLI METRE]
    Connection Length = 50. [MILLI METRE]
    Connection Position X = 489.5 [MILLI METRE]
    Connection Position Y = 660.4 [MILLI METRE]
    Connection Position Z = 553.4 [MILLI METRE]
    Connector Depth = 0. [MILLI METRE]
    Connector Height = 30. [MILLI METRE]
    Connector Width = 0. [MILLI METRE]
    Dimension 1 = 900. [MILLI METRE]
    Dimension 2 = 500. [MILLI METRE]
    Height = 920. [MILLI METRE]
    Inner Height = 80. [MILLI METRE]
    Inner Width = 170. [MILLI METRE]
    Nominal Depth = 0. [MILLI METRE]
    Top Level = 970.0000000000001 [MILLI METRE]
    Wall Thickness = 1. [MILLI METRE]
  AC_Pset_Standing_Cabinet_Block_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 1 (IFCINTEGER)
    3D Detail Level = 1 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Cabinet (matCabinet) = "Haast Half" (IFCLABEL)
    Cabinet Contour Line = 1 (IFCINTEGER)
    Cabinet Contour Pen = "Objects - General" (IFCLABEL)
    Carcass Contour Line = 21 (IFCINTEGER)
    Carcass Contour Pen = "Objects - General" (IFCLABEL)
    Cold Water Connection = FALSE (IFCBOOLEAN)
    Connection = "Foliage - Leaves Tree Small" (IFCLABEL)
    Connection Contour Line = 1 (IFCINTEGER)
    Connection Type (ConConnectorType_1) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_2) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_3) = "Welded" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Double Face = FALSE (IFCBOOLEAN)
    Drawer Structure = "Haast Half" (IFCLABEL)
    Equal Heights = FALSE (IFCBOOLEAN)
    Fill Background Pen = "Window Background" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Footing (bFooting) = TRUE (IFCBOOLEAN)
    Footing (matFooting) = "Haast Half" (IFCLABEL)
    Footing Type = 1 (IFCINTEGER)
    Front Joint = 1 (IFCINTEGER)
    Front Panel Position = 2 (IFCINTEGER)
    Group Type (FM_Type) = "Furniture" (IFCLABEL)
    Group Type (iFMType) = 16 (IFCINTEGER)
    Hot Water Connection = FALSE (IFCBOOLEAN)
    Inner Shelf Material 1 = "Insulation - Solid Brown" (IFCLABEL)
    Inner Shelf Material 2 = "Insulation - Solid Brown" (IFCLABEL)
    Inner Shelf Material 3 = "Insulation - Solid Brown" (IFCLABEL)
    Inner Shelf Material 4 = "Insulation - Solid Brown" (IFCLABEL)
    Inner Shelf Material 5 = "Insulation - Solid Brown" (IFCLABEL)
    Inner Shelf Material 6 = "Insulation - Solid Brown" (IFCLABEL)
    Inner Shelf Material 7 = "Insulation - Solid Brown" (IFCLABEL)
    Inner Shelf Material 8 = "Insulation - Solid Brown" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Knob = "Haast Half" (IFCLABEL)
    Left Panel = FALSE (IFCBOOLEAN)
    Location = "" (IFCLABEL)
    MEP System (ConSystem_1) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_2) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_3) = "Undefined" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_1) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_2) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_3) = "" (IFCLABEL)
    Nominal Size = 3 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 3 (IFCINTEGER)
    Number of Inner Segments (nSubsegment1) = 1 (IFCINTEGER)
    Number of Inner Segments (nSubsegment2) = 1 (IFCINTEGER)
    Number of Inner Segments (nSubsegment3) = 1 (IFCINTEGER)
    Number of Inner Segments (nSubsegment4) = 1 (IFCINTEGER)
    Number of Inner Segments (nSubsegment5) = 1 (IFCINTEGER)
    Number of Inner Segments (nSubsegment6) = 1 (IFCINTEGER)
    Number of Inner Segments (nSubsegment7) = 1 (IFCINTEGER)
    Number of Inner Segments (nSubsegment8) = 1 (IFCINTEGER)
    Number of Legs Row 1 = 2 (IFCINTEGER)
    Number of Legs Row 2 = 0 (IFCINTEGER)
    Number of Legs Row 3 = 2 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Opening Symbol (bShowOpeningSymbol) = TRUE (IFCBOOLEAN)
    Opening Symbol (penOpeningSymbol) = "Objects - Symbols and Separators" (IFCLABEL)
    Opening Symbol Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Opening Symbol Line = 1 (IFCINTEGER)
    Opening Symbol Type Front = 10 (IFCINTEGER)
    Opening Symbol Type Rear = 0 (IFCINTEGER)
    Plinth (matPlinth) = "Tiles - Mosaic Blue" (IFCLABEL)
    Plinth on Front = FALSE (IFCBOOLEAN)
    Plinth on Left = FALSE (IFCBOOLEAN)
    Plinth on Rear = FALSE (IFCBOOLEAN)
    Plinth on Right = FALSE (IFCBOOLEAN)
    Production Year = "" (IFCLABEL)
    Rear Joint = 1 (IFCINTEGER)
    Rear Panel = FALSE (IFCBOOLEAN)
    Rear Panel Position = 2 (IFCINTEGER)
    Resolution = 36 (IFCINTEGER)
    Right Panel = FALSE (IFCBOOLEAN)
    Segment Opening Type (iSegmentOpeningType1) = 2 (IFCINTEGER)
    Segment Opening Type (iSegmentOpeningType2) = 2 (IFCINTEGER)
    Segment Opening Type (iSegmentOpeningType3) = 2 (IFCINTEGER)
    Segment Opening Type (iSegmentOpeningType4) = 2 (IFCINTEGER)
    Segment Opening Type (iSegmentOpeningType5) = 2 (IFCINTEGER)
    Segment Opening Type (iSegmentOpeningType6) = 2 (IFCINTEGER)
    Segment Opening Type (iSegmentOpeningType7) = 2 (IFCINTEGER)
    Segment Opening Type (iSegmentOpeningType8) = 2 (IFCINTEGER)
    Segment Opening Type on Rear Side (iSegmentOpeningTypeRear1) = 0 (IFCINTEGER)
    Segment Opening Type on Rear Side (iSegmentOpeningTypeRear2) = 0 (IFCINTEGER)
    Segment Opening Type on Rear Side (iSegmentOpeningTypeRear3) = 0 (IFCINTEGER)
    Segment Opening Type on Rear Side (iSegmentOpeningTypeRear4) = 0 (IFCINTEGER)
    Segment Opening Type on Rear Side (iSegmentOpeningTypeRear5) = 0 (IFCINTEGER)
    Segment Opening Type on Rear Side (iSegmentOpeningTypeRear6) = 0 (IFCINTEGER)
    Segment Opening Type on Rear Side (iSegmentOpeningTypeRear7) = 0 (IFCINTEGER)
    Segment Opening Type on Rear Side (iSegmentOpeningTypeRear8) = 0 (IFCINTEGER)
    Segment Type (iSegmentType1) = 3 (IFCINTEGER)
    Segment Type (iSegmentType2) = 3 (IFCINTEGER)
    Segment Type (iSegmentType3) = 3 (IFCINTEGER)
    Segment Type (iSegmentType4) = 3 (IFCINTEGER)
    Segment Type (iSegmentType5) = 3 (IFCINTEGER)
    Segment Type (iSegmentType6) = 3 (IFCINTEGER)
    Segment Type (iSegmentType7) = 3 (IFCINTEGER)
    Segment Type (iSegmentType8) = 3 (IFCINTEGER)
    Segment Type on Rear Side (iSegmentTypeRear1) = 4 (IFCINTEGER)
    Segment Type on Rear Side (iSegmentTypeRear2) = 4 (IFCINTEGER)
    Segment Type on Rear Side (iSegmentTypeRear3) = 4 (IFCINTEGER)
    Segment Type on Rear Side (iSegmentTypeRear4) = 4 (IFCINTEGER)
    Segment Type on Rear Side (iSegmentTypeRear5) = 4 (IFCINTEGER)
    Segment Type on Rear Side (iSegmentTypeRear6) = 4 (IFCINTEGER)
    Segment Type on Rear Side (iSegmentTypeRear7) = 4 (IFCINTEGER)
    Segment Type on Rear Side (iSegmentTypeRear8) = 4 (IFCINTEGER)
    Segments Number = 2 (IFCINTEGER)
    Serial Number = "" (IFCLABEL)
    Set Program = FALSE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Shape Type (ConType_1) = "Circle" (IFCLABEL)
    Shape Type (ConType_2) = "Circle" (IFCLABEL)
    Shape Type (ConType_3) = "Circle" (IFCLABEL)
    Shelf = "Haast Half" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Left Cabinet Edge = TRUE (IFCBOOLEAN)
    Show Rear Cabinet Edge = TRUE (IFCBOOLEAN)
    Show Right Cabinet Edge = TRUE (IFCBOOLEAN)
    Symbol Contour Line = 1 (IFCINTEGER)
    Symbol Contour Pen = "Objects - General" (IFCLABEL)
    Symbol Type = 1 (IFCINTEGER)
    System Surface = "Brick - Classic Tongariro" (IFCLABEL)
    Tool Type (ConToolType_1) = 2 (IFCINTEGER)
    Tool Type (ConToolType_2) = 2 (IFCINTEGER)
    Tool Type (ConToolType_3) = 2 (IFCINTEGER)
    Uniform Fronts = FALSE (IFCBOOLEAN)
    Uniform Functions (bLinkSegmentTypes) = TRUE (IFCBOOLEAN)
    Uniform Functions (bLinkSegmentTypesRear) = FALSE (IFCBOOLEAN)
    Uniform Style = FALSE (IFCBOOLEAN)
    Use System Surface = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Waste Water Connection = FALSE (IFCBOOLEAN)
  AC_Pset_Oven_Standard_#1015 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Assembly Date = "" (IFCLABEL)
    Background Pen = "Objects - Fill Backgrounds" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Collection of Specifications ID = "" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cooktop View Attributes = "Objects - Extras" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Egress = 0. (IFCREAL)
    Fill = "Background Fill (2)" (IFCLABEL)
    Fill Background Pen = "Objects - Fill Backgrounds" (IFCLABEL)
    Fill Pen (cooktopFillPen) = "Objects - Cut Fills" (IFCLABEL)
    Fill Pen (gs_fill_pen) = "Objects - Cut Fills" (IFCLABEL)
    Fill Type = "Background Fill (2)" (IFCLABEL)
    GUID = "7d1077c8-24ad-471c-92bc-eec0ce39a104" (IFCLABEL)
    Group Type (FM_Type) = "Electric Facilities" (IFCLABEL)
    Group Type (iFMType) = 8 (IFCINTEGER)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Label Category = "Appliances" (IFCLABEL)
    Label Orientation = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Label Text (full) = "stove" (IFCLABEL)
    Label Text (short) = "St" (IFCLABEL)
    Line Type (cooktopLineType) = 1 (IFCINTEGER)
    Line Type (gs_line_type) = 1 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    ONORM Description = "" (IFCLABEL)
    ONORM Manufacturer = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "" (IFCLABEL)
    Onorm Base Height = "" (IFCLABEL)
    Onorm Number = "" (IFCLABEL)
    Outline Pen = "Objects - Uncut and Overhead" (IFCLABEL)
    Product Name = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Save Attributes = 0 (IFCINTEGER)
    Save View Attributes = FALSE (IFCBOOLEAN)
    Serial Number = "" (IFCLABEL)
    Showing 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    To Zone Number = "" (IFCLABEL)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Version Number = 1 (IFCINTEGER)
    View Attributes = "Objects - Electrical Appliances" (IFCLABEL)
    View Attributes GUID = "e0d07294-ffc1-49cf-ad64-ffadd1eebf05" (IFCLABEL)
    Volts = 0. (IFCREAL)
    Wattage = 0. (IFCREAL)
    Width/Depth/Height = "" (IFCLABEL)
    Zone Name = "" (IFCLABEL)
    Zone Number = "" (IFCLABEL)
  AC_Equantity_Oven_Standard_#1015 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Control Panel Height = 320. [MILLI METRE]
    Oven Depth = 600. [MILLI METRE]
    Oven Door Height = 560. [MILLI METRE]
    Oven Height = 910. [MILLI METRE]
    Oven Width = 600. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Equantity_Standing_Cabinet_Block_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 100. [MILLI METRE]
    Cabinet Depth = 667.9999999999773 [MILLI METRE]
    Cabinet Height = 2100. [MILLI METRE]
    Cabinet Width = 450. [MILLI METRE]
    Carcass Depth = 649.9999999999773 [MILLI METRE]
    Carcass Height = 2000. [MILLI METRE]
    Carcass Thickness = 18. [MILLI METRE]
    Carcass Width = 450. [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Length (ConLength_3) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = 200. [MILLI METRE]
    Connection Position X (ConPosX_2) = 400. [MILLI METRE]
    Connection Position X (ConPosX_3) = 300. [MILLI METRE]
    Connection Position Y (ConPosY_1) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_2) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_3) = 0. [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 700. [MILLI METRE]
    Connection Position Z (ConPosZ_2) = 700. [MILLI METRE]
    Connection Position Z (ConPosZ_3) = 600. [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_3) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_3) = 42. [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_3) = 5. [MILLI METRE]
    Dimension 1 = 450. [MILLI METRE]
    Dimension 2 = 649.9999999999773 [MILLI METRE]
    Door Panel Thickness = 18. [MILLI METRE]
    Footing Height = 100. [MILLI METRE]
    Footing Setback from Carcass Front = 90. [MILLI METRE]
    Footing Setback from Carcass Left = 0. [MILLI METRE]
    Footing Setback from Carcass Rear = 0. [MILLI METRE]
    Footing Setback from Carcass Right = 0. [MILLI METRE]
    Front Panel Left Offset = 0. [MILLI METRE]
    Front Panel Right Offset = 0. [MILLI METRE]
    Full Height = 2100. [MILLI METRE]
    Height = 2000. [MILLI METRE]
    Inner Shelf Thickness (subShelfThickness1) = 18. [MILLI METRE]
    Inner Shelf Thickness (subShelfThickness2) = 18. [MILLI METRE]
    Inner Shelf Thickness (subShelfThickness3) = 18. [MILLI METRE]
    Inner Shelf Thickness (subShelfThickness4) = 18. [MILLI METRE]
    Inner Shelf Thickness (subShelfThickness5) = 18. [MILLI METRE]
    Inner Shelf Thickness (subShelfThickness6) = 18. [MILLI METRE]
    Inner Shelf Thickness (subShelfThickness7) = 18. [MILLI METRE]
    Inner Shelf Thickness (subShelfThickness8) = 18. [MILLI METRE]
    Left Panel Bottom Offset = 0. [MILLI METRE]
    Left Panel Front Offset = 0. [MILLI METRE]
    Left Panel Rear Offset = 0. [MILLI METRE]
    Left Panel Thickness = 18. [MILLI METRE]
    Left Panel Top Offset = 0. [MILLI METRE]
    Leg Depth = 25. [MILLI METRE]
    Leg Diameter = 30. [MILLI METRE]
    Leg Radius = 15. [MILLI METRE]
    Leg Width = 25. [MILLI METRE]
    Minimal Space Rear on Side Left = 0. [MILLI METRE]
    Minimal Space Rear on Side Right = 0. [MILLI METRE]
    Minimal Space in Front = 900. [MILLI METRE]
    Minimal Space in Rear = 900. [MILLI METRE]
    Minimal Space on Side Left = 0. [MILLI METRE]
    Minimal Space on Side Right = 0. [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_3) = 40. [MILLI METRE]
    Outer Depth (ConDepth_1) = 27. [MILLI METRE]
    Outer Depth (ConDepth_2) = 27. [MILLI METRE]
    Outer Depth (ConDepth_3) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_1) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_2) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_3) = 42. [MILLI METRE]
    Plinth Setback from Carcass Front = 90. [MILLI METRE]
    Plinth Setback from Carcass Left = 0. [MILLI METRE]
    Plinth Setback from Carcass Rear = 0. [MILLI METRE]
    Plinth Setback from Carcass Right = 0. [MILLI METRE]
    Plinth Thickness = 18. [MILLI METRE]
    Position of rows (1) = 50. [MILLI METRE]
    Position of rows (2) = 200. [MILLI METRE]
    Position of rows (3) = 400. [MILLI METRE]
    Rear Panel / Double Face Left Offset = 0. [MILLI METRE]
    Rear Panel / Double Face Right Offset = 0. [MILLI METRE]
    Rear Panel Bottom Offset = 0. [MILLI METRE]
    Rear Panel Thickness = 18. [MILLI METRE]
    Rear Panel Top Offset = 0. [MILLI METRE]
    Right Panel Bottom Offset = 0. [MILLI METRE]
    Right Panel Front Offset = 0. [MILLI METRE]
    Right Panel Rear Offset = 0. [MILLI METRE]
    Right Panel Thickness = 18. [MILLI METRE]
    Right Panel Top Offset = 0. [MILLI METRE]
    Segment Height 1 = 800. [MILLI METRE]
    Segment Height 2 = 1200. [MILLI METRE]
    Segment Height 3 = 0. [MILLI METRE]
    Segment Height 4 = 0. [MILLI METRE]
    Segment Height 5 = 0. [MILLI METRE]
    Segment Height 6 = 0. [MILLI METRE]
    Segment Height 7 = 0. [MILLI METRE]
    Segment Height 8 = 0. [MILLI METRE]
    Shelf Thickness = 18. [MILLI METRE]
    Top Level = 2100. [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_3) = 1. [MILLI METRE]
  AC_Pset_Cabinet_Base_Double_Door_24 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    'A' 'B' Size = = "Counter" (IFCLABEL)
    'A' 'B' Size=Cabinet Size = FALSE (IFCBOOLEAN)
    2D Detail Level = 1 (IFCINTEGER)
    2D Hidden Edges = 0 (IFCINTEGER)
    3D Detail Level = 1 (IFCINTEGER)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Base Height = "" (IFCLABEL)
    Additional Description = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Additional Manufacturer = "" (IFCLABEL)
    Additional Number = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Area = 0. (IFCREAL)
    Assembly Date = "" (IFCLABEL)
    Backsplash = "Plastic - Laminate" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Cabinet (gs_cabinet_mat) = "Paint - Glossy White" (IFCLABEL)
    Cabinet Symbol Type = "Type 1" (IFCLABEL)
    Cold Water Connection = TRUE (IFCBOOLEAN)
    Collection of Specifications ID = "" (IFCLABEL)
    Connection = "Metal - Stainless Steel" (IFCLABEL)
    Connection Type (ConConnectorType_1) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_2) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_3) = "Welded" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Counter (bCounter) = TRUE (IFCBOOLEAN)
    Counter (count_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Counter Edge Visibility in 3D (side_vis) = "None" (IFCLABEL)
    Counter Edge Visibility in 3D (side_vis_mirror) = "None" (IFCLABEL)
    Counter Type (gs_count_type) = "Rectangular" (IFCLABEL)
    Counter Type (gs_count_type_m) = 1 (IFCINTEGER)
    Custom Knob Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_p) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_p_end) = "" (IFCLABEL)
    Dimensions W/D/H = "" (IFCLABEL)
    Door (Frame) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Door (Glazing) = "Glass - Clear Fast" (IFCLABEL)
    Door (bDoor) = TRUE (IFCBOOLEAN)
    Door (gs_door_type) = "Style 1" (IFCLABEL)
    Door Opening Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Door Style = 1 (IFCINTEGER)
    Double Faced = FALSE (IFCBOOLEAN)
    Drawer (DrawerMat) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Drawer (bDrawer) = TRUE (IFCBOOLEAN)
    Drawer No. = 2 (IFCINTEGER)
    Edge Bevel = FALSE (IFCBOOLEAN)
    Edge Visibility in 2D (side_vis2D) = "None" (IFCLABEL)
    Edge Visibility in 2D (side_vis2D_m) = 0 (IFCINTEGER)
    Edge Visibility in 2D (side_vis2D_mirror) = "None" (IFCLABEL)
    End Panel = "Wood - Pine Grained Horizontal" (IFCLABEL)
    End Panel Type = "Style 1" (IFCLABEL)
    Extra Hotspot Editing = TRUE (IFCBOOLEAN)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Background" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Group Type (FM_Type) = "HVAC Equipment" (IFCLABEL)
    Group Type (iFMType) = 12 (IFCINTEGER)
    Hidden Edges Contour = "Objects - General" (IFCLABEL)
    Hidden Edges Line Type = 4 (IFCINTEGER)
    Hot Water Connection = TRUE (IFCBOOLEAN)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Knob (bKnob) = TRUE (IFCBOOLEAN)
    Knob (gs_knob_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Knob (gs_knob_type) = "Style 1" (IFCLABEL)
    Knob Style = 1 (IFCINTEGER)
    Left End Panel (left_panel) = FALSE (IFCBOOLEAN)
    Left End Panel (left_panel_mirror) = FALSE (IFCBOOLEAN)
    Left End Panel is in Cabinet Size = TRUE (IFCBOOLEAN)
    Leg and Panel Relative Situation = 0 (IFCINTEGER)
    Location = "" (IFCLABEL)
    MEP System (ConSystem_1) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_2) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_3) = "Undefined" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    No. of Hor. Door Grids = 2 (IFCINTEGER)
    No. of Shelves = 1 (IFCINTEGER)
    No. of Vert. Door Grids = 1 (IFCINTEGER)
    Nominal Size (ConNominalWidth_1) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_2) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_3) = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 3 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Placing = 0 (IFCINTEGER)
    Product ID = "" (IFCLABEL)
    Product Name (FM_ProductName) = "" (IFCLABEL)
    Product Name (gs_onorm_product) = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Rear End Panel = FALSE (IFCBOOLEAN)
    Rear End Panel is in Cabinet Size = TRUE (IFCBOOLEAN)
    Resolution = 16 (IFCINTEGER)
    Right End Panel (right_panel) = FALSE (IFCBOOLEAN)
    Right End Panel (right_panel_mirror) = FALSE (IFCBOOLEAN)
    Right End Panel is in Cabinet Size = TRUE (IFCBOOLEAN)
    Same Door Widths = TRUE (IFCBOOLEAN)
    Same Drawer Front as Door = TRUE (IFCBOOLEAN)
    Serial Number = "" (IFCLABEL)
    Set Program = FALSE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Shape Type (ConType_1) = "Circle" (IFCLABEL)
    Shape Type (ConType_2) = "Circle" (IFCLABEL)
    Shape Type (ConType_3) = "Circle" (IFCLABEL)
    Shelf = "Paint - Glossy White" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Sides Visible = 0 (IFCINTEGER)
    Sink (bSink) = TRUE (IFCBOOLEAN)
    Sink (gs_sink_mat) = "Metal - Chrome 01" (IFCLABEL)
    Sink Style = 2 (IFCINTEGER)
    Sink Symbol Type (SinkSymbol) = "Detailed" (IFCLABEL)
    Sink Symbol Type (SinkSymbol_m) = 2 (IFCINTEGER)
    Sink Type = "Style 2" (IFCLABEL)
    Sink Undermounted = FALSE (IFCBOOLEAN)
    System Surface = "Paint - Cadmium Yellow" (IFCLABEL)
    Tap (bTap) = TRUE (IFCBOOLEAN)
    Tap (gs_tap_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Tap Style = 1 (IFCINTEGER)
    Tap Symbol Type (TapSymbol) = "Detailed" (IFCLABEL)
    Tap Symbol Type (TapSymbol_m) = 2 (IFCINTEGER)
    Tap Type = "Style 1" (IFCLABEL)
    To Zone Number = "" (IFCLABEL)
    Toe (bToeOn) = TRUE (IFCBOOLEAN)
    Toe (toe_mat) = "Mtl-Stainless Steel (2)" (IFCLABEL)
    Toe Type (gs_toe_type) = "Full" (IFCLABEL)
    Toe Type (gs_toe_type_m) = 1 (IFCINTEGER)
    Tool Type (ConToolType_1) = 2 (IFCINTEGER)
    Tool Type (ConToolType_2) = 2 (IFCINTEGER)
    Tool Type (ConToolType_3) = 2 (IFCINTEGER)
    Use System Surface = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Volume = 0. (IFCREAL)
    Waste Water Connection = TRUE (IFCBOOLEAN)
  AC_Equantity_Cabinet_Base_Double_Door_24 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Backsplash Height (0-None) = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Cabinet Depth = 600. [MILLI METRE]
    Cabinet Width = 1825. [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Length (ConLength_3) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = 500. [MILLI METRE]
    Connection Position X (ConPosX_2) = 700. [MILLI METRE]
    Connection Position X (ConPosX_3) = 600. [MILLI METRE]
    Connection Position Y (ConPosY_1) = 600. [MILLI METRE]
    Connection Position Y (ConPosY_2) = 600. [MILLI METRE]
    Connection Position Y (ConPosY_3) = 600. [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 800. [MILLI METRE]
    Connection Position Z (ConPosZ_2) = 800. [MILLI METRE]
    Connection Position Z (ConPosZ_3) = 600. [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_3) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_3) = 42. [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_3) = 5. [MILLI METRE]
    Counter Thickness = 50. [MILLI METRE]
    Countertop Height = 900. [MILLI METRE]
    Custom Knob Depth = 20. [MILLI METRE]
    Custom Knob Height = 15. [MILLI METRE]
    Custom Knob Length = 100. [MILLI METRE]
    Door Frame Width (doorframe_w) = 90. [MILLI METRE]
    Door Frame Width (doorframe_w_end) = 90. [MILLI METRE]
    Door Panel Height = 630. [MILLI METRE]
    Door Thickness = 20. [MILLI METRE]
    Drawer Height = 130. [MILLI METRE]
    Knob Horizontal Position = 50. [MILLI METRE]
    Knob Size = 100. [MILLI METRE]
    Knob Vertical Position = 520. [MILLI METRE]
    Left Door Width = 912.5 [MILLI METRE]
    Left End Panel Thickness = 20. [MILLI METRE]
    Minimal Space in Front = 900. [MILLI METRE]
    Minimal Space on Side 1 = 0. [MILLI METRE]
    Minimal Space on Side 2 = 0. [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 25.4 [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_3) = 40. [MILLI METRE]
    Outer Depth (ConDepth_1) = 27. [MILLI METRE]
    Outer Depth (ConDepth_2) = 27. [MILLI METRE]
    Outer Depth (ConDepth_3) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_1) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_2) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_3) = 42. [MILLI METRE]
    Overhang to Front of Cabinet = 0. [MILLI METRE]
    Overhang to Left of Cabinet (left_cab) = 0. [MILLI METRE]
    Overhang to Left of Cabinet (left_cab_mirror) = 0. [MILLI METRE]
    Overhang to Rear of Cabinet = 0. [MILLI METRE]
    Overhang to Right of Cabinet (right_cab) = 0. [MILLI METRE]
    Overhang to Right of Cabinet (right_cab_mirror) = 0. [MILLI METRE]
    Rear End Panel Thickness = 20. [MILLI METRE]
    Rear Minimal Space = 900. [MILLI METRE]
    Rear Minimal Space on Side 1 = 0. [MILLI METRE]
    Rear Minimal Space on Side 2 = 0. [MILLI METRE]
    Right End Panel Thickness = 20. [MILLI METRE]
    Sink X Dist. from Center = 238.1072525772549 [MILLI METRE]
    Sink Y Dist. from Center = -1.498801083243961E-12 [MILLI METRE]
    Tap Offset X = 4.440892098500626E-13 [MILLI METRE]
    Toe Height = 90. [MILLI METRE]
    Toe Setback = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_3) = 1. [MILLI METRE]
  AC_Pset_Refrigerator_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 1 (IFCINTEGER)
    3D Detail Level = 3 (IFCINTEGER)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Base Height = "" (IFCLABEL)
    Additional Description = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Additional Manufacturer = "" (IFCLABEL)
    Additional Number = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Appliance = "Paint - Titanium White" (IFCLABEL)
    Assembly Date = "" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Collection of Specifications ID = "" (IFCLABEL)
    Contour Pen = "General - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Display Text = FALSE (IFCBOOLEAN)
    Door Symbol Type = 2 (IFCINTEGER)
    Egress = 0. (IFCREAL)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Background Fill (2)" (IFCLABEL)
    Font Style Bold = FALSE (IFCBOOLEAN)
    Font Style Italic = FALSE (IFCBOOLEAN)
    Font Style Underline = FALSE (IFCBOOLEAN)
    Font Type = "Arial" (IFCLABEL)
    Freezer = TRUE (IFCBOOLEAN)
    Freezer Type = 1 (IFCINTEGER)
    Fridge Door = "Paint - Titanium White" (IFCLABEL)
    Group Type (FM_Type) = "Electric Facilities" (IFCLABEL)
    Group Type (iFMType) = 8 (IFCINTEGER)
    Handle (bHandle) = TRUE (IFCBOOLEAN)
    Handle (handle_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Handle Type (gs_handle_style) = "Square" (IFCLABEL)
    Handle Type (gs_handle_style_m) = 1 (IFCINTEGER)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Product Name = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Symbol Fill Type = "Foreground Fill (2)" (IFCLABEL)
    Symbol Line Type = 1 (IFCINTEGER)
    Symbol Pen = "Objects - General" (IFCLABEL)
    Symbol Type = "Style 1" (IFCLABEL)
    Text = "F" (IFCLABEL)
    Text Orientation on Symbol (typeTextRotation) = "Readable" (IFCLABEL)
    Text Orientation on Symbol (typeTextRotation_m) = 2 (IFCINTEGER)
    Text Pen = "Annotation text - notes" (IFCLABEL)
    To Zone Number = "" (IFCLABEL)
    Toe (bToe) = TRUE (IFCBOOLEAN)
    Toe (toe_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Top Panel (topp) = TRUE (IFCBOOLEAN)
    Top Panel (toppmat) = "Paint - Titanium White" (IFCLABEL)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Volts = 0. (IFCREAL)
    Wattage = 0. (IFCREAL)
    Width/Depth/Height = "" (IFCLABEL)
  AC_Equantity_Refrigerator_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 750. [MILLI METRE]
    Dimension 2 = 700. [MILLI METRE]
    Door Thickness = 60. [MILLI METRE]
    Font Size = 120. [MILLI METRE]
    Freezer Height = 400. [MILLI METRE]
    Handle Height = 200. [MILLI METRE]
    Handle Vertical Position = 1000. [MILLI METRE]
    Minimal Space in Front = 900. [MILLI METRE]
    Minimal Space on Side 1 = 0. [MILLI METRE]
    Minimal Space on Side 2 = 0. [MILLI METRE]
    Text Position X = 0. [MILLI METRE]
    Text Position Y = 0. [MILLI METRE]
    Toe Height = 90. [MILLI METRE]
    Toe Setback = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Total Height = 1800. [MILLI METRE]
  AC_Pset_CI_Tools_Window | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    2D Symbol Frame Profile = 1 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Acoustic Rating = "" (IFCLABEL)
    Cavity Closure = "none" (IFCLABEL)
    Cavity Closure Exterior = "regular" (IFCLABEL)
    Cavity Closure Interior = "regular" (IFCLABEL)
    Cavity Closure Left = TRUE (IFCBOOLEAN)
    Cavity Closure Right = TRUE (IFCBOOLEAN)
    Cavity Closure Skins turn In = 0 (IFCINTEGER)
    Cavity Closure Skins turn Out = 0 (IFCINTEGER)
    Code (widoCode) = "-" (IFCLABEL)
    Code Format = "<C>-<H><W><M>" (IFCLABEL)
    Code Size Format = 1 (IFCINTEGER)
    Code for Configuration = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Current Page = 29 (IFCINTEGER)
    Door Leaf Number Left = 1 (IFCINTEGER)
    Door Leaf Number Right = 0 (IFCINTEGER)
    Door Type = "Standard" (IFCLABEL)
    Door UI Editing Set = 1 (IFCINTEGER)
    Doors and Windows Remain Open in Section/Elevation = FALSE (IFCBOOLEAN)
    Double Hung Sash Ratio = 0.4 (IFCREAL)
    Elevation = "" (IFCLABEL)
    Exterior Handle = "None" (IFCLABEL)
    Exterior Handle Plate = "None" (IFCLABEL)
    Exterior Handle Plate Position = 0 (IFCINTEGER)
    Exterior Reveal Link Dimensions = TRUE (IFCBOOLEAN)
    Exterior Trim = "None" (IFCLABEL)
    Exterior Trim Bricks = FALSE (IFCBOOLEAN)
    Exterior Trim Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Exterior Trim Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Exterior Trim Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Exterior Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim View Pen = "Openings - General" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Frame Mitre Left = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Mitre Right = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Pen = "2D Elements - General" (IFCLABEL)
    Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame Section Fill = "Background Fill" (IFCLABEL)
    Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame Section Line Type = 1 (IFCINTEGER)
    Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Frame Surface = "Paint - Titanium White" (IFCLABEL)
    Frame Type Head = "Frame" (IFCLABEL)
    Frame Type Left = "Frame" (IFCLABEL)
    Frame Type Right = "Frame" (IFCLABEL)
    Frame Type Sill = "Frame" (IFCLABEL)
    Frame View Background Pen = "Transparent" (IFCLABEL)
    Frame View Fill = "Background Fill" (IFCLABEL)
    Frame View Fill Pen = "Openings - General" (IFCLABEL)
    Frame View Line Type = 1 (IFCINTEGER)
    Frame View Pen = "Openings - General" (IFCLABEL)
    Glass Pane Number = 1 (IFCINTEGER)
    Glass Pen = "2D Elements - General" (IFCLABEL)
    Glass Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Glass Section Fill = "Air Space" (IFCLABEL)
    Glass Section Fill Pen = "General - General" (IFCLABEL)
    Glass Section Line Type = 1 (IFCINTEGER)
    Glass Section Pen = "General - General" (IFCLABEL)
    Glass Surface (gs_glass_mat) = "Glass - Clear Fast" (IFCLABEL)
    Glass View Pen = "General - General" (IFCLABEL)
    Glazing = "" (IFCLABEL)
    Glazing Bars Full Window = TRUE (IFCBOOLEAN)
    Glazing Bars View Pen = "General - General" (IFCLABEL)
    Group Type = "Others" (IFCLABEL)
    Handle Placement to Right Leaf = FALSE (IFCBOOLEAN)
    Handle Placement to Second Leaf = FALSE (IFCBOOLEAN)
    Handle View Pen = "Openings - General" (IFCLABEL)
    Hardware Pen = "2D Elements - General" (IFCLABEL)
    Hardware Set = "" (IFCLABEL)
    Hardware Surface = "Metal - Stainless Steel" (IFCLABEL)
    Head Moulding = "None" (IFCLABEL)
    Head Moulding Bricks = FALSE (IFCBOOLEAN)
    Head Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding Position = "No Return" (IFCLABEL)
    Head Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Head Moulding Section Fill = "Background Fill" (IFCLABEL)
    Head Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Head Moulding Section Line Type = 1 (IFCINTEGER)
    Head Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Head Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding View Pen = "Openings - General" (IFCLABEL)
    Header Detail = "" (IFCLABEL)
    Heat Transfer Rate = "" (IFCLABEL)
    Hinges = "" (IFCLABEL)
    Hole Has Wall's Side Surface = FALSE (IFCBOOLEAN)
    Hole Surface's Split is Curved = FALSE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    IFC Operation (ifc_optype) = 12 (IFCINTEGER)
    IFC Operation (ifc_optypestr) = "Other" (IFCLABEL)
    Inner Frame Head and Sill Dimensions Differ = FALSE (IFCBOOLEAN)
    Inner Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame Section Fill = "Background Fill" (IFCLABEL)
    Inner Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame Section Line Type = 1 (IFCINTEGER)
    Inner Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Inner Frame View Background Pen = "Transparent" (IFCLABEL)
    Inner Frame View Fill = "Background Fill" (IFCLABEL)
    Inner Frame View Fill Pen = "Openings - General" (IFCLABEL)
    Inner Frame View Line Type = 1 (IFCINTEGER)
    Inner Frame View Pen = "Openings - General" (IFCLABEL)
    Interior Handle = "None" (IFCLABEL)
    Interior Handle Plate = "None" (IFCLABEL)
    Interior Handle Plate Position = 0 (IFCINTEGER)
    Inventory No. = "" (IFCLABEL)
    Jamb Detail = "" (IFCLABEL)
    Jamb Moulding = "X" (IFCLABEL)
    Jamb Moulding Bricks = FALSE (IFCBOOLEAN)
    Jamb Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Jamb Moulding Section Fill = "Background Fill" (IFCLABEL)
    Jamb Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Jamb Moulding Section Line Type = 1 (IFCINTEGER)
    Jamb Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Jamb Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding View Pen = "Walls - Outlines" (IFCLABEL)
    Kick Plate Surface = "Metal - Stainless Steel" (IFCLABEL)
    Kick Plate View Pen = "Openings - General" (IFCLABEL)
    Kick Plate to Exterior = FALSE (IFCBOOLEAN)
    Kick Plate to Interior = FALSE (IFCBOOLEAN)
    Layout Dimensions to Centres/ Panel Widths = 0 (IFCINTEGER)
    Layout Repeat Integer = 1 (IFCINTEGER)
    Layout Repeat Method = 1 (IFCINTEGER)
    Layout Repeating Integer = FALSE (IFCBOOLEAN)
    Layout Repeating Unit = FALSE (IFCBOOLEAN)
    LayoutSingle Unit = TRUE (IFCBOOLEAN)
    Leaf Edit Set = 1 (IFCINTEGER)
    Leaf Glazing Bars Surface = "Paint - Titanium White" (IFCLABEL)
    Leaf Panel View Pen = "Openings - General" (IFCLABEL)
    Leaf Pen (gs_leaf_pen) = "2D Elements - General" (IFCLABEL)
    Leaf Pen (gs_sash_pen) = "2D Elements - General" (IFCLABEL)
    Leaf Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Leaf Section Fill = "Air Space" (IFCLABEL)
    Leaf Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Leaf Section Line Type = 1 (IFCINTEGER)
    Leaf Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Leaf Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Leaf View Pen = "Openings - General" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lockset = "" (IFCLABEL)
    Louvre Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Louvres View Pen = "General - General" (IFCLABEL)
    Main Frame Flange = FALSE (IFCBOOLEAN)
    Manufacturer = "" (IFCLABEL)
    Mount Exterior = TRUE (IFCBOOLEAN)
    Mount Interior = FALSE (IFCBOOLEAN)
    Mullion/Transom Width Differs from Main Frame = FALSE (IFCBOOLEAN)
    Note/Remarks = "" (IFCLABEL)
    Number of Product Sizes = 1 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Opening Line Style = 0 (IFCINTEGER)
    Operation Type = "" (IFCLABEL)
    Panel edit menu = 0 (IFCINTEGER)
    Previous selection mode = 1 (IFCINTEGER)
    Production Year = "" (IFCLABEL)
    Rotate Window = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Rotate Window by 90 degrees = FALSE (IFCBOOLEAN)
    Sash Opening Direction Custom = TRUE (IFCBOOLEAN)
    Sash Surface = "Paint - Titanium White" (IFCLABEL)
    Selected Edge for Polygon Shape (uiBtmEdge) = 1 (IFCINTEGER)
    Selected Edge for Polygon Shape (uiTopEdge) = 1 (IFCINTEGER)
    Selected Size = 1 (IFCINTEGER)
    Selection mode = 2 (IFCINTEGER)
    Serial No. = "" (IFCLABEL)
    Shape Head = "Flat" (IFCLABEL)
    Shape Sill = "Flat" (IFCLABEL)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show the Menu = TRUE (IFCBOOLEAN)
    Sill Detail = "" (IFCLABEL)
    Snap Height First Listed = 0 (IFCINTEGER)
    Snap Height Number = 10 (IFCINTEGER)
    Snap Size Edit Values = 1 (IFCINTEGER)
    Snap Size Exclusion Number = 0 (IFCINTEGER)
    Snap Width First Listed = 0 (IFCINTEGER)
    Snap Width Number = 15 (IFCINTEGER)
    Symbol Pen = "Openings - General" (IFCLABEL)
    Timber Sill Type = 0 (IFCINTEGER)
    Total Glass Area = 0. (IFCREAL)
    Total Glass Perimeter = 5.869199999999999 (IFCREAL)
    Trims Pen = "2D Elements - General" (IFCLABEL)
    Trims Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Type ID (original field for presetCode) = "" (IFCLABEL)
    Use local settings = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    User Defined 6 = "" (IFCLABEL)
    User Defined 7 = "" (IFCLABEL)
    User Defined 8 = "" (IFCLABEL)
    User Defined 9 = "" (IFCLABEL)
    Version = 25 (IFCINTEGER)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Window belongs to the Zone into which it opens = TRUE (IFCBOOLEAN)
  AC_Pset_CI_Tools_Window | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    2D Symbol Frame Profile = 1 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Acoustic Rating = "" (IFCLABEL)
    Cavity Closure = "none" (IFCLABEL)
    Cavity Closure Exterior = "regular" (IFCLABEL)
    Cavity Closure Interior = "regular" (IFCLABEL)
    Cavity Closure Left = TRUE (IFCBOOLEAN)
    Cavity Closure Right = TRUE (IFCBOOLEAN)
    Cavity Closure Skins turn In = 0 (IFCINTEGER)
    Cavity Closure Skins turn Out = 0 (IFCINTEGER)
    Code (widoCode) = "-" (IFCLABEL)
    Code Format = "<C>-<H><W><M>" (IFCLABEL)
    Code Size Format = 1 (IFCINTEGER)
    Code for Configuration = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Current Page = 29 (IFCINTEGER)
    Door Leaf Number Left = 1 (IFCINTEGER)
    Door Leaf Number Right = 0 (IFCINTEGER)
    Door Type = "Standard" (IFCLABEL)
    Door UI Editing Set = 1 (IFCINTEGER)
    Doors and Windows Remain Open in Section/Elevation = FALSE (IFCBOOLEAN)
    Double Hung Sash Ratio = 0.4 (IFCREAL)
    Elevation = "" (IFCLABEL)
    Exterior Handle = "None" (IFCLABEL)
    Exterior Handle Plate = "None" (IFCLABEL)
    Exterior Handle Plate Position = 0 (IFCINTEGER)
    Exterior Reveal Link Dimensions = TRUE (IFCBOOLEAN)
    Exterior Trim = "None" (IFCLABEL)
    Exterior Trim Bricks = FALSE (IFCBOOLEAN)
    Exterior Trim Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Exterior Trim Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Exterior Trim Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Exterior Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim View Pen = "Openings - General" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Frame Mitre Left = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Mitre Right = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Pen = "2D Elements - General" (IFCLABEL)
    Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame Section Fill = "Background Fill" (IFCLABEL)
    Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame Section Line Type = 1 (IFCINTEGER)
    Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Frame Surface = "Paint - Titanium White" (IFCLABEL)
    Frame Type Head = "Frame" (IFCLABEL)
    Frame Type Left = "Frame" (IFCLABEL)
    Frame Type Right = "Frame" (IFCLABEL)
    Frame Type Sill = "Frame" (IFCLABEL)
    Frame View Background Pen = "Transparent" (IFCLABEL)
    Frame View Fill = "Background Fill" (IFCLABEL)
    Frame View Fill Pen = "Openings - General" (IFCLABEL)
    Frame View Line Type = 1 (IFCINTEGER)
    Frame View Pen = "Openings - General" (IFCLABEL)
    Glass Pane Number = 1 (IFCINTEGER)
    Glass Pen = "2D Elements - General" (IFCLABEL)
    Glass Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Glass Section Fill = "Air Space" (IFCLABEL)
    Glass Section Fill Pen = "General - General" (IFCLABEL)
    Glass Section Line Type = 1 (IFCINTEGER)
    Glass Section Pen = "General - General" (IFCLABEL)
    Glass Surface (gs_glass_mat) = "Glass - Clear Fast" (IFCLABEL)
    Glass View Pen = "General - General" (IFCLABEL)
    Glazing = "" (IFCLABEL)
    Glazing Bars Full Window = TRUE (IFCBOOLEAN)
    Glazing Bars View Pen = "General - General" (IFCLABEL)
    Group Type = "Others" (IFCLABEL)
    Handle Placement to Right Leaf = FALSE (IFCBOOLEAN)
    Handle Placement to Second Leaf = FALSE (IFCBOOLEAN)
    Handle View Pen = "Openings - General" (IFCLABEL)
    Hardware Pen = "2D Elements - General" (IFCLABEL)
    Hardware Set = "" (IFCLABEL)
    Hardware Surface = "Metal - Stainless Steel" (IFCLABEL)
    Head Moulding = "None" (IFCLABEL)
    Head Moulding Bricks = FALSE (IFCBOOLEAN)
    Head Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding Position = "No Return" (IFCLABEL)
    Head Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Head Moulding Section Fill = "Background Fill" (IFCLABEL)
    Head Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Head Moulding Section Line Type = 1 (IFCINTEGER)
    Head Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Head Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding View Pen = "Openings - General" (IFCLABEL)
    Header Detail = "" (IFCLABEL)
    Heat Transfer Rate = "" (IFCLABEL)
    Hinges = "" (IFCLABEL)
    Hole Has Wall's Side Surface = FALSE (IFCBOOLEAN)
    Hole Surface's Split is Curved = FALSE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    IFC Operation (ifc_optype) = 12 (IFCINTEGER)
    IFC Operation (ifc_optypestr) = "Other" (IFCLABEL)
    Inner Frame Head and Sill Dimensions Differ = FALSE (IFCBOOLEAN)
    Inner Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame Section Fill = "Background Fill" (IFCLABEL)
    Inner Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame Section Line Type = 1 (IFCINTEGER)
    Inner Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Inner Frame View Background Pen = "Transparent" (IFCLABEL)
    Inner Frame View Fill = "Background Fill" (IFCLABEL)
    Inner Frame View Fill Pen = "Openings - General" (IFCLABEL)
    Inner Frame View Line Type = 1 (IFCINTEGER)
    Inner Frame View Pen = "Openings - General" (IFCLABEL)
    Interior Handle = "None" (IFCLABEL)
    Interior Handle Plate = "None" (IFCLABEL)
    Interior Handle Plate Position = 0 (IFCINTEGER)
    Inventory No. = "" (IFCLABEL)
    Jamb Detail = "" (IFCLABEL)
    Jamb Moulding = "X" (IFCLABEL)
    Jamb Moulding Bricks = FALSE (IFCBOOLEAN)
    Jamb Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Jamb Moulding Section Fill = "Background Fill" (IFCLABEL)
    Jamb Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Jamb Moulding Section Line Type = 1 (IFCINTEGER)
    Jamb Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Jamb Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding View Pen = "Walls - Outlines" (IFCLABEL)
    Kick Plate Surface = "Metal - Stainless Steel" (IFCLABEL)
    Kick Plate View Pen = "Openings - General" (IFCLABEL)
    Kick Plate to Exterior = FALSE (IFCBOOLEAN)
    Kick Plate to Interior = FALSE (IFCBOOLEAN)
    Layout Dimensions to Centres/ Panel Widths = 0 (IFCINTEGER)
    Layout Repeat Integer = 1 (IFCINTEGER)
    Layout Repeat Method = 1 (IFCINTEGER)
    Layout Repeating Integer = FALSE (IFCBOOLEAN)
    Layout Repeating Unit = FALSE (IFCBOOLEAN)
    LayoutSingle Unit = TRUE (IFCBOOLEAN)
    Leaf Edit Set = 1 (IFCINTEGER)
    Leaf Glazing Bars Surface = "Paint - Titanium White" (IFCLABEL)
    Leaf Panel View Pen = "Openings - General" (IFCLABEL)
    Leaf Pen (gs_leaf_pen) = "2D Elements - General" (IFCLABEL)
    Leaf Pen (gs_sash_pen) = "2D Elements - General" (IFCLABEL)
    Leaf Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Leaf Section Fill = "Air Space" (IFCLABEL)
    Leaf Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Leaf Section Line Type = 1 (IFCINTEGER)
    Leaf Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Leaf Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Leaf View Pen = "Openings - General" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lockset = "" (IFCLABEL)
    Louvre Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Louvres View Pen = "General - General" (IFCLABEL)
    Main Frame Flange = FALSE (IFCBOOLEAN)
    Manufacturer = "" (IFCLABEL)
    Mount Exterior = TRUE (IFCBOOLEAN)
    Mount Interior = FALSE (IFCBOOLEAN)
    Mullion/Transom Width Differs from Main Frame = FALSE (IFCBOOLEAN)
    Note/Remarks = "" (IFCLABEL)
    Number of Product Sizes = 1 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Opening Line Style = 0 (IFCINTEGER)
    Operation Type = "" (IFCLABEL)
    Panel edit menu = 0 (IFCINTEGER)
    Previous selection mode = 1 (IFCINTEGER)
    Production Year = "" (IFCLABEL)
    Rotate Window = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Rotate Window by 90 degrees = FALSE (IFCBOOLEAN)
    Sash Opening Direction Custom = TRUE (IFCBOOLEAN)
    Sash Surface = "Paint - Titanium White" (IFCLABEL)
    Selected Edge for Polygon Shape (uiBtmEdge) = 1 (IFCINTEGER)
    Selected Edge for Polygon Shape (uiTopEdge) = 1 (IFCINTEGER)
    Selected Size = 1 (IFCINTEGER)
    Selection mode = 2 (IFCINTEGER)
    Serial No. = "" (IFCLABEL)
    Shape Head = "Flat" (IFCLABEL)
    Shape Sill = "Flat" (IFCLABEL)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show the Menu = TRUE (IFCBOOLEAN)
    Sill Detail = "" (IFCLABEL)
    Snap Height First Listed = 0 (IFCINTEGER)
    Snap Height Number = 10 (IFCINTEGER)
    Snap Size Edit Values = 1 (IFCINTEGER)
    Snap Size Exclusion Number = 0 (IFCINTEGER)
    Snap Width First Listed = 0 (IFCINTEGER)
    Snap Width Number = 15 (IFCINTEGER)
    Symbol Pen = "Openings - General" (IFCLABEL)
    Timber Sill Type = 0 (IFCINTEGER)
    Total Glass Area = 0. (IFCREAL)
    Total Glass Perimeter = 2.8296 (IFCREAL)
    Trims Pen = "2D Elements - General" (IFCLABEL)
    Trims Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Type ID (original field for presetCode) = "" (IFCLABEL)
    Use local settings = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    User Defined 6 = "" (IFCLABEL)
    User Defined 7 = "" (IFCLABEL)
    User Defined 8 = "" (IFCLABEL)
    User Defined 9 = "" (IFCLABEL)
    Version = 25 (IFCINTEGER)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Window belongs to the Zone into which it opens = TRUE (IFCBOOLEAN)
  AC_Pset_CI_Tools_Window | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    2D Symbol Frame Profile = 1 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Acoustic Rating = "" (IFCLABEL)
    Cavity Closure = "none" (IFCLABEL)
    Cavity Closure Exterior = "regular" (IFCLABEL)
    Cavity Closure Interior = "regular" (IFCLABEL)
    Cavity Closure Left = TRUE (IFCBOOLEAN)
    Cavity Closure Right = TRUE (IFCBOOLEAN)
    Cavity Closure Skins turn In = 0 (IFCINTEGER)
    Cavity Closure Skins turn Out = 0 (IFCINTEGER)
    Code (widoCode) = "-" (IFCLABEL)
    Code Format = "<C>-<H><W><M>" (IFCLABEL)
    Code Size Format = 1 (IFCINTEGER)
    Code for Configuration = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Current Page = 29 (IFCINTEGER)
    Door Leaf Number Left = 1 (IFCINTEGER)
    Door Leaf Number Right = 0 (IFCINTEGER)
    Door Type = "Standard" (IFCLABEL)
    Door UI Editing Set = 1 (IFCINTEGER)
    Doors and Windows Remain Open in Section/Elevation = FALSE (IFCBOOLEAN)
    Double Hung Sash Ratio = 0.4 (IFCREAL)
    Elevation = "" (IFCLABEL)
    Exterior Handle = "None" (IFCLABEL)
    Exterior Handle Plate = "None" (IFCLABEL)
    Exterior Handle Plate Position = 0 (IFCINTEGER)
    Exterior Reveal Link Dimensions = TRUE (IFCBOOLEAN)
    Exterior Trim = "None" (IFCLABEL)
    Exterior Trim Bricks = FALSE (IFCBOOLEAN)
    Exterior Trim Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Exterior Trim Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Exterior Trim Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Exterior Trim Surface = "Paint - Titanium White" (IFCLABEL)
    Exterior Trim View Pen = "Openings - General" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Fire Rating = "" (IFCLABEL)
    Frame Mitre Left = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Mitre Right = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Frame Pen = "2D Elements - General" (IFCLABEL)
    Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Frame Section Fill = "Background Fill" (IFCLABEL)
    Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Frame Section Line Type = 1 (IFCINTEGER)
    Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Frame Surface = "Paint - Titanium White" (IFCLABEL)
    Frame Type Head = "Frame" (IFCLABEL)
    Frame Type Left = "Frame" (IFCLABEL)
    Frame Type Right = "Frame" (IFCLABEL)
    Frame Type Sill = "Frame" (IFCLABEL)
    Frame View Background Pen = "Transparent" (IFCLABEL)
    Frame View Fill = "Background Fill" (IFCLABEL)
    Frame View Fill Pen = "Openings - General" (IFCLABEL)
    Frame View Line Type = 1 (IFCINTEGER)
    Frame View Pen = "Openings - General" (IFCLABEL)
    Glass Pane Number = 1 (IFCINTEGER)
    Glass Pen = "2D Elements - General" (IFCLABEL)
    Glass Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Glass Section Fill = "Air Space" (IFCLABEL)
    Glass Section Fill Pen = "General - General" (IFCLABEL)
    Glass Section Line Type = 1 (IFCINTEGER)
    Glass Section Pen = "General - General" (IFCLABEL)
    Glass Surface (gs_glass_mat) = "Glass - Clear Fast" (IFCLABEL)
    Glass View Pen = "General - General" (IFCLABEL)
    Glazing = "" (IFCLABEL)
    Glazing Bars Full Window = TRUE (IFCBOOLEAN)
    Glazing Bars View Pen = "General - General" (IFCLABEL)
    Group Type = "Others" (IFCLABEL)
    Handle Placement to Right Leaf = FALSE (IFCBOOLEAN)
    Handle Placement to Second Leaf = FALSE (IFCBOOLEAN)
    Handle View Pen = "Openings - General" (IFCLABEL)
    Hardware Pen = "2D Elements - General" (IFCLABEL)
    Hardware Set = "" (IFCLABEL)
    Hardware Surface = "Metal - Stainless Steel" (IFCLABEL)
    Head Moulding = "None" (IFCLABEL)
    Head Moulding Bricks = FALSE (IFCBOOLEAN)
    Head Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding Position = "No Return" (IFCLABEL)
    Head Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Head Moulding Section Fill = "Background Fill" (IFCLABEL)
    Head Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Head Moulding Section Line Type = 1 (IFCINTEGER)
    Head Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Head Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Head Moulding View Pen = "Openings - General" (IFCLABEL)
    Header Detail = "" (IFCLABEL)
    Heat Transfer Rate = "" (IFCLABEL)
    Hinges = "" (IFCLABEL)
    Hole Has Wall's Side Surface = FALSE (IFCBOOLEAN)
    Hole Surface's Split is Curved = FALSE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    IFC Operation (ifc_optype) = 12 (IFCINTEGER)
    IFC Operation (ifc_optypestr) = "Other" (IFCLABEL)
    Inner Frame Head and Sill Dimensions Differ = FALSE (IFCBOOLEAN)
    Inner Frame Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Inner Frame Section Fill = "Background Fill" (IFCLABEL)
    Inner Frame Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Inner Frame Section Line Type = 1 (IFCINTEGER)
    Inner Frame Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Inner Frame View Background Pen = "Transparent" (IFCLABEL)
    Inner Frame View Fill = "Background Fill" (IFCLABEL)
    Inner Frame View Fill Pen = "Openings - General" (IFCLABEL)
    Inner Frame View Line Type = 1 (IFCINTEGER)
    Inner Frame View Pen = "Openings - General" (IFCLABEL)
    Interior Handle = "None" (IFCLABEL)
    Interior Handle Plate = "None" (IFCLABEL)
    Interior Handle Plate Position = 0 (IFCINTEGER)
    Inventory No. = "" (IFCLABEL)
    Jamb Detail = "" (IFCLABEL)
    Jamb Moulding = "X" (IFCLABEL)
    Jamb Moulding Bricks = FALSE (IFCBOOLEAN)
    Jamb Moulding Mortar Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Jamb Moulding Section Fill = "Background Fill" (IFCLABEL)
    Jamb Moulding Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Jamb Moulding Section Line Type = 1 (IFCINTEGER)
    Jamb Moulding Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Jamb Moulding Surface = "Paint - Titanium White" (IFCLABEL)
    Jamb Moulding View Pen = "Walls - Outlines" (IFCLABEL)
    Kick Plate Surface = "Metal - Stainless Steel" (IFCLABEL)
    Kick Plate View Pen = "Openings - General" (IFCLABEL)
    Kick Plate to Exterior = FALSE (IFCBOOLEAN)
    Kick Plate to Interior = FALSE (IFCBOOLEAN)
    Layout Dimensions to Centres/ Panel Widths = 0 (IFCINTEGER)
    Layout Repeat Integer = 1 (IFCINTEGER)
    Layout Repeat Method = 1 (IFCINTEGER)
    Layout Repeating Integer = FALSE (IFCBOOLEAN)
    Layout Repeating Unit = FALSE (IFCBOOLEAN)
    LayoutSingle Unit = TRUE (IFCBOOLEAN)
    Leaf Edit Set = 1 (IFCINTEGER)
    Leaf Glazing Bars Surface = "Paint - Titanium White" (IFCLABEL)
    Leaf Panel View Pen = "Openings - General" (IFCLABEL)
    Leaf Pen (gs_leaf_pen) = "2D Elements - General" (IFCLABEL)
    Leaf Pen (gs_sash_pen) = "2D Elements - General" (IFCLABEL)
    Leaf Section Background Pen = "Openings- Fill backgrounds" (IFCLABEL)
    Leaf Section Fill = "Air Space" (IFCLABEL)
    Leaf Section Fill Pen = "Openings- Cut Fills" (IFCLABEL)
    Leaf Section Line Type = 1 (IFCINTEGER)
    Leaf Section Pen = "Openings- Cut Non-Structural" (IFCLABEL)
    Leaf Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Leaf View Pen = "Openings - General" (IFCLABEL)
    Location = "" (IFCLABEL)
    Lockset = "" (IFCLABEL)
    Louvre Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Louvres View Pen = "General - General" (IFCLABEL)
    Main Frame Flange = FALSE (IFCBOOLEAN)
    Manufacturer = "" (IFCLABEL)
    Mount Exterior = TRUE (IFCBOOLEAN)
    Mount Interior = FALSE (IFCBOOLEAN)
    Mullion/Transom Width Differs from Main Frame = FALSE (IFCBOOLEAN)
    Note/Remarks = "" (IFCLABEL)
    Number of Product Sizes = 1 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Opening Line Style = 0 (IFCINTEGER)
    Operation Type = "" (IFCLABEL)
    Panel edit menu = 0 (IFCINTEGER)
    Previous selection mode = 1 (IFCINTEGER)
    Production Year = "" (IFCLABEL)
    Rotate Window = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Rotate Window by 90 degrees = FALSE (IFCBOOLEAN)
    Sash Opening Direction Custom = TRUE (IFCBOOLEAN)
    Sash Surface = "Paint - Titanium White" (IFCLABEL)
    Selected Edge for Polygon Shape (uiBtmEdge) = 1 (IFCINTEGER)
    Selected Edge for Polygon Shape (uiTopEdge) = 1 (IFCINTEGER)
    Selected Size = 1 (IFCINTEGER)
    Selection mode = 2 (IFCINTEGER)
    Serial No. = "" (IFCLABEL)
    Shape Head = "Flat" (IFCLABEL)
    Shape Sill = "Flat" (IFCLABEL)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show the Menu = TRUE (IFCBOOLEAN)
    Sill Detail = "" (IFCLABEL)
    Snap Height First Listed = 0 (IFCINTEGER)
    Snap Height Number = 10 (IFCINTEGER)
    Snap Size Edit Values = 1 (IFCINTEGER)
    Snap Size Exclusion Number = 0 (IFCINTEGER)
    Snap Width First Listed = 0 (IFCINTEGER)
    Snap Width Number = 15 (IFCINTEGER)
    Symbol Pen = "Openings - General" (IFCLABEL)
    Timber Sill Type = 0 (IFCINTEGER)
    Total Glass Area = 0. (IFCREAL)
    Total Glass Perimeter = 8.1892 (IFCREAL)
    Trims Pen = "2D Elements - General" (IFCLABEL)
    Trims Surface = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Type ID (original field for presetCode) = "" (IFCLABEL)
    Use local settings = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    User Defined 6 = "" (IFCLABEL)
    User Defined 7 = "" (IFCLABEL)
    User Defined 8 = "" (IFCLABEL)
    User Defined 9 = "" (IFCLABEL)
    Version = 25 (IFCINTEGER)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Window belongs to the Zone into which it opens = TRUE (IFCBOOLEAN)
  AC_Equantity_CI_Tools_Window | quantities | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Camera proximity when fully open = 0. [MILLI METRE]
    Camera proximity when fully shut = 0. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset = 10. [MILLI METRE]
    Door Stop Thickness = 15. [MILLI METRE]
    Exterior Handle Length = 200. [MILLI METRE]
    Exterior Handle Plate Length = 250. [MILLI METRE]
    Exterior Handle Plate Thickness = 0. [MILLI METRE]
    Exterior Handle Plate Width = 80. [MILLI METRE]
    Exterior Handle Projection = 50. [MILLI METRE]
    Exterior Handle Thickness = 20. [MILLI METRE]
    Exterior Handle Width = 20. [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 18. [MILLI METRE]
    Exterior Trim Width = 80. [MILLI METRE]
    Fixed Glass Position = 5. [MILLI METRE]
    Frame Thickness = 50. [MILLI METRE]
    Frame Width = 70. [MILLI METRE]
    Frame extension (extendFrameL) = 0. [MILLI METRE]
    Frame extension (extendFrameR) = 0. [MILLI METRE]
    Framed Glass Position = 0. [MILLI METRE]
    Glass Pane Spacing = 19. [MILLI METRE]
    Glass Pane Thickness = 17. [MILLI METRE]
    Glass Thickness = 20. [MILLI METRE]
    Glazing Panel Width Default = 0. [MILLI METRE]
    Glazing Sill Height above Opening Base = 0. [MILLI METRE]
    Head Moulding Brick Width = 100. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 40. [MILLI METRE]
    Head Moulding Width = 80. [MILLI METRE]
    Inner Frame Backset = 50. [MILLI METRE]
    Inner Frame Depth = 35. [MILLI METRE]
    Inner Frame Head Width = 60. [MILLI METRE]
    Inner Frame Sill Width = 100. [MILLI METRE]
    Inner Frame Width = 40. [MILLI METRE]
    Interior Handle Length = 200. [MILLI METRE]
    Interior Handle Plate Length = 250. [MILLI METRE]
    Interior Handle Plate Thickness = 0. [MILLI METRE]
    Interior Handle Plate Width = 80. [MILLI METRE]
    Interior Handle Projection = 50. [MILLI METRE]
    Interior Handle Thickness = 20. [MILLI METRE]
    Interior Handle Width = 20. [MILLI METRE]
    Interior Reveal = 18. [MILLI METRE]
    Interior Sill Extension = 20. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 20. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 15. [MILLI METRE]
    Interior Trim Width = 50. [MILLI METRE]
    Jamb Liner Projection beyond Wall Face = 0. [MILLI METRE]
    Jamb Moulding Brick Width = 100. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Layout Repeat Length = 1200. [MILLI METRE]
    Louvre Width = 100. [MILLI METRE]
    Main Frame Backset from Wall Exterior = 0. [MILLI METRE]
    Main Frame Backset from Wall Interior = 0. [MILLI METRE]
    Main Frame Depth (FD) = 90. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 90. [MILLI METRE]
    Main Frame Flange Thickness = 5. [MILLI METRE]
    Main Frame Flange Width = 0. [MILLI METRE]
    Main Frame Width = 40. [MILLI METRE]
    Mullion Width = 35. [MILLI METRE]
    Mullion/Transom Depth = 10. [MILLI METRE]
    Offset point at the end of the opening = 0. [MILLI METRE]
    Opening Oversize Bottom = 5. [MILLI METRE]
    Opening Oversize Left = 5. [MILLI METRE]
    Opening Oversize Right = 5. [MILLI METRE]
    Opening Oversize Top = 5. [MILLI METRE]
    Pivot Lines Dash Length = 50. [MILLI METRE]
    Pivot Offset = 0. [MILLI METRE]
    Reveal Height = 1200. [MILLI METRE]
    Reveal Width = 1135. [MILLI METRE]
    Sash Frame Thickness = 50. [MILLI METRE]
    Sash Frame Width = 50. [MILLI METRE]
    Sash Height Bottom = 0. [MILLI METRE]
    Sash Height Lower = 390. [MILLI METRE]
    Sash Height Top = 0. [MILLI METRE]
    Sash Height Upper = 400. [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 600. [MILLI METRE]
    Shape Sill Height Left = 0. [MILLI METRE]
    Shape Sill Height Right = 0. [MILLI METRE]
    Shape Sill Inset Left = 0. [MILLI METRE]
    Shape Sill Inset Right = 0. [MILLI METRE]
    Shape Sill Mid Height = 0. [MILLI METRE]
    Shape Sill Midpoint = 600. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 10. [MILLI METRE]
    Shutter Position Offset = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extension Left = 50. [MILLI METRE]
    Sill Extension Right = 50. [MILLI METRE]
    Sill Height = 999.9999999999886 [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 50. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 35. [MILLI METRE]
    Unit Height = 1200. [MILLI METRE]
    Unit Width = 1135. [MILLI METRE]
    Ventillation Unit Thickness = 50. [MILLI METRE]
    Ventillation Unit Width = 200. [MILLI METRE]
    Wall Hole Height = 1220. [MILLI METRE]
    Wall Hole Width = 1155. [MILLI METRE]
    X Dimension = 1135. [MILLI METRE]
    Y Dimension = 1200. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_CI_Tools_Window | quantities | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Camera proximity when fully open = 0. [MILLI METRE]
    Camera proximity when fully shut = 0. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset = 10. [MILLI METRE]
    Door Stop Thickness = 15. [MILLI METRE]
    Exterior Handle Length = 200. [MILLI METRE]
    Exterior Handle Plate Length = 250. [MILLI METRE]
    Exterior Handle Plate Thickness = 0. [MILLI METRE]
    Exterior Handle Plate Width = 80. [MILLI METRE]
    Exterior Handle Projection = 50. [MILLI METRE]
    Exterior Handle Thickness = 20. [MILLI METRE]
    Exterior Handle Width = 20. [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 18. [MILLI METRE]
    Exterior Trim Width = 80. [MILLI METRE]
    Fixed Glass Position = 5. [MILLI METRE]
    Frame Thickness = 50. [MILLI METRE]
    Frame Width = 70. [MILLI METRE]
    Frame extension (extendFrameL) = 0. [MILLI METRE]
    Frame extension (extendFrameR) = 0. [MILLI METRE]
    Framed Glass Position = 0. [MILLI METRE]
    Glass Pane Spacing = 19. [MILLI METRE]
    Glass Pane Thickness = 17. [MILLI METRE]
    Glass Thickness = 20. [MILLI METRE]
    Glazing Panel Width Default = 0. [MILLI METRE]
    Glazing Sill Height above Opening Base = 0. [MILLI METRE]
    Head Moulding Brick Width = 100. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 40. [MILLI METRE]
    Head Moulding Width = 80. [MILLI METRE]
    Inner Frame Backset = 50. [MILLI METRE]
    Inner Frame Depth = 35. [MILLI METRE]
    Inner Frame Head Width = 60. [MILLI METRE]
    Inner Frame Sill Width = 100. [MILLI METRE]
    Inner Frame Width = 40. [MILLI METRE]
    Interior Handle Length = 200. [MILLI METRE]
    Interior Handle Plate Length = 250. [MILLI METRE]
    Interior Handle Plate Thickness = 0. [MILLI METRE]
    Interior Handle Plate Width = 80. [MILLI METRE]
    Interior Handle Projection = 50. [MILLI METRE]
    Interior Handle Thickness = 20. [MILLI METRE]
    Interior Handle Width = 20. [MILLI METRE]
    Interior Reveal = 18. [MILLI METRE]
    Interior Sill Extension = 20. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 20. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 15. [MILLI METRE]
    Interior Trim Width = 50. [MILLI METRE]
    Jamb Liner Projection beyond Wall Face = 0. [MILLI METRE]
    Jamb Moulding Brick Width = 100. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Layout Repeat Length = 1200. [MILLI METRE]
    Louvre Width = 100. [MILLI METRE]
    Main Frame Backset from Wall Exterior = 0. [MILLI METRE]
    Main Frame Backset from Wall Interior = 0. [MILLI METRE]
    Main Frame Depth (FD) = 90. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 90. [MILLI METRE]
    Main Frame Flange Thickness = 5. [MILLI METRE]
    Main Frame Flange Width = 0. [MILLI METRE]
    Main Frame Width = 40. [MILLI METRE]
    Mullion Width = 35. [MILLI METRE]
    Mullion/Transom Depth = 10. [MILLI METRE]
    Offset point at the end of the opening = 0. [MILLI METRE]
    Opening Oversize Bottom = 5. [MILLI METRE]
    Opening Oversize Left = 5. [MILLI METRE]
    Opening Oversize Right = 5. [MILLI METRE]
    Opening Oversize Top = 5. [MILLI METRE]
    Pivot Lines Dash Length = 50. [MILLI METRE]
    Pivot Offset = 0. [MILLI METRE]
    Reveal Height = 1200. [MILLI METRE]
    Reveal Width = 535. [MILLI METRE]
    Sash Frame Thickness = 50. [MILLI METRE]
    Sash Frame Width = 50. [MILLI METRE]
    Sash Height Bottom = 0. [MILLI METRE]
    Sash Height Lower = 390. [MILLI METRE]
    Sash Height Top = 0. [MILLI METRE]
    Sash Height Upper = 400. [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 600. [MILLI METRE]
    Shape Sill Height Left = 0. [MILLI METRE]
    Shape Sill Height Right = 0. [MILLI METRE]
    Shape Sill Inset Left = 0. [MILLI METRE]
    Shape Sill Inset Right = 0. [MILLI METRE]
    Shape Sill Mid Height = 0. [MILLI METRE]
    Shape Sill Midpoint = 600. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 10. [MILLI METRE]
    Shutter Position Offset = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extension Left = 50. [MILLI METRE]
    Sill Extension Right = 50. [MILLI METRE]
    Sill Height = 999.9999999999886 [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 50. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 35. [MILLI METRE]
    Unit Height = 1200. [MILLI METRE]
    Unit Width = 535. [MILLI METRE]
    Ventillation Unit Thickness = 50. [MILLI METRE]
    Ventillation Unit Width = 200. [MILLI METRE]
    Wall Hole Height = 1220. [MILLI METRE]
    Wall Hole Width = 555. [MILLI METRE]
    X Dimension = 535. [MILLI METRE]
    Y Dimension = 1200. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_CI_Tools_Window | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    2D Symbol Frame Thickness = 3. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Brick Mortar Gap = 10. [MILLI METRE]
    Camera proximity when fully open = 0. [MILLI METRE]
    Camera proximity when fully shut = 0. [MILLI METRE]
    Composite Skins Extend Exterior = 0. [MILLI METRE]
    Composite Skins Extend Interior = 0. [MILLI METRE]
    Composite Skins Origin Exterior = 0. [MILLI METRE]
    Composite Skins Origin Interior = 0. [MILLI METRE]
    Door Leaf Inset = 10. [MILLI METRE]
    Door Stop Thickness = 15. [MILLI METRE]
    Exterior Handle Length = 200. [MILLI METRE]
    Exterior Handle Plate Length = 250. [MILLI METRE]
    Exterior Handle Plate Thickness = 0. [MILLI METRE]
    Exterior Handle Plate Width = 80. [MILLI METRE]
    Exterior Handle Projection = 50. [MILLI METRE]
    Exterior Handle Thickness = 20. [MILLI METRE]
    Exterior Handle Width = 20. [MILLI METRE]
    Exterior Reveal Head Depth = 0. [MILLI METRE]
    Exterior Reveal Left Jamb = 0. [MILLI METRE]
    Exterior Reveal Right Jamb = 0. [MILLI METRE]
    Exterior Reveal Threshold Depth = 0. [MILLI METRE]
    Exterior Trim Brick Width = 0. [MILLI METRE]
    Exterior Trim Offset = 0. [MILLI METRE]
    Exterior Trim Thickness = 18. [MILLI METRE]
    Exterior Trim Width = 80. [MILLI METRE]
    Fixed Glass Position = 5. [MILLI METRE]
    Frame Thickness = 50. [MILLI METRE]
    Frame Width = 70. [MILLI METRE]
    Frame extension (extendFrameL) = 0. [MILLI METRE]
    Frame extension (extendFrameR) = 0. [MILLI METRE]
    Framed Glass Position = 0. [MILLI METRE]
    Glass Pane Spacing = 19. [MILLI METRE]
    Glass Pane Thickness = 17. [MILLI METRE]
    Glass Thickness = 20. [MILLI METRE]
    Glazing Panel Width Default = 0. [MILLI METRE]
    Glazing Sill Height above Opening Base = 0. [MILLI METRE]
    Head Moulding Brick Width = 100. [MILLI METRE]
    Head Moulding Extension = 0. [MILLI METRE]
    Head Moulding Thickness = 40. [MILLI METRE]
    Head Moulding Width = 80. [MILLI METRE]
    Inner Frame Backset = 50. [MILLI METRE]
    Inner Frame Depth = 35. [MILLI METRE]
    Inner Frame Head Width = 60. [MILLI METRE]
    Inner Frame Sill Width = 100. [MILLI METRE]
    Inner Frame Width = 40. [MILLI METRE]
    Interior Handle Length = 200. [MILLI METRE]
    Interior Handle Plate Length = 250. [MILLI METRE]
    Interior Handle Plate Thickness = 0. [MILLI METRE]
    Interior Handle Plate Width = 80. [MILLI METRE]
    Interior Handle Projection = 50. [MILLI METRE]
    Interior Handle Thickness = 20. [MILLI METRE]
    Interior Handle Width = 20. [MILLI METRE]
    Interior Reveal = 18. [MILLI METRE]
    Interior Sill Extension = 20. [MILLI METRE]
    Interior Sill Thickness = 16. [MILLI METRE]
    Interior Sill Width = 20. [MILLI METRE]
    Interior Trim Offset = 0. [MILLI METRE]
    Interior Trim Thickness = 15. [MILLI METRE]
    Interior Trim Width = 50. [MILLI METRE]
    Jamb Liner Projection beyond Wall Face = 0. [MILLI METRE]
    Jamb Moulding Brick Width = 100. [MILLI METRE]
    Jamb Moulding Thickness = 20. [MILLI METRE]
    Jamb Moulding Width = 50. [MILLI METRE]
    Kick Plate Height = 152.4 [MILLI METRE]
    Kick Plate Inset = 3.175 [MILLI METRE]
    Kick Plate Thickness = 3.175 [MILLI METRE]
    Layout Repeat Length = 1200. [MILLI METRE]
    Louvre Width = 100. [MILLI METRE]
    Main Frame Backset from Wall Exterior = 0. [MILLI METRE]
    Main Frame Backset from Wall Interior = 0. [MILLI METRE]
    Main Frame Depth (FD) = 90. [MILLI METRE]
    Main Frame Depth (FD_wkg) = 90. [MILLI METRE]
    Main Frame Flange Thickness = 5. [MILLI METRE]
    Main Frame Flange Width = 0. [MILLI METRE]
    Main Frame Width = 40. [MILLI METRE]
    Mullion Width = 35. [MILLI METRE]
    Mullion/Transom Depth = 10. [MILLI METRE]
    Offset point at the end of the opening = 0. [MILLI METRE]
    Opening Oversize Bottom = 5. [MILLI METRE]
    Opening Oversize Left = 5. [MILLI METRE]
    Opening Oversize Right = 5. [MILLI METRE]
    Opening Oversize Top = 5. [MILLI METRE]
    Pivot Lines Dash Length = 50. [MILLI METRE]
    Pivot Offset = 0. [MILLI METRE]
    Reveal Height = 1400. [MILLI METRE]
    Reveal Width = 1735. [MILLI METRE]
    Sash Frame Thickness = 50. [MILLI METRE]
    Sash Frame Width = 50. [MILLI METRE]
    Sash Height Bottom = 0. [MILLI METRE]
    Sash Height Lower = 390. [MILLI METRE]
    Sash Height Top = 0. [MILLI METRE]
    Sash Height Upper = 400. [MILLI METRE]
    Shape Head Height Left = 0. [MILLI METRE]
    Shape Head Height Right = 0. [MILLI METRE]
    Shape Head Inset Left = 0. [MILLI METRE]
    Shape Head Inset Right = 0. [MILLI METRE]
    Shape Head Mid Height = 0. [MILLI METRE]
    Shape Head Midpoint = 600. [MILLI METRE]
    Shape Sill Height Left = 0. [MILLI METRE]
    Shape Sill Height Right = 0. [MILLI METRE]
    Shape Sill Inset Left = 0. [MILLI METRE]
    Shape Sill Inset Right = 0. [MILLI METRE]
    Shape Sill Mid Height = 0. [MILLI METRE]
    Shape Sill Midpoint = 600. [MILLI METRE]
    Shim Space Head = 10. [MILLI METRE]
    Shim Space Left = 10. [MILLI METRE]
    Shim Space Right = 10. [MILLI METRE]
    Shim Space Sill = 10. [MILLI METRE]
    Shutter Position Offset = 0. [MILLI METRE]
    Sill Brick Width = 80. [MILLI METRE]
    Sill Extension Left = 50. [MILLI METRE]
    Sill Extension Right = 50. [MILLI METRE]
    Sill Height = 799.9999999999887 [MILLI METRE]
    Sill Thickness = 35. [MILLI METRE]
    Sill Width = 50. [MILLI METRE]
    Timber Sill Margin = 10. [MILLI METRE]
    Timber Sill Width = 30. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Width = 35. [MILLI METRE]
    Unit Height = 1400. [MILLI METRE]
    Unit Width = 1735. [MILLI METRE]
    Ventillation Unit Thickness = 50. [MILLI METRE]
    Ventillation Unit Width = 200. [MILLI METRE]
    Wall Hole Height = 1420. [MILLI METRE]
    Wall Hole Width = 1755. [MILLI METRE]
    X Dimension = 1735. [MILLI METRE]
    Y Dimension = 1400. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_Cabinet_Base_Corner_S_24 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Back Splash Height (0-None) = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Cabinet Depth = 599.9999999999999 [MILLI METRE]
    Cabinet Width = 699.9999999999984 [MILLI METRE]
    Con. Cab. Depth/Left = 50. [MILLI METRE]
    Con. Cab. Depth/Right = 599.8253517848973 [MILLI METRE]
    Counter Thickness = 50. [MILLI METRE]
    Countertop Height = 900. [MILLI METRE]
    Custom Knob Depth = 20. [MILLI METRE]
    Custom Knob Height = 15. [MILLI METRE]
    Custom Knob Length = 100. [MILLI METRE]
    Door Frame Width (doorframe_w) = 90. [MILLI METRE]
    Door Frame Width (doorframe_w_end) = 90. [MILLI METRE]
    Door Thickness = 20. [MILLI METRE]
    Drawer Height = 130. [MILLI METRE]
    Knob Horizontal Position = 50. [MILLI METRE]
    Knob Size = 100. [MILLI METRE]
    Knob Vertical Position = 550. [MILLI METRE]
    Left End Panel Thickness = 20. [MILLI METRE]
    Minimal Space in Front = 900. [MILLI METRE]
    Overhang to Front of Cabinet = 0. [MILLI METRE]
    Overhang to Left of Cabinet (left_cab) = 0. [MILLI METRE]
    Overhang to Left of Cabinet (left_cab_mirror) = 0. [MILLI METRE]
    Overhang to Left-Rear of Cab. (lrear_cab) = 0. [MILLI METRE]
    Overhang to Left-Rear of Cab. (lrear_cab_mirror) = 0. [MILLI METRE]
    Overhang to Right of Cabinet (right_cab) = 0. [MILLI METRE]
    Overhang to Right of Cabinet (right_cab_mirror) = 0. [MILLI METRE]
    Overhang to Right-Rear of Cab. (rrear_cab) = 0. [MILLI METRE]
    Overhang to Right-Rear of Cab. (rrear_cab_mirror) = 0. [MILLI METRE]
    Rear End Panel Thickness = 20. [MILLI METRE]
    Rear Minimal Space = 900. [MILLI METRE]
    Right End Panel Thickness = 20. [MILLI METRE]
    Toe Height = 90. [MILLI METRE]
    Toe Setback (0-None) = 20. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Pset_Cabinet_Base_Corner_S_24 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    'A' 'B' Size= (cab_size) = FALSE (IFCBOOLEAN)
    'A' 'B' Size= (cab_size_) = "Counter" (IFCLABEL)
    2D Hidden Edges = 0 (IFCINTEGER)
    2D Symbol Type = "Type 1" (IFCLABEL)
    3D Detail Level = 3 (IFCINTEGER)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Base Height = "" (IFCLABEL)
    Additional Description = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Additional Manufacturer = "" (IFCLABEL)
    Additional Number = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Assembly Date = "" (IFCLABEL)
    Backsplash = "Plastic - Laminate" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Cabinet (gs_cabinet_mat) = "Paint - Glossy White" (IFCLABEL)
    Collection of Specifications ID = "" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Counter (bCounter) = TRUE (IFCBOOLEAN)
    Counter (count_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Counter Edge Visibility in 3D (side_vis) = "None" (IFCLABEL)
    Counter Edge Visibility in 3D (side_vis_mirror) = "None" (IFCLABEL)
    Counter Type (gs_count_type) = "Rectangular" (IFCLABEL)
    Counter Type (gs_count_type_m) = 1 (IFCINTEGER)
    Custom Knob Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_p) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_p_end) = "" (IFCLABEL)
    Door (Frame) = "Paint - Titanium White" (IFCLABEL)
    Door (Glazing) = "Glass - Clear Fast" (IFCLABEL)
    Door (bDoor) = TRUE (IFCBOOLEAN)
    Door (gs_door_type) = "Style 1" (IFCLABEL)
    Door Opening Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Door Style = 1 (IFCINTEGER)
    Double Faced = FALSE (IFCBOOLEAN)
    Drawer (DrawerMat) = "Paint - Titanium White" (IFCLABEL)
    Drawer (bDrawer) = TRUE (IFCBOOLEAN)
    Edge Bevel = FALSE (IFCBOOLEAN)
    Edge Visibility in 2D (side_vis2D) = "None" (IFCLABEL)
    Edge Visibility in 2D (side_vis2D_mirror) = "Left" (IFCLABEL)
    Edge Visibility in 2D (side_vis2d_m) = 2 (IFCINTEGER)
    End Panel = "Wood - Pine Grained Horizontal" (IFCLABEL)
    End Panel Type = "Style 1" (IFCLABEL)
    Extra Hotspot Editing = TRUE (IFCBOOLEAN)
    Fill Background Pen = "Window Background" (IFCLABEL)
    Fill Pen = "Window Background" (IFCLABEL)
    Fill Type = "Background Fill (2)" (IFCLABEL)
    Group Type (FM_Type) = "Furniture" (IFCLABEL)
    Group Type (iFMType) = 16 (IFCINTEGER)
    Hidden Edges Contour = "Objects - General" (IFCLABEL)
    Hidden Edges Line Type = 4 (IFCINTEGER)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Knob (bKnob) = TRUE (IFCBOOLEAN)
    Knob (gs_knob_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Knob (gs_knob_type) = "Style 4" (IFCLABEL)
    Knob Style = 4 (IFCINTEGER)
    Left End Panel (left_panel) = FALSE (IFCBOOLEAN)
    Left End Panel (left_panel_mirror) = FALSE (IFCBOOLEAN)
    Left End Panel is in Cabinet Size = TRUE (IFCBOOLEAN)
    Left-Rear End Panel (lrear_panel) = FALSE (IFCBOOLEAN)
    Left-Rear End Panel (lrear_panel_mirror) = FALSE (IFCBOOLEAN)
    Left-Rear End Panel is in Cabinet Size = TRUE (IFCBOOLEAN)
    Leg and Panel Relative Situation = 0 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    No. of Hor. Door Grids = 2 (IFCINTEGER)
    No. of Shelves = 1 (IFCINTEGER)
    No. of Vert. Door Grids = 1 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Placing = 0 (IFCINTEGER)
    Product Name = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Resolution = 16 (IFCINTEGER)
    Right End Panel (right_panel) = FALSE (IFCBOOLEAN)
    Right End Panel (right_panel_mirror) = FALSE (IFCBOOLEAN)
    Right End Panel is in Cabinet Size = TRUE (IFCBOOLEAN)
    Right-Rear End Panel (rrear_panel) = FALSE (IFCBOOLEAN)
    Right-Rear End Panel (rrear_panel_mirror) = FALSE (IFCBOOLEAN)
    Right-Rear End Panel is in Cabinet Size = TRUE (IFCBOOLEAN)
    Same Drawer Front as Door = TRUE (IFCBOOLEAN)
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Shelf = "Paint - Glossy White" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Sides Visible = 0 (IFCINTEGER)
    To Zone Number = "" (IFCLABEL)
    Toe (bToeOn) = TRUE (IFCBOOLEAN)
    Toe (toe_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Toe Type (gs_toe_type) = "Full" (IFCLABEL)
    Toe Type (gs_toe_type_m) = 1 (IFCINTEGER)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Width/Depth/Height = "" (IFCLABEL)
  AC_Pset_Bed_01_26 | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 6 (IFCINTEGER)
    2D Symbol Type (iSymbolType) = 1 (IFCINTEGER)
    2D Symbol Type (styp) = "Type 1" (IFCLABEL)
    3D Detail Level = 4 (IFCINTEGER)
    Accessories (gs_list_accessories) = "" (IFCLABEL)
    Bed Frame (frmat) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Bed Frame (gs_frame_mat) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Fill Background Pen Bed = "Backgrounds - color 1" (IFCLABEL)
    Fill Background Pen Blanket = "Backgrounds - color 1" (IFCLABEL)
    Fill Background Pen Pillow = "Backgrounds - color 1" (IFCLABEL)
    Fill Background Pen Uniform = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Bed = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Blanket = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Pillow = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Uniform = "Backgrounds - color 1" (IFCLABEL)
    Fill Type Bed = "Background Fill" (IFCLABEL)
    Fill Type Blanket = "Background Fill" (IFCLABEL)
    Fill Type Pillow = "Background Fill" (IFCLABEL)
    Fill Type Uniform = "Background Fill" (IFCLABEL)
    Fill for (fillFor) = "Bed" (IFCLABEL)
    Fill for (iFillFor) = 1 (IFCINTEGER)
    Frame Type = 1 (IFCINTEGER)
    Group Type (FM_Type) = "Furniture" (IFCLABEL)
    Group Type (iFMType) = 16 (IFCINTEGER)
    Headboard (bHeadboard) = TRUE (IFCBOOLEAN)
    Headboard (hb) = "On Rear Side" (IFCLABEL)
    Headboard (hbmat) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Headboard (iHeadboard) = 3 (IFCINTEGER)
    Headboard Edge = FALSE (IFCBOOLEAN)
    Headboard Style (hboard_type) = "Style 1" (IFCLABEL)
    Headboard Style (hboard_type_m) = 1 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Leg = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Leg Style (iBedLegType) = 1 (IFCINTEGER)
    Leg Style (stBedLegType) = "Style 1" (IFCLABEL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Mattress (gs_matrace_mat) = "Paint - Sand Beige" (IFCLABEL)
    Mattress (mmat) = "Paint - Titanium White" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Pillow (pillow_mat) = "Paint - Titanium White" (IFCLABEL)
    Pillow (pw) = FALSE (IFCBOOLEAN)
    Production Year = "" (IFCLABEL)
    Resolution = 8 (IFCINTEGER)
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Support Type (iBedType) = 1 (IFCINTEGER)
    Support Type (stBedType) = "Frame" (IFCLABEL)
    Uniform Fill Settings = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Equantity_Bed_01_26 | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Bed Frame Height (frh) = 320. [MILLI METRE]
    Bed Frame Height (frhLeg) = 160. [MILLI METRE]
    Bed Height = 400. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 900. [MILLI METRE]
    Dimension 2 = 2000. [MILLI METRE]
    Edge Radius of Mattress = 20. [MILLI METRE]
    Fillet Radius of Mattress = 20. [MILLI METRE]
    Frontal Headboard Height = 340. [MILLI METRE]
    Height = 660. [MILLI METRE]
    Leg Height = 160. [MILLI METRE]
    Leg Width/Diameter = 50. [MILLI METRE]
    Mattress Distance from Edge = 20. [MILLI METRE]
    Mattress Height = 120. [MILLI METRE]
    Minimal Space Length 1 = 1200. [MILLI METRE]
    Minimal Space Length 2 = 300. [MILLI METRE]
    Minimal Space Width 1 on Side 1 = 1200. [MILLI METRE]
    Minimal Space Width 2 on Side 1 = 700. [MILLI METRE]
    Minimal Space in Front = 600. [MILLI METRE]
    Minimal Space on Side 2 = 600. [MILLI METRE]
    Rear Headboard Height = 340. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Pset_Bed_Layout_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 6 (IFCINTEGER)
    3D Detail Level = 4 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Base = TRUE (IFCBOOLEAN)
    Bed 2D Symbol Type (iSymbolType) = 1 (IFCINTEGER)
    Bed 2D Symbol Type (styp) = "Type 1" (IFCLABEL)
    Bed Frame = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Bed Frame Type = 1 (IFCINTEGER)
    Bed Headboard = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Bed Leg = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Bed Mattress = "Paint - Titanium White" (IFCLABEL)
    Bed Pillow = "Paint - Titanium White" (IFCLABEL)
    Bed Type = 2 (IFCINTEGER)
    Bed Type for Bed/Double bed objects = "" (IFCLABEL)
    Contour Pen = "Objects - General" (IFCLABEL)
    Cornice = TRUE (IFCBOOLEAN)
    Cornice Style = "Style 1" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Drawer Position = 2 (IFCINTEGER)
    Drawer Style (gs_door_type) = "Style 1" (IFCLABEL)
    Drawer Style (gs_door_type_m) = 1 (IFCINTEGER)
    Drawers and Table on the same Side = FALSE (IFCBOOLEAN)
    Edge Bevel = TRUE (IFCBOOLEAN)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Background Pen Blanket = "Backgrounds - color 1" (IFCLABEL)
    Fill Background Pen Lamp = "Backgrounds - color 1" (IFCLABEL)
    Fill Background Pen Night Table = "Backgrounds - color 1" (IFCLABEL)
    Fill Background Pen Pillow = "Backgrounds - color 1" (IFCLABEL)
    Fill Background Pen Uniform = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Blanket = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Lamp = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Night Table = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Pillow = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen Uniform = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Fill Type Blanket = "Background Fill" (IFCLABEL)
    Fill Type Lamp = "Background Fill" (IFCLABEL)
    Fill Type Night Table = "Background Fill" (IFCLABEL)
    Fill Type Pillow = "Background Fill" (IFCLABEL)
    Fill Type Uniform = "Background Fill" (IFCLABEL)
    Fill for (fillFor) = "Bed" (IFCLABEL)
    Fill for (iFillFor) = 1 (IFCINTEGER)
    Group Type (FM_Type) = "Furniture" (IFCLABEL)
    Group Type (iFMType) = 16 (IFCINTEGER)
    Headboard (bHeadboard) = TRUE (IFCBOOLEAN)
    Headboard (hb) = "Both Sides" (IFCLABEL)
    Headboard (iHeadboard) = 1 (IFCINTEGER)
    Headboard Edge = FALSE (IFCBOOLEAN)
    Headboard Style (hboard_type) = "Style 1" (IFCLABEL)
    Headboard Style (hboard_type_m) = 1 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Knob = TRUE (IFCBOOLEAN)
    Knob Style (gs_knob_type) = "Style 1" (IFCLABEL)
    Knob Style (gs_knob_type_m) = 1 (IFCINTEGER)
    Lamps (iLampOnSides) = 1 (IFCINTEGER)
    Lamps (sLampOnSides) = "None" (IFCLABEL)
    Leg Style (gs_leg_type) = "Style 1" (IFCLABEL)
    Leg Style (gs_leg_type_m) = 1 (IFCINTEGER)
    Leg Style (iBedLegType) = 1 (IFCINTEGER)
    Leg Style (stBedLegType) = "Style 1" (IFCLABEL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Night Table Base = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Night Table Cabinet = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Night Table Cornice = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Night Table Drawer (Frame) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Night Table Drawer (Inset) = "Glass - Clear Fast" (IFCLABEL)
    Night Table Knob = "Metal - Stainless Steel" (IFCLABEL)
    Night Table Lamp Base = "Metal - Stainless Steel" (IFCLABEL)
    Night Table Lampshade = "Paint - Glossy White" (IFCLABEL)
    Night Tables (iNightTableOnSides) = 2 (IFCINTEGER)
    Night Tables (sNightTableOnSides) = "On both sides" (IFCLABEL)
    No. of Drawers (0=None) = 2 (IFCINTEGER)
    No. of Hor. Grids = 0 (IFCINTEGER)
    No. of Vert. Grids = 0 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Pillow = FALSE (IFCBOOLEAN)
    Production Year = "" (IFCLABEL)
    Resolution = 12 (IFCINTEGER)
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Support Type = 1 (IFCINTEGER)
    Table Type (iNightTableType) = 2 (IFCINTEGER)
    Table Type (sNightTableType) = "Open" (IFCLABEL)
    Table Type for Night Table object = "Open" (IFCLABEL)
    Tabletop Style = 1 (IFCINTEGER)
    Uniform Fill Settings = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Equantity_Bed_Layout_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bed Frame Height (frh) = 320. [MILLI METRE]
    Bed Frame Height (frhLeg) = 10. [MILLI METRE]
    Bed Front Distance = 900. [MILLI METRE]
    Bed Height = 710. [MILLI METRE]
    Bed Length = 2030. [MILLI METRE]
    Bed Width / 2 = 750. [MILLI METRE]
    Bed Width = 1500. [MILLI METRE]
    Bed-Table Distance = 50. [MILLI METRE]
    Bedside Space Length = 1500. [MILLI METRE]
    Bedside Space Width 1 = 1200. [MILLI METRE]
    Bedside Space Width 2 = 700. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 2400. [MILLI METRE]
    Dimension 2 = 2030. [MILLI METRE]
    Drawer Frame Width = 50. [MILLI METRE]
    Drawer Thickness = 20. [MILLI METRE]
    Edge Radius of Mattress = 20. [MILLI METRE]
    Fillet Radius of Mattress = 20. [MILLI METRE]
    Front Headboard Height = 340. [MILLI METRE]
    Height (ZZYZX) = 710. [MILLI METRE]
    Height (leg_h) = 50. [MILLI METRE]
    Knob Size = 100. [MILLI METRE]
    Lamp Diameter = 200. [MILLI METRE]
    Lamp Height = 600. [MILLI METRE]
    Lampshade Height = 200. [MILLI METRE]
    Lampshade Upper Diameter = 100. [MILLI METRE]
    Lampshade Upper Radius = 50. [MILLI METRE]
    Leg Height = 160. [MILLI METRE]
    Leg Width/Diameter = 50. [MILLI METRE]
    Mattress Dist. from Edge = 20. [MILLI METRE]
    Mattress Height = 120. [MILLI METRE]
    Night Table Depth = 400. [MILLI METRE]
    Night Table Height = 500. [MILLI METRE]
    Night Table Width = 400. [MILLI METRE]
    Overhang Length = 10. [MILLI METRE]
    Rear Headboard Height = 390. [MILLI METRE]
    Thickness = 20. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Upper Drawer Height = 190. [MILLI METRE]
    Width/Diameter = 20. [MILLI METRE]
  AC_Pset_Basin_Cabinet_21 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    'A' 'B' Size= (cab_size) = FALSE (IFCBOOLEAN)
    'A' 'B' Size= (cab_size_) = "Counter" (IFCLABEL)
    2D Detail Level (gs_detlevel_2D) = "Scale Sensitive" (IFCLABEL)
    2D Detail Level (gs_detlevel_2D_m) = 0 (IFCINTEGER)
    3D (gs_detlevel_3D) = "Detailed" (IFCLABEL)
    3D (gs_detlevel_3D_m) = 2 (IFCINTEGER)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Base Height = "" (IFCLABEL)
    Additional Description = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Additional Manufacturer = "" (IFCLABEL)
    Additional Number = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Area = 0. (IFCREAL)
    Assembly Date = "" (IFCLABEL)
    Backsplash = "Plastic - Laminate" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Basin = "Rectangular" (IFCLABEL)
    Cabinet (gs_cabinet_mat) = "Paint - Titanium White" (IFCLABEL)
    Cabinet Symbol Type = "Type 1" (IFCLABEL)
    Cold Water Connection = TRUE (IFCBOOLEAN)
    Collection of Specifications ID = "" (IFCLABEL)
    Connection = "Metal - Stainless Steel" (IFCLABEL)
    Connection Type (ConConnectorType_1) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_2) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_3) = "Welded" (IFCLABEL)
    Contour Pen = "Mechanical - Plumbing" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Counter Type (gs_count_type) = "Rectangular" (IFCLABEL)
    Counter Type (gs_count_type_m) = 1 (IFCINTEGER)
    Countertop = "Plastic - Laminate" (IFCLABEL)
    Custom Panel Name (gs_cust_p) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_p_end) = "" (IFCLABEL)
    Dimensions W/D/H = "" (IFCLABEL)
    Door (Frame) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Door (Glazing) = "Glass - Clear Fast" (IFCLABEL)
    Door (door) = TRUE (IFCBOOLEAN)
    Door (gs_door_type) = "Style 1" (IFCLABEL)
    Door Opening Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Door Style = 1 (IFCINTEGER)
    Double Faced = FALSE (IFCBOOLEAN)
    Drain = "Metal - Stainless Steel" (IFCLABEL)
    Drawer (DrawerMat) = "Wood - Pine Grained Horizontal" (IFCLABEL)
    Drawer (bDrawer) = FALSE (IFCBOOLEAN)
    Drawer No. = 1 (IFCINTEGER)
    Edge Bevel = FALSE (IFCBOOLEAN)
    Edge Visibility in 2D (side_vis2D) = "Both" (IFCLABEL)
    Edge Visibility in 2D (side_vis2D_m) = 4 (IFCINTEGER)
    Edge Visibility in 2D (side_vis2D_mirror) = "Both" (IFCLABEL)
    Edge Visibility in 3D (side_vis) = "Both" (IFCLABEL)
    Edge Visibility in 3D (side_vis_mirror) = "Both" (IFCLABEL)
    End Panel = "Wood - Pine Grained Horizontal" (IFCLABEL)
    End Panel Type = "Style 1" (IFCLABEL)
    Extra Hotspot Editing = TRUE (IFCBOOLEAN)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Group Type (FM_Type) = "Sanitation" (IFCLABEL)
    Group Type (iFMType) = 13 (IFCINTEGER)
    Hot Water Connection = TRUE (IFCBOOLEAN)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Knob (gs_knob_mat) = "Metal - Stainless Steel" (IFCLABEL)
    Knob (gs_knob_type) = "Style 1" (IFCLABEL)
    Knob Position (gs_knob_p) = "Vertical" (IFCLABEL)
    Knob Position (gs_knob_p_m) = 0 (IFCINTEGER)
    Knob Style = 1 (IFCINTEGER)
    Left End Panel (left_panel) = FALSE (IFCBOOLEAN)
    Left End Panel (left_panel_mirror) = FALSE (IFCBOOLEAN)
    Location = "" (IFCLABEL)
    MEP System (ConSystem_1) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_2) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_3) = "Undefined" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    No. of Hor. Door Grids = 2 (IFCINTEGER)
    No. of Shelves = 2 (IFCINTEGER)
    No. of Vert. Door Grids = 1 (IFCINTEGER)
    Nominal Size (ConNominalWidth_1) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_2) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_3) = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 3 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Product ID = "" (IFCLABEL)
    Product Name (FM_ProductName) = "" (IFCLABEL)
    Product Name (gs_onorm_product) = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Rear End Panel = FALSE (IFCBOOLEAN)
    Resolution = 12 (IFCINTEGER)
    Right End Panel (right_panel) = FALSE (IFCBOOLEAN)
    Right End Panel (right_panel_mirror) = FALSE (IFCBOOLEAN)
    Same Door Widths = FALSE (IFCBOOLEAN)
    Serial Number = "" (IFCLABEL)
    Set Program = FALSE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Shape Type (ConType_1) = "Circle" (IFCLABEL)
    Shape Type (ConType_2) = "Circle" (IFCLABEL)
    Shape Type (ConType_3) = "Circle" (IFCLABEL)
    Shelf = "Paint - Titanium White" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Sides Visible = 4 (IFCINTEGER)
    Sink = "Ceramic - Porcelain" (IFCLABEL)
    Sink Style = 3 (IFCINTEGER)
    System Surface = "Paint - Cadmium Yellow" (IFCLABEL)
    Tap = "Metal - Stainless Steel" (IFCLABEL)
    Tap Style (gs_tap_type) = "Style 1" (IFCLABEL)
    Tap Style (gs_tap_type_m) = 1 (IFCINTEGER)
    Tap Symbol Type (TapSymbol) = "Detailed" (IFCLABEL)
    Tap Symbol Type (TapSymbol_m) = 2 (IFCINTEGER)
    Tap Type (iTapGroup) = 1 (IFCINTEGER)
    Tap Type (tapGroup) = "Single Level Mixer" (IFCLABEL)
    To Zone Number = "" (IFCLABEL)
    Toe = "Plastic - Laminate" (IFCLABEL)
    Toe Style = 1 (IFCINTEGER)
    Toe Type = "Full" (IFCLABEL)
    Tool Type (ConToolType_1) = 2 (IFCINTEGER)
    Tool Type (ConToolType_2) = 2 (IFCINTEGER)
    Tool Type (ConToolType_3) = 2 (IFCINTEGER)
    Use System Surface = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Volume = 0. (IFCREAL)
    Waste Water Connection = TRUE (IFCBOOLEAN)
  AC_Equantity_Basin_Cabinet_21 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Backsplash Height (0-None) = 100. [MILLI METRE]
    Basin Distance from Center = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Cabinet Depth = 460. [MILLI METRE]
    Cabinet Width = 750. [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Length (ConLength_3) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = 350. [MILLI METRE]
    Connection Position X (ConPosX_2) = 550. [MILLI METRE]
    Connection Position X (ConPosX_3) = 450. [MILLI METRE]
    Connection Position Y (ConPosY_1) = 460. [MILLI METRE]
    Connection Position Y (ConPosY_2) = 460. [MILLI METRE]
    Connection Position Y (ConPosY_3) = 460. [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 786.5 [MILLI METRE]
    Connection Position Z (ConPosZ_2) = 786.5 [MILLI METRE]
    Connection Position Z (ConPosZ_3) = 630. [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_3) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_3) = 42. [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_3) = 5. [MILLI METRE]
    Counter Thickness = 50. [MILLI METRE]
    Countertop Height = 850. [MILLI METRE]
    Door Frame Width = 80. [MILLI METRE]
    Door Panel Height = 700. [MILLI METRE]
    Door Thickness = 20. [MILLI METRE]
    Knob Position Hor. = 50. [MILLI METRE]
    Knob Position Vert. = 650. [MILLI METRE]
    Knob Size = 100. [MILLI METRE]
    Left Door Width = 500. [MILLI METRE]
    Minimal Space in Front = 900. [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 25.4 [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_3) = 40. [MILLI METRE]
    Outer Depth (ConDepth_1) = 27. [MILLI METRE]
    Outer Depth (ConDepth_2) = 27. [MILLI METRE]
    Outer Depth (ConDepth_3) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_1) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_2) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_3) = 42. [MILLI METRE]
    Overhang to Front of Cabinet = 50. [MILLI METRE]
    Overhang to Left of Cabinet (left_cab) = 0. [MILLI METRE]
    Overhang to Left of Cabinet (left_cab_mirror) = 0. [MILLI METRE]
    Overhang to Rear of Cabinet = 0. [MILLI METRE]
    Overhang to Right of Cabinet (right_cab) = 0. [MILLI METRE]
    Overhang to Right of Cabinet (right_cab_mirror) = 0. [MILLI METRE]
    Panel Frame Width = 30. [MILLI METRE]
    Rear Minimal Space = 900. [MILLI METRE]
    Sink Depth = 280. [MILLI METRE]
    Sink Width = 550. [MILLI METRE]
    Tap Height = 1100. [MILLI METRE]
    Tap X Position = 0. [MILLI METRE]
    Tap Y Position = -39.99999999999999 [MILLI METRE]
    Tap Z Position = 0. [MILLI METRE]
    Toe Height = 100. [MILLI METRE]
    Toe Setback = 20. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_3) = 1. [MILLI METRE]
  AC_Pset_WC_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 2 (IFCINTEGER)
    3D Detail Level = 3 (IFCINTEGER)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Base Height = "" (IFCLABEL)
    Additional Description = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Additional Manufacturer = "" (IFCLABEL)
    Additional Number = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Area = 0. (IFCREAL)
    Assembly Date = "" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Bowl (gs_bowl_mat) = "Ceramic - Porcelain" (IFCLABEL)
    Button = "Paint - Titanium White" (IFCLABEL)
    Button Position = "Front" (IFCLABEL)
    Cistern = "Paint - Titanium White" (IFCLABEL)
    Cistern Pipe = "Metal - Stainless Steel" (IFCLABEL)
    Cistern Type = 1 (IFCINTEGER)
    Collection of Specifications ID = "" (IFCLABEL)
    Connection = "Metal - Stainless Steel" (IFCLABEL)
    Connection Type (ConConnectorType_1) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_2) = "Welded" (IFCLABEL)
    Contour Pen = "Mechanical - Plumbing" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Dimensions W/D/H = "" (IFCLABEL)
    Elevated Cistern Type = "Type 1" (IFCLABEL)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Floor Mounted Bowl Type = 1 (IFCINTEGER)
    Flush Type = "Cistern" (IFCLABEL)
    Flushometer Pipe = "Metal - Stainless Steel" (IFCLABEL)
    Flushometer Type = "Simple" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Group Type (FM_Type) = "Sanitation" (IFCLABEL)
    Group Type (iFMType) = 13 (IFCINTEGER)
    ID Number = "" (IFCLABEL)
    In-Wall Carrier Button Type = "Type 1" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Lid = TRUE (IFCBOOLEAN)
    Location = "" (IFCLABEL)
    MEP System (ConSystem_1) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_2) = "Undefined" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    Mounting Type = "Floor Mounted" (IFCLABEL)
    Nominal Diameter (ConNominalWidth_1) = "" (IFCLABEL)
    Nominal Diameter (ConNominalWidth_2) = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 2 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Product ID = "" (IFCLABEL)
    Product Name (FM_ProductName) = "" (IFCLABEL)
    Product Name (gs_onorm_product) = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Resolution = 32 (IFCINTEGER)
    Seat (bSeat) = TRUE (IFCBOOLEAN)
    Seat (gs_seat) = "Closed" (IFCLABEL)
    Seat (matSeatCover) = "Plastic - Laminate" (IFCLABEL)
    Sensor = "Paint - Anthracite" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Set Program = FALSE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Shape Type (ConType_1) = "Circle" (IFCLABEL)
    Shape Type (ConType_2) = "Circle" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show 3D (2D Projection) = TRUE (IFCBOOLEAN)
    Show In-Wall Carrier in 2D = FALSE (IFCBOOLEAN)
    Show In-Wall Carrier in 3D = FALSE (IFCBOOLEAN)
    To Zone Number = "" (IFCLABEL)
    Tool Type (ConToolType_1) = 2 (IFCINTEGER)
    Tool Type (ConToolType_2) = 2 (IFCINTEGER)
    Type of Effluent = "In the Back" (IFCLABEL)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Volume = 0. (IFCREAL)
    Wall Hung Bowl Type = "Type 1" (IFCLABEL)
    Waste Water Connection = TRUE (IFCBOOLEAN)
    Water Connection = TRUE (IFCBOOLEAN)
  AC_Equantity_WC_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Bowl Depth = 700. [MILLI METRE]
    Bowl Height = 400. [MILLI METRE]
    Bowl Width = 380. [MILLI METRE]
    Carrier Depth = 120. [MILLI METRE]
    Carrier Height = 1200. [MILLI METRE]
    Carrier Width = 500. [MILLI METRE]
    Cistern Depth = 180. [MILLI METRE]
    Cistern Elevation = 1200. [MILLI METRE]
    Cistern Height = 390. [MILLI METRE]
    Cistern Width = 410. [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = 0. [MILLI METRE]
    Connection Position X (ConPosX_2) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_1) = -0. [MILLI METRE]
    Connection Position Y (ConPosY_2) = 0. [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 666. [MILLI METRE]
    Connection Position Z (ConPosZ_2) = 205.1282051282052 [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 130. [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 5. [MILLI METRE]
    Dimension 1 = 380. [MILLI METRE]
    Dimension 2 = 700. [MILLI METRE]
    Distance from Wall = 0. [MILLI METRE]
    Height = 400. [MILLI METRE]
    Minimal Space in Front 2 = 1000. [MILLI METRE]
    Minimal Space in Front = 1000. [MILLI METRE]
    Minimal Space in Width 2 = 1000. [MILLI METRE]
    Minimal Space on Side 1 = 300. [MILLI METRE]
    Minimal Space on Side 2 = 900. [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 30. [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 110. [MILLI METRE]
    Outer Depth (ConDepth_1) = 32. [MILLI METRE]
    Outer Depth (ConDepth_2) = 114. [MILLI METRE]
    Outer Diameter (ConWidth_1) = 32. [MILLI METRE]
    Outer Diameter (ConWidth_2) = 114. [MILLI METRE]
    Pipe Diameter = 30. [MILLI METRE]
    Seat Height = 400. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 2. [MILLI METRE]
    Water Connection Height = 755. [MILLI METRE]
  AC_Equantity_Shower_Cabin_26 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Cabin Depth = 900. [MILLI METRE]
    Cabin Frame Width = 30. [MILLI METRE]
    Cabin Height = 1950. [MILLI METRE]
    Cabin Width = 900. [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Length (ConLength_3) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = 75.00000000000001 [MILLI METRE]
    Connection Position X (ConPosX_2) = -75.00000000000001 [MILLI METRE]
    Connection Position X (ConPosX_3) = -275. [MILLI METRE]
    Connection Position Y (ConPosY_1) = 450. [MILLI METRE]
    Connection Position Y (ConPosY_2) = 450. [MILLI METRE]
    Connection Position Y (ConPosY_3) = 275. [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 1000. [MILLI METRE]
    Connection Position Z (ConPosZ_2) = 1000. [MILLI METRE]
    Connection Position Z (ConPosZ_3) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_3) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_3) = 54. [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_3) = 5. [MILLI METRE]
    Default Cabin Size 1 = 800. [MILLI METRE]
    Default Cabin Size 2 = 900. [MILLI METRE]
    Default Cabin Size 3 = 1000. [MILLI METRE]
    Default Door Width 1 = 450. [MILLI METRE]
    Default Door Width 2 = 500. [MILLI METRE]
    Default Door Width 3 = 550. [MILLI METRE]
    Default Door Width 4 = 600. [MILLI METRE]
    Default Door Width 5 = 565.6999999999999 [MILLI METRE]
    Default Door Width 6 = 636.4 [MILLI METRE]
    Default Door Width 7 = 707.0999999999999 [MILLI METRE]
    Door Frame Width = 15. [MILLI METRE]
    Door Width = 636.4 [MILLI METRE]
    Half Door Width = 318.2 [MILLI METRE]
    Minimal Space in Front = 1000. [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_3) = 50. [MILLI METRE]
    Opening Width in 3D = 0. [MILLI METRE]
    Outer Depth (ConDepth_1) = 27. [MILLI METRE]
    Outer Depth (ConDepth_2) = 27. [MILLI METRE]
    Outer Depth (ConDepth_3) = 54. [MILLI METRE]
    Outer Diameter (ConWidth_1) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_2) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_3) = 54. [MILLI METRE]
    Shower Tray Thickness = 100. [MILLI METRE]
    Side Panel Width 1 = 449.9972444528812 [MILLI METRE]
    Side Panel Width 2 = 449.9972444528812 [MILLI METRE]
    Tap Distance from Corner = 400. [MILLI METRE]
    Tap Height = 1000. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_3) = 2. [MILLI METRE]
  AC_Pset_Shower_Cabin_26 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2D Detail Level = 3 (IFCINTEGER)
    3D Detail Level = 1 (IFCINTEGER)
    AKS Number = "" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional Base Height = "" (IFCLABEL)
    Additional Description = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Additional Manufacturer = "" (IFCLABEL)
    Additional Number = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Area = 0. (IFCREAL)
    Assembly Date = "" (IFCLABEL)
    Base Height Value = "" (IFCLABEL)
    Bracket = TRUE (IFCBOOLEAN)
    Cabin Form (cabinForm) = "Squared Corner" (IFCLABEL)
    Cabin Form (iCabinForm) = 2 (IFCINTEGER)
    Cabin Frame = "Paint - Titanium White" (IFCLABEL)
    Cabin Glass = "Glass - Clear Fast" (IFCLABEL)
    Cabin Size (cabinSize) = "900 x 900" (IFCLABEL)
    Cabin Size (iCabinSize) = 2 (IFCINTEGER)
    Cabin Type (cabinType) = "Corner" (IFCLABEL)
    Cabin Type (iCabinType) = 2 (IFCINTEGER)
    Ceiling = FALSE (IFCBOOLEAN)
    Cold Water Connection = TRUE (IFCBOOLEAN)
    Collection of Specifications ID = "" (IFCLABEL)
    Connection = "Paint - Grey Light" (IFCLABEL)
    Connection Type (ConConnectorType_1) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_2) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_3) = "Welded" (IFCLABEL)
    Contour Pen = "Mechanical - Plumbing" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Dimensions W/D/H = "" (IFCLABEL)
    Door Type (doorType) = "Simple Leaf" (IFCLABEL)
    Door Type (iDoorType) = 1 (IFCINTEGER)
    Fill Background Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Pen = "Backgrounds - color 1" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Grab Bar = FALSE (IFCBOOLEAN)
    Group Type (FM_Type) = "Sanitation" (IFCLABEL)
    Group Type (iFMType) = 13 (IFCINTEGER)
    Handle = "Paint - Grey Light" (IFCLABEL)
    Handle Type (handleType) = "Style 1" (IFCLABEL)
    Handle Type (iHandleType) = 1 (IFCINTEGER)
    Hot Water Connection = TRUE (IFCBOOLEAN)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    MEP System (ConSystem_1) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_2) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_3) = "Undefined" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Mirror Door = FALSE (IFCBOOLEAN)
    Modification Date = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_1) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_2) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_3) = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 3 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Open Door on Detailed 2D = FALSE (IFCBOOLEAN)
    Opening Angle in 3D = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Panel Type (iPanelType) = 2 (IFCINTEGER)
    Panel Type (panelType) = "Fully Glazed" (IFCLABEL)
    Product ID = "" (IFCLABEL)
    Product Name (FM_ProductName) = "" (IFCLABEL)
    Product Name (gs_onorm_product) = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Resolution = 24 (IFCINTEGER)
    Serial Number = "" (IFCLABEL)
    Set Program = FALSE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Shape Type (ConType_1) = "Circle" (IFCLABEL)
    Shape Type (ConType_2) = "Circle" (IFCLABEL)
    Shape Type (ConType_3) = "Circle" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Grab Bar on Detailed 2D = TRUE (IFCBOOLEAN)
    Show Shower Kit on Detailed 2D = FALSE (IFCBOOLEAN)
    Shower Kit = "Paint - Grey Light" (IFCLABEL)
    Shower Tray = "Paint - Titanium White" (IFCLABEL)
    Shower Type (gs_tap_type) = "Wall Mounted Thermostatic" (IFCLABEL)
    Shower Type (gs_tap_type_m) = 24 (IFCINTEGER)
    System Surface = "Brick - Classic Tongariro" (IFCLABEL)
    To Zone Number = "" (IFCLABEL)
    Tool Type (ConToolType_1) = 2 (IFCINTEGER)
    Tool Type (ConToolType_2) = 2 (IFCINTEGER)
    Tool Type (ConToolType_3) = 2 (IFCINTEGER)
    Tray = TRUE (IFCBOOLEAN)
    Use System Surface = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Volume = 0. (IFCREAL)
    Waste Water Connection = TRUE (IFCBOOLEAN)
  AC_Pset_CI_Tools_Roof_Covering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    3D Detail = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional information (gs_list_custom1) = "" (IFCLABEL)
    Additional information (gs_list_custom2) = "" (IFCLABEL)
    Additional information (gs_list_custom3) = "" (IFCLABEL)
    Additional information (gs_list_custom4) = "" (IFCLABEL)
    Additional information (gs_list_custom5) = "" (IFCLABEL)
    Apron Flashing Perpendicular = FALSE (IFCBOOLEAN)
    Apron Flashing Type = "Realistic" (IFCLABEL)
    Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Barge Board Cut Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Barge Board Finish = "" (IFCLABEL)
    Barge Board Material (barge_colour) = "Ohakea" (IFCLABEL)
    Barge Board Material (barge_material) = "" (IFCLABEL)
    Barge Flashing Material = "Ohakea" (IFCLABEL)
    Barge Flashing Type = "Flat Square" (IFCLABEL)
    Calculated Downpipe Number = 2 (IFCINTEGER)
    Calculated Soffit Area = 4.272067158462209 (IFCREAL)
    Calculated Verge Area = 4.891499999999997 (IFCREAL)
    Cladding Preset = "" (IFCLABEL)
    Cladding Type = "Ribbed" (IFCLABEL)
    Clicked Cell = 337 (IFCINTEGER)
    Cost = 0. (IFCREAL)
    Default Barge Edge = "Barge" (IFCLABEL)
    Default Gutter Edge = "Gutter" (IFCLABEL)
    Default Hip Edge = "Hip" (IFCLABEL)
    Default Ridge Edge = "Ridge" (IFCLABEL)
    Default Roof Style = "Custom" (IFCLABEL)
    Default Valley Edge = "Valley" (IFCLABEL)
    Downpipe 3D Attributes = "Custom" (IFCLABEL)
    Downpipe 3D Attributes GUID = "" (IFCLABEL)
    Downpipe 3D Pen = "General - General" (IFCLABEL)
    Downpipe Material = "Ohakea" (IFCLABEL)
    Downpipe Neck Angle = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Downpipe Profile = "Circular" (IFCLABEL)
    Downpipe Section Attributes = "GA - Cut Steel (Folded)" (IFCLABEL)
    Downpipe Section Attributes GUID = "F204B6BC-1D61-45A5-BE0D-C92FE6FE3644" (IFCLABEL)
    Downpipe Section Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Downpipe Section Fill = "Steel" (IFCLABEL)
    Downpipe Section Fill Pen = "Structural - Hatching" (IFCLABEL)
    Downpipe Section Line Type = 1 (IFCINTEGER)
    Downpipe Section Pen = "Structural - Cut Non-Construction" (IFCLABEL)
    Downpipe Toe Angle = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Downpipe has Brackets = TRUE (IFCBOOLEAN)
    Downpipes = "" (IFCLABEL)
    Downpipes Total Length = 1 (IFCINTEGER)
    Edge Boards = "" (IFCLABEL)
    End Angles = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    FM Inventory Number = "" (IFCLABEL)
    FM Production Year = "" (IFCLABEL)
    FM Serial Number = "" (IFCLABEL)
    FM Type = "Others" (IFCLABEL)
    FM Weight = 0. (IFCREAL)
    FM Weight Unit = "kg" (IFCLABEL)
    Fascia Board Finish = "" (IFCLABEL)
    Fascia Board Material (fascia_colour) = "Ohakea" (IFCLABEL)
    Fascia Board Material (fascia_material) = "" (IFCLABEL)
    Fascia Board Profile = "Timber" (IFCLABEL)
    Fascia Section Attributes = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Finial = FALSE (IFCBOOLEAN)
    Finials = 1 (IFCINTEGER)
    Flashing Echo = "" (IFCLABEL)
    Flashing Finish = "" (IFCLABEL)
    Flashing Material = "" (IFCLABEL)
    Flashing Section Attributes = "" (IFCLABEL)
    Flashings Preset (flashingPreset) = "" (IFCLABEL)
    Floor Plan Display = 0 (IFCINTEGER)
    Framing = "" (IFCLABEL)
    Framing Grade = "" (IFCLABEL)
    Framing Material (frame_colour) = "Wood - Oak Light" (IFCLABEL)
    Framing Material (framing_mat) = "" (IFCLABEL)
    Framing Treatment = "" (IFCLABEL)
    Freize Style = 1 (IFCINTEGER)
    Group Type = 25 (IFCINTEGER)
    Gutter Ends at Apron Flashing = TRUE (IFCBOOLEAN)
    Gutter Finish = "" (IFCLABEL)
    Gutter Material (gutter_colour) = "Ohakea" (IFCLABEL)
    Gutter Material (gutter_material) = "" (IFCLABEL)
    Gutter Pen = "Annotation Text - general" (IFCLABEL)
    Gutter Pen GUID = "ffb1c35b-2eba-406a-86b3-ba42b97a5538" (IFCLABEL)
    Gutter Pen Preset = "GA - Steel (Folded)" (IFCLABEL)
    Gutter Profile = "Brick Wall" (IFCLABEL)
    Gutter Section Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Gutter Section Fill = "Steel" (IFCLABEL)
    Gutter Section Fill Pen = "Structural - Hatching" (IFCLABEL)
    Gutter Section GUID = "f204b6bc-1d61-45a5-be0d-c92fe6fe3644" (IFCLABEL)
    Gutter Section Line Type = 1 (IFCINTEGER)
    Gutter Section Pen = "Structural - Cut Non-Construction" (IFCLABEL)
    Gutter Section Preset = "GA - Cut Steel (Folded)" (IFCLABEL)
    Gutter Type = "Square" (IFCLABEL)
    Holes = 1 (IFCINTEGER)
    Image Index = 1 (IFCINTEGER)
    Listing Option for Barge & Fascia = 1 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Menu (menu) = 1000 (IFCINTEGER)
    Note = "" (IFCLABEL)
    Page = 2 (IFCINTEGER)
    Part = 1 (IFCINTEGER)
    Property = 2 (IFCINTEGER)
    Purlin Type = "Timber" (IFCLABEL)
    Relation of Brackets to downpipe = "Align" (IFCLABEL)
    Ridge/Hip Flashing Matches Barge = FALSE (IFCBOOLEAN)
    Ridge/Hip Flashing Material (ridge_colour) = "Ohakea" (IFCLABEL)
    Ridge/Hip Flashing Material (ridge_material) = "" (IFCLABEL)
    Ridge/Hip Flashing Type = "Flat" (IFCLABEL)
    Roof Area ignoring Holes (m2) = 24.84227630875221 (IFCREAL)
    Roof Area with Holes Removed (m2) = 24.84227630875221 (IFCREAL)
    Selection Mode = 4 (IFCINTEGER)
    Shadow Casting = FALSE (IFCBOOLEAN)
    Show Framing = TRUE (IFCBOOLEAN)
    Show Framing in 3D = FALSE (IFCBOOLEAN)
    Show Framing in Section/Elevation = FALSE (IFCBOOLEAN)
    Show Projection = 0 (IFCINTEGER)
    Soffit Finish = "" (IFCLABEL)
    Soffit Material (Ends) = "Okarito Double" (IFCLABEL)
    Soffit Material (soffit_colour) = "Okarito Double" (IFCLABEL)
    Soffit Material (soffit_material) = "" (IFCLABEL)
    Soffit Materials Linked = TRUE (IFCBOOLEAN)
    Soffit Section Attributes = "GA - Cut Ceiling" (IFCLABEL)
    Soffit Section Attributes GUID = "03b6d67b-4bc5-4f65-9fb1-f4cd19acd7c0" (IFCLABEL)
    Soffit Section Background Pen = "Roofs- Fill backgrounds" (IFCLABEL)
    Soffit Section Fill = "Plaster" (IFCLABEL)
    Soffit Section Fill Pen = "Roof - Cut Fills" (IFCLABEL)
    Soffit Section Line Type = 1 (IFCINTEGER)
    Soffit Section Pen = "Roof - Cut Non-Structuralr" (IFCLABEL)
    Soffit Type (Ends) = "Boxed Fascia" (IFCLABEL)
    Soffit Type = "Flat" (IFCLABEL)
    Soffit View Attributes = "GA - Timber (Dressed)" (IFCLABEL)
    Soffit View Attributes GUID = "adca6221-b281-4eac-9cf7-28b4b883134c" (IFCLABEL)
    Soffit View Pen = "Objects - General" (IFCLABEL)
    Soffits = "Sloping 450" (IFCLABEL)
    Soffits Area = 4.072100000600026 (IFCREAL)
    Start Angles = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Story Sensitive Symbol = TRUE (IFCBOOLEAN)
    Tile Capping Material = "Ohakea" (IFCLABEL)
    USED FOR VERSIONING = "USED FOR VERSIONING" (IFCLABEL)
    Update Calculated Parameters = 2 (IFCINTEGER)
    Use Same Pens for All Views = TRUE (IFCBOOLEAN)
    Valley Flashing Finish = "" (IFCLABEL)
    Valley Flashing Material (valley_colour) = "Ohakea" (IFCLABEL)
    Valley Flashing Material (valley_material) = "" (IFCLABEL)
    Valley Flashing Type = "Internal" (IFCLABEL)
    Version Number = 2400 (IFCINTEGER)
    Wall Cladding Surface = "Paint - Titanium White" (IFCLABEL)
    Wall Cladding Type = 1 (IFCINTEGER)
    Zoom Buttons = 3 (IFCINTEGER)
    Zoom Level = 1 (IFCINTEGER)
    reset = FALSE (IFCBOOLEAN)
    type = "" (IFCLABEL)
  AC_Pset_CI_Tools_Roof_Covering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    3D Detail = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional information (gs_list_custom1) = "" (IFCLABEL)
    Additional information (gs_list_custom2) = "" (IFCLABEL)
    Additional information (gs_list_custom3) = "" (IFCLABEL)
    Additional information (gs_list_custom4) = "" (IFCLABEL)
    Additional information (gs_list_custom5) = "" (IFCLABEL)
    Apron Flashing Perpendicular = FALSE (IFCBOOLEAN)
    Apron Flashing Type = "Realistic" (IFCLABEL)
    Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Barge Board Cut Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Barge Board Finish = "" (IFCLABEL)
    Barge Board Material (barge_colour) = "Ohakea" (IFCLABEL)
    Barge Board Material (barge_material) = "" (IFCLABEL)
    Barge Flashing Material = "Ohakea" (IFCLABEL)
    Barge Flashing Type = "Flat Square" (IFCLABEL)
    Calculated Downpipe Number = 2 (IFCINTEGER)
    Calculated Soffit Area = 4.272067158462209 (IFCREAL)
    Calculated Verge Area = 4.891499999999997 (IFCREAL)
    Cladding Preset = "" (IFCLABEL)
    Cladding Type = "Ribbed" (IFCLABEL)
    Clicked Cell = 337 (IFCINTEGER)
    Cost = 0. (IFCREAL)
    Default Barge Edge = "Barge" (IFCLABEL)
    Default Gutter Edge = "Gutter" (IFCLABEL)
    Default Hip Edge = "Hip" (IFCLABEL)
    Default Ridge Edge = "Ridge" (IFCLABEL)
    Default Roof Style = "Custom" (IFCLABEL)
    Default Valley Edge = "Valley" (IFCLABEL)
    Downpipe 3D Attributes = "Custom" (IFCLABEL)
    Downpipe 3D Attributes GUID = "" (IFCLABEL)
    Downpipe 3D Pen = "General - General" (IFCLABEL)
    Downpipe Material = "Ohakea" (IFCLABEL)
    Downpipe Neck Angle = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Downpipe Profile = "Circular" (IFCLABEL)
    Downpipe Section Attributes = "GA - Cut Steel (Folded)" (IFCLABEL)
    Downpipe Section Attributes GUID = "F204B6BC-1D61-45A5-BE0D-C92FE6FE3644" (IFCLABEL)
    Downpipe Section Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Downpipe Section Fill = "Steel" (IFCLABEL)
    Downpipe Section Fill Pen = "Structural - Hatching" (IFCLABEL)
    Downpipe Section Line Type = 1 (IFCINTEGER)
    Downpipe Section Pen = "Structural - Cut Non-Construction" (IFCLABEL)
    Downpipe Toe Angle = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Downpipe has Brackets = TRUE (IFCBOOLEAN)
    Downpipes = "" (IFCLABEL)
    Downpipes Total Length = 1 (IFCINTEGER)
    Edge Boards = "" (IFCLABEL)
    End Angles = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    FM Inventory Number = "" (IFCLABEL)
    FM Production Year = "" (IFCLABEL)
    FM Serial Number = "" (IFCLABEL)
    FM Type = "Others" (IFCLABEL)
    FM Weight = 0. (IFCREAL)
    FM Weight Unit = "kg" (IFCLABEL)
    Fascia Board Finish = "" (IFCLABEL)
    Fascia Board Material (fascia_colour) = "Ohakea" (IFCLABEL)
    Fascia Board Material (fascia_material) = "" (IFCLABEL)
    Fascia Board Profile = "Timber" (IFCLABEL)
    Fascia Section Attributes = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Finial = FALSE (IFCBOOLEAN)
    Finials = 1 (IFCINTEGER)
    Flashing Echo = "" (IFCLABEL)
    Flashing Finish = "" (IFCLABEL)
    Flashing Material = "" (IFCLABEL)
    Flashing Section Attributes = "" (IFCLABEL)
    Flashings Preset (flashingPreset) = "" (IFCLABEL)
    Floor Plan Display = 0 (IFCINTEGER)
    Framing = "" (IFCLABEL)
    Framing Grade = "" (IFCLABEL)
    Framing Material (frame_colour) = "Wood - Oak Light" (IFCLABEL)
    Framing Material (framing_mat) = "" (IFCLABEL)
    Framing Treatment = "" (IFCLABEL)
    Freize Style = 1 (IFCINTEGER)
    Group Type = 25 (IFCINTEGER)
    Gutter Ends at Apron Flashing = TRUE (IFCBOOLEAN)
    Gutter Finish = "" (IFCLABEL)
    Gutter Material (gutter_colour) = "Ohakea" (IFCLABEL)
    Gutter Material (gutter_material) = "" (IFCLABEL)
    Gutter Pen = "Annotation Text - general" (IFCLABEL)
    Gutter Pen GUID = "ffb1c35b-2eba-406a-86b3-ba42b97a5538" (IFCLABEL)
    Gutter Pen Preset = "GA - Steel (Folded)" (IFCLABEL)
    Gutter Profile = "Brick Wall" (IFCLABEL)
    Gutter Section Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Gutter Section Fill = "Steel" (IFCLABEL)
    Gutter Section Fill Pen = "Structural - Hatching" (IFCLABEL)
    Gutter Section GUID = "f204b6bc-1d61-45a5-be0d-c92fe6fe3644" (IFCLABEL)
    Gutter Section Line Type = 1 (IFCINTEGER)
    Gutter Section Pen = "Structural - Cut Non-Construction" (IFCLABEL)
    Gutter Section Preset = "GA - Cut Steel (Folded)" (IFCLABEL)
    Gutter Type = "Square" (IFCLABEL)
    Holes = 1 (IFCINTEGER)
    Image Index = 1 (IFCINTEGER)
    Listing Option for Barge & Fascia = 1 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Menu (menu) = 1000 (IFCINTEGER)
    Note = "" (IFCLABEL)
    Page = 2 (IFCINTEGER)
    Part = 1 (IFCINTEGER)
    Property = 2 (IFCINTEGER)
    Purlin Type = "Timber" (IFCLABEL)
    Relation of Brackets to downpipe = "Align" (IFCLABEL)
    Ridge/Hip Flashing Matches Barge = FALSE (IFCBOOLEAN)
    Ridge/Hip Flashing Material (ridge_colour) = "Ohakea" (IFCLABEL)
    Ridge/Hip Flashing Material (ridge_material) = "" (IFCLABEL)
    Ridge/Hip Flashing Type = "Flat" (IFCLABEL)
    Roof Area ignoring Holes (m2) = 17.1984989802278 (IFCREAL)
    Roof Area with Holes Removed (m2) = 17.1984989802278 (IFCREAL)
    Selection Mode = 4 (IFCINTEGER)
    Shadow Casting = FALSE (IFCBOOLEAN)
    Show Framing = TRUE (IFCBOOLEAN)
    Show Framing in 3D = FALSE (IFCBOOLEAN)
    Show Framing in Section/Elevation = FALSE (IFCBOOLEAN)
    Show Projection = 0 (IFCINTEGER)
    Soffit Finish = "" (IFCLABEL)
    Soffit Material (Ends) = "Okarito Double" (IFCLABEL)
    Soffit Material (soffit_colour) = "Okarito Double" (IFCLABEL)
    Soffit Material (soffit_material) = "" (IFCLABEL)
    Soffit Materials Linked = TRUE (IFCBOOLEAN)
    Soffit Section Attributes = "GA - Cut Ceiling" (IFCLABEL)
    Soffit Section Attributes GUID = "03b6d67b-4bc5-4f65-9fb1-f4cd19acd7c0" (IFCLABEL)
    Soffit Section Background Pen = "Roofs- Fill backgrounds" (IFCLABEL)
    Soffit Section Fill = "Plaster" (IFCLABEL)
    Soffit Section Fill Pen = "Roof - Cut Fills" (IFCLABEL)
    Soffit Section Line Type = 1 (IFCINTEGER)
    Soffit Section Pen = "Roof - Cut Non-Structuralr" (IFCLABEL)
    Soffit Type (Ends) = "Boxed Fascia" (IFCLABEL)
    Soffit Type = "Flat" (IFCLABEL)
    Soffit View Attributes = "GA - Timber (Dressed)" (IFCLABEL)
    Soffit View Attributes GUID = "adca6221-b281-4eac-9cf7-28b4b883134c" (IFCLABEL)
    Soffit View Pen = "Objects - General" (IFCLABEL)
    Soffits = "Sloping 450" (IFCLABEL)
    Soffits Area = 3.298100000464907 (IFCREAL)
    Start Angles = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Story Sensitive Symbol = TRUE (IFCBOOLEAN)
    Tile Capping Material = "Ohakea" (IFCLABEL)
    USED FOR VERSIONING = "USED FOR VERSIONING" (IFCLABEL)
    Update Calculated Parameters = 2 (IFCINTEGER)
    Use Same Pens for All Views = TRUE (IFCBOOLEAN)
    Valley Flashing Finish = "" (IFCLABEL)
    Valley Flashing Material (valley_colour) = "Ohakea" (IFCLABEL)
    Valley Flashing Material (valley_material) = "" (IFCLABEL)
    Valley Flashing Type = "Internal" (IFCLABEL)
    Version Number = 2400 (IFCINTEGER)
    Wall Cladding Surface = "Paint - Titanium White" (IFCLABEL)
    Wall Cladding Type = 1 (IFCINTEGER)
    Zoom Buttons = 3 (IFCINTEGER)
    Zoom Level = 1 (IFCINTEGER)
    reset = FALSE (IFCBOOLEAN)
    type = "" (IFCLABEL)
  AC_Pset_CI_Tools_Roof_Covering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    3D Detail = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional information (gs_list_custom1) = "" (IFCLABEL)
    Additional information (gs_list_custom2) = "" (IFCLABEL)
    Additional information (gs_list_custom3) = "" (IFCLABEL)
    Additional information (gs_list_custom4) = "" (IFCLABEL)
    Additional information (gs_list_custom5) = "" (IFCLABEL)
    Apron Flashing Perpendicular = FALSE (IFCBOOLEAN)
    Apron Flashing Type = "Realistic" (IFCLABEL)
    Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Barge Board Cut Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Barge Board Finish = "" (IFCLABEL)
    Barge Board Material (barge_colour) = "Ohakea" (IFCLABEL)
    Barge Board Material (barge_material) = "" (IFCLABEL)
    Barge Flashing Material = "Ohakea" (IFCLABEL)
    Barge Flashing Type = "Flat Square" (IFCLABEL)
    Calculated Downpipe Number = 2 (IFCINTEGER)
    Calculated Soffit Area = 4.272067158462209 (IFCREAL)
    Calculated Verge Area = 4.891499999999997 (IFCREAL)
    Cladding Preset = "" (IFCLABEL)
    Cladding Type = "Ribbed" (IFCLABEL)
    Clicked Cell = 337 (IFCINTEGER)
    Cost = 0. (IFCREAL)
    Default Barge Edge = "Barge" (IFCLABEL)
    Default Gutter Edge = "Gutter" (IFCLABEL)
    Default Hip Edge = "Hip" (IFCLABEL)
    Default Ridge Edge = "Ridge" (IFCLABEL)
    Default Roof Style = "Custom" (IFCLABEL)
    Default Valley Edge = "Valley" (IFCLABEL)
    Downpipe 3D Attributes = "Custom" (IFCLABEL)
    Downpipe 3D Attributes GUID = "" (IFCLABEL)
    Downpipe 3D Pen = "General - General" (IFCLABEL)
    Downpipe Material = "Ohakea" (IFCLABEL)
    Downpipe Neck Angle = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Downpipe Profile = "Circular" (IFCLABEL)
    Downpipe Section Attributes = "GA - Cut Steel (Folded)" (IFCLABEL)
    Downpipe Section Attributes GUID = "F204B6BC-1D61-45A5-BE0D-C92FE6FE3644" (IFCLABEL)
    Downpipe Section Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Downpipe Section Fill = "Steel" (IFCLABEL)
    Downpipe Section Fill Pen = "Structural - Hatching" (IFCLABEL)
    Downpipe Section Line Type = 1 (IFCINTEGER)
    Downpipe Section Pen = "Structural - Cut Non-Construction" (IFCLABEL)
    Downpipe Toe Angle = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Downpipe has Brackets = TRUE (IFCBOOLEAN)
    Downpipes = "" (IFCLABEL)
    Downpipes Total Length = 0 (IFCINTEGER)
    Edge Boards = "" (IFCLABEL)
    End Angles = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    FM Inventory Number = "" (IFCLABEL)
    FM Production Year = "" (IFCLABEL)
    FM Serial Number = "" (IFCLABEL)
    FM Type = "Others" (IFCLABEL)
    FM Weight = 0. (IFCREAL)
    FM Weight Unit = "kg" (IFCLABEL)
    Fascia Board Finish = "" (IFCLABEL)
    Fascia Board Material (fascia_colour) = "Ohakea" (IFCLABEL)
    Fascia Board Material (fascia_material) = "" (IFCLABEL)
    Fascia Board Profile = "Timber" (IFCLABEL)
    Fascia Section Attributes = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Finial = FALSE (IFCBOOLEAN)
    Finials = 1 (IFCINTEGER)
    Flashing Echo = "" (IFCLABEL)
    Flashing Finish = "" (IFCLABEL)
    Flashing Material = "" (IFCLABEL)
    Flashing Section Attributes = "" (IFCLABEL)
    Flashings Preset (flashingPreset) = "" (IFCLABEL)
    Floor Plan Display = 0 (IFCINTEGER)
    Framing = "" (IFCLABEL)
    Framing Grade = "" (IFCLABEL)
    Framing Material (frame_colour) = "Wood - Oak Light" (IFCLABEL)
    Framing Material (framing_mat) = "" (IFCLABEL)
    Framing Treatment = "" (IFCLABEL)
    Freize Style = 1 (IFCINTEGER)
    Group Type = 25 (IFCINTEGER)
    Gutter Ends at Apron Flashing = TRUE (IFCBOOLEAN)
    Gutter Finish = "" (IFCLABEL)
    Gutter Material (gutter_colour) = "Ohakea" (IFCLABEL)
    Gutter Material (gutter_material) = "" (IFCLABEL)
    Gutter Pen = "Annotation Text - general" (IFCLABEL)
    Gutter Pen GUID = "ffb1c35b-2eba-406a-86b3-ba42b97a5538" (IFCLABEL)
    Gutter Pen Preset = "GA - Steel (Folded)" (IFCLABEL)
    Gutter Profile = "Brick Wall" (IFCLABEL)
    Gutter Section Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Gutter Section Fill = "Steel" (IFCLABEL)
    Gutter Section Fill Pen = "Structural - Hatching" (IFCLABEL)
    Gutter Section GUID = "f204b6bc-1d61-45a5-be0d-c92fe6fe3644" (IFCLABEL)
    Gutter Section Line Type = 1 (IFCINTEGER)
    Gutter Section Pen = "Structural - Cut Non-Construction" (IFCLABEL)
    Gutter Section Preset = "GA - Cut Steel (Folded)" (IFCLABEL)
    Gutter Type = "Square" (IFCLABEL)
    Holes = 1 (IFCINTEGER)
    Image Index = 1 (IFCINTEGER)
    Listing Option for Barge & Fascia = 1 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Menu (menu) = 1000 (IFCINTEGER)
    Note = "" (IFCLABEL)
    Page = 2 (IFCINTEGER)
    Part = 1 (IFCINTEGER)
    Property = 2 (IFCINTEGER)
    Purlin Type = "Timber" (IFCLABEL)
    Relation of Brackets to downpipe = "Align" (IFCLABEL)
    Ridge/Hip Flashing Matches Barge = FALSE (IFCBOOLEAN)
    Ridge/Hip Flashing Material (ridge_colour) = "Ohakea" (IFCLABEL)
    Ridge/Hip Flashing Material (ridge_material) = "" (IFCLABEL)
    Ridge/Hip Flashing Type = "Flat" (IFCLABEL)
    Roof Area ignoring Holes (m2) = 24.84227630128948 (IFCREAL)
    Roof Area with Holes Removed (m2) = 24.84227630128948 (IFCREAL)
    Selection Mode = 4 (IFCINTEGER)
    Shadow Casting = FALSE (IFCBOOLEAN)
    Show Framing = TRUE (IFCBOOLEAN)
    Show Framing in 3D = FALSE (IFCBOOLEAN)
    Show Framing in Section/Elevation = FALSE (IFCBOOLEAN)
    Show Projection = 0 (IFCINTEGER)
    Soffit Finish = "" (IFCLABEL)
    Soffit Material (Ends) = "Okarito Double" (IFCLABEL)
    Soffit Material (soffit_colour) = "Okarito Double" (IFCLABEL)
    Soffit Material (soffit_material) = "" (IFCLABEL)
    Soffit Materials Linked = TRUE (IFCBOOLEAN)
    Soffit Section Attributes = "GA - Cut Ceiling" (IFCLABEL)
    Soffit Section Attributes GUID = "03b6d67b-4bc5-4f65-9fb1-f4cd19acd7c0" (IFCLABEL)
    Soffit Section Background Pen = "Roofs- Fill backgrounds" (IFCLABEL)
    Soffit Section Fill = "Plaster" (IFCLABEL)
    Soffit Section Fill Pen = "Roof - Cut Fills" (IFCLABEL)
    Soffit Section Line Type = 1 (IFCINTEGER)
    Soffit Section Pen = "Roof - Cut Non-Structuralr" (IFCLABEL)
    Soffit Type (Ends) = "Boxed Fascia" (IFCLABEL)
    Soffit Type = "Flat" (IFCLABEL)
    Soffit View Attributes = "GA - Timber (Dressed)" (IFCLABEL)
    Soffit View Attributes GUID = "adca6221-b281-4eac-9cf7-28b4b883134c" (IFCLABEL)
    Soffit View Pen = "Objects - General" (IFCLABEL)
    Soffits = "Sloping 450" (IFCLABEL)
    Soffits Area = 4.072100000544482 (IFCREAL)
    Start Angles = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Story Sensitive Symbol = TRUE (IFCBOOLEAN)
    Tile Capping Material = "Ohakea" (IFCLABEL)
    USED FOR VERSIONING = "USED FOR VERSIONING" (IFCLABEL)
    Update Calculated Parameters = 2 (IFCINTEGER)
    Use Same Pens for All Views = TRUE (IFCBOOLEAN)
    Valley Flashing Finish = "" (IFCLABEL)
    Valley Flashing Material (valley_colour) = "Ohakea" (IFCLABEL)
    Valley Flashing Material (valley_material) = "" (IFCLABEL)
    Valley Flashing Type = "Internal" (IFCLABEL)
    Version Number = 2400 (IFCINTEGER)
    Wall Cladding Surface = "Paint - Titanium White" (IFCLABEL)
    Wall Cladding Type = 1 (IFCINTEGER)
    Zoom Buttons = 3 (IFCINTEGER)
    Zoom Level = 1 (IFCINTEGER)
    reset = FALSE (IFCBOOLEAN)
    type = "" (IFCLABEL)
  AC_Pset_CI_Tools_Roof_Covering | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    3D Detail = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Additional information (gs_list_custom1) = "" (IFCLABEL)
    Additional information (gs_list_custom2) = "" (IFCLABEL)
    Additional information (gs_list_custom3) = "" (IFCLABEL)
    Additional information (gs_list_custom4) = "" (IFCLABEL)
    Additional information (gs_list_custom5) = "" (IFCLABEL)
    Apron Flashing Perpendicular = FALSE (IFCBOOLEAN)
    Apron Flashing Type = "Realistic" (IFCLABEL)
    Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Barge Board Cut Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Barge Board Finish = "" (IFCLABEL)
    Barge Board Material (barge_colour) = "Ohakea" (IFCLABEL)
    Barge Board Material (barge_material) = "" (IFCLABEL)
    Barge Flashing Material = "Ohakea" (IFCLABEL)
    Barge Flashing Type = "Flat Square" (IFCLABEL)
    Calculated Downpipe Number = 2 (IFCINTEGER)
    Calculated Soffit Area = 4.272067158462209 (IFCREAL)
    Calculated Verge Area = 4.891499999999997 (IFCREAL)
    Cladding Preset = "" (IFCLABEL)
    Cladding Type = "Ribbed" (IFCLABEL)
    Clicked Cell = 337 (IFCINTEGER)
    Cost = 0. (IFCREAL)
    Default Barge Edge = "Barge" (IFCLABEL)
    Default Gutter Edge = "Gutter" (IFCLABEL)
    Default Hip Edge = "Hip" (IFCLABEL)
    Default Ridge Edge = "Ridge" (IFCLABEL)
    Default Roof Style = "Custom" (IFCLABEL)
    Default Valley Edge = "Valley" (IFCLABEL)
    Downpipe 3D Attributes = "Custom" (IFCLABEL)
    Downpipe 3D Attributes GUID = "" (IFCLABEL)
    Downpipe 3D Pen = "General - General" (IFCLABEL)
    Downpipe Material = "Ohakea" (IFCLABEL)
    Downpipe Neck Angle = 5. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Downpipe Profile = "Circular" (IFCLABEL)
    Downpipe Section Attributes = "GA - Cut Steel (Folded)" (IFCLABEL)
    Downpipe Section Attributes GUID = "F204B6BC-1D61-45A5-BE0D-C92FE6FE3644" (IFCLABEL)
    Downpipe Section Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Downpipe Section Fill = "Steel" (IFCLABEL)
    Downpipe Section Fill Pen = "Structural - Hatching" (IFCLABEL)
    Downpipe Section Line Type = 1 (IFCINTEGER)
    Downpipe Section Pen = "Structural - Cut Non-Construction" (IFCLABEL)
    Downpipe Toe Angle = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Downpipe has Brackets = TRUE (IFCBOOLEAN)
    Downpipes = "" (IFCLABEL)
    Downpipes Total Length = 0 (IFCINTEGER)
    Edge Boards = "" (IFCLABEL)
    End Angles = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    FM Inventory Number = "" (IFCLABEL)
    FM Production Year = "" (IFCLABEL)
    FM Serial Number = "" (IFCLABEL)
    FM Type = "Others" (IFCLABEL)
    FM Weight = 0. (IFCREAL)
    FM Weight Unit = "kg" (IFCLABEL)
    Fascia Board Finish = "" (IFCLABEL)
    Fascia Board Material (fascia_colour) = "Ohakea" (IFCLABEL)
    Fascia Board Material (fascia_material) = "" (IFCLABEL)
    Fascia Board Profile = "Timber" (IFCLABEL)
    Fascia Section Attributes = "" (IFCLABEL)
    Fill Type = "Background Fill" (IFCLABEL)
    Finial = FALSE (IFCBOOLEAN)
    Finials = 1 (IFCINTEGER)
    Flashing Echo = "" (IFCLABEL)
    Flashing Finish = "" (IFCLABEL)
    Flashing Material = "" (IFCLABEL)
    Flashing Section Attributes = "" (IFCLABEL)
    Flashings Preset (flashingPreset) = "" (IFCLABEL)
    Floor Plan Display = 0 (IFCINTEGER)
    Framing = "" (IFCLABEL)
    Framing Grade = "" (IFCLABEL)
    Framing Material (frame_colour) = "Wood - Oak Light" (IFCLABEL)
    Framing Material (framing_mat) = "" (IFCLABEL)
    Framing Treatment = "" (IFCLABEL)
    Freize Style = 1 (IFCINTEGER)
    Group Type = 25 (IFCINTEGER)
    Gutter Ends at Apron Flashing = TRUE (IFCBOOLEAN)
    Gutter Finish = "" (IFCLABEL)
    Gutter Material (gutter_colour) = "Ohakea" (IFCLABEL)
    Gutter Material (gutter_material) = "" (IFCLABEL)
    Gutter Pen = "Annotation Text - general" (IFCLABEL)
    Gutter Pen GUID = "ffb1c35b-2eba-406a-86b3-ba42b97a5538" (IFCLABEL)
    Gutter Pen Preset = "GA - Steel (Folded)" (IFCLABEL)
    Gutter Profile = "Brick Wall" (IFCLABEL)
    Gutter Section Background Pen = "Structural - fill backgrounds" (IFCLABEL)
    Gutter Section Fill = "Steel" (IFCLABEL)
    Gutter Section Fill Pen = "Structural - Hatching" (IFCLABEL)
    Gutter Section GUID = "f204b6bc-1d61-45a5-be0d-c92fe6fe3644" (IFCLABEL)
    Gutter Section Line Type = 1 (IFCINTEGER)
    Gutter Section Pen = "Structural - Cut Non-Construction" (IFCLABEL)
    Gutter Section Preset = "GA - Cut Steel (Folded)" (IFCLABEL)
    Gutter Type = "Square" (IFCLABEL)
    Holes = 1 (IFCINTEGER)
    Image Index = 1 (IFCINTEGER)
    Listing Option for Barge & Fascia = 1 (IFCINTEGER)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Menu (menu) = 1000 (IFCINTEGER)
    Note = "" (IFCLABEL)
    Page = 2 (IFCINTEGER)
    Part = 1 (IFCINTEGER)
    Property = 2 (IFCINTEGER)
    Purlin Type = "Timber" (IFCLABEL)
    Relation of Brackets to downpipe = "Align" (IFCLABEL)
    Ridge/Hip Flashing Matches Barge = FALSE (IFCBOOLEAN)
    Ridge/Hip Flashing Material (ridge_colour) = "Ohakea" (IFCLABEL)
    Ridge/Hip Flashing Material (ridge_material) = "" (IFCLABEL)
    Ridge/Hip Flashing Type = "Flat" (IFCLABEL)
    Roof Area ignoring Holes (m2) = 17.19849897691962 (IFCREAL)
    Roof Area with Holes Removed (m2) = 17.19849897691962 (IFCREAL)
    Selection Mode = 4 (IFCINTEGER)
    Shadow Casting = FALSE (IFCBOOLEAN)
    Show Framing = TRUE (IFCBOOLEAN)
    Show Framing in 3D = FALSE (IFCBOOLEAN)
    Show Framing in Section/Elevation = FALSE (IFCBOOLEAN)
    Show Projection = 0 (IFCINTEGER)
    Soffit Finish = "" (IFCLABEL)
    Soffit Material (Ends) = "Okarito Double" (IFCLABEL)
    Soffit Material (soffit_colour) = "Okarito Double" (IFCLABEL)
    Soffit Material (soffit_material) = "" (IFCLABEL)
    Soffit Materials Linked = TRUE (IFCBOOLEAN)
    Soffit Section Attributes = "GA - Cut Ceiling" (IFCLABEL)
    Soffit Section Attributes GUID = "03b6d67b-4bc5-4f65-9fb1-f4cd19acd7c0" (IFCLABEL)
    Soffit Section Background Pen = "Roofs- Fill backgrounds" (IFCLABEL)
    Soffit Section Fill = "Plaster" (IFCLABEL)
    Soffit Section Fill Pen = "Roof - Cut Fills" (IFCLABEL)
    Soffit Section Line Type = 1 (IFCINTEGER)
    Soffit Section Pen = "Roof - Cut Non-Structuralr" (IFCLABEL)
    Soffit Type (Ends) = "Boxed Fascia" (IFCLABEL)
    Soffit Type = "Flat" (IFCLABEL)
    Soffit View Attributes = "GA - Timber (Dressed)" (IFCLABEL)
    Soffit View Attributes GUID = "adca6221-b281-4eac-9cf7-28b4b883134c" (IFCLABEL)
    Soffit View Pen = "Objects - General" (IFCLABEL)
    Soffits = "Sloping 450" (IFCLABEL)
    Soffits Area = 3.29810000042934 (IFCREAL)
    Start Angles = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Story Sensitive Symbol = TRUE (IFCBOOLEAN)
    Tile Capping Material = "Ohakea" (IFCLABEL)
    USED FOR VERSIONING = "USED FOR VERSIONING" (IFCLABEL)
    Update Calculated Parameters = 2 (IFCINTEGER)
    Use Same Pens for All Views = TRUE (IFCBOOLEAN)
    Valley Flashing Finish = "" (IFCLABEL)
    Valley Flashing Material (valley_colour) = "Ohakea" (IFCLABEL)
    Valley Flashing Material (valley_material) = "" (IFCLABEL)
    Valley Flashing Type = "Internal" (IFCLABEL)
    Version Number = 2400 (IFCINTEGER)
    Wall Cladding Surface = "Paint - Titanium White" (IFCLABEL)
    Wall Cladding Type = 1 (IFCINTEGER)
    Zoom Buttons = 3 (IFCINTEGER)
    Zoom Level = 1 (IFCINTEGER)
    reset = FALSE (IFCBOOLEAN)
    type = "" (IFCLABEL)
  AC_Equantity_CI_Tools_Roof_Covering | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Apron Flashing Depth = 12. [MILLI METRE]
    Apron Flashing Height = 200. [MILLI METRE]
    Apron Flashing Height around Holes = 20. [MILLI METRE]
    Apron Flashing Thickness = 5. [MILLI METRE]
    Apron Flashing Width = 150. [MILLI METRE]
    Aprons Total Length = 0. [MILLI METRE]
    Barge Board Extension = 100. [MILLI METRE]
    Barge Flashing Cap = 0. [MILLI METRE]
    Barge Flashing Cap Depth = 0. [MILLI METRE]
    Barge Flashing Depth = 12. [MILLI METRE]
    Barge Flashing Drop = 70. [MILLI METRE]
    Barge Flashing Thickness = 3. [MILLI METRE]
    Barge Flashing Width = 150. [MILLI METRE]
    Barge Total Length = 0. [MILLI METRE]
    Batten Depth = 70. [MILLI METRE]
    Batten Width = 45. [MILLI METRE]
    Bottom Level = -2933.748127855773 [MILLI METRE]
    Calculated Apron Length = 0. [MILLI METRE]
    Calculated Barge Length = 12960.03722867854 [MILLI METRE]
    Calculated Fascia Length = 9170.000000000005 [MILLI METRE]
    Calculated Gutter Length = 9170.000000000005 [MILLI METRE]
    Calculated Hip Length = 0. [MILLI METRE]
    Calculated Ridge Length = 4585.000000000002 [MILLI METRE]
    Calculated Valley Length = 0. [MILLI METRE]
    Cladding Overhang at Barges = 0. [MILLI METRE]
    Cladding Overhang at Fascias = 40. [MILLI METRE]
    Cladding Overhang at Valley = 0. [MILLI METRE]
    Cladding Rib Height = 36. [MILLI METRE]
    Cladding Rib Spacing = 150. [MILLI METRE]
    Cladding Rib Width at Base = 50. [MILLI METRE]
    Cladding Rib Width at Top = 0. [MILLI METRE]
    Cladding Tile Height = 20. [MILLI METRE]
    Cladding Tile Length = 350. [MILLI METRE]
    Cladding Tile Thickness = 2. [MILLI METRE]
    Cladding Tile Width = 300. [MILLI METRE]
    Downpipe Bracket Spacing = 800. [MILLI METRE]
    Downpipe Depth = 50. [MILLI METRE]
    Downpipe Diameter = 80. [MILLI METRE]
    Downpipe Dropper Length = 200. [MILLI METRE]
    Downpipe Toe Length = 0. [MILLI METRE]
    Downpipe Width = 80. [MILLI METRE]
    Dowpipe Extension to Wall = 55. [MILLI METRE]
    Eaves Total Length = 9900.000001303855 [MILLI METRE]
    Extend beyond barge boards = 0. [MILLI METRE]
    Fascia Offset = 20. [MILLI METRE]
    Fascias Total Length = 9900.000001303855 [MILLI METRE]
    Finial Thickness = 90. [MILLI METRE]
    Framing Allowance = 0. [MILLI METRE]
    Framing Spacing = 0. [MILLI METRE]
    Framing Thickness = 0. [MILLI METRE]
    Framing Width = 0. [MILLI METRE]
    Freize Beam Thickness = 70. [MILLI METRE]
    Freize Beam Width = 45. [MILLI METRE]
    Freize Drop below Apex = 900. [MILLI METRE]
    Freize Height = 450. [MILLI METRE]
    Freize Post Extension = 50. [MILLI METRE]
    Freize Post Spacing = 150. [MILLI METRE]
    Freize Post Thickness = 40. [MILLI METRE]
    Freize Post Width = 40. [MILLI METRE]
    Frieze Inset = 0. [MILLI METRE]
    Gables Total Length = 0. [MILLI METRE]
    Gutter Depth (back face) = 120. [MILLI METRE]
    Gutter Drop below Fascia = 0. [MILLI METRE]
    Gutter End Extension = 0. [MILLI METRE]
    Gutter Height (front face) = 82. [MILLI METRE]
    Gutter Lip = 12. [MILLI METRE]
    Gutter Width = 120. [MILLI METRE]
    Gutters Total Length = 9900.000001303855 [MILLI METRE]
    Hips Total Length = 11736.3754364881 [MILLI METRE]
    Offset from Fascia Edge = 20. [MILLI METRE]
    Origin X = 0. [MILLI METRE]
    Origin Y = 0. [MILLI METRE]
    Purlin Depth = 45. [MILLI METRE]
    Purlin Spacing = 900. [MILLI METRE]
    Purlin Width = 90. [MILLI METRE]
    Ridge/Hip Flashing Cap = 0. [MILLI METRE]
    Ridge/Hip Flashing Depth = 12. [MILLI METRE]
    Ridge/Hip Flashing Thickness = 3. [MILLI METRE]
    Ridge/Hip Flashing Width = 150. [MILLI METRE]
    Ridges Total Length = 1800.000000745058 [MILLI METRE]
    Roof Length along Rafters = 4288.484123023038 [MILLI METRE]
    Roof Width along Purlins = 9900.000001303855 [MILLI METRE]
    Soffit Default Width (eave_width) = 450. [MILLI METRE]
    Soffit Default Width (soffit_width) = 430. [MILLI METRE]
    Soffit Thickness = 4.5 [MILLI METRE]
    Tile Capping Length = 250. [MILLI METRE]
    Tile Capping Thickness = 12. [MILLI METRE]
    Tile Capping Width = 300. [MILLI METRE]
    Top Level = 1183.307979737147 [MILLI METRE]
    Valley Flashing Depth = 25. [MILLI METRE]
    Valley Flashing Thickness = 2. [MILLI METRE]
    Valley Flashing Width = 150. [MILLI METRE]
    Valleys Total Length = 0. [MILLI METRE]
  AC_Equantity_CI_Tools_Roof_Covering | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Apron Flashing Depth = 12. [MILLI METRE]
    Apron Flashing Height = 200. [MILLI METRE]
    Apron Flashing Height around Holes = 20. [MILLI METRE]
    Apron Flashing Thickness = 5. [MILLI METRE]
    Apron Flashing Width = 150. [MILLI METRE]
    Aprons Total Length = 0. [MILLI METRE]
    Barge Board Extension = 100. [MILLI METRE]
    Barge Flashing Cap = 0. [MILLI METRE]
    Barge Flashing Cap Depth = 0. [MILLI METRE]
    Barge Flashing Depth = 12. [MILLI METRE]
    Barge Flashing Drop = 70. [MILLI METRE]
    Barge Flashing Thickness = 3. [MILLI METRE]
    Barge Flashing Width = 150. [MILLI METRE]
    Barge Total Length = 0. [MILLI METRE]
    Batten Depth = 70. [MILLI METRE]
    Batten Width = 45. [MILLI METRE]
    Bottom Level = -93.65211542254833 [MILLI METRE]
    Calculated Apron Length = 0. [MILLI METRE]
    Calculated Barge Length = 12960.03722867854 [MILLI METRE]
    Calculated Fascia Length = 9170.000000000005 [MILLI METRE]
    Calculated Gutter Length = 9170.000000000005 [MILLI METRE]
    Calculated Hip Length = 0. [MILLI METRE]
    Calculated Ridge Length = 4585.000000000002 [MILLI METRE]
    Calculated Valley Length = 0. [MILLI METRE]
    Cladding Overhang at Barges = 0. [MILLI METRE]
    Cladding Overhang at Fascias = 40. [MILLI METRE]
    Cladding Overhang at Valley = 0. [MILLI METRE]
    Cladding Rib Height = 36. [MILLI METRE]
    Cladding Rib Spacing = 150. [MILLI METRE]
    Cladding Rib Width at Base = 50. [MILLI METRE]
    Cladding Rib Width at Top = 0. [MILLI METRE]
    Cladding Tile Height = 20. [MILLI METRE]
    Cladding Tile Length = 350. [MILLI METRE]
    Cladding Tile Thickness = 2. [MILLI METRE]
    Cladding Tile Width = 300. [MILLI METRE]
    Downpipe Bracket Spacing = 800. [MILLI METRE]
    Downpipe Depth = 50. [MILLI METRE]
    Downpipe Diameter = 80. [MILLI METRE]
    Downpipe Dropper Length = 200. [MILLI METRE]
    Downpipe Toe Length = 0. [MILLI METRE]
    Downpipe Width = 80. [MILLI METRE]
    Dowpipe Extension to Wall = 55. [MILLI METRE]
    Eaves Total Length = 8100.000001066793 [MILLI METRE]
    Extend beyond barge boards = 0. [MILLI METRE]
    Fascia Offset = 20. [MILLI METRE]
    Fascias Total Length = 8100.000001066793 [MILLI METRE]
    Finial Thickness = 90. [MILLI METRE]
    Framing Allowance = 0. [MILLI METRE]
    Framing Spacing = 0. [MILLI METRE]
    Framing Thickness = 0. [MILLI METRE]
    Framing Width = 0. [MILLI METRE]
    Freize Beam Thickness = 70. [MILLI METRE]
    Freize Beam Width = 45. [MILLI METRE]
    Freize Drop below Apex = 900. [MILLI METRE]
    Freize Height = 450. [MILLI METRE]
    Freize Post Extension = 50. [MILLI METRE]
    Freize Post Spacing = 150. [MILLI METRE]
    Freize Post Thickness = 40. [MILLI METRE]
    Freize Post Width = 40. [MILLI METRE]
    Frieze Inset = 0. [MILLI METRE]
    Gables Total Length = 0. [MILLI METRE]
    Gutter Depth (back face) = 120. [MILLI METRE]
    Gutter Drop below Fascia = 0. [MILLI METRE]
    Gutter End Extension = 0. [MILLI METRE]
    Gutter Height (front face) = 82. [MILLI METRE]
    Gutter Lip = 12. [MILLI METRE]
    Gutter Width = 120. [MILLI METRE]
    Gutters Total Length = 8100.000001066793 [MILLI METRE]
    Hips Total Length = 11736.37543612121 [MILLI METRE]
    Offset from Fascia Edge = 20. [MILLI METRE]
    Origin X = 0. [MILLI METRE]
    Origin Y = 0. [MILLI METRE]
    Purlin Depth = 45. [MILLI METRE]
    Purlin Spacing = 900. [MILLI METRE]
    Purlin Width = 90. [MILLI METRE]
    Ridge/Hip Flashing Cap = 0. [MILLI METRE]
    Ridge/Hip Flashing Depth = 12. [MILLI METRE]
    Ridge/Hip Flashing Thickness = 3. [MILLI METRE]
    Ridge/Hip Flashing Width = 150. [MILLI METRE]
    Ridges Total Length = 0. [MILLI METRE]
    Roof Length along Rafters = 4288.484122527294 [MILLI METRE]
    Roof Width along Purlins = 8100.000001066793 [MILLI METRE]
    Soffit Default Width (eave_width) = 450. [MILLI METRE]
    Soffit Default Width (soffit_width) = 430. [MILLI METRE]
    Soffit Thickness = 4.5 [MILLI METRE]
    Tile Capping Length = 250. [MILLI METRE]
    Tile Capping Thickness = 12. [MILLI METRE]
    Tile Capping Width = 300. [MILLI METRE]
    Top Level = 1183.307979748243 [MILLI METRE]
    Valley Flashing Depth = 25. [MILLI METRE]
    Valley Flashing Thickness = 2. [MILLI METRE]
    Valley Flashing Width = 150. [MILLI METRE]
    Valleys Total Length = 0. [MILLI METRE]
  AC_Equantity_CI_Tools_Roof_Covering | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Apron Flashing Depth = 12. [MILLI METRE]
    Apron Flashing Height = 200. [MILLI METRE]
    Apron Flashing Height around Holes = 20. [MILLI METRE]
    Apron Flashing Thickness = 5. [MILLI METRE]
    Apron Flashing Width = 150. [MILLI METRE]
    Aprons Total Length = 0. [MILLI METRE]
    Barge Board Extension = 100. [MILLI METRE]
    Barge Flashing Cap = 0. [MILLI METRE]
    Barge Flashing Cap Depth = 0. [MILLI METRE]
    Barge Flashing Depth = 12. [MILLI METRE]
    Barge Flashing Drop = 70. [MILLI METRE]
    Barge Flashing Thickness = 3. [MILLI METRE]
    Barge Flashing Width = 150. [MILLI METRE]
    Barge Total Length = 0. [MILLI METRE]
    Batten Depth = 70. [MILLI METRE]
    Batten Width = 45. [MILLI METRE]
    Bottom Level = -2933.748127855773 [MILLI METRE]
    Calculated Apron Length = 0. [MILLI METRE]
    Calculated Barge Length = 12960.03722867854 [MILLI METRE]
    Calculated Fascia Length = 9170.000000000005 [MILLI METRE]
    Calculated Gutter Length = 9170.000000000005 [MILLI METRE]
    Calculated Hip Length = 0. [MILLI METRE]
    Calculated Ridge Length = 4585.000000000002 [MILLI METRE]
    Calculated Valley Length = 0. [MILLI METRE]
    Cladding Overhang at Barges = 0. [MILLI METRE]
    Cladding Overhang at Fascias = 40. [MILLI METRE]
    Cladding Overhang at Valley = 0. [MILLI METRE]
    Cladding Rib Height = 36. [MILLI METRE]
    Cladding Rib Spacing = 150. [MILLI METRE]
    Cladding Rib Width at Base = 50. [MILLI METRE]
    Cladding Rib Width at Top = 0. [MILLI METRE]
    Cladding Tile Height = 20. [MILLI METRE]
    Cladding Tile Length = 350. [MILLI METRE]
    Cladding Tile Thickness = 2. [MILLI METRE]
    Cladding Tile Width = 300. [MILLI METRE]
    Downpipe Bracket Spacing = 800. [MILLI METRE]
    Downpipe Depth = 50. [MILLI METRE]
    Downpipe Diameter = 80. [MILLI METRE]
    Downpipe Dropper Length = 200. [MILLI METRE]
    Downpipe Toe Length = 0. [MILLI METRE]
    Downpipe Width = 80. [MILLI METRE]
    Dowpipe Extension to Wall = 55. [MILLI METRE]
    Eaves Total Length = 9900.000001303855 [MILLI METRE]
    Extend beyond barge boards = 0. [MILLI METRE]
    Fascia Offset = 20. [MILLI METRE]
    Fascias Total Length = 9900.000001303855 [MILLI METRE]
    Finial Thickness = 90. [MILLI METRE]
    Framing Allowance = 0. [MILLI METRE]
    Framing Spacing = 0. [MILLI METRE]
    Framing Thickness = 0. [MILLI METRE]
    Framing Width = 0. [MILLI METRE]
    Freize Beam Thickness = 70. [MILLI METRE]
    Freize Beam Width = 45. [MILLI METRE]
    Freize Drop below Apex = 900. [MILLI METRE]
    Freize Height = 450. [MILLI METRE]
    Freize Post Extension = 50. [MILLI METRE]
    Freize Post Spacing = 150. [MILLI METRE]
    Freize Post Thickness = 40. [MILLI METRE]
    Freize Post Width = 40. [MILLI METRE]
    Frieze Inset = 0. [MILLI METRE]
    Gables Total Length = 0. [MILLI METRE]
    Gutter Depth (back face) = 120. [MILLI METRE]
    Gutter Drop below Fascia = 0. [MILLI METRE]
    Gutter End Extension = 0. [MILLI METRE]
    Gutter Height (front face) = 82. [MILLI METRE]
    Gutter Lip = 12. [MILLI METRE]
    Gutter Width = 120. [MILLI METRE]
    Gutters Total Length = 9900.000001303855 [MILLI METRE]
    Hips Total Length = 11736.3754346418 [MILLI METRE]
    Offset from Fascia Edge = 20. [MILLI METRE]
    Origin X = 0. [MILLI METRE]
    Origin Y = 0. [MILLI METRE]
    Purlin Depth = 45. [MILLI METRE]
    Purlin Spacing = 900. [MILLI METRE]
    Purlin Width = 90. [MILLI METRE]
    Ridge/Hip Flashing Cap = 0. [MILLI METRE]
    Ridge/Hip Flashing Depth = 12. [MILLI METRE]
    Ridge/Hip Flashing Thickness = 3. [MILLI METRE]
    Ridge/Hip Flashing Width = 150. [MILLI METRE]
    Ridges Total Length = 1800.000000745058 [MILLI METRE]
    Roof Length along Rafters = 4288.484121747359 [MILLI METRE]
    Roof Width along Purlins = 9900.000001303855 [MILLI METRE]
    Soffit Default Width (eave_width) = 450. [MILLI METRE]
    Soffit Default Width (soffit_width) = 430. [MILLI METRE]
    Soffit Thickness = 4.5 [MILLI METRE]
    Tile Capping Length = 250. [MILLI METRE]
    Tile Capping Thickness = 12. [MILLI METRE]
    Tile Capping Width = 300. [MILLI METRE]
    Top Level = 1183.307979513713 [MILLI METRE]
    Valley Flashing Depth = 25. [MILLI METRE]
    Valley Flashing Thickness = 2. [MILLI METRE]
    Valley Flashing Width = 150. [MILLI METRE]
    Valleys Total Length = 0. [MILLI METRE]
  AC_Equantity_CI_Tools_Roof_Covering | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Apron Flashing Depth = 12. [MILLI METRE]
    Apron Flashing Height = 200. [MILLI METRE]
    Apron Flashing Height around Holes = 20. [MILLI METRE]
    Apron Flashing Thickness = 5. [MILLI METRE]
    Apron Flashing Width = 150. [MILLI METRE]
    Aprons Total Length = 0. [MILLI METRE]
    Barge Board Extension = 100. [MILLI METRE]
    Barge Flashing Cap = 0. [MILLI METRE]
    Barge Flashing Cap Depth = 0. [MILLI METRE]
    Barge Flashing Depth = 12. [MILLI METRE]
    Barge Flashing Drop = 70. [MILLI METRE]
    Barge Flashing Thickness = 3. [MILLI METRE]
    Barge Flashing Width = 150. [MILLI METRE]
    Barge Total Length = 0. [MILLI METRE]
    Batten Depth = 70. [MILLI METRE]
    Batten Width = 45. [MILLI METRE]
    Bottom Level = -93.65211542254819 [MILLI METRE]
    Calculated Apron Length = 0. [MILLI METRE]
    Calculated Barge Length = 12960.03722867854 [MILLI METRE]
    Calculated Fascia Length = 9170.000000000005 [MILLI METRE]
    Calculated Gutter Length = 9170.000000000005 [MILLI METRE]
    Calculated Hip Length = 0. [MILLI METRE]
    Calculated Ridge Length = 4585.000000000002 [MILLI METRE]
    Calculated Valley Length = 0. [MILLI METRE]
    Cladding Overhang at Barges = 0. [MILLI METRE]
    Cladding Overhang at Fascias = 40. [MILLI METRE]
    Cladding Overhang at Valley = 0. [MILLI METRE]
    Cladding Rib Height = 36. [MILLI METRE]
    Cladding Rib Spacing = 150. [MILLI METRE]
    Cladding Rib Width at Base = 50. [MILLI METRE]
    Cladding Rib Width at Top = 0. [MILLI METRE]
    Cladding Tile Height = 20. [MILLI METRE]
    Cladding Tile Length = 350. [MILLI METRE]
    Cladding Tile Thickness = 2. [MILLI METRE]
    Cladding Tile Width = 300. [MILLI METRE]
    Downpipe Bracket Spacing = 800. [MILLI METRE]
    Downpipe Depth = 50. [MILLI METRE]
    Downpipe Diameter = 80. [MILLI METRE]
    Downpipe Dropper Length = 200. [MILLI METRE]
    Downpipe Toe Length = 0. [MILLI METRE]
    Downpipe Width = 80. [MILLI METRE]
    Dowpipe Extension to Wall = 55. [MILLI METRE]
    Eaves Total Length = 8100.000001066789 [MILLI METRE]
    Extend beyond barge boards = 0. [MILLI METRE]
    Fascia Offset = 20. [MILLI METRE]
    Fascias Total Length = 8100.000001066789 [MILLI METRE]
    Finial Thickness = 90. [MILLI METRE]
    Framing Allowance = 0. [MILLI METRE]
    Framing Spacing = 0. [MILLI METRE]
    Framing Thickness = 0. [MILLI METRE]
    Framing Width = 0. [MILLI METRE]
    Freize Beam Thickness = 70. [MILLI METRE]
    Freize Beam Width = 45. [MILLI METRE]
    Freize Drop below Apex = 900. [MILLI METRE]
    Freize Height = 450. [MILLI METRE]
    Freize Post Extension = 50. [MILLI METRE]
    Freize Post Spacing = 150. [MILLI METRE]
    Freize Post Thickness = 40. [MILLI METRE]
    Freize Post Width = 40. [MILLI METRE]
    Frieze Inset = 0. [MILLI METRE]
    Gables Total Length = 0. [MILLI METRE]
    Gutter Depth (back face) = 120. [MILLI METRE]
    Gutter Drop below Fascia = 0. [MILLI METRE]
    Gutter End Extension = 0. [MILLI METRE]
    Gutter Height (front face) = 82. [MILLI METRE]
    Gutter Lip = 12. [MILLI METRE]
    Gutter Width = 120. [MILLI METRE]
    Gutters Total Length = 8100.000001066789 [MILLI METRE]
    Hips Total Length = 11736.37543493899 [MILLI METRE]
    Offset from Fascia Edge = 20. [MILLI METRE]
    Origin X = 0. [MILLI METRE]
    Origin Y = 0. [MILLI METRE]
    Purlin Depth = 45. [MILLI METRE]
    Purlin Spacing = 900. [MILLI METRE]
    Purlin Width = 90. [MILLI METRE]
    Ridge/Hip Flashing Cap = 0. [MILLI METRE]
    Ridge/Hip Flashing Depth = 12. [MILLI METRE]
    Ridge/Hip Flashing Thickness = 3. [MILLI METRE]
    Ridge/Hip Flashing Width = 150. [MILLI METRE]
    Ridges Total Length = 0. [MILLI METRE]
    Roof Length along Rafters = 4288.484121710458 [MILLI METRE]
    Roof Width along Purlins = 8100.000001066789 [MILLI METRE]
    Soffit Default Width (eave_width) = 450. [MILLI METRE]
    Soffit Default Width (soffit_width) = 430. [MILLI METRE]
    Soffit Thickness = 4.5 [MILLI METRE]
    Tile Capping Length = 250. [MILLI METRE]
    Tile Capping Thickness = 12. [MILLI METRE]
    Tile Capping Width = 300. [MILLI METRE]
    Top Level = 1183.307979502616 [MILLI METRE]
    Valley Flashing Depth = 25. [MILLI METRE]
    Valley Flashing Thickness = 2. [MILLI METRE]
    Valley Flashing Width = 150. [MILLI METRE]
    Valleys Total Length = 0. [MILLI METRE]