IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "Prueba_Multicapa_Visor.ifc"
Time stamp: "2025-12-11T17:57:28+01:00"
Preprocessor: "IfcOpenShell 0.8.5-alpha251202"
Originating system: "Bonsai 0.8.5-alpha251202-f50bbe8"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 3 elements
          1 x IFCWINDOW | type IFCWINDOWTYPE "Window_Type 1" | SINGLE_PANEL | names: "Window"
          1 x IFCDOOR | type IFCDOORTYPE "Door_Type 1" | SINGLE_SWING_LEFT | names: "Door"
          1 x IFCWALL | type IFCWALLTYPE "Muro compuesto_1" | names: "Wall" | material: layers ("Gris_MAT" 0.0149999996647239, "Rojo_MAT" 0.119999997317791, "Amarillo_MAT" 0.0799999982118607, "Azul_MAT" 0.100000001490116) | property sets: EPset_Parametric

Types
  IFCWINDOWTYPE "Window_Type 1" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCDOORTYPE "Door_Type 1" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: BBIM_Door
  IFCWALLTYPE "Muro compuesto_1" | SOLIDWALL | 1 occurrence | material: layers ("Gris_MAT" 0.0149999996647239, "Rojo_MAT" 0.119999997317791, "Amarillo_MAT" 0.0799999982118607, "Azul_MAT" 0.100000001490116) | property sets: EPset_Parametric

Property sets
  EPset_Parametric | properties | on 1 object (1 IFCWALL)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS2" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 1.2000000476837158, "overall_width": 1.2000000476837158, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2.200000047683716, "overall_width": 0.8999999761581421, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.0, "casing_thickness": 0.07500000298023224, "casing_depth": 0.004999999888241291, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)