IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
File name: "Test_Material_Parameter_optimized.ifc (Edited by Simplebim 8.2 SR1)"
Time stamp: "2021-01-12T12:07:53"
Organization: "mh-software"
Preprocessor: "mh-IfcEngine 2020"
Originating system: "mh-Bim 6.7 (Solibri IFC Optimizer)"
Authorization: "ZWP Ingenieur AG"
Application: "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist"
Application: "mh-Bim" version "6.0" identifier "mh-software GmbH" by Organization "mh-Bim"

People and organizations
  Person (no name given) of Organization "Simplebim"
  Person "mh" of Organization "ZWP Ingenieur AG"
  Owner history of Person (no name given) of Organization "Simplebim" | application "Not Defined" version "Not Defined" identifier "Not Defined" by Organization "Datacubist" | change ADDED | created 1610988605 (2021-01-18T16:50:05Z)
  Owner history of Person "mh" of Organization "ZWP Ingenieur AG" | application "mh-Bim" version "6.0" identifier "mh-software GmbH" by Organization "mh-Bim" | change ADDED | created 1610449673 (2021-01-12T11:07:53Z)

Units
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: SQUARE_METRE
  LENGTHUNIT: MILLI METRE
  MASSUNIT: KILO GRAM
  POWERUNIT: WATT
  PRESSUREUNIT: KILO PASCAL
  FORCEUNIT: KILO NEWTON
  ELECTRICVOLTAGEUNIT: VOLT
  ELECTRICCURRENTUNIT: AMPERE
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  TIMEUNIT: SECOND
  VOLUMEUNIT: CUBIC_METRE
  LINEARVELOCITYUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  THERMALTRANSMITTANCEUNIT: derived
  SOUNDPRESSUREUNIT: derived

Spatial structure
IFCPROJECT "Projekt" | phase "LP2"
  IFCSITE "Liegenschaft" | latitude 51° 28′ 52.763671″ | longitude 7° 12′ 54.577331″ | elevation above sea level 2038.6 | postal address: "Haus des Wissens"
    IFCBUILDING "AB"
      IFCBUILDINGSTOREY "1. Untergeschoss" | elevation -3850.
        contains 446 elements
          98 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP , DN 50 <Rc>" | RIGIDSEGMENT | names: "36", "39", "1285" (+95 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Allgemein, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, Pset_PipeSegmentTypeCommon, mhEigenschaften-ifcParameter
          1 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (1800/1450/900)" | USERDEFINED | names: "3234" | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_SpaceHeaterTypeCommon
          2 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (1000/30/1800)" | USERDEFINED | names: "3249", "3258" | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_SpaceHeaterTypeCommon
          2 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (1000/30/900)" | USERDEFINED | names: "3259", "3269" | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_SpaceHeaterTypeCommon
          8 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 15 <Rc>" | RIGIDSEGMENT | names: "3260", "3261", "3264" (+5 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Rohr, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, Pset_PipeSegmentTypeCommon, mhEigenschaften-Allgemein
          1 x IFCVALVE | type IFCVALVETYPE "- - DN 0" | REGULATING | names: "Thermostatventil" | property sets: Pset_ValveTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-Ventil, mhEigenschaften-Ergebnisse
          1 x IFCVALVE | type IFCVALVETYPE "- - DN 0" | USERDEFINED | names: "Rücklaufverschraubung" | property sets: Pset_ValveTypeCommon, mhEigenschaften-Ventil, mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein
          1 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (4000/1800/2000)" | USERDEFINED | names: "3273" | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, Pset_SpaceHeaterTypeCommon, mhEigenschaften-Allgemein
          2 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 1500 <Rc>" | RIGIDSEGMENT | names: "3278", "3281" | property sets: mhEigenschaften-Drücke, mhEigenschaften-Rohr, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-ifcParameter, mhEigenschaften-Allgemein
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Boden, DN 1500 <Rc>" | USERDEFINED | names: "3279", "3282" | property sets: Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein
          6 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 15 <Rc>" | BEND | names: "3284", "3285", "5265" (+3 more) | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Bogen, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, mhEigenschaften-ifcParameter
          10 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 1880 <Rc>" | RIGIDSEGMENT | names: "3311", "3314", "3317" (+7 more) | property sets: mhEigenschaften-Drücke, Pset_PipeSegmentTypeCommon, mhEigenschaften-Rohr, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-ifcParameter
          10 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Boden, DN 1880 <Rc>" | USERDEFINED | names: "3312", "3315", "3318" (+7 more) | property sets: Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein
          3 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (2870/1020/920)" | USERDEFINED | names: "3345", "3351", "3357" | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, Pset_SpaceHeaterTypeCommon, mhEigenschaften-Allgemein
          5 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (1000/30/2870)" | USERDEFINED | names: "3346", "3348", "3352" (+2 more) | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_SpaceHeaterTypeCommon
          6 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (1000/30/920)" | USERDEFINED | names: "3349", "3350", "3354" (+3 more) | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, Pset_SpaceHeaterTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-Diverses
          1 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (3000/2000/1000)" | USERDEFINED | names: "3362" | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, Pset_SpaceHeaterTypeCommon, mhEigenschaften-Diverses
          39 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 50 <Rc>" | RIGIDSEGMENT | names: "3365", "3366", "3368" (+36 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Rohr, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          75 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 90°, DN 50 <Rc>" | BEND | names: "3673", "3676", "3678" (+72 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Bogen, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          2 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (4000/500/1000)" | USERDEFINED | names: "4414", "4415" | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, Pset_SpaceHeaterTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-Allgemein
          76 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" | RIGIDSEGMENT | names: "4471", "4478", "4492" (+73 more) | property sets: mhEigenschaften-Drücke, Pset_PipeSegmentTypeCommon, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, mhEigenschaften-Rohr
          46 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 100 <Rc>" | BEND | names: "4553", "4555", "4556" (+43 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter, mhEigenschaften-Allgemein, mhEigenschaften-Bogen
          27 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 50 <Rc>" | BEND | names: "4564", "4567", "8212" (+24 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter, mhEigenschaften-Bogen
          10 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 100/100/100 <Rc>" | JUNCTION | names: "4955", "4958", "7568" (+7 more) | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter, mhEigenschaften-Allgemein
          4 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "8263", "8267", "8427" (+1 more) | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter, mhEigenschaften-Allgemein
          7 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "8421", "8424", "8434" (+4 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Standard" | object type "NOTDEFINED" | names: "3" | property sets: Pset_BuildingElementProxyCommon, mhEigenschaften-Allgemein
      IFCBUILDINGSTOREY "Erdgeschoss" | elevation -190.
        contains 205 elements
          92 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP , DN 50 <Rc>" | RIGIDSEGMENT | names: "1090", "1374", "1376" (+89 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_PipeSegmentTypeCommon, mhEigenschaften-ifcParameter
          18 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "1822", "4183", "5810" (+15 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-T-Stück, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter
          57 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 90°, DN 50 <Rc>" | BEND | names: "4182", "5807", "5809" (+54 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-Bogen, mhEigenschaften-ifcParameter
          23 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" | RIGIDSEGMENT | names: "4459", "4462", "4469" (+20 more) | property sets: mhEigenschaften-Drücke, Pset_PipeSegmentTypeCommon, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Rohr, mhEigenschaften-Allgemein
          5 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 100 <Rc>" | BEND | names: "4485", "4486", "4487" (+2 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-Bogen, mhEigenschaften-ifcParameter
          9 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 100/100/100 <Rc>" | JUNCTION | names: "4490", "4491", "4864" (+6 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Liegenschafts-Ursprung" | object type "NOTDEFINED" | names: "Liegenschafts-Ursprung" | property sets: Pset_BuildingElementProxyCommon
      IFCBUILDINGSTOREY "1. Obergeschoss" | elevation 3800.
        contains 184 elements
          89 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP , DN 50 <Rc>" | RIGIDSEGMENT | names: "126", "129", "259" (+86 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Rohr, Pset_PipeSegmentTypeCommon, mhEigenschaften-ifcParameter
          53 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 90°, DN 50 <Rc>" | BEND | names: "1060", "1228", "1235" (+50 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Bogen, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 85°, DN 50 <Rc>" | BEND | names: "1229", "1234" | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-Bogen, mhEigenschaften-ifcParameter
          16 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "1580", "4160", "4209" (+13 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          12 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" | RIGIDSEGMENT | names: "4453", "4456", "4457" (+9 more) | property sets: mhEigenschaften-Drücke, Pset_PipeSegmentTypeCommon, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          6 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 100/100/100 <Rc>" | JUNCTION | names: "4458", "4461", "4517" (+3 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          4 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 50 <Rc>" | RIGIDSEGMENT | names: "7186", "7189", "7206" (+1 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, mhEigenschaften-Rohr, mhEigenschaften-ifcParameter
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "7207", "7210" | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
      IFCBUILDINGSTOREY "2. Obergeschoss" | elevation 7600.
        contains 172 elements
          82 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP , DN 50 <Rc>" | RIGIDSEGMENT | names: "146", "148", "150" (+79 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Rohr, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_PipeSegmentTypeCommon
          48 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 90°, DN 50 <Rc>" | BEND | names: "777", "778", "1266" (+45 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Bogen, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter, mhEigenschaften-Allgemein
          17 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "1139", "4210", "5230" (+14 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          12 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" | RIGIDSEGMENT | names: "4447", "4450", "4451" (+9 more) | property sets: mhEigenschaften-Drücke, Pset_PipeSegmentTypeCommon, mhEigenschaften-Rohr, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein
          6 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 100/100/100 <Rc>" | JUNCTION | names: "4452", "4455", "4511" (+3 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          4 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 50 <Rc>" | RIGIDSEGMENT | names: "7166", "7169", "7184" (+1 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Rohr, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "7185", "7188" | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 85°, DN 50 <Rc>" | BEND | names: "7797" | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Bogen, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
      IFCBUILDINGSTOREY "3. Obergeschoss" | elevation 11820.
        contains 230 elements
          91 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP , DN 50 <Rc>" | RIGIDSEGMENT | names: "191", "192", "200" (+88 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Allgemein, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Rohr, Pset_PipeSegmentTypeCommon
          14 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "1728", "2021", "4337" (+11 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter, mhEigenschaften-Allgemein
          58 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 90°, DN 50 <Rc>" | BEND | names: "1951", "1956", "2029" (+55 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Bogen, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP X-Stück 90° 90°, DN 50/50/50/50 <Rc>" | JUNCTION | names: "X-Stueck ohne Reduzierung" | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-X-Stück, mhEigenschaften-Diverses, mhEigenschaften-ifcParameter
          30 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" | RIGIDSEGMENT | names: "4441", "4443", "4445" (+27 more) | property sets: mhEigenschaften-Drücke, Pset_PipeSegmentTypeCommon, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Rohr, mhEigenschaften-Allgemein
          6 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 100/100/100 <Rc>" | JUNCTION | names: "4446", "4449", "4505" (+3 more) | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Diverses, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter, mhEigenschaften-Allgemein
          18 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 100 <Rc>" | BEND | names: "5659", "5660", "5661" (+15 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter, mhEigenschaften-Bogen
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 85°, DN 50 <Rc>" | BEND | names: "6726" | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, mhEigenschaften-Bogen, mhEigenschaften-ifcParameter
          6 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 50 <Rc>" | RIGIDSEGMENT | names: "7157", "7161", "7164" (+3 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Rohr, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "7180", "7182" | property sets: mhEigenschaften-Ergebnisse, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 50 <Rc>" | BEND | names: "7181", "7183" | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter, mhEigenschaften-Bogen
      IFCBUILDINGSTOREY "4. Obergeschoss" | elevation 15460.
        contains 231 elements
          102 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP , DN 50 <Rc>" | RIGIDSEGMENT | names: "169", "170", "223" (+99 more) | property sets: mhEigenschaften-Drücke, mhEigenschaften-Allgemein, mhEigenschaften-Rohr, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, Pset_PipeSegmentTypeCommon
          72 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 90°, DN 50 <Rc>" | BEND | names: "1134", "2691", "5050" (+69 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Bogen, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          13 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" | RIGIDSEGMENT | names: "4439", "4440", "4498" (+10 more) | property sets: mhEigenschaften-Drücke, Pset_PipeSegmentTypeCommon, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          13 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 100 <Rc>" | BEND | names: "4442", "4444", "6676" (+10 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter, mhEigenschaften-Bogen
          24 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 45°, DN 50 <Rc>" | BEND | names: "5014", "5117", "5120" (+21 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Bogen, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter, mhEigenschaften-Allgemein
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 40°, DN 50 <Rc>" | BEND | names: "7147" | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Bogen, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-Allgemein, mhEigenschaften-ifcParameter
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 50°, DN 50 <Rc>" | BEND | names: "7150" | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, mhEigenschaften-Bogen, mhEigenschaften-ifcParameter, Pset_PipeFittingTypeCommon
          2 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 50 <Rc>" | RIGIDSEGMENT | names: "7158", "7162" | property sets: mhEigenschaften-Drücke, mhEigenschaften-Allgemein, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Rohr, mhEigenschaften-ifcParameter
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | names: "7494" | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_PipeFittingTypeCommon, mhEigenschaften-T-Stück, mhEigenschaften-ifcParameter
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 50 <Rc>" | BEND | names: "8184", "8185" | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter, mhEigenschaften-Bogen
      IFCBUILDINGSTOREY "5. Obergeschoss" | elevation 18710.
        contains 63 elements
          3 x IFCSPACEHEATER | type IFCSPACEHEATERTYPE "- (6000/1040/2400)" | USERDEFINED | names: "3340", "3342", "3344" | property sets: mhEigenschaften-Leistung, mhEigenschaften-Ergebnisse, mhEigenschaften-Allgemein, mhEigenschaften-Diverses, Pset_SpaceHeaterTypeCommon
          30 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" | RIGIDSEGMENT | names: "3747", "3748", "3752" (+27 more) | property sets: mhEigenschaften-Drücke, Pset_PipeSegmentTypeCommon, mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Rohr, mhEigenschaften-ifcParameter
          30 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 100 <Rc>" | BEND | names: "5587", "5589", "6479" (+27 more) | property sets: mhEigenschaften-Ergebnisse, mhEigenschaften-Diverses, mhEigenschaften-Allgemein, Pset_PipeFittingTypeCommon, mhEigenschaften-ifcParameter, mhEigenschaften-Bogen

Types
  IFCPIPESEGMENTTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP , DN 50 <Rc>" | RIGIDSEGMENT | 554 occurrences
  IFCSPACEHEATERTYPE "- (1800/1450/900)" | 1 occurrence
  IFCSPACEHEATERTYPE "- (1000/30/1800)" | 2 occurrences
  IFCSPACEHEATERTYPE "- (1000/30/900)" | 2 occurrences
  IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 15 <Rc>" | RIGIDSEGMENT | 8 occurrences
  IFCVALVETYPE "- - DN 0" | REGULATING | 1 occurrence
  IFCVALVETYPE "- - DN 0" | 1 occurrence
  IFCSPACEHEATERTYPE "- (4000/1800/2000)" | 1 occurrence
  IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 1500 <Rc>" | RIGIDSEGMENT | 2 occurrences
  IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Boden, DN 1500 <Rc>" | 2 occurrences
  IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 15 <Rc>" | BEND | 6 occurrences
  IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 1880 <Rc>" | RIGIDSEGMENT | 10 occurrences
  IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Boden, DN 1880 <Rc>" | 10 occurrences
  IFCSPACEHEATERTYPE "- (2870/1020/920)" | 3 occurrences
  IFCSPACEHEATERTYPE "- (1000/30/2870)" | 5 occurrences
  IFCSPACEHEATERTYPE "- (1000/30/920)" | 6 occurrences
  IFCSPACEHEATERTYPE "- (3000/2000/1000)" | 1 occurrence
  IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 50 <Rc>" | RIGIDSEGMENT | 55 occurrences
  IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 90°, DN 50 <Rc>" | BEND | 363 occurrences
  IFCSPACEHEATERTYPE "- (4000/500/1000)" | 2 occurrences
  IFCPIPESEGMENTTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" | RIGIDSEGMENT | 196 occurrences
  IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 100 <Rc>" | BEND | 112 occurrences
  IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 50 <Rc>" | BEND | 31 occurrences
  IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 100/100/100 <Rc>" | JUNCTION | 37 occurrences
  IFCPIPEFITTINGTYPE "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | 10 occurrences
  IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP T-Stück 90°, DN 50/50/50 <Rc>" | JUNCTION | 73 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Standard" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Liegenschafts-Ursprung" | 1 occurrence
  IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 85°, DN 50 <Rc>" | BEND | 4 occurrences
  IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP X-Stück 90° 90°, DN 50/50/50/50 <Rc>" | JUNCTION | 2 occurrences
  IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 45°, DN 50 <Rc>" | BEND | 24 occurrences
  IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 40°, DN 50 <Rc>" | BEND | 1 occurrence
  IFCPIPEFITTINGTYPE "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 50°, DN 50 <Rc>" | BEND | 1 occurrence
  IFCSPACEHEATERTYPE "- (6000/1040/2400)" | 3 occurrences

Property sets
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Liegenschafts-Ursprung" (IFCIDENTIFIER)
  mhEigenschaften-Allgemein | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Element-Id = "3" (IFCLABEL)
    System = "<leer>" (IFCLABEL)
  mhEigenschaften-Allgemein | properties | on 1 object (1 IFCPIPEFITTING)
    Element-Id = "7538" (IFCLABEL)
    System = "KX_HK-VL" (IFCLABEL)
  mhEigenschaften-Allgemein | properties | on 1 object (1 IFCPIPEFITTING)
    Element-Id = "6202" (IFCLABEL)
    System = "HX_STAT-HZG-RL" (IFCLABEL)
  mhEigenschaften-Allgemein | properties | on 1 object (1 IFCPIPEFITTING)
    Element-Id = "8438" (IFCLABEL)
    System = "HX_FB-HZG-RL" (IFCLABEL)
  mhEigenschaften-Allgemein | properties | on 1 object (1 IFCPIPEFITTING)
    Element-Id = "7833" (IFCLABEL)
    System = "KX_HK-RL" (IFCLABEL)
  mhEigenschaften-Allgemein | properties | on 1 object (1 IFCPIPEFITTING)
    Element-Id = "8221" (IFCLABEL)
    System = "HX_WW-VL" (IFCLABEL)
  mhEigenschaften-Allgemein | properties | on 1 object (1 IFCPIPEFITTING)
    Element-Id = "8588" (IFCLABEL)
    System = "KX_GLY-RL" (IFCLABEL)
  mhEigenschaften-Allgemein | properties | on 1 object (1 IFCPIPEFITTING)
    Element-Id = "8598" (IFCLABEL)
    System = "KX_GLY-RL" (IFCLABEL)
  mhEigenschaften-Allgemein: 1522 more contents on 1522 objects not shown
  mhEigenschaften-Ergebnisse | properties | on 825 objects (825 IFCPIPESEGMENT)
    Q-Verlust (Str) [W] = 0. (IFCPOWERMEASURE) [WATT]
    Zeta = "0.00" (IFCLABEL)
    mIdeal [kg/h] = 0. (IFCREAL)
    mReal [kg/h] = 0. (IFCREAL)
    t [°C] = 0. (IFCREAL)
    w [m/s] = 0. (IFCLINEARVELOCITYMEASURE) [derived]
  mhEigenschaften-Ergebnisse | properties | on 664 objects (664 IFCPIPEFITTING)
    mIdeal [kg/h] = 0. (IFCREAL)
    mReal [kg/h] = 0. (IFCREAL)
    t [°C] = 0. (IFCREAL)
    w [m/s] = 0. (IFCLINEARVELOCITYMEASURE) [derived]
  mhEigenschaften-Ergebnisse | properties | on 26 objects (26 IFCSPACEHEATER)
    Druckabfall [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
    Leistung [W] = 0. (IFCPOWERMEASURE) [WATT]
    m-Ideal [kg/h] = 0. (IFCREAL)
    m-Real [kg/h] = 0. (IFCREAL)
    tRücklauf tr [°C] = 0. (IFCREAL)
    tVorlauf tv [°C] = 0. (IFCREAL)
  mhEigenschaften-Ergebnisse | properties | on 2 objects (2 IFCVALVE)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Druckabfall [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
    P-Abweichung [K] = 0. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
    Soll-Diff. [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
    kv-Wert [m3/h] = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    mIdeal [kg/h] = 0. (IFCREAL)
    mReal [kg/h] = 0. (IFCREAL)
    pRest [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
  mhEigenschaften-Bogen | properties | on 276 objects (276 IFCPIPEFITTING)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Wandstärke [mm] = 2.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Winkel [°] = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Bogen | properties | on 120 objects (120 IFCPIPEFITTING)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Winkel [°] = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Bogen | properties | on 16 objects (16 IFCPIPEFITTING)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Wandstärke [mm] = 2.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Winkel [°] = 91.6 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Bogen | properties | on 12 objects (12 IFCPIPEFITTING)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Wandstärke [mm] = 2.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Winkel [°] = 89.9 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Bogen | properties | on 10 objects (10 IFCPIPEFITTING)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Wandstärke [mm] = 2.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Winkel [°] = 90.1 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Bogen | properties | on 9 objects (9 IFCPIPEFITTING)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Wandstärke [mm] = 2.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Winkel [°] = 88.9 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Bogen | properties | on 7 objects (7 IFCPIPEFITTING)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Winkel [°] = 91.7 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Bogen | properties | on 6 objects (6 IFCPIPEFITTING)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Winkel [°] = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da [mm] = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 16. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Bogen: 43 more contents on 86 objects not shown
  Pset_PipeFittingTypeCommon | properties | on 363 objects (363 IFCPIPEFITTING)
    Reference = "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 90°, DN 50 <Rc>" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 112 objects (112 IFCPIPEFITTING)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 100 <Rc>" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 73 objects (73 IFCPIPEFITTING)
    Reference = "Stahlrohr-Stahlrohr Vorgabe ZWP T-Stück 90°, DN 50/50/50 <Rc>" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 37 objects (37 IFCPIPEFITTING)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 100/100/100 <Rc>" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 31 objects (31 IFCPIPEFITTING)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 Bogen 90°, DN 50 <Rc>" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 24 objects (24 IFCPIPEFITTING)
    Reference = "Stahlrohr-Stahlrohr Vorgabe ZWP Bogen 45°, DN 50 <Rc>" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 10 objects (10 IFCPIPEFITTING)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 T-Stück 90°, DN 50/50/50 <Rc>" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon | properties | on 10 objects (10 IFCPIPEFITTING)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 Boden, DN 1880 <Rc>" (IFCIDENTIFIER)
  Pset_PipeFittingTypeCommon: 6 more contents on 16 objects not shown
  mhEigenschaften-T-Stück | properties | on 66 objects (66 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Winkel [°] = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da 1 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-T-Stück | properties | on 43 objects (43 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Winkel [°] = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da 1 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-T-Stück | properties | on 2 objects (2 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Winkel [°] = 89.9 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da 1 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-T-Stück | properties | on 2 objects (2 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Winkel [°] = 88.4 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da 1 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-T-Stück | properties | on 2 objects (2 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Winkel [°] = 88.5 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da 1 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-T-Stück | properties | on 2 objects (2 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Winkel [°] = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da 1 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-T-Stück | properties | on 2 objects (2 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Winkel [°] = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da 1 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-T-Stück | properties | on 1 object (1 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Winkel [°] = 89.9 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    da 1 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-X-Stück | properties | on 2 objects (2 IFCPIPEFITTING)
    DN 1 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 2 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 3 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    DN 4 [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    da 1 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 2 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 3 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    da 4 [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di 1 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 2 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 3 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
    di 4 [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Diverses | properties | on 1489 objects (825 IFCPIPESEGMENT, 664 IFCPIPEFITTING)
    Gleichzeitigkeit = "1.00" (IFCLABEL)
    tUmgebung [°C] = 20. (IFCREAL)
  mhEigenschaften-Diverses | properties | on 26 objects (26 IFCSPACEHEATER)
    Leergewicht [kg] = 0. (IFCMASSMEASURE) [KILO GRAM]
    Wasserinhalt [l] = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Zeta = "0.00" (IFCLABEL)
    pZusätzlich [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
  mhEigenschaften-ifcParameter | properties | on 1489 objects (825 IFCPIPESEGMENT, 664 IFCPIPEFITTING)
    ifcMaterial = "Aluminum_420" (IFCLABEL)
  Qto_PipeFittingBaseQuantities | quantities | on 54 objects (54 IFCPIPEFITTING)
    GrossCrossSectionArea = 2.85577840907697E-3 [SQUARE_METRE]
    GrossWeight = 2.33447452765486 [KILO GRAM]
    Length = 2.42E-1 [MILLI METRE]
    NetCrossSectionArea = 5.22949626504176E-4 [SQUARE_METRE]
    NetWeight = 1.48925854835445 [KILO GRAM]
    OuterSurfaceArea = 6.86428727235453E-2 [SQUARE_METRE]
  Qto_PipeFittingBaseQuantities | quantities | on 35 objects (35 IFCPIPEFITTING)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 4.E-1 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeFittingBaseQuantities | quantities | on 9 objects (9 IFCPIPEFITTING)
    GrossCrossSectionArea = 2.85577840907697E-3 [SQUARE_METRE]
    GrossWeight = 2.23461429534012 [KILO GRAM]
    Length = 2.42E-1 [MILLI METRE]
    NetCrossSectionArea = 5.22949626504176E-4 [SQUARE_METRE]
    NetWeight = 1.42555354628497 [KILO GRAM]
    OuterSurfaceArea = 6.57065831492871E-2 [SQUARE_METRE]
  Qto_PipeFittingBaseQuantities | quantities | on 8 objects (8 IFCPIPEFITTING)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 2.E-1 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeFittingBaseQuantities | quantities | on 2 objects (2 IFCPIPEFITTING)
    GrossCrossSectionArea = 2.85577840907697E-3 [SQUARE_METRE]
    GrossWeight = 1.55073276883659 [KILO GRAM]
    Length = 1.21E-1 [MILLI METRE]
    NetCrossSectionArea = 5.22949626504176E-4 [SQUARE_METRE]
    NetWeight = 9.89277032087922E-1 [KILO GRAM]
    OuterSurfaceArea = 4.55977355154156E-2 [SQUARE_METRE]
  Qto_PipeFittingBaseQuantities | quantities | on 2 objects (2 IFCPIPEFITTING)
    GrossCrossSectionArea = 2.85577840907697E-3 [SQUARE_METRE]
    GrossWeight = 1.55910814323656 [KILO GRAM]
    Length = 2.42E-1 [MILLI METRE]
    NetCrossSectionArea = 5.22949626504176E-4 [SQUARE_METRE]
    NetWeight = 9.94620032310486E-1 [KILO GRAM]
    OuterSurfaceArea = 4.58440049658375E-2 [SQUARE_METRE]
  Qto_PipeFittingBaseQuantities | quantities | on 2 objects (2 IFCPIPEFITTING)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 3.99E-1 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeFittingBaseQuantities | quantities | on 1 object (1 IFCPIPEFITTING)
    GrossCrossSectionArea = 2.85577840907697E-3 [SQUARE_METRE]
    GrossWeight = 2.33776440367419 [KILO GRAM]
    Length = 2.4E-1 [MILLI METRE]
    NetCrossSectionArea = 5.22949626504176E-4 [SQUARE_METRE]
    NetWeight = 1.49135729731348 [KILO GRAM]
    OuterSurfaceArea = 6.87396082150642E-2 [SQUARE_METRE]
  Qto_PipeFittingBaseQuantities: 9 more contents on 9 objects not shown
  mhEigenschaften-Rohr | properties | on 12 objects (12 IFCPIPESEGMENT)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Länge [m] = 1.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Rohr | properties | on 4 objects (4 IFCPIPESEGMENT)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Länge [m] = 4.059 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Wandstärke [mm] = 2.9 (IFCLENGTHMEASURE) [MILLI METRE]
    da [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Rohr | properties | on 4 objects (4 IFCPIPESEGMENT)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Länge [m] = 3.98 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Rohr | properties | on 4 objects (4 IFCPIPESEGMENT)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Länge [m] = 8.E-1 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Rohr | properties | on 4 objects (4 IFCPIPESEGMENT)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Länge [m] = 2.455 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    da [mm] = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 16. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Rohr | properties | on 4 objects (4 IFCPIPESEGMENT)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "sta - Stahlrohr" (IFCLABEL)
    Länge [m] = 4.099 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "sta - Stahlrohr Vorgabe ZWP" (IFCLABEL)
    Wandstärke [mm] = 2.9 (IFCLENGTHMEASURE) [MILLI METRE]
    da [mm] = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 54.5 (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Rohr | properties | on 4 objects (4 IFCPIPESEGMENT)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Länge [m] = 2.25 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Rohr | properties | on 4 objects (4 IFCPIPESEGMENT)
    DN [mm] = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Hersteller = "cu - Kupferrohr" (IFCLABEL)
    Länge [m] = 3.62 (IFCLENGTHMEASURE) [MILLI METRE]
    Material = "cu - Kupferrohr nach DIN EN 1057" (IFCLABEL)
    Wandstärke [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    da [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    di [mm] = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  mhEigenschaften-Rohr: 659 more contents on 785 objects not shown
  mhEigenschaften-Drücke | properties | on 825 objects (825 IFCPIPESEGMENT)
    R-Wert(Str) [Pa/m] = 0. (IFCREAL)
    pDiff(Str) [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
    pDrossel(Str) [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
    pRest(Str) [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
    pStatisch(Str) [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
    pStrecke(Str) [Pa] = 0. (IFCPRESSUREMEASURE) [KILO PASCAL]
  Pset_PipeSegmentTypeCommon | properties | on 554 objects (554 IFCPIPESEGMENT)
    Reference = "Stahlrohr-Stahlrohr Vorgabe ZWP , DN 50 <Rc>" (IFCIDENTIFIER)
  Pset_PipeSegmentTypeCommon | properties | on 196 objects (196 IFCPIPESEGMENT)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 100 <Rc>" (IFCIDENTIFIER)
  Pset_PipeSegmentTypeCommon | properties | on 55 objects (55 IFCPIPESEGMENT)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 50 <Rc>" (IFCIDENTIFIER)
  Pset_PipeSegmentTypeCommon | properties | on 10 objects (10 IFCPIPESEGMENT)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 1880 <Rc>" (IFCIDENTIFIER)
  Pset_PipeSegmentTypeCommon | properties | on 8 objects (8 IFCPIPESEGMENT)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 15 <Rc>" (IFCIDENTIFIER)
  Pset_PipeSegmentTypeCommon | properties | on 2 objects (2 IFCPIPESEGMENT)
    Reference = "Kupferrohr-Kupferrohr nach DIN EN 1057 , DN 1500 <Rc>" (IFCIDENTIFIER)
  Qto_PipeSegmentBaseQuantities | quantities | on 12 objects (12 IFCPIPESEGMENT)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 1.7 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 4 objects (4 IFCPIPESEGMENT)
    GrossCrossSectionArea = 2.85577840907697E-3 [SQUARE_METRE]
    GrossWeight = 26.1504957735013 [KILO GRAM]
    Length = 4.059 [MILLI METRE]
    NetCrossSectionArea = 5.22949626504176E-4 [SQUARE_METRE]
    NetWeight = 16.6824906046486 [KILO GRAM]
    OuterSurfaceArea = 7.68928995272142E-1 [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 4 objects (4 IFCPIPESEGMENT)
    GrossCrossSectionArea = 2.54468983032113E-4 [SQUARE_METRE]
    GrossWeight = 1.67195764561506 [KILO GRAM]
    Length = 2.455 [MILLI METRE]
    NetCrossSectionArea = 5.34070341025069E-5 [SQUARE_METRE]
    NetWeight = 1.17839993703961 [KILO GRAM]
    OuterSurfaceArea = 1.38826969071616E-1 [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 4 objects (4 IFCPIPESEGMENT)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 3.62 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 4 objects (4 IFCPIPESEGMENT)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 8.E-1 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 4 objects (4 IFCPIPESEGMENT)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 2.25 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 4 objects (4 IFCPIPESEGMENT)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 2.2 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 4 objects (4 IFCPIPESEGMENT)
    GrossCrossSectionArea = 0. [SQUARE_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 3.98 [MILLI METRE]
    NetCrossSectionArea = 0. [SQUARE_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0. [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities: 674 more contents on 785 objects not shown
  mhEigenschaften-Leistung | properties | on 26 objects (26 IFCSPACEHEATER)
    Leistung-Vorgabe Q [W] = 0. (IFCPOWERMEASURE) [WATT]
    Massenstrom m [kg/h] = 0. (IFCREAL)
  Pset_SpaceHeaterTypeCommon | properties | on 6 objects (6 IFCSPACEHEATER)
    Reference = "- (1000/30/920)" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 5 objects (5 IFCSPACEHEATER)
    Reference = "- (1000/30/2870)" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 3 objects (3 IFCSPACEHEATER)
    Reference = "- (2870/1020/920)" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 3 objects (3 IFCSPACEHEATER)
    Reference = "- (6000/1040/2400)" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 2 objects (2 IFCSPACEHEATER)
    Reference = "- (4000/500/1000)" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 2 objects (2 IFCSPACEHEATER)
    Reference = "- (1000/30/900)" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 2 objects (2 IFCSPACEHEATER)
    Reference = "- (1000/30/1800)" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACEHEATER)
    Reference = "- (3000/2000/1000)" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon: 2 more contents on 2 objects not shown
  Pset_ValveTypeCommon | properties | on 2 objects (2 IFCVALVE)
    Reference = "- - DN 0" (IFCIDENTIFIER)
  mhEigenschaften-Ventil | properties | on 1 object (1 IFCVALVE)
    Armaturenart = 0. (IFCREAL)
    Armaturentyp = 0. (IFCREAL)
    Typ = "<2> - Verschraubung" (IFCLABEL)
  mhEigenschaften-Ventil | properties | on 1 object (1 IFCVALVE)
    Armaturenart = 0. (IFCREAL)
    Armaturentyp = 0. (IFCREAL)
    Typ = "<1> - Thermostat" (IFCLABEL)