IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "6-13_SimQ.ifc"
Time stamp: "2024-06-13T18:24:10+02:00"
Preprocessor: "IfcOpenShell v0.7.0-c7830e9e5"
Originating system: "BlenderBIM 0.0.240602-47704b1"
Authorization: "Nobody"

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE

Spatial structure
IFCPROJECT "SimQ_Gebauede_neu"
  IFCSITE "Default"
    IFCBUILDING "SimQ_Gebaeude"
      IFCBUILDINGSTOREY "DG"
        contains 15 elements
          8 x IFCWALL | type IFCWALLTYPE "SIMQ_4" | names: "Wall" | material: layers "Wall_SIMQ_4" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.100000001490116, "Plaster_800_MA" 0.00499999988824129) | property sets: EPset_Parametric
          5 x IFCWINDOW | type IFCWINDOWTYPE "window_160x120_MA" | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "Wintergarten_Fenster" | names: "Window"
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke" | FLOOR | names: "Slab" | material: layers "Slab_SIMQ_Geschossdecke" ("Screed_1.40_MA" 0.0500000007450581, "Insulation_040_MA" 0.0199999995529652, "Concrete_1.2_MA" 0.180000007152557) | property sets: EPset_Parametric
      IFCBUILDINGSTOREY "1.OG"
        contains 47 elements
          6 x IFCWINDOW | type IFCWINDOWTYPE "window_445x160_MA" | names: "Window"
          6 x IFCWALL | type IFCWALLTYPE "SIMQ_4" | names: "Wall" | material: layers "Wall_SIMQ_4" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.100000001490116, "Plaster_800_MA" 0.00499999988824129) | property sets: EPset_Parametric
          14 x IFCWALL | type IFCWALLTYPE "IW_schwer" | names: "Wall" | material: layers "Wall_SIMQ_IW_schwer" ("Concrete_1.2_MA" 0.200000002980232) | property sets: EPset_Parametric
          2 x IFCWALL | type IFCWALLTYPE "IW_Treppenhaus" | names: "Wall" | material: layers "Wall_IW_Treppenhaus" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.200000002980232) | property sets: EPset_Parametric
          3 x IFCWINDOW | type IFCWINDOWTYPE "window_295x160_MA" | names: "Window"
          6 x IFCWALL | type IFCWALLTYPE "IW_leicht" | names: "Wall" | material: layers "Wall_SIMQ_IW_leicht" ("Brick_0.5_MA" 0.200000002980232) | property sets: EPset_Parametric
          2 x IFCWINDOW | type IFCWINDOWTYPE "window_160x55" | names: "Window" | material: constituents "window_160x55_MA" ("Glass": "Glass_1.1_MA", "Frame": "Frame_MA")
          3 x IFCWINDOW | type IFCWINDOWTYPE "window_640x160_MA" | names: "Window"
          2 x IFCWINDOW | type IFCWINDOWTYPE "window_400x160_MA" | names: "Window"
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke" | FLOOR | names: "Slab.001" | material: layers "Slab_SIMQ_Geschossdecke" ("Screed_1.40_MA" 0.0500000007450581, "Insulation_040_MA" 0.0199999995529652, "Concrete_1.2_MA" 0.180000007152557) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_70x160_MA" | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_130x160_MA" | names: "Window"
        IFCSPACE "Buero111"
        IFCSPACE "Buero104"
        IFCSPACE "Buero108"
        IFCSPACE "TeekuecheOG1"
        IFCSPACE "Buero102"
        IFCSPACE "Buero106"
        IFCSPACE "FlurOG1"
        IFCSPACE "Buero109"
        IFCSPACE "Buero105"
        IFCSPACE "WC_Damen1"
        IFCSPACE "Buero101"
        IFCSPACE "Buero107"
        IFCSPACE "WC_Herren1"
        IFCSPACE "Buero103"
        IFCSPACE "Buero110"
      IFCBUILDINGSTOREY "2.OG"
        contains 37 elements
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_130x160_MA" | names: "Window"
          10 x IFCWALL | type IFCWALLTYPE "SIMQ_4" | names: "Wall" | material: layers "Wall_SIMQ_4" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.100000001490116, "Plaster_800_MA" 0.00499999988824129) | property sets: EPset_Parametric, BBIM_Boolean
          2 x IFCWINDOW | type IFCWINDOWTYPE "window_160x55" | names: "Window"
          9 x IFCWALL | type IFCWALLTYPE "IW_schwer" | names: "Wall" | material: layers "Wall_SIMQ_IW_schwer" ("Concrete_1.2_MA" 0.200000002980232) | property sets: EPset_Parametric
          4 x IFCWINDOW | type IFCWINDOWTYPE "window_445x160_MA" | names: "Window"
          3 x IFCWINDOW | type IFCWINDOWTYPE "window_295x160_MA" | names: "Window"
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke" | FLOOR | names: "Slab" | material: layers "Slab_SIMQ_Geschossdecke" ("Screed_1.40_MA" 0.0500000007450581, "Insulation_040_MA" 0.0199999995529652, "Concrete_1.2_MA" 0.180000007152557) | property sets: EPset_Parametric
          2 x IFCWALL | type IFCWALLTYPE "IW_Treppenhaus" | names: "Wall" | material: layers "Wall_IW_Treppenhaus" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.200000002980232) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_70x160_MA" | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_20000x570_MA" | names: "Window"
          2 x IFCWINDOW | type IFCWINDOWTYPE "window_400x160_MA" | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_20000x113_MA" | names: "Window"
        IFCSPACE "Buero202"
        IFCSPACE "WC_Herren2"
        IFCSPACE "FlurOG2"
        IFCSPACE "Wintergarten"
        IFCSPACE "WC_Damen2"
        IFCSPACE "TeekuecheOG2"
      IFCBUILDINGSTOREY "EG"
        contains 35 elements
          4 x IFCWALL | type IFCWALLTYPE "IW_schwer" | names: "Wall" | material: layers "Wall_SIMQ_IW_schwer" ("Concrete_1.2_MA" 0.200000002980232) | property sets: EPset_Parametric
          10 x IFCWALL | type IFCWALLTYPE "SIMQ_4" | names: "Wall" | material: layers "Wall_SIMQ_4" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.100000001490116, "Plaster_800_MA" 0.00499999988824129) | property sets: EPset_Parametric
          11 x IFCWINDOW | type IFCWINDOWTYPE "window_435x240_MA" | names: "Window"
          2 x IFCWALL | type IFCWALLTYPE "IW_Treppenhaus" | names: "Wall" | material: layers "Wall_IW_Treppenhaus" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.200000002980232) | property sets: EPset_Parametric
          2 x IFCWINDOW | type IFCWINDOWTYPE "window_140x240_MA" | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_420x240_MA" | TRIPLE_PANEL_VERTICAL | names: "Window"
          2 x IFCWINDOW | type IFCWINDOWTYPE "window_160x55" | WINDOW | names: "Window.030", "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_420x240_MA" | names: "Window" | material: constituents "window_420x240_MA" ("Glass": "Glass_1.1_MA", "Frame": "Frame_MA")
          1 x IFCSLAB | type IFCSLABTYPE "Bodenplatte" | BASESLAB | names: "Slab" | material: layers "Slab_SIMQ_Bodenplatte" ("Screed_1.40_MA" 0.0500000007450581, "Insulation_040_MA" 0.0199999995529652, "Concrete_1.2_MA" 0.180000007152557, "Insulation_040_MA" 0.200000002980232) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "window_9x140x240_MA" | names: "Window" | material: constituents "window_9x140x240_MA" ("Glass": "Glass_1.1_MA", "Frame": "Frame_MA")
        IFCSPACE "Treppenhaus"
        IFCSPACE "HVAC"
        IFCSPACE "Aufzug"
        IFCSPACE "Empfang"
        IFCSPACE "Restaurant"

Types
  IFCWALLTYPE "SIMQ_4" | 34 occurrences | material: layers "Wall_SIMQ_4" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.100000001490116, "Plaster_800_MA" 0.00499999988824129)
  IFCWINDOWTYPE "window_160x120_MA" | WINDOW | SINGLE_PANEL | 5 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "Wintergarten_Fenster" | USERDEFINED | 1 occurrence
  IFCSLABTYPE "Geschossdecke" | 3 occurrences | material: layers "Slab_SIMQ_Geschossdecke" ("Screed_1.40_MA" 0.0500000007450581, "Insulation_040_MA" 0.0199999995529652, "Concrete_1.2_MA" 0.180000007152557)
  IFCWINDOWTYPE "window_445x160_MA" | WINDOW | SINGLE_PANEL | 10 occurrences | property sets: BBIM_Window
  IFCWALLTYPE "IW_schwer" | 27 occurrences | material: layers "Wall_SIMQ_IW_schwer" ("Concrete_1.2_MA" 0.200000002980232)
  IFCWALLTYPE "IW_Treppenhaus" | 6 occurrences | material: layers "Wall_IW_Treppenhaus" ("Concrete_1.2_MA" 0.200000002980232, "Insulation_040_MA" 0.200000002980232)
  IFCWINDOWTYPE "window_295x160_MA" | WINDOW | SINGLE_PANEL | 6 occurrences | property sets: BBIM_Window
  IFCWALLTYPE "IW_leicht" | 6 occurrences | material: layers "Wall_SIMQ_IW_leicht" ("Brick_0.5_MA" 0.200000002980232)
  IFCWINDOWTYPE "window_160x55" | WINDOW | SINGLE_PANEL | 6 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "window_640x160_MA" | WINDOW | SINGLE_PANEL | 3 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "window_400x160_MA" | WINDOW | SINGLE_PANEL | 4 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "window_70x160_MA" | WINDOW | SINGLE_PANEL | 2 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "window_130x160_MA" | WINDOW | SINGLE_PANEL | 2 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "window_20000x570_MA" | WINDOW | 1 occurrence
  IFCWINDOWTYPE "window_20000x113_MA" | WINDOW | 1 occurrence
  IFCWINDOWTYPE "window_435x240_MA" | WINDOW | SINGLE_PANEL | 11 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "window_140x240_MA" | WINDOW | SINGLE_PANEL | 2 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "window_420x240_MA" | WINDOW | SINGLE_PANEL | 2 occurrences | property sets: BBIM_Window
  IFCSLABTYPE "Bodenplatte" | 1 occurrence | material: layers "Slab_SIMQ_Bodenplatte" ("Screed_1.40_MA" 0.0500000007450581, "Insulation_040_MA" 0.0199999995529652, "Concrete_1.2_MA" 0.180000007152557, "Insulation_040_MA" 0.200000002980232)
  IFCWINDOWTYPE "window_9x140x240_MA" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window

Property sets
  EPset_Parametric | properties | on 73 objects (73 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 4 objects (4 IFCSLAB)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  BBIM_Boolean | properties | on 1 object (1 IFCWALL)
    Data = "[37284]" (IFCTEXT)
  BBIM_Boolean | properties | on 1 object (1 IFCWALL)
    Data = "[37294]" (IFCTEXT)
  BBIM_Boolean | properties | on 1 object (1 IFCWALL)
    Data = "[37569]" (IFCTEXT)
  BBIM_Boolean | properties | on 1 object (1 IFCSPACE)
    Data = "[37579]" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 1.2000000476837158, "overall_width": 1.600000023841858, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_VERTICAL", "overall_height": 1.600000023841858, "overall_width": 4.449999809265137, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "mullion_thickness": 0.05000000074505806, "first_mullion_offset": 1.4800000190734863, "second_mullion_offset": 2.9700000286102295}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 1.600000023841858, "overall_width": 2.950000047683716, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "mullion_thickness": 0.05000000074505806, "first_mullion_offset": 1.475000023841858}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 0.550000011920929, "overall_width": 1.600000023841858, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 1.600000023841858, "overall_width": 6.400000095367432, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_VERTICAL", "overall_height": 1.600000023841858, "overall_width": 4.0, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "mullion_thickness": 0.05000000074505806, "first_mullion_offset": 1.3300000429153442, "second_mullion_offset": 2.6700000762939453}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 1.600000023841858, "overall_width": 0.699999988079071, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 1.600000023841858, "overall_width": 1.2999999523162842, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window: 4 more contents on 0 objects not shown