IFC building model
Schema: "IFC4X3"
Description: "ViewDefinition [CoordinationView]"
Description: "RevitIdentifiers [VersionGUID: ae5f772d-fa3a-4a3d-939d-1b5da769d716, NumberOfSaves: 9]"
Description: "CoordinateReference [CoordinateBase: Sdílené souřadnice, ProjectSite: Default Site]"
File name: "testing_model_adjusted_BBIM.ifc"
Time stamp: "2023-09-30T16:03:50+02:00"
Preprocessor: "IfcOpenShell v0.7.0-9cc1f5f0e"
Originating system: "BlenderBIM 0.0.230922-6d14c2d"
Application: "Autodesk Revit 2024 (CSY)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (CSY)"

People and organizations
  Person "tomas.polakCMEY6" of Organization "Organization Name" description "Organization Description"
  Owner history of Person "tomas.polakCMEY6" of Organization "Organization Name" description "Organization Description" | application "Autodesk Revit 2024 (CSY)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (CSY)" | change NOCHANGE | created 1694008506 (2023-09-06T13:55:06Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "TEST" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.401672″ | longitude -71° 3′ 24.345703″ | elevation above sea level 0.
    IFCBUILDING "Building Name" | long name "Building Name" | postal address: "Enter address hereAddress Line 2", "Boston", "MA"
      IFCBUILDINGSTOREY "L1" | long name "L1" | object type "Podlaží:8mm Head" | elevation 0.
        contains 25 elements
          4 x IFCWALL | type IFCWALLTYPE "Základní stěna:Concrete 300mm" | object type "Základní stěna:Concrete 300mm" | names: "Základní stěna:Concrete 300mm:1588862", "Základní stěna:Concrete 300mm:1588863", "Základní stěna:Concrete 300mm:1588864" (+1 more) | material: layers "Základní stěna:Concrete 300mm" ("Concrete, Cast-in-Place gray" 300.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, A1, B1, W1
          2 x IFCWALL | type IFCWALLTYPE "Základní stěna:Interior - 125mm Partition" | object type "Základní stěna:Interior - 125mm Partition" | names: "Základní stěna:Interior - 125mm Partition:1588937", "Základní stěna:Interior - 125mm Partition:1588984" | material: layers "Základní stěna:Interior - 125mm Partition" ("Gypsum Wall Board" 12.5, "Metal Stud Layer" 100., "Gypsum Wall Board" 12.5) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, A1, B1, M1
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Concrete 250mm" | object type "Podlaha:Concrete 250mm" | FLOOR | names: "Podlaha:Concrete 250mm:1588996" | material: layers "Podlaha:Concrete 250mm" ("Concrete, Cast-in-Place gray" 250.00000000000003) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, A1, B1, W1
          1 x IFCDOOR | type IFCDOORTYPE "M_Door-Passage-Double-Flush:1800 x 2000mm" | object type "DOOR" | DOOR | names: "M_Door-Passage-Double-Flush:1800 x 2000mm:1589305" | material: constituents ("Aluminum": "Aluminum", "Metal Door - Brindle": "Metal Door - Brindle", "Metal - Painted - Grey": "Metal - Painted - Grey") | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "M_Door-Passage-Single-Flush:900 x 2000mm" | object type "DOOR" | DOOR | SINGLE_SWING_RIGHT | names: "M_Door-Passage-Single-Flush:900 x 2000mm:1589398" | material: constituents ("Aluminum": "Aluminum", "Wood - Birch": "Wood - Birch", "Metal - Paint Finish - Grey": "Metal - Paint Finish - Grey") | property sets: Pset_EnvironmentalImpactIndicators
          3 x IFCWINDOW | type IFCWINDOWTYPE "M_Window-Fixed:900 x 1650mm" | object type "M_Window-Fixed:900 x 1650mm" | WINDOW | names: "M_Window-Fixed:900 x 1650mm:1589512", "M_Window-Fixed:900 x 1650mm:1589598", "M_Window-Fixed:900 x 1650mm:1589649" | material: constituents ("Wood - Stained": "Wood - Stained", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2" | object type "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2" | names: "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:1589515", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:1589601", "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2:1589652" (+1 more) | material: constituents ("Clad - White": "Clad - White", "Wood - Stained": "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Trim-Window-Exterior-Flat:with Sill" | object type "M_Trim-Window-Exterior-Flat:with Sill" | names: "M_Trim-Window-Exterior-Flat:with Sill:1589516", "M_Trim-Window-Exterior-Flat:with Sill:1589602", "M_Trim-Window-Exterior-Flat:with Sill:1589653" (+1 more) | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Trim-Window-Interior-Flat:Picture Frame" | object type "M_Trim-Window-Interior-Flat:Picture Frame" | names: "M_Trim-Window-Interior-Flat:Picture Frame:1589517", "M_Trim-Window-Interior-Flat:Picture Frame:1589603", "M_Trim-Window-Interior-Flat:Picture Frame:1589654" (+1 more) | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "M_Window-Fixed:900 x 1650mm" | object type "M_Window-Fixed:900 x 1650mm" | names: "M_Window-Fixed:900 x 1650mm:1589692" | material: constituents ("Wood - Stained": "Wood - Stained", "Glass": "Glass") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
      IFCBUILDINGSTOREY "L2" | long name "L2" | object type "Podlaží:8mm Head" | elevation 3600.0000000000005

Types
  IFCWALLTYPE "Základní stěna:Concrete 300mm" | STANDARD | 4 occurrences | material: layers "Základní stěna:Concrete 300mm" ("Concrete, Cast-in-Place gray" 300.) | property sets: Pset_WallCommon
  IFCWALLTYPE "Základní stěna:Interior - 125mm Partition" | STANDARD | 2 occurrences | material: layers "Základní stěna:Interior - 125mm Partition" ("Gypsum Wall Board" 12.5, "Metal Stud Layer" 100., "Gypsum Wall Board" 12.5) | property sets: Pset_WallCommon
  IFCSLABTYPE "Podlaha:Concrete 250mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Concrete 250mm" ("Concrete, Cast-in-Place gray" 250.00000000000003) | property sets: Pset_SlabCommon
  IFCDOORTYPE "M_Door-Passage-Double-Flush:1800 x 2000mm" | DOOR | DOUBLE_PANEL_SINGLE_SWING_OPPOSITE_LEFT | 1 occurrence | material: constituents ("Hardware": "Aluminum", "Panel": "Metal Door - Brindle", "Rám/Příčel": "Metal - Painted - Grey") | property sets: M_Door-Passage-Double-Flush:1800 x 2000mm:1589305, M_Door-Passage-Double-Flush:1800 x 2000mm:1589305:1, Pset_DoorCommon
  IFCDOORTYPE "M_Door-Passage-Single-Flush:900 x 2000mm" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents ("Hardware": "Aluminum", "Panel": "Wood - Birch", "Rám/Příčel": "Metal - Paint Finish - Grey") | property sets: M_Door-Passage-Single-Flush:900 x 2000mm:1589398, M_Door-Passage-Single-Flush:900 x 2000mm:1589398:1, Pset_DoorCommon
  IFCWINDOWTYPE "M_Window-Fixed:900 x 1650mm" | WINDOW | 3 occurrences | material: constituents ("Rám/Příčel": "Wood - Stained", "Sklo": "Glass") | property sets: M_Window-Fixed:900 x 1650mm:1589512, Pset_WindowCommon
  IFCBUILDINGELEMENTPROXYTYPE "M_Muntin Pattern_2x2:M_Muntin Pattern_2x2" | 4 occurrences | material: constituents ("Clad - White": "Clad - White", "Wood - Stained": "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "M_Trim-Window-Exterior-Flat:with Sill" | 4 occurrences | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "M_Trim-Window-Interior-Flat:Picture Frame" | 4 occurrences | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon
  IFCDOORTYPE "M_Window-Fixed:900 x 1650mm" | 1 occurrence | material: constituents ("Rám/Příčel": "Wood - Stained", "Sklo": "Glass") | property sets: M_Window-Fixed:900 x 1650mm:1589692, M_Window-Fixed:900 x 1650mm:1589692:1, Pset_DoorCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Informace o projektu" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Informace o projektu" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "8mm Head" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 4 objects (4 IFCWALL)
    Reference = "Concrete 300mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 4 objects (3 IFCWINDOW, 1 IFCDOOR)
    Reference = "900 x 1650mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "M_Muntin Pattern_2x2" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "with Sill" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "Picture Frame" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 2 objects (2 IFCWALL)
    Reference = "Interior - 125mm Partition" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCSLAB)
    Reference = "Concrete 250mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCDOOR)
    Reference = "1800 x 2000mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 1 more content on 1 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALL)
    Reference = "Concrete 300mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALL)
    Reference = "Interior - 125mm Partition" (IFCLABEL)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Concrete 300mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - 125mm Partition" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 3.4866666666666668 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0.24761904761904763 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  A1 | properties | on 7 objects (6 IFCWALL, 1 IFCSLAB)
    Construction phase = "Phase 2" (IFCTEXT)
    Schedule duration = "4 months" (IFCTEXT)
    Scheduled end = "3/21/2024" (IFCTEXT)
    Scheduled start = "9/6/2023" (IFCTEXT)
  B1 | properties | on 6 objects (6 IFCWALL)
    Classification code = "B" (IFCTEXT)
    Classification system = "CCI" (IFCTEXT)
  B1 | properties | on 1 object (1 IFCSLAB)
    Classification code = "C" (IFCTEXT)
    Classification system = "CCI" (IFCTEXT)
  W1 | properties | on 2 objects (2 IFCWALL)
    Height = "3500" (IFCTEXT)
    Length = "6000" (IFCTEXT)
    Width = "300" (IFCTEXT)
  W1 | properties | on 2 objects (2 IFCWALL)
    Height = "3500" (IFCTEXT)
    Length = "8000" (IFCTEXT)
    Width = "300" (IFCTEXT)
  W1 | properties | on 1 object (1 IFCSLAB)
    Area = "48" (IFCTEXT)
    Height = "250" (IFCTEXT)
    Length = "6000" (IFCTEXT)
    Volume = "12" (IFCTEXT)
    Width = "8000" (IFCTEXT)
  W2 | properties | on 4 objects (4 IFCWALL)
    Concrete specification = "C30" (IFCTEXT)
    Reinforcement = "Yes" (IFCTEXT)
    Technology = "monolith" (IFCTEXT)
  M1 | properties | on 4 objects (4 IFCWALL)
    Design lifetime = "70 years" (IFCTEXT)
    Material = "Concrete" (IFCTEXT)
  M1 | properties | on 2 objects (2 IFCWALL)
    Design lifetime = "50 years" (IFCTEXT)
    Material = "Drywall on Steel Studs" (IFCTEXT)
  M1 | properties | on 1 object (1 IFCSLAB)
    Design lifetime = "70 years" (IFCTEXT)
    Material = "Concrete reinforced" (IFCTEXT)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Concrete 250mm" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Concrete 250mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 4.1840000000000002 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "900 x 1650mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "M_Muntin Pattern_2x2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "with Sill" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Picture Frame" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Informace o projektu" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "900 x 1650mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 1 type object
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "8mm Head" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Informace o projektu" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCCOUNTMEASURE)
    Reference = "Informace o projektu" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Informace o projektu" (IFCIDENTIFIER)
  pset_CCI | properties | on 1 object (1 IFCWALL)
    StringProperty = "B" (IFCLABEL)
  M_Door-Passage-Double-Flush:1800 x 2000mm:1589305 | predefined | on 1 type object
  M_Door-Passage-Double-Flush:1800 x 2000mm:1589305:1 | predefined | on 1 type object
  M_Door-Passage-Single-Flush:900 x 2000mm:1589398 | predefined | on 1 type object
  M_Door-Passage-Single-Flush:900 x 2000mm:1589398:1 | predefined | on 1 type object
  M_Window-Fixed:900 x 1650mm:1589512 | predefined | on 1 type object
  M_Window-Fixed:900 x 1650mm:1589692 | predefined | on 1 type object
  M_Window-Fixed:900 x 1650mm:1589692:1 | predefined | on 1 type object