IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
File name: "House Dahl 2019 As Built-edied.ifc"
Time stamp: "2022-08-22T23:01:19+02:00"
Preprocessor: "IfcOpenShell v0.7.0-cb8cfd79"
Originating system: "BlenderBIM 0.0.220822"
Application: "Autodesk Revit LT 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit LT 2020 (ENU)"

People and organizations
  Person "sceye" of Organization (no name given)
  Owner history of Person "sceye" of Organization (no name given) | application "Autodesk Revit LT 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit LT 2020 (ENU)" | change NOCHANGE | created 1634036418 (2021-10-12T11:00:18Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Surface:143978" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Terrace" | long name "Terrace" | object type "Level:8mm Head" | elevation 812.000000000001
        contains 28 elements
          15 x IFCBUILDINGELEMENTPROXY | names: "123322", "123395", "123396" (+12 more) | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          10 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:150052", "Basic Wall:Retaining - 300mm Concrete:150078", "Basic Wall:Retaining - 300mm Concrete:150099" (+7 more) | material: layers "Basic Wall:Retaining - 300mm Concrete" ("Concrete, Cast In Situ" 300.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSTAIR | object type "Assembled Stair:190mm max riser 250mm going" | names: "Assembled Stair:Stair:348870" | parts: 2 IFCMEMBER, 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:220mm Brick Wall With Symmetrical Footing" | object type "Basic Wall:220mm Brick Wall With Symmetrical Footing" | names: "Basic Wall:220mm Brick Wall With Symmetrical Footing:351535", "Basic Wall:220mm Brick Wall With Symmetrical Footing:351608" | material: layers "Basic Wall:220mm Brick Wall With Symmetrical Footing" ("Masonry - Brick" 220.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "Ground Floor" | long name "Ground Floor" | object type "Level:8mm Head" | elevation 1381.81875
        contains 106 elements
          13 x IFCWALL | type IFCWALLTYPE "Basic Wall:280mm Brick Cavity Wall With Symmetrical Footing" | object type "Basic Wall:280mm Brick Cavity Wall With Symmetrical Footing" | names: "Basic Wall:280mm Brick Cavity Wall With Symmetrical Footing:69760", "Basic Wall:280mm Brick Cavity Wall With Symmetrical Footing:69783", "Basic Wall:280mm Brick Cavity Wall With Symmetrical Footing:69842" (+10 more) | material: layers "Basic Wall:280mm Brick Cavity Wall With Symmetrical Footing" ("Masonry - Brick Soldier Course" 110., "Default Wall" 60., "Masonry - Brick Soldier Course" 110.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:110mm Brick Wall" | object type "Basic Wall:110mm Brick Wall" | names: "Basic Wall:110mm Brick Wall:70576", "Basic Wall:110mm Brick Wall:70608", "Basic Wall:110mm Brick Wall:290673" (+2 more) | material: layers "Basic Wall:110mm Brick Wall" ("Masonry - Brick" 110.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSTAIR | object type "Stair:190mm max riser 250mm going" | names: "Stair:190mm max riser 250mm going:74600" | parts: 1 IFCRAILING, 1 IFCSTAIR | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete 225mm" | object type "Floor:Insitu Concrete 225mm" | FLOOR | names: "Floor:Insitu Concrete 225mm:86747" | material: layers "Floor:Insitu Concrete 225mm" ("Concrete, Sand/Cement Screed" 50., "Damp-proofing" 0., "Concrete, Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete 225mm" | object type "Floor:Insitu Concrete 225mm" | FLOOR | names: "Floor:Insitu Concrete 225mm:86747:2" | material: layers "Floor:Insitu Concrete 225mm" ("Concrete, Sand/Cement Screed" 50., "Damp-proofing" 0., "Concrete, Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete 225mm" | object type "Floor:Insitu Concrete 225mm" | FLOOR | names: "Floor:Insitu Concrete 225mm:86782" | material: layers "Floor:Insitu Concrete 225mm" ("Concrete, Sand/Cement Screed" 50., "Damp-proofing" 0., "Concrete, Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORTYPE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | DOOR | SINGLE_SWING_RIGHT | names: "M_Single-Flush:0915 x 2134mm:88428" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCFURNITURE | type IFCFURNITURETYPE "600mm Depth" | object type "M_Vanity Counter Top w Round Sink Hole:600mm Depth" | names: "M_Vanity Counter Top w Round Sink Hole:600mm Depth:89266" | material: "Counter Top" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCFLOWTERMINAL | object type "M_Sink Vanity-Round:482 x 482mm" | names: "M_Sink Vanity-Round:482 x 482mm:90119" | material: "Porcelain - Linen" | property sets: Pset_EnvironmentalImpactIndicators
          2 x IFCDOOR | type IFCDOORTYPE "1730 x 2032mm" | object type "M_Double-Panel 2:1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "M_Double-Panel 2:1730 x 2032mm:91039", "M_Double-Panel 2:1730 x 2032mm:91161" | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Refridgerator_398" | object type "Refridgerator_398:Refridgerator_398" | names: "Refridgerator_398:Refridgerator_398:93909" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCFLOWTERMINAL | object type "M_Sink Kitchen-Triple:1100 x 535mm" | names: "M_Sink Kitchen-Triple:1100 x 535mm:95057" | property sets: Pset_EnvironmentalImpactIndicators
          2 x IFCWINDOW | type IFCWINDOWTYPE "0915 x 0900mm" | object type "M_Double Hung:0915 x 0900mm" | WINDOW | names: "M_Double Hung:0915 x 0900mm:99859", "M_Double Hung:0915 x 0900mm:99914" | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWTYPE "0610 x 0900mm" | object type "M_Double Hung:0610 x 0900mm" | WINDOW | names: "M_Double Hung:0610 x 0900mm:99861", "M_Double Hung:0610 x 0900mm:99913", "M_Double Hung:0610 x 0900mm:104921" | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCDOOR | type IFCDOORTYPE "32"x96"" | object type "Single_Offset_Pivot_Door_650:32"x96"" | DOOR | names: "Single_Offset_Pivot_Door_650:32"x96":102313" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCFURNITURE | type IFCFURNITURETYPE "0915 x 1830mm" | object type "M_Table-Dining:0915 x 1830mm" | names: "M_Table-Dining:0915 x 1830mm:103830" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          3 x IFCFURNITURE | type IFCFURNITURETYPE "M_Chair-Breuer" | object type "M_Chair-Breuer:M_Chair-Breuer" | names: "M_Chair-Breuer:M_Chair-Breuer:104164", "M_Chair-Breuer:M_Chair-Breuer:104382", "M_Chair-Breuer:M_Chair-Breuer:104527" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          3 x IFCFURNITURE | type IFCFURNITURETYPE "M_Chair-Breuer" | object type "M_Chair-Breuer:M_Chair-Breuer" | names: "M_Chair-Breuer:M_Chair-Breuer:104487", "M_Chair-Breuer:M_Chair-Breuer:104525", "M_Chair-Breuer:M_Chair-Breuer:104526" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCDOOR | type IFCDOORTYPE "1730 x 2032mm" | object type "M_Double-Panel 2:1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "M_Double-Panel 2:1730 x 2032mm:106395" | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCDOOR | type IFCDOORTYPE "1730 x 2032mm" | object type "M_Double-Panel 2:1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "M_Double-Panel 2:1730 x 2032mm:110171", "M_Double-Panel 2:1730 x 2032mm:233576" | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "1730 x 2032mm" | object type "M_Double-Panel 2:1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "M_Double-Panel 2:1730 x 2032mm:110172" | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCFURNITURE | type IFCFURNITURETYPE "1830mm" | object type "M_Sofa:1830mm" | names: "M_Sofa:1830mm:116146", "M_Sofa:1830mm:116197" | material: "Textile - Linen, Smooth" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCFURNITURE | type IFCFURNITURETYPE "0787 x 0711 x 0610mm" | object type "M_Table-Coffee:0787 x 0711 x 0610mm" | names: "M_Table-Coffee:0787 x 0711 x 0610mm:116790" | material: "Glass - Clear, Grey" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:152321", "Basic Wall:Retaining - 300mm Concrete:152356", "Basic Wall:Retaining - 300mm Concrete:152389" | material: layers "Basic Wall:Retaining - 300mm Concrete" ("Concrete, Cast In Situ" 300.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCSITE | object type "6PSP Paling Fence :6PSP Paling Fence 39.4m" | names: "6PSP Paling Fence :6PSP Paling Fence 39.4m:162523", "6PSP Paling Fence :6PSP Paling Fence 39.4m:180425" | material: "Timber" | property sets: Pset_SiteCommon
          1 x IFCSITE | object type "6PSP Paling Fence :6PSP Paling Fence 6.32m" | names: "6PSP Paling Fence :6PSP Paling Fence 6.32m:162710" | material: "Timber" | property sets: Pset_SiteCommon
          1 x IFCSITE | object type "6PSP Paling Fence :6PSP Paling Fence 10.2m" | names: "6PSP Paling Fence :6PSP Paling Fence 10.2m:163520" | material: "Timber" | property sets: Pset_SiteCommon
          1 x IFCSITE | object type "6PSP Paling Fence :6PSP Paling Fence 3m" | names: "6PSP Paling Fence :6PSP Paling Fence 3m:164551" | material: "Timber" | property sets: Pset_SiteCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "152mm Diameter" | object type "M_Round Column:152mm Diameter" | names: "M_Round Column:152mm Diameter:168549" | material: profiles "152mm Diameter" ("152mm Diameter": "Plastic - Vinyl Cove Base") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "152mm Diameter" | object type "M_Round Column:152mm Diameter" | names: "M_Round Column:152mm Diameter:169204" | material: "Plastic - Vinyl Cove Base" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSITE | object type "M_Manhole:M_Manhole" | names: "M_Manhole:M_Manhole:170473" | property sets: Pset_SiteCommon
          1 x IFCDOOR | type IFCDOORTYPE "0915 x 2134mm - FIRE DOOR" | object type "M_Single-Flush:0915 x 2134mm - FIRE DOOR" | DOOR | SINGLE_SWING_LEFT | names: "M_Single-Flush:0915 x 2134mm - FIRE DOOR:171948" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Dishwasher_172" | object type "Dishwasher_172:Dishwasher_172" | names: "Dishwasher_172:Dishwasher_172:175453", "Dishwasher_172:Dishwasher_172:175800", "Dishwasher_172:Dishwasher_172:226807" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Standard Timber - Deck" | object type "Floor:Standard Timber - Deck" | FLOOR | names: "Floor:Standard Timber - Deck:176978" | material: layers "Floor:Standard Timber - Deck" ("Default Floor" 32., "Structure - Timber Joist/Rafter Layer" 200.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSITE | object type "6PSP Paling Fence :6PSP Paling Fence 31.5m" | names: "6PSP Paling Fence :6PSP Paling Fence 31.5m:180252" | material: "Timber" | property sets: Pset_SiteCommon
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "50x150mm" | object type "M_Dimension Lumber-Column:50x150mm" | names: "M_Dimension Lumber-Column:50x150mm:181230", "M_Dimension Lumber-Column:50x150mm:181622" | material: profiles "50x150mm" ("50x150mm": "<Unnamed>") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Beam and Block 200mm Timber Finish" | object type "Floor:Beam and Block 200mm Timber Finish" | FLOOR | names: "Floor:Beam and Block 200mm Timber Finish:195913" | material: layers "Floor:Beam and Block 200mm Timber Finish" ("Default Floor" 22., "Structure - Timber Joist/Rafter Layer" 75., "Default Floor" 50., "Masonry - Concrete Blocks" 75., "Structure - Steel Bar Joist Layer" 75.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:90 mm Plasterboard Partition" | object type "Basic Wall:90 mm Plasterboard Partition" | names: "Basic Wall:90 mm Plasterboard Partition:221402", "Basic Wall:90 mm Plasterboard Partition:225159" | material: layers "Basic Wall:90 mm Plasterboard Partition" ("Finishes - Interior - Plasterboard" 12., "Default Wall" 66., "Finishes - Interior - Plasterboard" 12.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCFLOWTERMINAL | object type "M_Tub-Free Standing-3D:900 x 1850mm" | names: "M_Tub-Free Standing-3D:900 x 1850mm:221742" | material: "Porcelain - Ivory" | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCFLOWTERMINAL | object type "M_Toilet-Domestic-3D:M_Toilet-Domestic-3D" | names: "M_Toilet-Domestic-3D:M_Toilet-Domestic-3D:224538" | material: constituents "MaterialConstituentSet" ("Porcelain - Linen": "Porcelain - Linen", "Laminate - Linen,Matte": "Laminate - Linen,Matte") | property sets: Pset_EnvironmentalImpactIndicators
          2 x IFCDOOR | type IFCDOORTYPE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | DOOR | SINGLE_SWING_LEFT | names: "M_Single-Flush:0915 x 2134mm:225592", "M_Single-Flush:0915 x 2134mm:225649" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWINDOW | type IFCWINDOWTYPE "0915 x 1200mm" | object type "M_Double Hung:0915 x 1200mm" | WINDOW | names: "M_Double Hung:0915 x 1200mm:225698", "M_Double Hung:0915 x 1200mm:225776" | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "0915 x 1200mm" | object type "M_Double Hung:0915 x 1200mm" | WINDOW | names: "M_Double Hung:0915 x 1200mm:225774" | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          20 x IFCWINDOW | type IFCWINDOWTYPE "0400 x 0400mm" | object type "M_Fixed:0400 x 0400mm" | WINDOW | names: "M_Fixed:0400 x 0400mm:231097", "M_Fixed:0400 x 0400mm:231098", "M_Fixed:0400 x 0400mm:231127" (+17 more) | material: "Glass, Clear Glazing, Low E" | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCDOOR | type IFCDOORTYPE "0915 x 2134mm EXTERNAL" | object type "M_Single-Flush:0915 x 2134mm EXTERNAL" | DOOR | SINGLE_SWING_LEFT | names: "M_Single-Flush:0915 x 2134mm EXTERNAL:245679" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCWINDOW | type IFCWINDOWTYPE "1360x910mm" | object type "Windows_Tpl_Variable_Casement:1360x910mm" | WINDOW | names: "Windows_Tpl_Variable_Casement:1360x910mm:279385", "Windows_Tpl_Variable_Casement:1360x910mm:279450", "Windows_Tpl_Variable_Casement:1360x910mm:279466" | material: constituents "MaterialConstituentSet" ("Aluminium - White Annodized": "Aluminium - White Annodized", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "1810x1810mm" | object type "Windows_SCO_Horz_Bar_Dbl:1810x1810mm" | WINDOW | names: "Windows_SCO_Horz_Bar_Dbl:1810x1810mm:286812" | material: "Glass, Clear Glazing, Low E" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_WindowCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "330x330mm" | object type "M_Dimension Lumber-Column:330x330mm" | names: "M_Dimension Lumber-Column:330x330mm:298761" | material: profiles "330x330mm" ("330x330mm": "<Unnamed>") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          2 x IFCRAILING | object type "Railing:1100mm" | names: "Railing:1100mm:345085", "Railing:1100mm:351999" | property sets: Pset_EnvironmentalImpactIndicators, Pset_RailingCommon
        IFCSPACE "1" | long name "GF Living Area" | SPACE
        IFCSPACE "3" | long name "Garage" | SPACE
      IFCBUILDINGSTOREY "First Floor" | long name "First Floor" | object type "Level:8mm Head" | elevation 4211.99999999569
        contains 148 elements
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:140mm Timber Frame - Internal" | object type "Basic Wall:140mm Timber Frame - Internal" | names: "Basic Wall:140mm Timber Frame - Internal:72122", "Basic Wall:140mm Timber Frame - Internal:72199", "Basic Wall:140mm Timber Frame - Internal:247695" | material: layers "Basic Wall:140mm Timber Frame - Internal" ("Finishes - Interior - Plasterboard" 9., "Structure - Timber Joist/Rafter Layer" 122., "Finishes - Interior - Plasterboard" 9.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCFLOWTERMINAL | object type "M_Toilet-Domestic-3D:M_Toilet-Domestic-3D" | names: "M_Toilet-Domestic-3D:M_Toilet-Domestic-3D:76739", "M_Toilet-Domestic-3D:M_Toilet-Domestic-3D:76886" | material: constituents "MaterialConstituentSet" ("Porcelain - Linen": "Porcelain - Linen", "Laminate - Linen,Matte": "Laminate - Linen,Matte") | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | DOOR | SINGLE_SWING_LEFT | names: "M_Single-Flush:0915 x 2134mm:78568" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCFLOWTERMINAL | object type "M_Tub-Free Standing-3D:900 x 1850mm" | names: "M_Tub-Free Standing-3D:900 x 1850mm:80360", "M_Tub-Free Standing-3D:900 x 1850mm:339391" | material: "Porcelain - Ivory" | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Beam and Block 200mm Timber Finish" | object type "Floor:Beam and Block 200mm Timber Finish" | FLOOR | names: "Floor:Beam and Block 200mm Timber Finish:83028" | material: layers "Floor:Beam and Block 200mm Timber Finish" ("Default Floor" 22., "Structure - Timber Joist/Rafter Layer" 75., "Default Floor" 50., "Masonry - Concrete Blocks" 75., "Structure - Steel Bar Joist Layer" 75.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Standard Timber - Deck" | object type "Floor:Standard Timber - Deck" | FLOOR | names: "Floor:Standard Timber - Deck:83531" | material: layers "Floor:Standard Timber - Deck" ("Default Floor" 32., "Structure - Timber Joist/Rafter Layer" 200.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          12 x IFCFURNITURE | type IFCFURNITURETYPE "Aluminium / Grey-Blue" | object type "BIC Unit 1:Aluminium / Grey-Blue" | names: "BIC Unit 1:Aluminium / Grey-Blue:97846", "BIC Unit 1:Aluminium / Grey-Blue:97847", "BIC Unit 1:Aluminium / Grey-Blue:97848" (+9 more) | material: constituents "MaterialConstituentSet" ("Stacking Cabinet - Grey-Blue": "Stacking Cabinet - Grey-Blue", "Stacking Cabinet - Aluminium": "Stacking Cabinet - Aluminium") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCFURNITURE | type IFCFURNITURETYPE "600mm Depth" | object type "M_Vanity Counter Top w Round Sink Hole:600mm Depth" | names: "M_Vanity Counter Top w Round Sink Hole:600mm Depth:113135" | material: "Counter Top" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          3 x IFCFLOWTERMINAL | object type "M_Sink Vanity-Round:482 x 482mm" | names: "M_Sink Vanity-Round:482 x 482mm:113136", "M_Sink Vanity-Round:482 x 482mm:113660", "M_Sink Vanity-Round:482 x 482mm:339310" | material: "Porcelain - Linen" | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCFURNITURE | type IFCFURNITURETYPE "600mm Depth" | object type "M_Vanity Counter Top w Round Sink Hole:600mm Depth" | names: "M_Vanity Counter Top w Round Sink Hole:600mm Depth:113659" | material: "Counter Top" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "0610 x 1200mm" | object type "M_Double Hung:0610 x 1200mm" | WINDOW | names: "M_Double Hung:0610 x 1200mm:114399" | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "0610 x 1200mm" | object type "M_Double Hung:0610 x 1200mm" | WINDOW | names: "M_Double Hung:0610 x 1200mm:114496" | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:280 Timber Frame Wall (Stairwell)" | object type "Basic Wall:280 Timber Frame Wall (Stairwell)" | names: "Basic Wall:280 Timber Frame Wall (Stairwell):233877", "Basic Wall:280 Timber Frame Wall (Stairwell):260656", "Basic Wall:280 Timber Frame Wall (Stairwell):343348" | material: layers "Basic Wall:280 Timber Frame Wall (Stairwell)" ("Masonry - Brick" 20., "Structure - Timber Joist/Rafter Layer" 114., "Masonry - Brick" 12., "Structure - Timber Joist/Rafter Layer" 114., "Masonry - Brick" 20.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | DOOR | SINGLE_SWING_LEFT | names: "M_Single-Flush:0915 x 2134mm:233919" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          13 x IFCWALL | type IFCWALLTYPE "Basic Wall:140mm Timber Frame - With Cladding" | object type "Basic Wall:140mm Timber Frame - With Cladding" | names: "Basic Wall:140mm Timber Frame - With Cladding:244003", "Basic Wall:140mm Timber Frame - With Cladding:246034", "Basic Wall:140mm Timber Frame - With Cladding:246091" (+10 more) | material: layers "Basic Wall:140mm Timber Frame - With Cladding" ("Wall material 1" 9., "Structure - Timber Joist/Rafter Layer" 140., "Gypsum Wall Board" 9.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | DOOR | SINGLE_SWING_RIGHT | names: "M_Single-Flush:0915 x 2134mm:247906" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCFURNITURE | type IFCFURNITURETYPE "Aluminium / Grey-Blue" | object type "BIC Unit 1:Aluminium / Grey-Blue" | names: "BIC Unit 1:Aluminium / Grey-Blue:247983", "BIC Unit 1:Aluminium / Grey-Blue:247984", "BIC Unit 1:Aluminium / Grey-Blue:247985" | material: constituents "MaterialConstituentSet" ("Stacking Cabinet - Grey-Blue": "Stacking Cabinet - Grey-Blue", "Stacking Cabinet - Aluminium": "Stacking Cabinet - Aluminium") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCDOOR | type IFCDOORTYPE "0915 x 2032mm" | object type "M_Single-Flush:0915 x 2032mm" | DOOR | SINGLE_SWING_RIGHT | names: "M_Single-Flush:0915 x 2032mm:247996" | material: constituents "MaterialConstituentSet" ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWINDOW | type IFCWINDOWTYPE "0450 x 0600mm" | object type "M_Fixed:0450 x 0600mm" | WINDOW | names: "M_Fixed:0450 x 0600mm:248063", "M_Fixed:0450 x 0600mm:352884" | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Beam and Block 200mm Timber Finish 2" | object type "Floor:Beam and Block 200mm Timber Finish 2" | FLOOR | names: "Floor:Beam and Block 200mm Timber Finish 2:248804" | material: layers "Floor:Beam and Block 200mm Timber Finish 2" ("Default Floor" 22., "Structure - Timber Joist/Rafter Layer" 225.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORTYPE "1730 x 2032mm" | object type "M_Double-Panel 2:1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "M_Double-Panel 2:1730 x 2032mm:253273" | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:Shower Wall" | object type "Basic Wall:Shower Wall" | names: "Basic Wall:Shower Wall:254156", "Basic Wall:Shower Wall:339141", "Basic Wall:Shower Wall:346570" | material: layers "Basic Wall:Shower Wall" ("Glazing - Curtain Wall Glazing" 15.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Curtain Wall - Simon" | object type "Basic Wall:Curtain Wall - Simon" | names: "Basic Wall:Curtain Wall - Simon:254539", "Basic Wall:Curtain Wall - Simon:339142" | material: layers "Basic Wall:Curtain Wall - Simon" ("Glazing - Curtain Wall Glazing" 15.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORTYPE "0915 x 2100mm Shower Door" | object type "M_Single-Flush:0915 x 2100mm Shower Door" | DOOR | SINGLE_SWING_RIGHT | names: "M_Single-Flush:0915 x 2100mm Shower Door:254931", "M_Single-Flush:0915 x 2100mm Shower Door:339143" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          6 x IFCWINDOW | type IFCWINDOWTYPE "0915 x 1200mm" | object type "M_Double Hung:0915 x 1200mm" | WINDOW | names: "M_Double Hung:0915 x 1200mm:257500", "M_Double Hung:0915 x 1200mm:391717", "M_Double Hung:0915 x 1200mm:392046" (+3 more) | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWTYPE "0915 x 1200mm" | object type "M_Double Hung:0915 x 1200mm" | WINDOW | names: "M_Double Hung:0915 x 1200mm:257645", "M_Double Hung:0915 x 1200mm:296654", "M_Double Hung:0915 x 1200mm:391652" | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Ceiling:Generic" | object type "Basic Ceiling:Generic" | CEILING | names: "Basic Ceiling:Generic:262924" | material: layers "Basic Ceiling:Generic" ("<Unnamed>" 0.) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Ceiling:Generic" | object type "Basic Ceiling:Generic" | CEILING | names: "Basic Ceiling:Generic:263296" | material: layers "Basic Ceiling:Generic" ("<Unnamed>" 0.) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          20 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "150mm_Diameter-60_Watt_Incandescent" | object type "Lighting_Fixtures_Downlight_Recessed_Can:150mm_Diameter-60_Watt_Incandescent" | names: "Lighting_Fixtures_Downlight_Recessed_Can:150mm_Diameter-60_Watt_Incandescent:264348", "Lighting_Fixtures_Downlight_Recessed_Can:150mm_Diameter-60_Watt_Incandescent:264571", "Lighting_Fixtures_Downlight_Recessed_Can:150mm_Diameter-60_Watt_Incandescent:264602" (+17 more) | property sets: Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon
          2 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "100_Watt_Incandescent" | object type "Lighting_Fixtures_Mdrn_Uplighter:100_Watt_Incandescent" | names: "Lighting_Fixtures_Mdrn_Uplighter:100_Watt_Incandescent:266661", "Lighting_Fixtures_Mdrn_Uplighter:100_Watt_Incandescent:266698" | property sets: Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Double" | object type "Elect_Equipment_Dbl_Socket:Double" | names: "Elect_Equipment_Dbl_Socket:Double:271087", "Elect_Equipment_Dbl_Socket:Double:271208" | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          11 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Double" | object type "Elect_Equipment_Dbl_Socket:Double" | names: "Elect_Equipment_Dbl_Socket:Double:271276", "Elect_Equipment_Dbl_Socket:Double:271338", "Elect_Equipment_Dbl_Socket:Double:271364" (+8 more) | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Single_Pole" | object type "Elect_Equipment_Switch_Sgl_Pole:Single_Pole" | names: "Elect_Equipment_Switch_Sgl_Pole:Single_Pole:272097", "Elect_Equipment_Switch_Sgl_Pole:Single_Pole:272156" | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Single_Pole" | object type "Elect_Equipment_Switch_Sgl_Pole:Single_Pole" | names: "Elect_Equipment_Switch_Sgl_Pole:Single_Pole:272244" | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Single_Pole" | object type "Elect_Equipment_Switch_Sgl_Pole:Single_Pole" | names: "Elect_Equipment_Switch_Sgl_Pole:Single_Pole:272288" | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "2_Gang" | object type "Elect_Equipment_Switch_Sgl_Pole_2-Gang:2_Gang" | names: "Elect_Equipment_Switch_Sgl_Pole_2-Gang:2_Gang:272978", "Elect_Equipment_Switch_Sgl_Pole_2-Gang:2_Gang:273015" | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Double" | object type "Elect_Equipment_Dbl_Socket:Double" | names: "Elect_Equipment_Dbl_Socket:Double:273133" | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Double" | object type "Elect_Equipment_Dbl_Socket:Double" | names: "Elect_Equipment_Dbl_Socket:Double:273372" | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          6 x IFCBUILDINGELEMENTPROXY | names: "273882", "273883", "274164" (+3 more) | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          1 x IFCBEAM | type IFCBEAMTYPE "79X305" | object type "Glulam (2):79X305" | names: "Glulam (2):79X305:298904" | material: profiles "79X305" ("79X305": "<Unnamed>") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCDOOR | type IFCDOORTYPE "0915 x 2032mm" | object type "M_Single-Flush:0915 x 2032mm" | DOOR | SINGLE_SWING_LEFT | names: "M_Single-Flush:0915 x 2032mm:338952" | material: constituents "MaterialConstituentSet" ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCFURNITURE | type IFCFURNITURETYPE "600mm Depth" | object type "M_Vanity Counter Top w Round Sink Hole:600mm Depth" | names: "M_Vanity Counter Top w Round Sink Hole:600mm Depth:339309" | material: "Counter Top" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          12 x IFCWINDOW | type IFCWINDOWTYPE "0400 x 0400mm" | object type "M_Fixed:0400 x 0400mm" | WINDOW | names: "M_Fixed:0400 x 0400mm:344403", "M_Fixed:0400 x 0400mm:344405", "M_Fixed:0400 x 0400mm:344407" (+9 more) | material: "Glass, Clear Glazing, Low E" | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete 297mm" | object type "Floor:Insitu Concrete 297mm" | FLOOR | names: "Floor:Insitu Concrete 297mm:344514" | material: layers "Floor:Insitu Concrete 297mm" ("Default Floor" 72., "Default Floor" 50., "Vapour / Moisture Barriers - Damp-proofing" 0., "Concrete - Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete 297mm" | object type "Floor:Insitu Concrete 297mm" | FLOOR | names: "Floor:Insitu Concrete 297mm:344514:2" | material: layers "Floor:Insitu Concrete 297mm" ("Default Floor" 72., "Default Floor" 50., "Vapour / Moisture Barriers - Damp-proofing" 0., "Concrete - Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete 297mm" | object type "Floor:Insitu Concrete 297mm" | FLOOR | names: "Floor:Insitu Concrete 297mm:344514:3" | material: layers "Floor:Insitu Concrete 297mm" ("Default Floor" 72., "Default Floor" 50., "Vapour / Moisture Barriers - Damp-proofing" 0., "Concrete - Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete 225mm" | object type "Floor:Insitu Concrete 225mm" | FLOOR | names: "Floor:Insitu Concrete 225mm:345368" | material: layers "Floor:Insitu Concrete 225mm" ("Concrete, Sand/Cement Screed" 50., "Damp-proofing" 0., "Concrete, Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Wet Floor" | object type "Floor:Wet Floor" | FLOOR | names: "Floor:Wet Floor:345967" | material: layers "Floor:Wet Floor" ("Default Floor" 75.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Wet Floor" | object type "Floor:Wet Floor" | FLOOR | names: "Floor:Wet Floor:345967:2" | material: layers "Floor:Wet Floor" ("Default Floor" 75.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          5 x IFCRAILING | object type "Railing:1100mm" | names: "Railing:1100mm:110645", "Railing:1100mm:154119", "Railing:1100mm:345488" (+2 more) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RailingCommon
        IFCSPACE "2" | long name "FF Living Area" | SPACE
      IFCBUILDINGSTOREY "Roof Eaves" | long name "Roof Eaves" | object type "Level:8mm Head" | elevation 6611.99999999996
        contains 21 elements
          4 x IFCROOF | object type "Basic Roof:Warm Roof - IBR on Timber Beams" | names: "Basic Roof:Warm Roof - IBR on Timber Beams:82070", "Basic Roof:Warm Roof - IBR on Timber Beams:249380", "Basic Roof:Warm Roof - IBR on Timber Beams:249712" (+1 more) | parts: 5 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 140mm Clerestory" | object type "Basic Wall:Generic - 140mm Clerestory" | names: "Basic Wall:Generic - 140mm Clerestory:252123", "Basic Wall:Generic - 140mm Clerestory:260828" | material: layers "Basic Wall:Generic - 140mm Clerestory" ("Finishes - Exterior - EIFS - Exterior Insulation and Finish System" 15., "Structure - Timber Joist/Rafter Layer" 110., "Finishes - Interior - Plasterboard" 15.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWINDOW | type IFCWINDOWTYPE "1000 x 450mm Clerestory" | object type "M_Fixed:1000 x 450mm Clerestory" | WINDOW | names: "M_Fixed:1000 x 450mm Clerestory:256705", "M_Fixed:1000 x 450mm Clerestory:256921", "M_Fixed:1000 x 450mm Clerestory:257133" (+3 more) | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWTYPE "1000 x 450mm Clerestory" | object type "M_Fixed:1000 x 450mm Clerestory" | WINDOW | names: "M_Fixed:1000 x 450mm Clerestory:257163", "M_Fixed:1000 x 450mm Clerestory:257164", "M_Fixed:1000 x 450mm Clerestory:259550" | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          4 x IFCBUILDINGELEMENTPROXY | object type "Fascia:Fascia" | names: "Fascia:Fascia:273533", "Fascia:Fascia:273535", "Fascia:Fascia:273579" (+1 more) | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Gutter:Gutter:19886" | object type "Gutter:Gutter" | names: "Gutter:Gutter:273538" | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Gutter:Gutter:19886" | object type "Gutter:Gutter" | names: "Gutter:Gutter:273540" | property sets: Pset_EnvironmentalImpactIndicators

Types
  IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | 13 occurrences | material: layers "Basic Wall:Retaining - 300mm Concrete" ("Concrete, Cast In Situ" 300.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:220mm Brick Wall With Symmetrical Footing" | 2 occurrences | material: layers "Basic Wall:220mm Brick Wall With Symmetrical Footing" ("Masonry - Brick" 220.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:280mm Brick Cavity Wall With Symmetrical Footing" | 13 occurrences | material: layers "Basic Wall:280mm Brick Cavity Wall With Symmetrical Footing" ("Masonry - Brick Soldier Course" 110., "Default Wall" 60., "Masonry - Brick Soldier Course" 110.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:110mm Brick Wall" | 5 occurrences | material: layers "Basic Wall:110mm Brick Wall" ("Masonry - Brick" 110.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Floor:Insitu Concrete 225mm" | FLOOR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:Insitu Concrete 225mm" | FLOOR | 1 occurrence | material: layers "Floor:Insitu Concrete 225mm" ("Concrete, Sand/Cement Screed" 50., "Damp-proofing" 0., "Concrete, Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:Insitu Concrete 225mm" | FLOOR | 1 occurrence | material: layers "Floor:Insitu Concrete 225mm" ("Concrete, Sand/Cement Screed" 50., "Damp-proofing" 0., "Concrete, Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORTYPE "0915 x 2134mm" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | property sets: M_Single-Flush:0915 x 2134mm:88428, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCFURNITURETYPE "600mm Depth" | 1 occurrence | material: "Counter Top" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCDOORTYPE "1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: M_Double-Panel 2:1730 x 2032mm:91039, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Refridgerator_398" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "0915 x 0900mm" | WINDOW | 2 occurrences | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Double Hung:0915 x 0900mm:99859, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "0610 x 0900mm" | WINDOW | 3 occurrences | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Double Hung:0610 x 0900mm:99861, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCDOORTYPE "32"x96"" | DOOR | 1 occurrence | property sets: Single_Offset_Pivot_Door_650:32"x96":102313, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCFURNITURETYPE "0915 x 1830mm" | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCFURNITURETYPE "M_Chair-Breuer" | 3 occurrences | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCFURNITURETYPE "M_Chair-Breuer" | 3 occurrences | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCDOORTYPE "1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: M_Double-Panel 2:1730 x 2032mm:106395, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: M_Double-Panel 2:1730 x 2032mm:110171, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: M_Double-Panel 2:1730 x 2032mm:110172, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCFURNITURETYPE "1830mm" | 2 occurrences | material: "Textile - Linen, Smooth" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCFURNITURETYPE "0787 x 0711 x 0610mm" | 1 occurrence | material: "Glass - Clear, Grey" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCCOLUMNTYPE "152mm Diameter" | COLUMN | 1 occurrence | material: profiles "152mm Diameter" ("152mm Diameter": "Plastic - Vinyl Cove Base") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "152mm Diameter" | COLUMN | 1 occurrence | material: profiles "152mm Diameter" ("152mm Diameter": "Plastic - Vinyl Cove Base") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCDOORTYPE "0915 x 2134mm - FIRE DOOR" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: M_Single-Flush:0915 x 2134mm - FIRE DOOR:171948, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Dishwasher_172" | 3 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCSLABTYPE "Floor:Standard Timber - Deck" | FLOOR | 1 occurrence | material: layers "Floor:Standard Timber - Deck" ("Default Floor" 32., "Structure - Timber Joist/Rafter Layer" 200.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "50x150mm" | COLUMN | 2 occurrences | material: profiles "50x150mm" ("50x150mm": "<Unnamed>") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCSLABTYPE "Floor:Beam and Block 200mm Timber Finish" | FLOOR | 1 occurrence | material: layers "Floor:Beam and Block 200mm Timber Finish" ("Default Floor" 22., "Structure - Timber Joist/Rafter Layer" 75., "Default Floor" 50., "Masonry - Concrete Blocks" 75., "Structure - Steel Bar Joist Layer" 75.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:90 mm Plasterboard Partition" | 2 occurrences | material: layers "Basic Wall:90 mm Plasterboard Partition" ("Finishes - Interior - Plasterboard" 12., "Default Wall" 66., "Finishes - Interior - Plasterboard" 12.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "0915 x 2134mm" | DOOR | SINGLE_SWING_LEFT | 2 occurrences | property sets: M_Single-Flush:0915 x 2134mm:225592, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "0915 x 1200mm" | WINDOW | 2 occurrences | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Double Hung:0915 x 1200mm:225698, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "0915 x 1200mm" | WINDOW | 1 occurrence | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Double Hung:0915 x 1200mm:225774, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "0400 x 0400mm" | WINDOW | 20 occurrences | material: "Glass, Clear Glazing, Low E" | property sets: M_Fixed:0400 x 0400mm:231097, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCDOORTYPE "0915 x 2134mm EXTERNAL" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: M_Single-Flush:0915 x 2134mm EXTERNAL:245679, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "1360x910mm" | WINDOW | 3 occurrences | material: constituents "MaterialConstituentSet" ("Aluminium - White Annodized": "Aluminium - White Annodized", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: Windows_Tpl_Variable_Casement:1360x910mm:279385, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "1810x1810mm" | WINDOW | 1 occurrence | material: "Glass, Clear Glazing, Low E" | property sets: Windows_SCO_Horz_Bar_Dbl:1810x1810mm:286812, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCCOLUMNTYPE "330x330mm" | COLUMN | 1 occurrence | material: profiles "330x330mm" ("330x330mm": "<Unnamed>") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCWALLTYPE "Basic Wall:140mm Timber Frame - Internal" | 3 occurrences | material: layers "Basic Wall:140mm Timber Frame - Internal" ("Finishes - Interior - Plasterboard" 9., "Structure - Timber Joist/Rafter Layer" 122., "Finishes - Interior - Plasterboard" 9.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "0915 x 2134mm" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: M_Single-Flush:0915 x 2134mm:78568, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCSLABTYPE "Floor:Beam and Block 200mm Timber Finish" | FLOOR | 1 occurrence | material: layers "Floor:Beam and Block 200mm Timber Finish" ("Default Floor" 22., "Structure - Timber Joist/Rafter Layer" 75., "Default Floor" 50., "Masonry - Concrete Blocks" 75., "Structure - Steel Bar Joist Layer" 75.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:Standard Timber - Deck" | FLOOR | 1 occurrence | material: layers "Floor:Standard Timber - Deck" ("Default Floor" 32., "Structure - Timber Joist/Rafter Layer" 200.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCFURNITURETYPE "Aluminium / Grey-Blue" | 12 occurrences | material: constituents "MaterialConstituentSet" ("Stacking Cabinet - Grey-Blue": "Stacking Cabinet - Grey-Blue", "Stacking Cabinet - Aluminium": "Stacking Cabinet - Aluminium") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCFURNITURETYPE "600mm Depth" | 1 occurrence | material: "Counter Top" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCFURNITURETYPE "600mm Depth" | 1 occurrence | material: "Counter Top" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCWINDOWTYPE "0610 x 1200mm" | WINDOW | 1 occurrence | property sets: M_Double Hung:0610 x 1200mm:114399, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "0610 x 1200mm" | WINDOW | 1 occurrence | property sets: M_Double Hung:0610 x 1200mm:114496, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWALLTYPE "Basic Wall:280 Timber Frame Wall (Stairwell)" | 3 occurrences | material: layers "Basic Wall:280 Timber Frame Wall (Stairwell)" ("Masonry - Brick" 20., "Structure - Timber Joist/Rafter Layer" 114., "Masonry - Brick" 12., "Structure - Timber Joist/Rafter Layer" 114., "Masonry - Brick" 20.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "0915 x 2134mm" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: M_Single-Flush:0915 x 2134mm:233919, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCWALLTYPE "Basic Wall:140mm Timber Frame - With Cladding" | 13 occurrences | material: layers "Basic Wall:140mm Timber Frame - With Cladding" ("Wall material 1" 9., "Structure - Timber Joist/Rafter Layer" 140., "Gypsum Wall Board" 9.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "0915 x 2134mm" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | property sets: M_Single-Flush:0915 x 2134mm:247906, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCFURNITURETYPE "Aluminium / Grey-Blue" | 3 occurrences | material: constituents "MaterialConstituentSet" ("Stacking Cabinet - Grey-Blue": "Stacking Cabinet - Grey-Blue", "Stacking Cabinet - Aluminium": "Stacking Cabinet - Aluminium") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCDOORTYPE "0915 x 2032mm" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: M_Single-Flush:0915 x 2032mm:247996, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "0450 x 0600mm" | WINDOW | 2 occurrences | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Fixed:0450 x 0600mm:248063, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCSLABTYPE "Floor:Beam and Block 200mm Timber Finish 2" | FLOOR | 1 occurrence | material: layers "Floor:Beam and Block 200mm Timber Finish 2" ("Default Floor" 22., "Structure - Timber Joist/Rafter Layer" 225.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORTYPE "1730 x 2032mm" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: constituents "MaterialConstituentSet" ("Door - Panel": "Door - Panel", "Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E") | property sets: M_Double-Panel 2:1730 x 2032mm:253273, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCWALLTYPE "Basic Wall:Shower Wall" | 3 occurrences | material: layers "Basic Wall:Shower Wall" ("Glazing - Curtain Wall Glazing" 15.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:Curtain Wall - Simon" | 2 occurrences | material: layers "Basic Wall:Curtain Wall - Simon" ("Glazing - Curtain Wall Glazing" 15.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "0915 x 2100mm Shower Door" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | property sets: M_Single-Flush:0915 x 2100mm Shower Door:254931, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "0915 x 1200mm" | WINDOW | 6 occurrences | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Double Hung:0915 x 1200mm:257500, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "0915 x 1200mm" | WINDOW | 3 occurrences | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Double Hung:0915 x 1200mm:257645, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCCOVERINGTYPE "Basic Ceiling:Generic" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Basic Ceiling:Generic" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCLIGHTFIXTURETYPE "150mm_Diameter-60_Watt_Incandescent" | 20 occurrences | property sets: Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon
  IFCLIGHTFIXTURETYPE "100_Watt_Incandescent" | 2 occurrences | property sets: Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon
  IFCBUILDINGELEMENTPROXYTYPE "Double" | 2 occurrences | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Double" | 11 occurrences | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Single_Pole" | 2 occurrences | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Single_Pole" | 1 occurrence | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Single_Pole" | 1 occurrence | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "2_Gang" | 2 occurrences | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Double" | 1 occurrence | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Double" | 1 occurrence | material: "Plastic - White" | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBEAMTYPE "79X305" | BEAM | 1 occurrence | material: profiles "79X305" ("79X305": "<Unnamed>") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCDOORTYPE "0915 x 2032mm" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: M_Single-Flush:0915 x 2032mm:338952, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCFURNITURETYPE "600mm Depth" | 1 occurrence | material: "Counter Top" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
  IFCWINDOWTYPE "0400 x 0400mm" | WINDOW | 12 occurrences | material: "Glass, Clear Glazing, Low E" | property sets: M_Fixed:0400 x 0400mm:344403, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCSLABTYPE "Floor:Insitu Concrete 297mm" | FLOOR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:Insitu Concrete 297mm" | FLOOR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:Insitu Concrete 297mm" | FLOOR | 1 occurrence | material: layers "Floor:Insitu Concrete 297mm" ("Default Floor" 72., "Default Floor" 50., "Vapour / Moisture Barriers - Damp-proofing" 0., "Concrete - Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:Insitu Concrete 225mm" | FLOOR | 1 occurrence | material: layers "Floor:Insitu Concrete 225mm" ("Concrete, Sand/Cement Screed" 50., "Damp-proofing" 0., "Concrete, Cast In Situ" 175.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:Wet Floor" | FLOOR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:Wet Floor" | FLOOR | 1 occurrence | material: layers "Floor:Wet Floor" ("Default Floor" 75.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:Generic - 140mm Clerestory" | 2 occurrences | material: layers "Basic Wall:Generic - 140mm Clerestory" ("Finishes - Exterior - EIFS - Exterior Insulation and Finish System" 15., "Structure - Timber Joist/Rafter Layer" 110., "Finishes - Interior - Plasterboard" 15.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWINDOWTYPE "1000 x 450mm Clerestory" | WINDOW | 6 occurrences | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Fixed:1000 x 450mm Clerestory:256705, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "1000 x 450mm Clerestory" | WINDOW | 3 occurrences | material: constituents "MaterialConstituentSet" ("Glass, Clear Glazing, Low E": "Glass, Clear Glazing, Low E", "Aluminium - White Annodized": "Aluminium - White Annodized") | property sets: M_Fixed:1000 x 450mm Clerestory:257163, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCPIPESEGMENTTYPE "Gutter:Gutter:19886" | element type "Gutter:Gutter:19886" | GUTTER | 1 occurrence
  IFCPIPESEGMENTTYPE "Gutter:Gutter:19886" | element type "Gutter:Gutter:19886" | GUTTER | 1 occurrence

Property sets
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "GF Living Area" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "FF Living Area" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "Garage" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GF Living Area 1" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "FF Living Area 2" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Garage 3" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 32 objects (32 IFCWINDOW) | on 2 type objects
    Reference = "0400 x 0400mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 25 objects (13 IFCWALL, 12 IFCOPENINGELEMENT) | on 1 type object
    Reference = "280mm Brick Cavity Wall With Symmetrical Footing" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    Reference = "" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 20 objects (20 IFCLIGHTFIXTURE) | on 1 type object
    Reference = "150mm_Diameter-60_Watt_Incandescent" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Reference = "Double" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 15 objects (15 IFCFURNITURE) | on 2 type objects
    Reference = "Aluminium / Grey-Blue" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 13 objects (13 IFCWALL) | on 1 type object
    Reference = "Retaining - 300mm Concrete" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 13 objects (13 IFCWALL) | on 1 type object
    Reference = "140mm Timber Frame - With Cladding" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 54 more contents on 178 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 13 objects (13 IFCWALL) | on 1 type object
    Reference = "280mm Brick Cavity Wall With Symmetrical Footing" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 13 objects (13 IFCWALL) | on 1 type object
    Reference = "Retaining - 300mm Concrete" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 13 objects (13 IFCWALL) | on 1 type object
    Reference = "140mm Timber Frame - With Cladding" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 5 objects (5 IFCWALL) | on 1 type object
    Reference = "110mm Brick Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL) | on 1 type object
    Reference = "140mm Timber Frame - Internal" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL) | on 1 type object
    Reference = "280 Timber Frame Wall (Stairwell)" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL) | on 1 type object
    Reference = "Shower Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALL) | on 1 type object
    Reference = "90 mm Plasterboard Partition" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 3 more contents on 6 objects not shown
  Pset_WallCommon | properties | on 13 objects (13 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Retaining - 300mm Concrete" (IFCIDENTIFIER)
    ThermalTransmittance = 3.48666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 13 objects (13 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "140mm Timber Frame - With Cladding" (IFCIDENTIFIER)
    ThermalTransmittance = 72.2222222222222 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 11 objects (11 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "280mm Brick Cavity Wall With Symmetrical Footing" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "110mm Brick Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "140mm Timber Frame - Internal" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "280 Timber Frame Wall (Stairwell)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Shower Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "280mm Brick Cavity Wall With Symmetrical Footing" (IFCIDENTIFIER)
  Pset_WallCommon: 17 more contents on 10 objects not shown
  Pset_OpeningElementCommon | properties | on 12 objects (12 IFCOPENINGELEMENT)
    Reference = "280mm Brick Cavity Wall With Symmetrical Footing" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 8 objects (8 IFCOPENINGELEMENT)
    Reference = "280 Timber Frame Wall (Stairwell)" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 4 objects (4 IFCOPENINGELEMENT)
    Reference = "600mm Depth" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Generic - 140mm Clerestory" (IFCIDENTIFIER)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 15. (IFCCOUNTMEASURE)
    NumberOfTreads = 14. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 188.678749999712 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 974.999999999987 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 487.499999999994 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 8. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 129.979861111111 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 974.999999999987 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 487.499999999994 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "1730 x 2032mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR) | on 5 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR) | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2032mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2100mm Shower Door" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "32"x96"" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm - FIRE DOOR" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm EXTERNAL" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 5 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1730 x 2032mm" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 4 objects (4 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Warm Roof - IBR on Timber Beams" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfSlab | properties | on 5 objects (5 IFCSLAB)
    Reference = "Warm Roof - IBR on Timber Beams" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB) | on 4 type objects
    Reference = "Insitu Concrete 225mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB) | on 3 type objects
    Reference = "Insitu Concrete 297mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "Beam and Block 200mm Timber Finish" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "Standard Timber - Deck" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "Wet Floor" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Beam and Block 200mm Timber Finish 2" (IFCLABEL)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Insitu Concrete 225mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.64888888888889 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 9.07475997113757 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Warm Roof - IBR on Timber Beams" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Insitu Concrete 297mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 13.2277729753144 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Warm Roof - IBR on Timber Beams" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Beam and Block 200mm Timber Finish" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Standard Timber - Deck" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Wet Floor" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Beam and Block 200mm Timber Finish 2" (IFCIDENTIFIER)
  Pset_SlabCommon: 7 more contents on 1 objects not shown
  Pset_FurnitureTypeCommon | properties | on 15 objects (15 IFCFURNITURE) | on 2 type objects
    Reference = "Aluminium / Grey-Blue" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 6 objects (6 IFCFURNITURE) | on 2 type objects
    Reference = "M_Chair-Breuer" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 4 objects (4 IFCFURNITURE) | on 4 type objects
    Reference = "600mm Depth" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 2 objects (2 IFCFURNITURE) | on 1 type object
    Reference = "1830mm" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 1 object (1 IFCFURNITURE) | on 1 type object
    Reference = "0915 x 1830mm" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 1 object (1 IFCFURNITURE) | on 1 type object
    Reference = "0787 x 0711 x 0610mm" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Double" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Single_Pole" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Fascia" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Dishwasher_172" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2_Gang" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Refridgerator_398" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Double" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 2 more contents on 0 objects not shown
  Pset_WindowCommon | properties | on 32 objects (32 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0400 x 0400mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 12 objects (12 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0915 x 1200mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 9 objects (9 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "1000 x 450mm Clerestory" (IFCIDENTIFIER)
    ThermalTransmittance = 2.2147 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0610 x 0900mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "1360x910mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0915 x 0900mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0610 x 1200mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0450 x 0600mm" (IFCIDENTIFIER)
  Pset_WindowCommon: 10 more contents on 1 objects not shown
  Pset_BuildingElementProxyProvisionForVoid | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Height = 85. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 170. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Depth = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Height = 85. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 85. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Depth = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 750. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Depth = 235. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 19. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 235. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 749.999999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 6957.47500000002 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 6957.47500000002 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 99.9999999999978 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 99.9999999999978 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyProvisionForVoid: 3 more contents on 4 objects not shown
  Pset_SiteCommon | properties | on 2 objects (2 IFCSITE)
    Reference = "6PSP Paling Fence 39.4m" (IFCIDENTIFIER)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Surface" (IFCIDENTIFIER)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "6PSP Paling Fence 6.32m" (IFCIDENTIFIER)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "6PSP Paling Fence 10.2m" (IFCIDENTIFIER)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "6PSP Paling Fence 3m" (IFCIDENTIFIER)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "M_Manhole" (IFCIDENTIFIER)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "6PSP Paling Fence 31.5m" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "152mm Diameter" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x150mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "330x330mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "152mm Diameter" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x150mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "330x330mm" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 2 objects (2 IFCCOLUMN) | on 2 type objects
    Reference = "152mm Diameter" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 2 objects (2 IFCCOLUMN) | on 1 type object
    Reference = "50x150mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN) | on 1 type object
    Reference = "330x330mm" (IFCLABEL)
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 20 objects (20 IFCLIGHTFIXTURE) | on 1 type object
    Reference = "150mm_Diameter-60_Watt_Incandescent" (IFCIDENTIFIER)
    TotalWattage = 60. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 2 objects (2 IFCLIGHTFIXTURE) | on 1 type object
    Reference = "100_Watt_Incandescent" (IFCIDENTIFIER)
    TotalWattage = 150. (IFCPOWERMEASURE) [WATT]
  Pset_ManufacturerTypeInformation | properties | on 4 objects (4 IFCWINDOW) | on 2 type objects
    Manufacturer = "Revit" (IFCLABEL)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "79X305" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6022. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "79X305" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM) | on 1 type object
    Reference = "79X305" (IFCLABEL)
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 8. (IFCCOUNTMEASURE)
    Reference = "50mm Tread 13mm Riser" (IFCIDENTIFIER)
    RiserHeight = 129.979861111111 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_RailingCommon | properties | on 10 objects (10 IFCRAILING)
    Height = 1100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100mm" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "8mm Head" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 4 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  M_Single-Flush:0915 x 2134mm:88428 | predefined | on 2 type objects
  M_Double-Panel 2:1730 x 2032mm:91039 | predefined | on 2 type objects
  M_Double Hung:0915 x 0900mm:99859 | predefined | on 1 type object
  M_Double Hung:0610 x 0900mm:99861 | predefined | on 1 type object
  Single_Offset_Pivot_Door_650:32"x96":102313 | predefined | on 2 type objects
  M_Double-Panel 2:1730 x 2032mm:106395 | predefined | on 2 type objects
  M_Double-Panel 2:1730 x 2032mm:110171 | predefined | on 2 type objects
  M_Double-Panel 2:1730 x 2032mm:110172 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm - FIRE DOOR:171948 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm:225592 | predefined | on 2 type objects
  M_Double Hung:0915 x 1200mm:225698 | predefined | on 1 type object
  M_Double Hung:0915 x 1200mm:225774 | predefined | on 1 type object
  M_Fixed:0400 x 0400mm:231097 | predefined | on 1 type object
  M_Single-Flush:0915 x 2134mm EXTERNAL:245679 | predefined | on 2 type objects
  Windows_Tpl_Variable_Casement:1360x910mm:279385 | predefined | on 1 type object
  Windows_SCO_Horz_Bar_Dbl:1810x1810mm:286812 | predefined | on 1 type object
  M_Single-Flush:0915 x 2134mm:78568 | predefined | on 2 type objects
  M_Double Hung:0610 x 1200mm:114399 | predefined | on 1 type object
  M_Double Hung:0610 x 1200mm:114496 | predefined | on 1 type object
  M_Single-Flush:0915 x 2134mm:233919 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm:247906 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2032mm:247996 | predefined | on 2 type objects
  M_Fixed:0450 x 0600mm:248063 | predefined | on 1 type object
  M_Double-Panel 2:1730 x 2032mm:253273 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2100mm Shower Door:254931 | predefined | on 2 type objects
  M_Double Hung:0915 x 1200mm:257500 | predefined | on 1 type object
  M_Double Hung:0915 x 1200mm:257645 | predefined | on 1 type object
  M_Single-Flush:0915 x 2032mm:338952 | predefined | on 2 type objects
  M_Fixed:0400 x 0400mm:344403 | predefined | on 1 type object
  M_Fixed:1000 x 450mm Clerestory:256705 | predefined | on 1 type object
  M_Fixed:1000 x 450mm Clerestory:257163 | predefined | on 1 type object

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"