IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "CSV2SoR_empty.ifc"
Time stamp: "2023-12-13T10:10:30+00:00"
Preprocessor: "IfcOpenShell v0.7.0-6c9e130ca"
Originating system: "BlenderBIM 0.0.231104-4e76f36"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Buidling"
      IFCBUILDINGSTOREY "1F"
        contains 9 elements
          4 x IFCBEAM | type IFCBEAMTYPE "BEM-01" | names: "Beam" | material: profiles ("C30-37") | property sets: EPset_Parametric, Qto_BeamBaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "SLB-02" | names: "Slab" | material: layers "raft slab" ("C25-30" 0.150000005960464) | property sets: EPset_Parametric, Qto_SlabBaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "WAL-03" | names: "Wall" | material: layers ("BLK-02" 0.150000005960464) | property sets: EPset_Parametric, Qto_WallBaseQuantities
      IFCBUILDINGSTOREY "GF"
        contains 10 elements
          1 x IFCSLAB | type IFCSLABTYPE "SLB-01" | names: "Slab" | material: layers "raft slab" ("C25-30" 0.150000005960464) | property sets: EPset_Parametric, Qto_SlabBaseQuantities
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "COL-01" | names: "Column" | material: profiles ("C30-37") | property sets: EPset_Parametric, Qto_ColumnBaseQuantities
          4 x IFCWALL | type IFCWALLTYPE "WAL-02" | names: "Wall" | material: layers ("BLK-02" 0.150000005960464) | property sets: EPset_Parametric, Qto_WallBaseQuantities

Types
  IFCBEAMTYPE "BEM-01" | BEAM | 4 occurrences | material: profiles ("C30-37")
  IFCSLABTYPE "SLB-02" | ROOF | 1 occurrence | material: layers "raft slab" ("C25-30" 0.150000005960464) | property sets: EPset_Parametric
  IFCWALLTYPE "WAL-03" | PARAPET | 4 occurrences | material: layers ("BLK-02" 0.150000005960464) | property sets: EPset_Parametric
  IFCSLABTYPE "SLB-01" | BASESLAB | 1 occurrence | material: layers "raft slab" ("C25-30" 0.150000005960464) | property sets: EPset_Parametric
  IFCCOLUMNTYPE "COL-01" | COLUMN | 5 occurrences | material: profiles ("C30-37")
  IFCWALLTYPE "WAL-02" | SOLIDWALL | 4 occurrences | material: layers ("BLK-02" 0.150000005960464) | property sets: EPset_Parametric

Property sets
  EPset_Parametric | properties | on 9 objects (5 IFCCOLUMN, 4 IFCBEAM)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 8 objects (8 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 2 objects (2 IFCSLAB)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.15 [METRE]
    GrossArea = 16. [SQUARE_METRE]
    GrossVolume = 2.4 [CUBIC_METRE]
    Length = 4. [METRE]
    NetArea = 16. [SQUARE_METRE]
    NetVolume = 2.4 [CUBIC_METRE]
    Perimeter = 16. [METRE]
    Width = 4. [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.15 [METRE]
    GrossArea = 12.96 [SQUARE_METRE]
    GrossVolume = 1.944 [CUBIC_METRE]
    Length = 3.6 [METRE]
    NetArea = 12.96 [SQUARE_METRE]
    NetVolume = 1.944 [CUBIC_METRE]
    Perimeter = 14.4 [METRE]
    Width = 3.6 [METRE]
  Qto_ColumnBaseQuantities | quantities | on 5 objects (5 IFCCOLUMN)
    CrossSectionArea = 0.08 [SQUARE_METRE]
    GrossSurfaceArea = 3.94 [SQUARE_METRE]
    GrossVolume = 0.252 [CUBIC_METRE]
    Length = 3.15 [METRE]
    NetSurfaceArea = 3.94 [SQUARE_METRE]
    NetVolume = 0.252 [CUBIC_METRE]
    OuterSurfaceArea = 3.78 [SQUARE_METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossFootprintArea = 0.48 [SQUARE_METRE]
    GrossSideArea = 9.12 [SQUARE_METRE]
    GrossVolume = 1.368 [CUBIC_METRE]
    Height = 2.85 [METRE]
    Length = 3.2 [METRE]
    NetFootprintArea = 0.48 [SQUARE_METRE]
    NetSideArea = 9.12 [SQUARE_METRE]
    NetVolume = 1.368 [CUBIC_METRE]
    Width = 0.15 [METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossFootprintArea = 0.54 [SQUARE_METRE]
    GrossSideArea = 10.26 [SQUARE_METRE]
    GrossVolume = 1.539 [CUBIC_METRE]
    Height = 2.85 [METRE]
    Length = 3.6 [METRE]
    NetFootprintArea = 0.54 [SQUARE_METRE]
    NetSideArea = 10.26 [SQUARE_METRE]
    NetVolume = 1.539 [CUBIC_METRE]
    Width = 0.15 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.6 [SQUARE_METRE]
    GrossSideArea = 4. [SQUARE_METRE]
    GrossVolume = 0.6 [CUBIC_METRE]
    Height = 1. [METRE]
    Length = 4. [METRE]
    NetFootprintArea = 0.6 [SQUARE_METRE]
    NetSideArea = 4. [SQUARE_METRE]
    NetVolume = 0.6 [CUBIC_METRE]
    Width = 0.15 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.578 [SQUARE_METRE]
    GrossSideArea = 3.85 [SQUARE_METRE]
    GrossVolume = 0.578 [CUBIC_METRE]
    Height = 1. [METRE]
    Length = 3.85 [METRE]
    NetFootprintArea = 0.578 [SQUARE_METRE]
    NetSideArea = 3.85 [SQUARE_METRE]
    NetVolume = 0.578 [CUBIC_METRE]
    Width = 0.15 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.577 [SQUARE_METRE]
    GrossSideArea = 3.85 [SQUARE_METRE]
    GrossVolume = 0.577 [CUBIC_METRE]
    Height = 1. [METRE]
    Length = 3.85 [METRE]
    NetFootprintArea = 0.577 [SQUARE_METRE]
    NetSideArea = 3.85 [SQUARE_METRE]
    NetVolume = 0.577 [CUBIC_METRE]
    Width = 0.15 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.555 [SQUARE_METRE]
    GrossSideArea = 3.7 [SQUARE_METRE]
    GrossVolume = 0.555 [CUBIC_METRE]
    Height = 1. [METRE]
    Length = 3.7 [METRE]
    NetFootprintArea = 0.555 [SQUARE_METRE]
    NetSideArea = 3.7 [SQUARE_METRE]
    NetVolume = 0.555 [CUBIC_METRE]
    Width = 0.15 [METRE]
  Qto_BeamBaseQuantities | quantities | on 2 objects (2 IFCBEAM)
    CrossSectionArea = 0.06 [SQUARE_METRE]
    GrossSurfaceArea = 3.72 [SQUARE_METRE]
    GrossVolume = 0.216 [CUBIC_METRE]
    Length = 3.6 [METRE]
    NetSurfaceArea = 3.72 [SQUARE_METRE]
    NetVolume = 0.216 [CUBIC_METRE]
    OuterSurfaceArea = 3.6 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 2 objects (2 IFCBEAM)
    CrossSectionArea = 0.06 [SQUARE_METRE]
    GrossSurfaceArea = 3.32 [SQUARE_METRE]
    GrossVolume = 0.192 [CUBIC_METRE]
    Length = 3.2 [METRE]
    NetSurfaceArea = 3.32 [SQUARE_METRE]
    NetVolume = 0.192 [CUBIC_METRE]
    OuterSurfaceArea = 3.2 [SQUARE_METRE]