IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "Verona_3_Season_Porch.ifc"
Time stamp: "2024-10-07T19:34:23-05:00"
Preprocessor: "IfcOpenShell 0.0.0"
Originating system: "Bonsai 0.8.1-alpha241001-a422636"
Authorization: "Nobody"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  836 x Person "ryan@openingdesign.com" of Organization (no name given)
  661 x Organization "Autodesk Revit 2020 (ENU)"
  Organization "Autodesk Revit 2022 (ENU)"
  180 x Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  Owner history | change NOCHANGE | created 1680878644 (2023-04-07T14:44:04Z)
  3 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1680878644 (2023-04-07T14:44:04Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1661457979 (2022-08-25T20:06:19Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1682123705 (2023-04-22T00:35:05Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1633996150 (2021-10-11T23:49:10Z)
  2 x Owner history | change NOCHANGE | created 1682305051 (2023-04-24T02:57:31Z)
  160 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1682305051 (2023-04-24T02:57:31Z)
  2 x Owner history | change NOCHANGE | created 1681941947 (2023-04-19T22:05:47Z)

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: square foot (conversion based)
  LENGTHUNIT: foot (conversion based)
  VOLUMEUNIT: cubic foot (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "Library"
    contains 82 elements
      2 x IFCDOOR | type IFCDOORTYPE "3080R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (e) Hinge Approach, Push Side - 22"" | names: "BuildingElementProxy"
      6 x IFCWALL | type IFCWALLTYPE "W1" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, EPset_Drawing
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (g) Latch Approach, Push Side - 24"" | names: "BuildingElementProxy"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (e* & **) Hinge Approach, Push Side - 22"" | names: "BuildingElementProxy"
      2 x IFCWINDOW | type IFCWINDOWTYPE "FIXED: 3'-0" X 4'-0"" | names: "Window"
      9 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "Structural Framing 17:Structural Fr", "Structural Framing 19:Structural Fr", "Structural Framing 22:Structural Fr" (+6 more) | material: "HEADER TRACK"; "VERTICAL METAL CRIPPLE STUD BEYOND"; "DOUBLE UP METAL STUDS @ JAMB"; "(2) BOXED STUDS\nSAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, EPset_Drawing
      1 x IFCDOOR | type IFCDOORTYPE "D6484" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "S9080" | names: "Door" | material: constituents "MaterialConstituentSet" ("DOOR JAMB", "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "DOOR TRIM") | property sets: EPset_Drawing
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (b)_M Front Approach, Push" | names: "BuildingElementProxy" | property sets: EPset_Drawing
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (c)_M Hinge Approach, Pull" | names: "BuildingElementProxy"
      1 x IFCWALL | type IFCWALLTYPE "M358BØB" | names: "Wall" | material: layers "poche" ("GYP. BD. - PAINTED - (PT-1)" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION) (mat)" 0.291666666666667, "GYP. BD. - PAINTED - (PT-1)" 0.0520833333333333) | property sets: EPset_Parametric
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (a) Front Approach, Pull Side - 18"" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "D6884" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "S8480" | names: "Door" | material: constituents "MaterialConstituentSet" ("DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "DOOR TRIM", "DOOR JAMB")
      1 x IFCDOOR | type IFCDOORTYPE "D6880" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "3284L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (e* & **)_M Hinge Approach," | names: "BuildingElementProxy"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (f)_M Latch Approach, Pull" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3084L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: EPset_Drawing
      1 x IFCDOOR | type IFCDOORTYPE "G36"80"R" | names: "Door"
      1 x IFCDOOR | type IFCDOORTYPE "S7280" | names: "Door" | material: constituents "MaterialConstituentSet" ("DOOR TRIM", "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "DOOR JAMB")
      1 x IFCDOOR | type IFCDOORTYPE "D7280" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (c) Hinge Approach, Pull Side - 36"" | names: "BuildingElementProxy"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (g)_M Latch Approach, Push" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3080L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "3484L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "3480R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "3680L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (f) Latch Approach, Pull Side - 24"" | names: "BuildingElementProxy"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - 30"x48"" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3284R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (g*) Latch Approach, Push Side - 24" (with" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3480L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "3684R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "D4880" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "D6084" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (d)_M Hinge Approach, Pull" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3084R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "3684L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "D4884" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (a)_M Front Approach, Pull" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3680R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "S6080" | names: "Door" | material: constituents "MaterialConstituentSet" ("DOOR JAMB", "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "DOOR TRIM")
      1 x IFCDOOR | type IFCDOORTYPE "D6080" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - 36"x48"" | names: "BuildingElementProxy"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (e)_M Hinge Approach, Push" | names: "BuildingElementProxy"
      1 x IFCBUILDINGELEMENTPROXY | PROVISIONFORSPACE | names: "Plane"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - 5ft Circle" | names: "BuildingElementProxy"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (b) Front Approach, Push Side - 12"" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "G3684L" | names: "Door"
      1 x IFCDOOR | type IFCDOORTYPE "S9680" | names: "Door" | material: constituents "MaterialConstituentSet" ("DOOR JAMB", "DOOR TRIM", "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (f*)_M Latch Approach, Pull" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3484R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "D7284" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "D6480" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCDOOR | type IFCDOORTYPE "DT01" | names: "Door"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (d) Hinge Approach, Pull Side - 42"" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3280L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (g*)_M Latch Approach, Push" | names: "BuildingElementProxy"
      1 x IFCDOOR | names: "Door"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - T-shape" | names: "BuildingElementProxy"
      1 x IFCDOOR | type IFCDOORTYPE "3280R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING")
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ADA - (f*) Latch Approach, Pull Side - 24" (with" | names: "BuildingElementProxy"
      1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "34" counter" | DISHWASHER | names: "BuildingElementProxy"
      1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "36" X 30"" | REFRIGERATOR | names: "BuildingElementProxy.001" | material: "REFRIG."
      1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "36" RANGE/OVEN" | ELECTRICCOOKER | names: "BuildingElementProxy.002" | material: constituents "MaterialConstituentSet" ("Appliance - Plastic - Red": "Appliance - Plastic - Red", "Appliance - Chrome": "Appliance - Chrome", "RANGE": "RANGE", "Appliance - Oven Glass": "Appliance - Oven Glass")
  IFCSITE "Details"
    contains 889 elements
      421 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "Generic Models 616:Generic Models 1:1823539", "Generic Models 490:Generic Models 1:1571399", "Generic Models 534:Generic Models 1:1579472" (+418 more) | material: "CEILING TRACK AS SCHEDULED"; "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC"; "EXISTING 5/8" GYP. BD \n@ CEILING (PT-1)"; "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION) (mat)"; "WALL BASE AS SCHEDULED"; "2X WOOD STUD" | property sets: BBIM_Array, EPset_Drawing, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 140:Structural Framing 7" | names: "Structural Framing 140:Structural Framing 7:1773754" | material: "BLOCKING TO BRIDGE AT LEAST\n(3) VERTICAL STUDS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Walls 127:Walls 126" | names: "Walls 127:Walls 126:1519197" | material: "Earth" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 266:Generic Models 1" | names: "Generic Models 266:Generic Models 1:1652123" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 114:Generic Models 65" | names: "Generic Models 114:Generic Models 65:1619509" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 191:Generic Models 65" | names: "Generic Models 191:Generic Models 65:1622486" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 177:Structural Framing 2" | names: "Structural Framing 177:Structural Framing 2:1774119" | material: "(2) BOXED STUDS\nSAME SIZE AS WALL STUDS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 390:Generic Models 1" | names: "Generic Models 390:Generic Models 1:1850535" | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 427:Generic Models 1" | names: "Generic Models 427:Generic Models 1:1507317" | material: "1/8" SOUND MAT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 127:Structural Framing 1" | names: "Structural Framing 127:Structural Framing 1:1773571" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 163:Generic Models 1" | names: "Generic Models 163:Generic Models 1:855558" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 110:Structural Framing 1" | names: "Structural Framing 110:Structural Framing 1:1773370" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      39 x IFCBUILDINGELEMENTPROXY | names: "BuildingElementProxy" | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: BBIM_Array
      1 x IFCWALL | object type "Generic Models 77:Generic Models 1" | names: "Generic Models 77:Generic Models 1:1616055" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 130:Generic Models 65" | names: "Generic Models 130:Generic Models 65:1622309" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 149:Structural Framing 1" | names: "Structural Framing 149:Structural Framing 1:1773850" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 429:Generic Models 1" | names: "Generic Models 429:Generic Models 1:1507517" | material: "3/4" GYP. CRETE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 190:Generic Models 1" | names: "Generic Models 190:Generic Models 1:1622477" | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 184:Generic Models 184" | names: "Generic Models 184:Generic Models 184:858653" | material: "GRADE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 160:Structural Framing 7" | names: "Structural Framing 160:Structural Framing 7:1773962" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 227:Generic Models 1" | names: "Generic Models 227:Generic Models 1:1633977" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 13:Structural Framing 2" | names: "Structural Framing 13:Structural Framing 2:1775703" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 318:Generic Models 1" | names: "Generic Models 318:Generic Models 1:1652390" | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel13:Dowel" | names: "Dowel13:Dowel:1619577" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 148:Structural Framing 1" | names: "Structural Framing 148:Structural Framing 1:1773840" | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 55:Generic Models 1" | names: "Generic Models 55:Generic Models 1:1622967" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 240:Generic Models 1" | names: "Generic Models 240:Generic Models 1:1651807" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 391:Generic Models 1" | names: "Generic Models 391:Generic Models 1:1850568" | material: "2X WOOD STUDS BEYOND" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      12 x IFCVIRTUALELEMENT | names: "Model Text:OD_Very Large:1595843", "Model Text:OD_Very Large:1595842", "Model Text:OD_Very Large:1595840" (+6 more)
      1 x IFCWALL | object type "Generic Models 164:Generic Models 1" | names: "Generic Models 164:Generic Models 1:855573" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 79:Generic Models 1" | names: "Generic Models 79:Generic Models 1:1616415" | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | PROVISIONFORSPACE | names: "Plane" | property sets: EPset_Drawing
      1 x IFCWALL | object type "Generic Models 306:Generic Models 263" | names: "Generic Models 306:Generic Models 263:1399821" | material: "EXISTING GRADE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel11:Dowel" | names: "Dowel11:Dowel:1622333" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 150:Structural Framing 1" | names: "Structural Framing 150:Structural Framing 1:1773860" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Light Pole Base Plate4:Light Pole Base Plate" | names: "Light Pole Base Plate4:Light Pole Base Plate:1586650" | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 342:Generic Models 1" | names: "Generic Models 342:Generic Models 1:1848940" | material: "5/8" GYP. BD @ CEILING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 151:Generic Models 1" | names: "Generic Models 151:Generic Models 1:832637" | material: "GRADE (SLOPE 2% MIN AWAY FROM BUILDING)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 269:Generic Models 263" | names: "Generic Models 269:Generic Models 263:1381148" | material: "CONCRETE CURB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 239:Generic Models 1" | names: "Generic Models 239:Generic Models 1:1651794" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 404:Generic Models 1" | names: "Generic Models 404:Generic Models 1:1659546" | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 56:Generic Models 1" | names: "Generic Models 56:Generic Models 1:1623516" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 179:Structural Framing 2" | names: "Structural Framing 179:Structural Framing 2:1774137" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 241:Generic Models 1" | names: "Generic Models 241:Generic Models 1:1651820" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 192:Generic Models 65" | names: "Generic Models 192:Generic Models 65:1622508" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 162:Structural Framing 7" | names: "Structural Framing 162:Structural Framing 7:1773980" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon, EPset_Drawing
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 132:Structural Framing 1" | names: "Structural Framing 132:Structural Framing 1:1773645" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 307:Generic Models 263" | names: "Generic Models 307:Generic Models 263:1400379" | material: "CONCRETE PAVEMENT HEAVY DUTY" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 131:Generic Models 65" | names: "Generic Models 131:Generic Models 65:1622340" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "060523 - W_P_C - Fastenings - Generic:_GROUND LUG" | names: "060523 - W_P_C - Fastenings - Generic:_GROUND LUG:1587577" | material: "GROUND WIRE BOLTED TO POLE'S GROUND LUG" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 64:Generic Models 1" | names: "Generic Models 64:Generic Models 1:1849353" | material: "CONDUIT/PIPE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 111:Structural Framing 1" | names: "Structural Framing 111:Structural Framing 1:1773380" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 128:Structural Framing 1" | names: "Structural Framing 128:Structural Framing 1:1773581" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 61:Generic Models 1" | names: "Generic Models 61:Generic Models 1:1848231" | material: "5/8" GYP. BD @ CEILING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 152:Generic Models 1" | names: "Generic Models 152:Generic Models 1:833476" | material: "1/2" GYP. BD" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 270:Generic Models 263" | names: "Generic Models 270:Generic Models 263:1381912" | material: "CONCRETE CURB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 321:Generic Models 1" | names: "Generic Models 321:Generic Models 1:1659594" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Pole:Pole" | names: "Pole:Pole:1510851" | material: "STEEL LIGHT POLE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 116:Structural Framing 1" | names: "Structural Framing 116:Structural Framing 1:1773432" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 14:Structural Framing 2" | names: "Structural Framing 14:Structural Framing 2:1775712" | material: "(2) BOXED STUDS\nSAME SIZE AS WALL STUDS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 213:Generic Models 1" | names: "Generic Models 213:Generic Models 1:1633830" | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 268:Generic Models 1" | names: "Generic Models 268:Generic Models 1:1652149" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 118:Generic Models 65" | names: "Generic Models 118:Generic Models 65:1619584" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel14:Dowel" | names: "Dowel14:Dowel:1622531" | material: "#4 REBARS @ 24" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 163:Structural Framing 7" | names: "Structural Framing 163:Structural Framing 7:1773989" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 392:Generic Models 1" | names: "Generic Models 392:Generic Models 1:1850653" | material: "2X WOOD STUDS BEYOND" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 308:Generic Models 263" | names: "Generic Models 308:Generic Models 263:1400384" | material: "MEDIUM BROOM FINISH" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 344:Generic Models 1" | names: "Generic Models 344:Generic Models 1:1849507" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 129:Structural Framing 1" | names: "Structural Framing 129:Structural Framing 1:1773591" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 112:Structural Framing 2" | names: "Structural Framing 112:Structural Framing 2:1773393" | material: "METAL SILL CHANNEL\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 165:Generic Models 1" | names: "Generic Models 165:Generic Models 1:855588" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 80:Generic Models 1" | names: "Generic Models 80:Generic Models 1:1616542" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 151:Structural Framing 1" | names: "Structural Framing 151:Structural Framing 1:1773870" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 63:Generic Models 1" | names: "Generic Models 63:Generic Models 1:1848259" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 153:Generic Models 1" | names: "Generic Models 153:Generic Models 1:852181" | material: "SILL PLATE GASKET" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Light Pole Base Plate:Light Pole Base Plate" | names: "Light Pole Base Plate:Light Pole Base Plate:1510904" | material: "STEEL BASE PLATE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 167:Generic Models 1" | names: "Generic Models 167:Generic Models 1:855618" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 230:Generic Models 1" | names: "Generic Models 230:Generic Models 1:1634117" | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 15:Structural Framing 2" | names: "Structural Framing 15:Structural Framing 2:1775721" | material: "(2) BOXED STUDS\nSAME SIZE AS WALL STUDS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 207:Generic Models 1" | names: "Generic Models 207:Generic Models 1:1773600" | material: "UNDERSIDE OF FLOOR ASSEMBLY\nSEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators, EPset_Drawing
      1 x IFCWALL | object type "Generic Models 119:Generic Models 65" | names: "Generic Models 119:Generic Models 65:1619606" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 193:Generic Models 65" | names: "Generic Models 193:Generic Models 65:1622538" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 181:Generic Models 65" | names: "Generic Models 181:Generic Models 65:854445" | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 205:Generic Models 1" | names: "Generic Models 205:Generic Models 1:1773486" | material: "UNDERSIDE OF FLOOR ASSEMBLY\nSEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 22:Structural Framing 1" | names: "Structural Framing 22:Structural Framing 1:1775774" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 180:Structural Framing 1" | names: "Structural Framing 180:Structural Framing 1:1774143" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 393:Generic Models 1" | names: "Generic Models 393:Generic Models 1:1850729" | material: "5/8" GYP. BD @ CEILING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      8 x IFCELEMENTASSEMBLY | ACCESSORY_ASSEMBLY | names: "WOOD TRUSS FLOOR" | material: "WOOD TRUSS - WEB"; "EXISTING WOOD TRUSS" | property sets: BBIM_Aggregate_Data
      1 x IFCWALL | object type "Generic Models 244:Generic Models 1" | names: "Generic Models 244:Generic Models 1:1651835" | material: "GALV. STEEL WITH TOTAL AREA OF DUCT OPENING NOT TO EXCEED 113 SQ. IN. PER 100 SQ. FT. OF CEILING AREA, AREA OF INDIVIDUAL DUCT OPENING NOT TO EXCEED 113 SQ. IN. MAX. DIMENSION OF OPENING 12" - SEE UL ..." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 166:Generic Models 1" | names: "Generic Models 166:Generic Models 1:855603" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 81:Generic Models 1" | names: "Generic Models 81:Generic Models 1:1616646" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 113:Structural Framing 2" | names: "Structural Framing 113:Structural Framing 2:1773402" | material: "METAL TRACK CHANNEL @ HEAD\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 288:Generic Models 263" | names: "Generic Models 288:Generic Models 263:1387393" | material: "7" CONC. SIDE WALK, IF PRESENT (SEE SITE PLAN)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 133:Generic Models 1" | names: "Generic Models 133:Generic Models 1:1622357" | material: "BEARING STRIP" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 152:Structural Framing 1" | names: "Structural Framing 152:Structural Framing 1:1773880" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 65:Generic Models 1" | names: "Generic Models 65:Generic Models 1:1848274" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 44:Generic Models 1" | names: "Generic Models 44:Generic Models 1:1601268" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 231:Generic Models 1" | names: "Generic Models 231:Generic Models 1:1634198" | material: "5/8" GYP. BD @ CEILING (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 271:Generic Models 263" | names: "Generic Models 271:Generic Models 263:1382304" | material: "EXISTING PAVEMENT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 322:Generic Models 1" | names: "Generic Models 322:Generic Models 1:1659680" | material: "BREAK EVERY OTHER REBAR AT JOINT (TOP AND BOTTOM REBAR TO BE CONT.)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 208:Generic Models 1" | names: "Generic Models 208:Generic Models 1:1773613" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 120:Generic Models 1" | names: "Generic Models 120:Generic Models 1:1619618" | material: "REINFORCEMENT GROUTED INTO BROKEN CORE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 183:Generic Models 1" | names: "Generic Models 183:Generic Models 1:854474" | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 218:Generic Models 1" | names: "Generic Models 218:Generic Models 1:1633868" | material: "RESILIENT CHANNEL - 25 GA - 24" O.C. INSTALLED PERPENDICULAR TO TRUSSES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 249:Generic Models 1" | names: "Generic Models 249:Generic Models 1:1651856" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 181:Structural Framing 2" | names: "Structural Framing 181:Structural Framing 2:1774156" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 394:Generic Models 1" | names: "Generic Models 394:Generic Models 1:1850742" | material: "5/8" GYP. BD @ CEILING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 164:Structural Framing 7" | names: "Structural Framing 164:Structural Framing 7:1773998" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 82:Generic Models 1" | names: "Generic Models 82:Generic Models 1:1616792" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 310:Generic Models 263" | names: "Generic Models 310:Generic Models 263:1400408" | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel12:Dowel" | names: "Dowel12:Dowel:1622372" | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 40:Generic Models 1" | names: "Generic Models 40:Generic Models 1:1601430" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 348:Generic Models 1" | names: "Generic Models 348:Generic Models 1:1849566" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 272:Generic Models 263" | names: "Generic Models 272:Generic Models 263:1384116" | material: "1.50" ASPHALT SURFACE COURSE (E-0.3)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 309:Generic Models 263" | names: "Generic Models 309:Generic Models 263:1400637" | material: "EPOXY COATED 6 X 6 X W2.9 X W2.9, PLACED 3" ABOVE SLAB BASE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 319:Generic Models 1" | names: "Generic Models 319:Generic Models 1:1660588" | material: "3/4" DEEP NOTCH AT EACH SIDE OF WALL (SPACE APART - 25FT MIN.)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      2 x IFCBUILDINGELEMENTPROXY | object type "060523 - W_P_C - Fastenings - Generic:_1" Light Pole Anchor Bolt" | names: "060523 - W_P_C - Fastenings - Generic:_1" Light Pole Anchor Bolt:1512772", "060523 - W_P_C - Fastenings - Generic:_1" Light Pole Anchor Bolt:1512896" | material: constituents ("5/8" GALV. ANCHOR BOLT @ 24" O.C. (6" MIN. EMBEDMENT)": "5/8" GALV. ANCHOR BOLT @ 24" O.C. (6" MIN. EMBEDMENT)", "<Unnamed>": "<Unnamed>") | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 353:Generic Models 1" | names: "Generic Models 353:Generic Models 1:1849609" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 130:Structural Framing 2" | names: "Structural Framing 130:Structural Framing 2:1773630" | material: "METAL SILL CHANNEL\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 142:Structural Framing 7" | names: "Structural Framing 142:Structural Framing 7:1773785" | material: "BLOCKING TO BRIDGE AT LEAST\n(3) VERTICAL STUDS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 16:Structural Framing 2" | names: "Structural Framing 16:Structural Framing 2:1775730" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      2 x IFCCOLUMN | names: "Column" | property sets: EPset_Parametric
      1 x IFCWALL | object type "Generic Models 219:Generic Models 1" | names: "Generic Models 219:Generic Models 1:1633873" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 253:Generic Models 1" | names: "Generic Models 253:Generic Models 1:1651877" | material: "20" X 48"/60" OR 24" X 48" - MAX OF 16 SQ FT PER 100 SQ FT OF CEILING AREA - OR - INCANDESCENT LAMP TYPE 6.5" DIA. X 7-1/2" HIGH - (4) FIXTURES PER 100 SQ FT OF CEILING AREA (USE FIXTURE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel10:Dowel" | names: "Dowel10:Dowel:1618061" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 409:Generic Models 1" | names: "Generic Models 409:Generic Models 1:1851602" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 206:Generic Models 1" | names: "Generic Models 206:Generic Models 1:1773499" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 165:Structural Framing 7" | names: "Structural Framing 165:Structural Framing 7:1774007" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 194:Generic Models 65" | names: "Generic Models 194:Generic Models 65:1622560" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 311:Generic Models 263" | names: "Generic Models 311:Generic Models 263:1400420" | material: "COMPACTED SUBGRADE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 45:Generic Models 1" | names: "Generic Models 45:Generic Models 1:1601478" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 351:Generic Models 1" | names: "Generic Models 351:Generic Models 1:1849596" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 114:Structural Framing 1" | names: "Structural Framing 114:Structural Framing 1:1773410" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 108:Generic Models 65" | names: "Generic Models 108:Generic Models 65:1619799" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 153:Structural Framing 1" | names: "Structural Framing 153:Structural Framing 1:1773890" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 66:Generic Models 1" | names: "Generic Models 66:Generic Models 1:1848287" | material: "1/8" SOUND MAT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 396:Generic Models 1" | names: "Generic Models 396:Generic Models 1:1850768" | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      2 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 183:Structural Framing 2" | names: "Structural Framing 183:Structural Framing 2:1774174" | material: "(2) BOXED STUDS\nSAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 127:Generic Models 1" | names: "Generic Models 127:Generic Models 1:1622300" | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 125:Generic Models 1" | names: "Generic Models 125:Generic Models 1:1773303" | material: "UNDERSIDE OF FLOOR ASSEMBLY\nSEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      2 x IFCBUILDINGELEMENTPROXY | object type "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8"" | names: "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8":1618148", "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8":1617861" | material: "5/8” GALV. BENT ANCHOR BOLT @ 4’ O.C. (WITHIN 8” OF EVERY CORNER) 7” MIN. EMBEDMENT" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 169:Generic Models 1" | names: "Generic Models 169:Generic Models 1:855648" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 430:Generic Models 1" | names: "Generic Models 430:Generic Models 1:1651556" | material: "NOMINAL 3/4" THICK, 48" WIDE GYPSUM BOARD - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 17:Structural Framing 2" | names: "Structural Framing 17:Structural Framing 2:1775739" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 101:Generic Models 1" | names: "Generic Models 101:Generic Models 1:1618681" | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 106:Generic Models 65" | names: "Generic Models 106:Generic Models 65:1619787" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 121:Structural Framing 2" | names: "Structural Framing 121:Structural Framing 2:1773516" | material: "METAL SILL CHANNEL\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 166:Structural Framing 2" | names: "Structural Framing 166:Structural Framing 2:1774016" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 154:Generic Models 1" | names: "Generic Models 154:Generic Models 1:855166" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 195:Generic Models 1" | names: "Generic Models 195:Generic Models 1:1622572" | material: "3" CONCRETE TOPPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 395:Generic Models 1" | names: "Generic Models 395:Generic Models 1:1850755" | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 84:Generic Models 1" | names: "Generic Models 84:Generic Models 1:1616808" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 216:Generic Models 1" | names: "Generic Models 216:Generic Models 1:3424124" | material: "7/8" FURRING CHANNELS @ 12" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 294:Generic Models 263" | names: "Generic Models 294:Generic Models 263:1388734" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 182:Generic Models 65" | names: "Generic Models 182:Generic Models 65:1622384" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 154:Structural Framing 1" | names: "Structural Framing 154:Structural Framing 1:1773900" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon, EPset_Drawing
      1 x IFCWALL | object type "Generic Models 68:Generic Models 1" | names: "Generic Models 68:Generic Models 1:1848300" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 397:Generic Models 1" | names: "Generic Models 397:Generic Models 1:1850781" | material: "2X WOOD STUDS BEYOND" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      2 x IFCWALL | object type "Generic Models 8:Generic Models 1" | names: "Generic Models 8:Generic Models 1:826903", "Generic Models 8:Generic Models 1:1622703" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 170:Generic Models 1" | names: "Generic Models 170:Generic Models 1:855663" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 232:Generic Models 1" | names: "Generic Models 232:Generic Models 1:1651569" | material: "EXISTING FLOOR SUBSTRATE - MIN 19/32 THICK WOOD STRUCTURAL PANELS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 18:Structural Framing 2" | names: "Structural Framing 18:Structural Framing 2:1775748" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 273:Generic Models 263" | names: "Generic Models 273:Generic Models 263:1384314" | material: "INSTALL TACK COAT PER WDOT SPECIFICATIONS IF LAYERS ARE NOT INSTALLED AT THE SAME TIME" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 267:Generic Models 1" | names: "Generic Models 267:Generic Models 1:1652136" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 312:Generic Models 263" | names: "Generic Models 312:Generic Models 263:1402220" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 343:Generic Models 1" | names: "Generic Models 343:Generic Models 1:1849666" | material: "UL RATED FIRE STOP" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 131:Structural Framing 2" | names: "Structural Framing 131:Structural Framing 2:1773639" | material: "METAL TRACK CHANNEL @ HEAD\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 196:Generic Models 65" | names: "Generic Models 196:Generic Models 65:1622594" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 158:Generic Models 1" | names: "Generic Models 158:Generic Models 1:855467" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 220:Generic Models 1" | names: "Generic Models 220:Generic Models 1:1633886" | material: "1/8" SOUND MAT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 254:Generic Models 1" | names: "Generic Models 254:Generic Models 1:1651918" | material: "EXISTING - FLOOR BRIDGING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 352:Generic Models 1" | names: "Generic Models 352:Generic Models 1:1851677" | material: "5/8" GYP. BD" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 90:Generic Models 1" | names: "Generic Models 90:Generic Models 1:1618070" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 19:Structural Framing 1" | names: "Structural Framing 19:Structural Framing 1:1775754" | material: "VERTICAL METAL CRIPPLE STUD BEYOND" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 295:Generic Models 263" | names: "Generic Models 295:Generic Models 263:1388746" | material: "CRUSHED AGGREGATE BASE COURSE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 50:Generic Models 1" | names: "Generic Models 50:Generic Models 1:1601574" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 222:Generic Models 1" | names: "Generic Models 222:Generic Models 1:1633912" | material: "3/4" GYP. CRETE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 109:Generic Models 65" | names: "Generic Models 109:Generic Models 65:1619830" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 797:Generic Models 1" | names: "Generic Models 797:Generic Models 1:1651582" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 263:Generic Models 263" | names: "Generic Models 263:Generic Models 263:1384500" | material: "1.50" ASPHALT BINDER COURSE (E-0.3)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 283:Generic Models 263" | names: "Generic Models 283:Generic Models 263:1403684" | material: "SLOPED - 7" CONC." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 204:Generic Models 1" | names: "Generic Models 204:Generic Models 1:1773316" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 354:Generic Models 1" | names: "Generic Models 354:Generic Models 1:1850205" | material: "3" CONCRETE TOPPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 119:Structural Framing 1" | names: "Structural Framing 119:Structural Framing 1:1773465" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 159:Generic Models 1" | names: "Generic Models 159:Generic Models 1:855498" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 221:Generic Models 1" | names: "Generic Models 221:Generic Models 1:1633899" | material: "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL -L521 FLOOR ASSEMBLY)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 255:Generic Models 1" | names: "Generic Models 255:Generic Models 1:1651932" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 92:Generic Models 1" | names: "Generic Models 92:Generic Models 1:1618083" | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 410:Generic Models 1" | names: "Generic Models 410:Generic Models 1:1851747" | material: "HATCHED AREA" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 167:Structural Framing 1" | names: "Structural Framing 167:Structural Framing 1:1774022" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 431:Generic Models 1" | names: "Generic Models 431:Generic Models 1:1651595" | material: "RESILIENT CHANNEL - FORMED FROM MIN. 25 MSG GALV. STEEL SPACED MAX 24" O.C. PERPENDICULAR TO JOISTS - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 122:Structural Framing 2" | names: "Structural Framing 122:Structural Framing 2:1773525" | material: "METAL TRACK CHANNEL @ HEAD\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 21:Structural Framing 1" | names: "Structural Framing 21:Structural Framing 1:1775764" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 53:Generic Models 1" | names: "Generic Models 53:Generic Models 1:1601636" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 110:Generic Models 65" | names: "Generic Models 110:Generic Models 65:1619842" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 37:Structural Framing 7" | names: "Structural Framing 37:Structural Framing 7:1773764" | material: "BLOCKING TO BRIDGE AT LEAST\n(3) VERTICAL STUDS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 185:Structural Framing 2" | names: "Structural Framing 185:Structural Framing 2:1774192" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon, EPset_Drawing
      1 x IFCWALL | object type "Generic Models 274:Generic Models 263" | names: "Generic Models 274:Generic Models 263:1384626" | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 398:Generic Models 1" | names: "Generic Models 398:Generic Models 1:1850794" | material: "2X WOOD STUDS BEYOND" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 81:Structural Framing 1" | names: "Structural Framing 81:Structural Framing 1:1773330" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Ground Rod:Ground Rod" | names: "Ground Rod:Ground Rod:1515191" | material: "5/8" x 8' GROUND ROD" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 34:Generic Models 1" | names: "Generic Models 34:Generic Models 1:828799" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 171:Generic Models 1" | names: "Generic Models 171:Generic Models 1:855678" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 95:Generic Models 1" | names: "Generic Models 95:Generic Models 1:1618109" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 198:Generic Models 65" | names: "Generic Models 198:Generic Models 65:1622616" | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 168:Structural Framing 7" | names: "Structural Framing 168:Structural Framing 7:1774035" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 433:Generic Models 1" | names: "Generic Models 433:Generic Models 1:1651607" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 289:Generic Models 263" | names: "Generic Models 289:Generic Models 263:1394121" | material: "7" CONC. DRIVE APPROACH" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 111:Generic Models 65" | names: "Generic Models 111:Generic Models 65:1619877" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 70:Generic Models 1" | names: "Generic Models 70:Generic Models 1:1848326" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 223:Generic Models 1" | names: "Generic Models 223:Generic Models 1:1633925" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 399:Generic Models 1" | names: "Generic Models 399:Generic Models 1:1850846" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 186:Structural Framing 1" | names: "Structural Framing 186:Structural Framing 1:1774198" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Anchor Bolt:1/2"" | names: "Anchor Bolt:1/2":829037" | material: "1/2" ANCHOR BOLTS (7" MIN. EMBED) AT 72" MIN O.C. SPACING (18" MAX. FROM CORNERS)" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 172:Generic Models 1" | names: "Generic Models 172:Generic Models 1:855693" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 296:Generic Models 1" | names: "Generic Models 296:Generic Models 1:1652164" | material: "AIR DUCT — MIN 0.029 IN. THICK (22 GAUGE) GALV STEEL AIR DUCT. TOTAL AREA OF DUCT OPENINGS NOT TO EXCEED 114 SQ IN. PER EACH 100 SQ FT OF CEILING AREA." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 284:Generic Models 263" | names: "Generic Models 284:Generic Models 263:1403706" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 387:Generic Models 1" | names: "Generic Models 387:Generic Models 1:1850257" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 133:Structural Framing 1" | names: "Structural Framing 133:Structural Framing 1:1773655" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 199:Generic Models 1" | names: "Generic Models 199:Generic Models 1:1622628" | material: "GROUT CORES AT REBAR" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 160:Generic Models 1" | names: "Generic Models 160:Generic Models 1:855513" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 256:Generic Models 1" | names: "Generic Models 256:Generic Models 1:1651956" | material: "EXISTING - FLOOR BRIDGING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 411:Generic Models 1" | names: "Generic Models 411:Generic Models 1:1852408" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 297:Generic Models 263" | names: "Generic Models 297:Generic Models 263:1394272" | material: "SLOPED - 7" CONC." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 71:Generic Models 1" | names: "Generic Models 71:Generic Models 1:1848339" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 54:Generic Models 1" | names: "Generic Models 54:Generic Models 1:1601706" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 224:Generic Models 1" | names: "Generic Models 224:Generic Models 1:1633938" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 74:Generic Models 1" | names: "Generic Models 74:Generic Models 1:1775660" | material: "UNDERSIDE OF FLOOR ASSEMBLY\nSEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 424:Generic Models 1" | names: "Generic Models 424:Generic Models 1:3405062" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 43:Generic Models 65" | names: "Generic Models 43:Generic Models 65:829101" | material: "2X6s WOOD JOISTS - 16" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 275:Generic Models 263" | names: "Generic Models 275:Generic Models 263:1384752" | material: "COMPACTED SUBGRADE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 285:Generic Models 263" | names: "Generic Models 285:Generic Models 263:1403728" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 388:Generic Models 1" | names: "Generic Models 388:Generic Models 1:1850301" | material: "UL RATED FIRE STOP" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 134:Structural Framing 1" | names: "Structural Framing 134:Structural Framing 1:1773665" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 161:Generic Models 1" | names: "Generic Models 161:Generic Models 1:855528" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 278:Generic Models 263" | names: "Generic Models 278:Generic Models 263:1385167" | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 257:Generic Models 1" | names: "Generic Models 257:Generic Models 1:1651969" | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 99:Generic Models 1" | names: "Generic Models 99:Generic Models 1:1618126" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 423:Generic Models 1" | names: "Generic Models 423:Generic Models 1:3405052" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 46:Generic Models 1" | names: "Generic Models 46:Generic Models 1:829188" | material: "1/2" CDX PLYWOOD" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 169:Structural Framing 7" | names: "Structural Framing 169:Structural Framing 7:1774044" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 796:Generic Models 1" | names: "Generic Models 796:Generic Models 1:1651622" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel5:Dowel" | names: "Dowel5:Dowel:1614630" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 117:Structural Framing 1" | names: "Structural Framing 117:Structural Framing 1:1773443" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 107:Generic Models 65" | names: "Generic Models 107:Generic Models 65:1620157" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 277:Generic Models 263" | names: "Generic Models 277:Generic Models 263:1385057" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 62:Generic Models 1" | names: "Generic Models 62:Generic Models 1:1850876" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 276:Generic Models 263" | names: "Generic Models 276:Generic Models 263:1405189" | material: "1" EXPANSION JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 135:Structural Framing 1" | names: "Structural Framing 135:Structural Framing 1:1773675" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 173:Generic Models 1" | names: "Generic Models 173:Generic Models 1:855708" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 299:Generic Models 263" | names: "Generic Models 299:Generic Models 263:1395691" | material: "CONCRETE CURB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 302:Generic Models 1" | names: "Generic Models 302:Generic Models 1:1652185" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 73:Generic Models 1" | names: "Generic Models 73:Generic Models 1:1848365" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 258:Generic Models 1" | names: "Generic Models 258:Generic Models 1:1651985" | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 100:Generic Models 1" | names: "Generic Models 100:Generic Models 1:1618136" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 51:Generic Models 1" | names: "Generic Models 51:Generic Models 1:829284" | material: "VINYL SIDING OVER AIR & MOISTURE BARRIER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 200:Generic Models 1" | names: "Generic Models 200:Generic Models 1:1622654" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 170:Structural Framing 7" | names: "Structural Framing 170:Structural Framing 7:1774053" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 421:Generic Models 1" | names: "Generic Models 421:Generic Models 1:1651662" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 78:Generic Models 1" | names: "Generic Models 78:Generic Models 1:1614654" | material: "BEARING STRIP" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel8:Dowel" | names: "Dowel8:Dowel:1617962" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 298:Generic Models 263" | names: "Generic Models 298:Generic Models 263:1394399" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 112:Generic Models 65" | names: "Generic Models 112:Generic Models 65:1620169" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 72:Generic Models 1" | names: "Generic Models 72:Generic Models 1:1848352" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 93:Generic Models 1" | names: "Generic Models 93:Generic Models 1:1775673" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 400:Generic Models 1" | names: "Generic Models 400:Generic Models 1:1850894" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 425:Generic Models 1" | names: "Generic Models 425:Generic Models 1:3405072" | material: "RESILIENT CHANNEL - 25 GA - 24" O.C. INSTALLED PERPENDICULAR TO TRUSSES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 174:Generic Models 1" | names: "Generic Models 174:Generic Models 1:855723" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel9:Dowel" | names: "Dowel9:Dowel:1617989" | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 300:Generic Models 263" | names: "Generic Models 300:Generic Models 263:1395728" | material: "CONCRETE CURB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 303:Generic Models 1" | names: "Generic Models 303:Generic Models 1:1652206" | material: "2' x 4' RECESSED LIGHT FIXTURE WITH STEEL HOUSING AND 'FIXTURE PROTECTION' - SPACED TO NOT EXCEED 24 SQ FT PER 100 SQ FT OF CEILING AREA - SEE UL LISTING FOR MORE INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 148:Generic Models 1" | names: "Generic Models 148:Generic Models 1:1848378" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Dowel7:Dowel" | names: "Dowel7:Dowel:1614828" | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 140:Generic Models 1" | names: "Generic Models 140:Generic Models 1:829357" | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION) (mat)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 201:Generic Models 1" | names: "Generic Models 201:Generic Models 1:1622672" | material: "(2) #5's" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 171:Structural Framing 1" | names: "Structural Framing 171:Structural Framing 1:1774059" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 422:Generic Models 1" | names: "Generic Models 422:Generic Models 1:1651685" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 279:Generic Models 263" | names: "Generic Models 279:Generic Models 263:1385327" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 115:Generic Models 65" | names: "Generic Models 115:Generic Models 65:1620201" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Light Pole Luminaire:Light Pole Luminaire" | names: "Light Pole Luminaire:Light Pole Luminaire:1513850" | material: "LUMINAIRE HOUSING AS SPECIFIED" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 226:Generic Models 1" | names: "Generic Models 226:Generic Models 1:1633964" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 401:Generic Models 1" | names: "Generic Models 401:Generic Models 1:1850912" | material: "CONDUIT/PIPE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 102:Generic Models 1" | names: "Generic Models 102:Generic Models 1:1618883" | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 115:Structural Framing 1" | names: "Structural Framing 115:Structural Framing 1:1773421" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 175:Generic Models 1" | names: "Generic Models 175:Generic Models 1:855738" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 305:Generic Models 1" | names: "Generic Models 305:Generic Models 1:1652247" | material: "EXISTING - FLOOR BRIDGING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      2 x IFCBUILDINGELEMENTPROXY | object type "Generic Models 299:Generic Models 263" | names: "Generic Models 299:Generic Models 2", "Generic Models 299:Generic Models 263:1451928" | material: "CONCRETE CURB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 91:Generic Models 1" | names: "Generic Models 91:Generic Models 1:1614869" | material: "3" CONCRETE TOPPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 136:Structural Framing 1" | names: "Structural Framing 136:Structural Framing 1:1773685" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 202:Generic Models 1" | names: "Generic Models 202:Generic Models 1:1622682" | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 280:Generic Models 263" | names: "Generic Models 280:Generic Models 263:1385413" | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 259:Generic Models 1" | names: "Generic Models 259:Generic Models 1:1651998" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 155:Structural Framing 2" | names: "Structural Framing 155:Structural Framing 2:1773913" | material: "METAL SILL CHANNEL\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Light Pole Base Plate3:Light Pole Base Plate" | names: "Light Pole Base Plate3:Light Pole Base Plate:1586248" | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 185:Generic Models 1" | names: "Generic Models 185:Generic Models 1:1622400" | material: "SOLID CMU AS NEEDED" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 261:Generic Models 1" | names: "Generic Models 261:Generic Models 1:1652062" | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 103:Generic Models 1" | names: "Generic Models 103:Generic Models 1:1619141" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 143:Structural Framing 2" | names: "Structural Framing 143:Structural Framing 2:1773795" | material: "SILL STUD" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 203:Generic Models 1" | names: "Generic Models 203:Generic Models 1:1622696" | material: "(2) #5's" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 173:Structural Framing 1" | names: "Structural Framing 173:Structural Framing 1:1774078" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 96:Generic Models 1" | names: "Generic Models 96:Generic Models 1:1614983" | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 137:Structural Framing 1" | names: "Structural Framing 137:Structural Framing 1:1773695" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 86:Generic Models 1" | names: "Generic Models 86:Generic Models 1:1617996" | material: "3" CONCRETE TOPPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 304:Generic Models 263" | names: "Generic Models 304:Generic Models 263:1396625" | material: "1" EXPANSION JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 161:Structural Framing 7" | names: "Structural Framing 161:Structural Framing 7:1773971" | material: "BLOCKING @ DOOR HINGE LOCATIONS\nEXTEND TO AT LEAST (3) VERT." | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 211:Generic Models 1" | names: "Generic Models 211:Generic Models 1:1848391" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 260:Generic Models 1" | names: "Generic Models 260:Generic Models 1:1652050" | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 186:Generic Models 65" | names: "Generic Models 186:Generic Models 65:1622412" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      2 x IFCWALL | object type "Generic Models 139:Generic Models 1" | names: "Generic Models 139:Generic Models 1:829521", "Generic Models 139:Generic Models 1:1622725" | material: "#4 CONT. STEEL REBAR" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 233:Generic Models 1" | names: "Generic Models 233:Generic Models 1:1651709" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 172:Structural Framing 2" | names: "Structural Framing 172:Structural Framing 2:1774072" | material: "METAL SILL CHANNEL\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 314:Generic Models 1" | names: "Generic Models 314:Generic Models 1:1652285" | material: "EXISTING - FLOOR BRIDGING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 69:Generic Models 1" | names: "Generic Models 69:Generic Models 1:1848313" | material: "3/4" GYP. CRETE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 116:Generic Models 65" | names: "Generic Models 116:Generic Models 65:1620213" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 144:Structural Framing 2" | names: "Structural Framing 144:Structural Framing 2:1773804" | material: "HEADER TRACK" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 174:Structural Framing 2" | names: "Structural Framing 174:Structural Framing 2:1774091" | material: "METAL SILL CHANNEL\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 402:Generic Models 1" | names: "Generic Models 402:Generic Models 1:1850921" | material: "UL RATED FIRE STOP" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Generic Models 285:Generic Models 263" | names: "Generic Models 285:Generic Models 263:1451950" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 209:Generic Models 1" | names: "Generic Models 209:Generic Models 1:1773704" | material: "UNDERSIDE OF FLOOR ASSEMBLY\nSEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 176:Generic Models 1" | names: "Generic Models 176:Generic Models 1:855753" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 87:Generic Models 1" | names: "Generic Models 87:Generic Models 1:1618017" | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 282:Generic Models 263" | names: "Generic Models 282:Generic Models 263:1398156" | material: "CONCRETE CURB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 313:Generic Models 1" | names: "Generic Models 313:Generic Models 1:1652261" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 212:Generic Models 1" | names: "Generic Models 212:Generic Models 1:1848411" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 123:Structural Framing 1" | names: "Structural Framing 123:Structural Framing 1:1773531" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      2 x IFCWALL | object type "Generic Models 141:Generic Models 1" | names: "Generic Models 141:Generic Models 1:830973", "Generic Models 141:Generic Models 1:1622735" | material: "#4 CONT. STEEL REBAR" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 234:Generic Models 1" | names: "Generic Models 234:Generic Models 1:1651722" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 281:Generic Models 263" | names: "Generic Models 281:Generic Models 263:1385588" | material: "3" TO 6" WASHED OR CLEAR STONE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 315:Generic Models 1" | names: "Generic Models 315:Generic Models 1:1652301" | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 12:Structural Framing 1" | names: "Structural Framing 12:Structural Framing 1:1775694" | material: "BEND DOWN FLANGE OF METAL TRACK\nOR USE CLIP ANGLES\nPER MANU. REQUIREMENT" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Qto_BuildingElementProxyQuantities
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 156:Structural Framing 1" | names: "Structural Framing 156:Structural Framing 1:1773919" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 117:Generic Models 1" | names: "Generic Models 117:Generic Models 1:1620261" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 145:Structural Framing 1" | names: "Structural Framing 145:Structural Framing 1:1773810" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Light Pole Base Plate1:Light Pole Base Plate" | names: "Light Pole Base Plate1:Light Pole Base Plate:1515308" | material: "(4) VERTICAL #6 REBAR" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 229:Generic Models 1" | names: "Generic Models 229:Generic Models 1:1633990" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 405:Generic Models 1" | names: "Generic Models 405:Generic Models 1:1851094" | material: "UL RATED FIRE STOP" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 262:Generic Models 1" | names: "Generic Models 262:Generic Models 1:1652080" | material: "GYPSUM BOARD — 5/8" X 4 FT WIDE GYPSUM BOARD, INSTALLED WITH LONG DIMENSION PERPENDICULAR TO CROSS TEES WITH SIDE JOINTS CENTERED ALONG MAIN RUNNERS." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 104:Generic Models 1" | names: "Generic Models 104:Generic Models 1:1619290" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 179:Generic Models 1" | names: "Generic Models 179:Generic Models 1:855824" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 301:Generic Models 263" | names: "Generic Models 301:Generic Models 263:1398203" | material: "CONCRETE CURB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 214:Generic Models 1" | names: "Generic Models 214:Generic Models 1:1848424" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 124:Structural Framing 1" | names: "Structural Framing 124:Structural Framing 1:1773541" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 82:Structural Framing 1" | names: "Structural Framing 82:Structural Framing 1:1773340" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 75:Generic Models 1" | names: "Generic Models 75:Generic Models 1:1615730" | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 235:Generic Models 1" | names: "Generic Models 235:Generic Models 1:1651751" | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 286:Generic Models 263" | names: "Generic Models 286:Generic Models 263:1386677" | material: "6" CRUSHED AGGREGATE BASE COURSE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 187:Generic Models 1" | names: "Generic Models 187:Generic Models 1:1622429" | material: "SOLID CMU AS NEEDED" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 157:Structural Framing 1" | names: "Structural Framing 157:Structural Framing 1:1773929" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 138:Structural Framing 2" | names: "Structural Framing 138:Structural Framing 2:1773734" | material: "METAL TRACK CHANNEL @ HEAD\nFASTENER PER MANU. REQUIREMENTS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Light Pole Base Plate2:Light Pole Base Plate" | names: "Light Pole Base Plate2:Light Pole Base Plate:1516878" | material: "STEEL BASE PLATE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 406:Generic Models 1" | names: "Generic Models 406:Generic Models 1:1851126" | material: "CONDUIT/PIPE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 105:Generic Models 1" | names: "Generic Models 105:Generic Models 1:1619338" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 264:Generic Models 1" | names: "Generic Models 264:Generic Models 1:1652093" | material: "EXISTING FLOOR SUBSTRATE - 15/32" THICK PLYWOOD OR 7/16" THICK ORIENTATED STRAND BOARD (OSB) WOOD STRUCTURAL PANELS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 120:Structural Framing 1" | names: "Structural Framing 120:Structural Framing 1:1773476" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 175:Structural Framing 1" | names: "Structural Framing 175:Structural Framing 1:1774097" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 180:Generic Models 65" | names: "Generic Models 180:Generic Models 65:856122" | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 414:Generic Models 1" | names: "Generic Models 414:Generic Models 1:1506002" | material: "5/8" GYP. BD @ CEILING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 76:Generic Models 1" | names: "Generic Models 76:Generic Models 1:1615830" | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 210:Generic Models 1" | names: "Generic Models 210:Generic Models 1:1773717" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 88:Generic Models 1" | names: "Generic Models 88:Generic Models 1:1618032" | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 188:Generic Models 65" | names: "Generic Models 188:Generic Models 65:1622441" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 158:Structural Framing 1" | names: "Structural Framing 158:Structural Framing 1:1773939" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      2 x IFCWALL | object type "Generic Models 144:Generic Models 1" | names: "Generic Models 144:Generic Models 1:830994", "Generic Models 144:Generic Models 1:1622740" | material: "#10 6x6 WIRE MESH" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 225:Generic Models 1" | names: "Generic Models 225:Generic Models 1:1633951" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 141:Structural Framing 7" | names: "Structural Framing 141:Structural Framing 7:1773775" | material: "BLOCKING TO BRIDGE AT LEAST\n(3) VERTICAL STUDS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 177:Generic Models 1" | names: "Generic Models 177:Generic Models 1:856630" | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 316:Generic Models 1" | names: "Generic Models 316:Generic Models 1:1652314" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 121:Generic Models 1" | names: "Generic Models 121:Generic Models 1:1621614" | material: "3" CONCRETE TOPPING" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 146:Structural Framing 1" | names: "Structural Framing 146:Structural Framing 1:1773820" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 176:Structural Framing 2" | names: "Structural Framing 176:Structural Framing 2:1774110" | material: "(2) BOXED STUDS\nSAME SIZE AS WALL STUDS" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 389:Generic Models 1" | names: "Generic Models 389:Generic Models 1:1850411" | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 426:Generic Models 1" | names: "Generic Models 426:Generic Models 1:1507267" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 162:Generic Models 1" | names: "Generic Models 162:Generic Models 1:855543" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 89:Generic Models 1" | names: "Generic Models 89:Generic Models 1:1618045" | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 290:Generic Models 263" | names: "Generic Models 290:Generic Models 263:1399522" | material: "GRADED BACKFILL" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 215:Generic Models 1" | names: "Generic Models 215:Generic Models 1:1848437" | material: "OPEN WEB WOOD TRUSS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 125:Structural Framing 1" | names: "Structural Framing 125:Structural Framing 1:1773551" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 108:Structural Framing 1" | names: "Structural Framing 108:Structural Framing 1:1773350" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 408:Generic Models 1" | names: "Generic Models 408:Generic Models 1:1851308" | material: "UL RATED FIRE STOP" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 189:Generic Models 65" | names: "Generic Models 189:Generic Models 65:1622463" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 145:Generic Models 1" | names: "Generic Models 145:Generic Models 1:831218" | material: "6 MIL VAPOR BARRIER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 178:Generic Models 155" | names: "Generic Models 178:Generic Models 155:856646" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 236:Generic Models 1" | names: "Generic Models 236:Generic Models 1:1651764" | material: "EXISTING FLOOR SUBSTRATE - 1 X 4 T&G LAID PERPENDICULAR TO JOISTS, OR 19/32" PLYWOOD WOOD STRUCTURAL PANELS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 317:Generic Models 1" | names: "Generic Models 317:Generic Models 1:1652367" | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 139:Structural Framing 1" | names: "Structural Framing 139:Structural Framing 1:1773740" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 123:Generic Models 1" | names: "Generic Models 123:Generic Models 1:1621813" | material: "#3 J's @ 24" O.C." | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 147:Structural Framing 1" | names: "Structural Framing 147:Structural Framing 1:1773830" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Walls 126:Walls 126" | names: "Walls 126:Walls 126:1518668" | material: "24" DIA. CONCRETE POLE BASE WITH THOROSEAL FINISH" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 168:Generic Models 1" | names: "Generic Models 168:Generic Models 1:855633" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 407:Generic Models 1" | names: "Generic Models 407:Generic Models 1:1851151" | material: "UL RATED FIRE STOP" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 265:Generic Models 1" | names: "Generic Models 265:Generic Models 1:1652106" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 113:Generic Models 65" | names: "Generic Models 113:Generic Models 65:1619487" | material: "MORTAR JOINT" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 118:Structural Framing 1" | names: "Structural Framing 118:Structural Framing 1:1773454" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Generic Models 291:Generic Models 263" | names: "Generic Models 291:Generic Models 263:1399720" | material: "GRADED BACKFILL" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 345:Generic Models 1" | names: "Generic Models 345:Generic Models 1:1848797" | material: "5/8" GYP. BD" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 126:Structural Framing 1" | names: "Structural Framing 126:Structural Framing 1:1773561" | material: "TYP. VERTICAL METAL STUD\nSEE WALL TAG FOR SPACING AND GUAGE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCBUILDINGELEMENTPROXY | object type "Structural Framing 109:Structural Framing 1" | names: "Structural Framing 109:Structural Framing 1:1773360" | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Qto_BuildingElementProxyQuantities, Pset_EnvironmentalImpactIndicators, Pset_BuildingElementProxyCommon
      1 x IFCWALL | object type "Dowel6:Dowel" | names: "Dowel6:Dowel:1615883" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 150:Generic Models 1" | names: "Generic Models 150:Generic Models 1:831484" | material: "6" COMPACTED CRUSHED STONE" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
      1 x IFCWALL | object type "Generic Models 237:Generic Models 1" | names: "Generic Models 237:Generic Models 1:1651777" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_ReinforcementBarPitchOfWall, Pset_EnvironmentalImpactIndicators
  IFCSITE "Tradesman_Warehouse_T"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "1ST FLOOR"
        contains 161 elements
          15 x IFCELEMENTASSEMBLY | names: "Default_Name" | parts: 34 IFCWALL
          12 x IFCBEAM | type IFCBEAMTYPE "2x10 - Floor" | names: "Beam" | material: profiles ("V_White Trim") | property sets: EPset_Parametric, BBIM_Array
          10 x IFCWALL | type IFCWALLTYPE "V_2x6 drywall Copy" | names: "Wall" | material: layers ("V_Air" 0.0833333358168602, "V_Plywood" 0.0416666679084301, "V_2x6" 0.458333343267441, "V_Drywall" 0.0520833320915699) | property sets: EPset_Parametric, EPset_Status
          17 x IFCWINDOW | type IFCWINDOWTYPE "w1" | names: "Window" | property sets: EPset_Status
          15 x IFCVIRTUALELEMENT | object type "REFERENCE_PLAN" | names: "Plane"
          1 x IFCWINDOW | type IFCWINDOWTYPE "Double Hung" | names: "Window" | material: constituents ("DOUBLE HUNG WINDOW")
          2 x IFCWINDOW | type IFCWINDOWTYPE "W6" | names: "Window" | property sets: EPset_Status
          4 x IFCWALL | type IFCWALLTYPE "V_porch wall" | names: "Wall" | material: layers ("V_White Trim" 0.0625, "V_2x6" 0.291666656732559, "V_White Trim" 0.0625) | property sets: EPset_Parametric
          4 x IFCBEAM | type IFCBEAMTYPE "beam 1" | names: "Beam" | material: profiles ("V_Steel_Galv.") | property sets: EPset_Parametric
          1 x IFCWALL | type IFCWALLTYPE "GENERIC 6"" | names: "Wall" | material: layers ("GENERIC POCHE" 0.5) | property sets: EPset_Parametric
          7 x IFCWINDOW | type IFCWINDOWTYPE "Cube" | names: "Window"
          14 x IFCWINDOW | type IFCWINDOWTYPE "w2" | names: "Window" | property sets: EPset_Status
          4 x IFCCOVERING | type IFCCOVERINGTYPE "SOFFIT" | names: "Covering" | material: layers ("EXISTING SOFFIT" 0.666666686534882) | property sets: EPset_Parametric
          9 x IFCWALL | type IFCWALLTYPE "V_brick" | names: "Wall" | material: layers ("V_Brick" 0.291666656732559) | property sets: EPset_Parametric, EPset_Status
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_254_183624_R" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)")
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_102_363424" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)")
          1 x IFCWALL | type IFCWALLTYPE "GEN 8"" | names: "Wall" | material: layers ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 1.4466667175293) | property sets: EPset_Parametric
          2 x IFCDOOR | type IFCDOORTYPE "SLIDING - PATIO" | names: "Door" | material: constituents "MaterialConstituentSet" ("_DESIGN TRIM - WHITE": "_DESIGN TRIM - WHITE", "INSULATED GLAZING": "INSULATED GLAZING")
          1 x IFCROOF | type IFCROOFTYPE "Hip - Shingles 2" | GABLE_ROOF | names: "Roof" | material: "V_Asphalt Shingles"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_253_183624_R" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)")
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_100_213424" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET SHELF")
          2 x IFCWINDOW | type IFCWINDOWTYPE "w3" | names: "Window" | property sets: EPset_Status
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_301_183612_L" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)")
          1 x IFCWALL | type IFCWALLTYPE "GENERIC 5"" | names: "Wall" | material: layers ("GENERIC POCHE" 0.416666656732559) | property sets: EPset_Parametric
          1 x IFCWALL | type IFCWALLTYPE "GENERIC 3"" | names: "Wall" | material: layers ("GENERIC POCHE" 0.25) | property sets: EPset_Parametric
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_152_363624" | names: "Furniture" | material: "BASE CABINET (PL-1)"
          2 x IFCWALL | type IFCWALLTYPE "W4BØD" | names: "Wall" | material: layers ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699, "2X WOOD STUD" 0.291666656732559, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699) | property sets: EPset_Parametric
          1 x IFCSLAB | type IFCSLABTYPE "SlabType" | names: "Slab" | material: layers ("V_Brick" 0.416666656732559) | property sets: EPset_Parametric
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_102_363624" | names: "Furniture" | material: "BASE CABINET (PL-1)"
          1 x IFCWALL | type IFCWALLTYPE "DIAGRAMMATIC WALL" | names: "Wall" | material: layers ("GENERIC POCHE" 0.0833333358168602) | property sets: EPset_Parametric
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_222_303624" | names: "Furniture" | material: "BASE CABINET (PL-1)"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_101_183624_L" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)")
          1 x IFCSLAB | type IFCSLABTYPE "Porch Floor" | names: "Slab" | material: layers ("V_Wood Flooring" 0.0416666679084301, "V_Plywood" 0.0625) | property sets: EPset_Parametric
          1 x IFCWALL | type IFCWALLTYPE "GENERIC 2"" | names: "Wall" | material: layers ("GENERIC POCHE" 0.16666667163372) | property sets: EPset_Parametric
          2 x IFCDOOR | type IFCDOORTYPE "SLIDING - PATIO Copy" | names: "Door" | material: constituents "MaterialConstituentSet" ("_DESIGN TRIM - WHITE": "_DESIGN TRIM - WHITE", "INSULATED GLAZING": "INSULATED GLAZING")
          1 x IFCWINDOW | type IFCWINDOWTYPE "W5" | names: "Window" | property sets: EPset_Status
          1 x IFCWALL | type IFCWALLTYPE "W4AØD" | names: "Wall" | material: layers ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION) (mat)" 0.291666656732559, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699) | property sets: EPset_Parametric
          1 x IFCWALL | type IFCWALLTYPE "EXT WALL - (HORZ. SIDING - 1/2 SHEATHING" | names: "Wall" | material: layers "Basic Wall:EXT WALL - (HORZ. SIDING - 1/2 SHEATHING - 2X6 WOOD(BATT) - 5/8 GYP)" ("SIDING - CLAPBOARD" 0.0416666679084301, "BUILDING WRAP OVER CDX SHEATHING" 0.0416666666666667, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION) (mat)" 0.458333343267441, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699) | property sets: EPset_Parametric
          1 x IFCDOOR | type IFCDOORTYPE "Double Inswing - 4073" | names: "Door"
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "column 1" | names: "Column" | material: profiles ("V_Steel_Galv.") | property sets: EPset_Parametric
          1 x IFCACTUATOR | ELECTRICACTUATOR | names: "Actuator" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_211_183624_R" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)")
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_101_183424_R" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)")
          1 x IFCWALL | type IFCWALLTYPE "EXT-VINYL" | names: "Wall" | material: layers "HorzLines6in96scale" ("GENERIC POCHE" 0.583333313465118) | property sets: EPset_Parametric, Pset_WallCommon
          1 x IFCFURNITURE | type IFCFURNITURETYPE "BC_302_363612" | names: "Furniture" | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)")
          1 x IFCROOF | type IFCROOFTYPE "Hip" | GABLE_ROOF | names: "Roof"
          1 x IFCWINDOW | type IFCWINDOWTYPE "w4" | names: "Window" | property sets: EPset_Status
          1 x IFCWINDOW | names: "Window"
          1 x IFCROOF | type IFCROOFTYPE "asphalt shingles" | names: "Roof" | material: layers ("V_Asphalt Shingles" 0.020833333954215) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "Sliding Window" | names: "Window"
          1 x IFCWALL | type IFCWALLTYPE "GENERIC 1"" | names: "Wall" | material: layers ("GENERIC POCHE" 0.0833333358168602) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "Casement or Awning or Fixed" | names: "Window"
          1 x IFCROOF | type IFCROOFTYPE "Porch Roof" | names: "Roof" | material: layers ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.833333313465118) | property sets: EPset_Parametric
          1 x IFCFOOTING | PAD_FOOTING | names: "Cube" | material: "V_Concrete"
          1 x IFCWALL | type IFCWALLTYPE "GENERIC 8"" | names: "Wall" | material: layers ("GENERIC POCHE (NEW)" 0.666666686534882) | property sets: EPset_Parametric
          1 x IFCWALL | type IFCWALLTYPE "GENERIC 4"" | names: "Wall" | material: layers ("GENERIC POCHE" 0.333333343267441) | property sets: EPset_Parametric

Types
  IFCDOORTYPE "3080R" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (e) Hinge Approach, Push Side - 22"" | PROVISIONFORSPACE | 1 occurrence
  IFCWALLTYPE "W1" | STANDARD | 6 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (g) Latch Approach, Push Side - 24"" | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (e* & **) Hinge Approach, Push Side - 22"" | PROVISIONFORSPACE | 1 occurrence
  IFCWINDOWTYPE "FIXED: 3'-0" X 4'-0"" | 2 occurrences | property sets: EPset_Drawing
  IFCDOORTYPE "D6484" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "S9080" | DOOR | DOUBLE_DOOR_SLIDING | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOOR JAMB", "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "DOOR TRIM") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (b)_M Front Approach, Push" | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (c)_M Hinge Approach, Pull" | PROVISIONFORSPACE | 1 occurrence
  IFCWALLTYPE "M358BØB" | STANDARD | 1 occurrence | material: layers "poche" ("GYP. BD. - PAINTED - (PT-1)" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION) (mat)" 0.291666666666667, "GYP. BD. - PAINTED - (PT-1)" 0.0520833333333333) | property sets: Pset_ElementShading, Pset_ProductRequirements, EPset_Drawing | description "5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP"
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (a) Front Approach, Pull Side - 18"" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "D6884" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "S8480" | DOOR | DOUBLE_DOOR_SLIDING | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "DOOR TRIM", "DOOR JAMB") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing
  IFCDOORTYPE "D6880" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "3284L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (e* & **)_M Hinge Approach," | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (f)_M Latch Approach, Pull" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3084L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "G36"80"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Qto_DoorBaseQuantities
  IFCDOORTYPE "S7280" | DOOR | DOUBLE_DOOR_SLIDING | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOOR TRIM", "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "DOOR JAMB") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing
  IFCDOORTYPE "D7280" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (c) Hinge Approach, Pull Side - 36"" | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (g)_M Latch Approach, Push" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3080L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "3484L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "3480R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "3680L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (f) Latch Approach, Pull Side - 24"" | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - 30"x48"" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3284R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (g*) Latch Approach, Push Side - 24" (with" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3480L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "3684R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing | description "HOLLOW METAL DOOR – WOOD PANEL"
  IFCDOORTYPE "D4880" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "D6084" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (d)_M Hinge Approach, Pull" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3084R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "3684L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing | description "HOLLOW METAL DOOR – WOOD PANEL"
  IFCDOORTYPE "D4884" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (a)_M Front Approach, Pull" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3680R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "S6080" | DOOR | DOUBLE_DOOR_SLIDING | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOOR JAMB", "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "DOOR TRIM") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing, Qto_DoorBaseQuantities | description "SLIDING CLOSET DOOR"
  IFCDOORTYPE "D6080" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - 36"x48"" | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (e)_M Hinge Approach, Push" | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - 5ft Circle" | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (b) Front Approach, Push Side - 12"" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "G3684L" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Qto_DoorBaseQuantities, EPset_Drawing | description "GLASS INSET (TEMPERED GLAZING)"
  IFCDOORTYPE "S9680" | DOOR | DOUBLE_DOOR_SLIDING | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOOR JAMB", "DOOR TRIM", "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing, Qto_DoorBaseQuantities | description "SLIDING CLOSET DOOR"
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (f*)_M Latch Approach, Pull" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3484R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "D7284" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "D6480" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "DT01" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (d) Hinge Approach, Pull Side - 42"" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3280L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (g*)_M Latch Approach, Push" | PROVISIONFORSPACE | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "ADA - T-shape" | PROVISIONFORSPACE | 1 occurrence
  IFCDOORTYPE "3280R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL (PAINT/STAIN - TBD) \nFRAME (REPAINTED - TBD)", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "ADA - (f*) Latch Approach, Pull Side - 24" (with" | PROVISIONFORSPACE | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "34" counter" | DISHWASHER | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCELECTRICAPPLIANCETYPE "36" X 30"" | REFRIGERATOR | 1 occurrence | material: "REFRIG." | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCELECTRICAPPLIANCETYPE "36" RANGE/OVEN" | ELECTRICCOOKER | 1 occurrence | material: constituents "MaterialConstituentSet" ("Appliance - Plastic - Red": "Appliance - Plastic - Red", "Appliance - Chrome": "Appliance - Chrome", "RANGE": "RANGE", "Appliance - Oven Glass": "Appliance - Oven Glass") | property sets: Pset_BuildingElementProxyCommon, Pset_BuildingElementProxyProvisionForVoid, Pset_EnvironmentalImpactIndicators
  IFCBEAMTYPE "2x10 - Floor" | BEAM | 12 occurrences | material: profiles ("V_White Trim")
  IFCWALLTYPE "V_2x6 drywall Copy" | ELEMENTEDWALL | 10 occurrences | material: layers ("V_Air" 0.0833333358168602, "V_Plywood" 0.0416666679084301, "V_2x6" 0.458333343267441, "V_Drywall" 0.0520833320915699) | property sets: EPset_Parametric
  IFCWINDOWTYPE "w1" | WINDOW | 17 occurrences
  IFCWINDOWTYPE "Double Hung" | WINDOW | 1 occurrence
  IFCWINDOWTYPE "W6" | WINDOW | 2 occurrences
  IFCWALLTYPE "V_porch wall" | ELEMENTEDWALL | 4 occurrences | material: layers ("V_White Trim" 0.0625, "V_2x6" 0.291666656732559, "V_White Trim" 0.0625) | property sets: EPset_Parametric
  IFCBEAMTYPE "beam 1" | 4 occurrences | material: profiles ("V_Steel_Galv.")
  IFCWALLTYPE "GENERIC 6"" | SOLIDWALL | 1 occurrence | material: layers ("GENERIC POCHE" 0.5)
  IFCWINDOWTYPE "Cube" | WINDOW | 7 occurrences
  IFCWINDOWTYPE "w2" | WINDOW | 14 occurrences
  IFCCOVERINGTYPE "SOFFIT" | CEILING | 4 occurrences | material: layers ("EXISTING SOFFIT" 0.666666686534882) | property sets: EPset_Parametric
  IFCWALLTYPE "V_brick" | ELEMENTEDWALL | 9 occurrences | material: layers ("V_Brick" 0.291666656732559) | property sets: EPset_Parametric
  IFCFURNITURETYPE "BC_254_183624_R" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "BC_102_363424" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)") | property sets: Pset_ManufacturerTypeInformation
  IFCWALLTYPE "GEN 8"" | ELEMENTEDWALL | 1 occurrence | material: layers ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 1.4466667175293) | property sets: EPset_Parametric
  IFCDOORTYPE "SLIDING - PATIO" | DOOR | 2 occurrences | material: constituents "MaterialConstituentSet" ("_DESIGN TRIM - WHITE": "_DESIGN TRIM - WHITE", "INSULATED GLAZING": "INSULATED GLAZING") | property sets: Door-Gliding-Andersen-A_Series-Double:_Type Name_:2741442, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
  IFCROOFTYPE "Hip - Shingles 2" | HIP_ROOF | 1 occurrence | property sets: BBIM_Roof
  IFCFURNITURETYPE "BC_253_183624_R" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "BC_100_213424" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET SHELF") | property sets: Pset_ManufacturerTypeInformation
  IFCWINDOWTYPE "w3" | WINDOW | 2 occurrences
  IFCFURNITURETYPE "BC_301_183612_L" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)") | property sets: Pset_ManufacturerTypeInformation
  IFCWALLTYPE "GENERIC 5"" | SOLIDWALL | 1 occurrence | material: layers ("GENERIC POCHE" 0.416666656732559)
  IFCWALLTYPE "GENERIC 3"" | SOLIDWALL | 1 occurrence | material: layers ("GENERIC POCHE" 0.25)
  IFCFURNITURETYPE "BC_152_363624" | element type "CABINET" | USERDEFINED | 1 occurrence | material: "BASE CABINET (PL-1)" | property sets: Pset_ManufacturerTypeInformation
  IFCWALLTYPE "W4BØD" | ELEMENTEDWALL | 2 occurrences | material: layers ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699, "2X WOOD STUD" 0.291666656732559, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699) | property sets: EPset_Parametric | description "5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP"
  IFCSLABTYPE "SlabType" | BASESLAB | 1 occurrence | material: layers ("V_Brick" 0.416666656732559) | property sets: EPset_Parametric
  IFCFURNITURETYPE "BC_102_363624" | element type "CABINET" | USERDEFINED | 1 occurrence | material: "BASE CABINET (PL-1)" | property sets: Pset_ManufacturerTypeInformation
  IFCWALLTYPE "DIAGRAMMATIC WALL" | SOLIDWALL | 1 occurrence | material: layers ("GENERIC POCHE" 0.0833333358168602)
  IFCFURNITURETYPE "BC_222_303624" | element type "CABINET" | USERDEFINED | 1 occurrence | material: "BASE CABINET (PL-1)" | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "BC_101_183624_L" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)") | property sets: Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Porch Floor" | FLOOR | 1 occurrence | material: layers ("V_Wood Flooring" 0.0416666679084301, "V_Plywood" 0.0625) | property sets: EPset_Parametric
  IFCWALLTYPE "GENERIC 2"" | SOLIDWALL | 1 occurrence | material: layers ("GENERIC POCHE" 0.16666667163372)
  IFCDOORTYPE "SLIDING - PATIO Copy" | DOOR | 2 occurrences | material: constituents "MaterialConstituentSet" ("_DESIGN TRIM - WHITE": "_DESIGN TRIM - WHITE", "INSULATED GLAZING": "INSULATED GLAZING") | property sets: Door-Gliding-Andersen-A_Series-Double:_Type Name_:2741442, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
  IFCWINDOWTYPE "W5" | WINDOW | 1 occurrence
  IFCWALLTYPE "W4AØD" | ELEMENTEDWALL | 1 occurrence | material: layers ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION) (mat)" 0.291666656732559, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699) | property sets: EPset_Parametric | description "5/8 GYP - 2X4 WOOD - 5/8 GYP"
  IFCWALLTYPE "EXT WALL - (HORZ. SIDING - 1/2 SHEATHING" | 1 occurrence | material: layers "Basic Wall:EXT WALL - (HORZ. SIDING - 1/2 SHEATHING - 2X6 WOOD(BATT) - 5/8 GYP)" ("SIDING - CLAPBOARD" 0.0416666679084301, "BUILDING WRAP OVER CDX SHEATHING" 0.0416666666666667, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION) (mat)" 0.458333343267441, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833320915699) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "Double Inswing - 4073" | DOOR | 1 occurrence
  IFCCOLUMNTYPE "column 1" | 1 occurrence | material: profiles ("V_Steel_Galv.")
  IFCFURNITURETYPE "BC_211_183624_R" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "BC_101_183424_R" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)") | property sets: Pset_ManufacturerTypeInformation
  IFCWALLTYPE "EXT-VINYL" | STANDARD | 1 occurrence | material: layers "HorzLines6in96scale" ("GENERIC POCHE" 0.583333313465118) | property sets: Pset_ElementShading, Pset_ProductRequirements
  IFCFURNITURETYPE "BC_302_363612" | element type "CABINET" | USERDEFINED | 1 occurrence | material: constituents ("PL-1", "CABINET PULL", "BASE CABINET (PL-1)", "CABINET SIDE", "CABINET BACK/BOTTOM", "CABINET BASE (WB-1)") | property sets: Pset_ManufacturerTypeInformation
  IFCROOFTYPE "Hip" | HIP_ROOF | 1 occurrence | property sets: BBIM_Roof
  IFCWINDOWTYPE "w4" | WINDOW | 1 occurrence
  IFCROOFTYPE "asphalt shingles" | FLAT_ROOF | 1 occurrence | material: layers ("V_Asphalt Shingles" 0.020833333954215) | property sets: EPset_Parametric
  IFCWINDOWTYPE "Sliding Window" | WINDOW | 1 occurrence
  IFCWALLTYPE "GENERIC 1"" | SOLIDWALL | 1 occurrence | material: layers ("GENERIC POCHE" 0.0833333358168602)
  IFCWINDOWTYPE "Casement or Awning or Fixed" | WINDOW | 1 occurrence
  IFCROOFTYPE "Porch Roof" | FLAT_ROOF | 1 occurrence | material: layers ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.833333313465118) | property sets: EPset_Parametric
  IFCWALLTYPE "GENERIC 8"" | SOLIDWALL | 1 occurrence | material: layers ("GENERIC POCHE (NEW)" 0.666666686534882)
  IFCWALLTYPE "GENERIC 4"" | SOLIDWALL | 1 occurrence | material: layers ("GENERIC POCHE" 0.333333343267441)

Property sets
  EPset_Drawing | properties | on 121 objects (99 IFCANNOTATION, 12 IFCBUILDINGELEMENTPROXY, 7 IFCWALL, 2 IFCDOOR) | on 32 type objects
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
  EPset_Drawing | properties | on 16 objects (16 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/2"=1'-0"" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Metadata = "predefined_type, EPset_Status.Status, mats.Name, mats.Category" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/24" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 3 objects (3 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "material.Category" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/32" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCTEXT)
    Metadata = "predefined_type, EPset_Status.Status, mats.Name, mats.Category" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCTEXT)
    Scale = "1/4" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCTEXT)
    Symbols = "drawings\assets\symbols.svg" (IFCTEXT)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "material.Category" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/4" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/2"=1'-0"" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/24" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    CurrentShadingStyle = "Plan" (IFCLABEL)
    Exclude = "IfcGeographicElement + IfcElement, "EPset_Status"."Status"="DEMOLISH" + IfcVirtualElement" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    ImperialPrecision = "1" (IFCLABEL)
    JoinCriteria = "EPset_Status.Status" (IFCTEXT)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Metadata = "predefined_type, EPset_Status.Status, mats.Name, mats.Category" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/48" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    Exclude = "IfcVirtualElement + IfcSpace + IfcGeographicElement + IfcElement , EPset_Status.Status=DEMOLISH" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/96" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "MODEL_VIEW" (IFCLABEL)
  EPset_Drawing: 18 more contents on 17 objects not shown
  EPset_Annotation | properties | on 39 objects (39 IFCANNOTATION)
    Classes = "small" (IFCLABEL)
  EPset_Annotation | properties | on 34 objects (34 IFCANNOTATION)
    Classes = "small fill-bg" (IFCLABEL)
  EPset_Annotation | properties | on 21 objects (21 IFCANNOTATION)
    Classes = "fill-bg" (IFCTEXT)
  EPset_Annotation | properties | on 13 objects (13 IFCANNOTATION)
    Classes = "fill-bg" (IFCLABEL)
  EPset_Annotation | properties | on 7 objects (7 IFCANNOTATION)
    Classes = "oblique, fill-bg" (IFCLABEL)
  EPset_Parametric | properties | on 70 objects (70 IFCWALL)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 17 objects (16 IFCBEAM, 1 IFCCOLUMN)
    Engine = "Bonsai.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 8 objects (8 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 8 objects (4 IFCCOVERING, 2 IFCROOF, 2 IFCSLAB)
    Engine = "Bonsai.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 2 objects (2 IFCCOLUMN)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 6 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  EPset_Parametric | properties | on 5 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  BBIM_Array | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "3iGRJZfy51iAd8K3LgiYDq" (IFCLABEL)
  BBIM_Array | properties | on 10 objects (10 IFCBEAM)
    Parent = "3vki5LfA571ALryRXaERyk" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "0zDYnHKt9D9xBQ0J7EbG8P" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "0QwQTUhPr6EAqfEjNat8se" (IFCLABEL)
  BBIM_Array | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "3QecqJiErB$9TeAgOjclzW" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Data = "[{"children": ["3syCb0d5zDaf1UuAsd_Fxo", "17OoJfbx1FQP_yhRVQqSYn", "3B9HHI1M56hgq$o59XcyAn", "11ASd3UDv9SAGo77xAa5iX", "2jpLr8LAD8MwpGy$UTclFu", "07VBrshCz3hRkEb_0Pb6kF", "2NjRZ17Sf7ZwBsVLJPcW$i", "02lIXz8VDCShBckuHCsAP0", "3jtKSi5qb5mOXZ7jPH28B7", "3FI_7o4Dz1keW3geVnqXHX"], "count": 11, "x": 0.0, "y": 0.0, "z": 0.6666666865348816, "use_local_space": true, "sync_children": false, "method": "OFFSET"}]" (IFCLABEL)
    Parent = "3iGRJZfy51iAd8K3LgiYDq" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Data = "[{"children": ["0Hu5OZfpXCjuqdz_xm5p6$", "04KRMMDiLFIgW7HB4S4vIL", "05a_Wn$f928BFxplue91xZ", "30b0rmoPbFDugJMwVmEMGA", "1sUMWnnaTFLu73DtV$Vg5E", "10Tedwphz2Xw6DSFVkA1zb", "0XSgQoVYLCIACcxDoGGY44", "3KSgklMnr3QOnLfDhxaRy9", "3HF$OKLd1E$fWQN2MAZkGf"], "count": 10, "x": 0.0, "y": 0.0, "z": 0.6666666865348816, "use_local_space": true, "sync_children": false, "method": "OFFSET"}]" (IFCLABEL)
    Parent = "0zDYnHKt9D9xBQ0J7EbG8P" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Data = "[{"children": ["0BUZvVwhLFcOcAqiojq8XJ", "2dC8Tk5z59oAn9EQGs3qxr", "3JyzZ3SZ51EQennn87_bZW", "1piov1eK9CPAWWpE35mYlv", "1NusYV31DBN8_z5_ldWhch", "2Ul6tH$JDBjuajb8WfB8xm", "1$pb4RBKTDtP_eEP_TkpAP", "2NKikJo1T31egFEKkEgv$3", "0d1KDqYRrCE9_7zIFzbh7M"], "count": 10, "x": 0.0, "y": 0.0, "z": 0.6666666865348816, "use_local_space": true, "sync_children": false, "method": "OFFSET"}]" (IFCLABEL)
    Parent = "0QwQTUhPr6EAqfEjNat8se" (IFCLABEL)
  BBIM_Array: 2 more contents on 2 objects not shown
  OD_Options | properties | on 1 object (1 IFCANNOTATION)
    OD_Option_1 = "" (IFCTEXT)
    OD_Option_2 = "N" (IFCTEXT)
  Pset_WallCommon | properties | on 218 objects (218 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 39 objects (39 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 263" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 28 objects (28 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 10 objects (10 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Dowel" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 5 objects (5 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Light Pole Base Plate" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 126" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Ground Rod" (IFCIDENTIFIER)
  Pset_WallCommon: 5 more contents on 4 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 51 objects (51 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Structural Framing 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 26 objects (26 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Structural Framing 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Structural Framing 7" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 263" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "5/8"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "_1" Light Pole Anchor Bolt" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 5 more contents on 2 objects not shown
  BBIM_Dimension | properties | on 4 objects (4 IFCANNOTATION)
    ShowDescriptionOnly = TRUE (IFCBOOLEAN)
  BBIM_Aggregate_Data | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Data = "[{"children": [], "instance_of": ["3fzeczmmTDzODy5MoOxgsJ"]}]" (IFCLABEL)
    Parent = "0fSC_1z0z88vOeLw0MY65G" (IFCLABEL)
  Qto_WallBaseQuantities | quantities | on 20 objects (20 IFCWALL)
    NetVolume = 0.17163085937498 [cubic foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 8 objects (8 IFCWALL)
    NetVolume = 0.145833333333371 [cubic foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 8 objects (8 IFCWALL)
    NetVolume = 0.338770136546469 [cubic foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 8 objects (8 IFCWALL)
    NetVolume = 0.0127494669677329 [cubic foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 7 objects (7 IFCWALL)
    NetVolume = 0.0577256944444402 [cubic foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 6 objects (6 IFCWALL)
    NetVolume = 0.311645507812511 [cubic foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 6 objects (6 IFCWALL)
    NetVolume = 0.833333333333236 [cubic foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 6 objects (6 IFCWALL)
    NetVolume = 0.00545389503946121 [cubic foot (conversion based)]
  Qto_WallBaseQuantities: 176 more contents on 238 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 218 objects (218 IFCWALL)
    Reference = "Generic Models 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 39 objects (39 IFCWALL)
    Reference = "Generic Models 263" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 28 objects (28 IFCWALL)
    Reference = "Generic Models 65" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 10 objects (10 IFCWALL)
    Reference = "Dowel" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 5 objects (5 IFCWALL)
    Reference = "Light Pole Base Plate" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALL)
    Reference = "Walls 126" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Ground Rod" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Light Pole Luminaire" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 4 more contents on 3 objects not shown
  Pset_EnvironmentalImpactIndicators | properties | on 218 objects (218 IFCWALL)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 52 objects (28 IFCWALL, 24 IFCOPENINGELEMENT)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 51 objects (51 IFCBUILDINGELEMENTPROXY)
    Reference = "Structural Framing 1" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 42 objects (39 IFCWALL, 3 IFCBUILDINGELEMENTPROXY)
    Reference = "Generic Models 263" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 26 objects (26 IFCBUILDINGELEMENTPROXY)
    Reference = "Structural Framing 2" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY)
    Reference = "Structural Framing 7" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 10 objects (10 IFCWALL)
    Reference = "Dowel" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 5 objects (5 IFCWALL)
    Reference = "Light Pole Base Plate" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 15 more contents on 14 objects not shown
  Qto_BuildingElementProxyQuantities | quantities | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 1.04513888888876 [square foot (conversion based)]
    NetVolume = 0.0425347222222167 [cubic foot (conversion based)]
  Qto_BuildingElementProxyQuantities | quantities | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 2.36763521613757 [square foot (conversion based)]
    NetVolume = 0.0119955046556136 [cubic foot (conversion based)]
  Qto_BuildingElementProxyQuantities | quantities | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 2.36763521613758 [square foot (conversion based)]
    NetVolume = 0.0119955046556134 [cubic foot (conversion based)]
  Qto_BuildingElementProxyQuantities | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 3.78052220799487 [square foot (conversion based)]
    NetVolume = 0.00966170478802033 [cubic foot (conversion based)]
  Qto_BuildingElementProxyQuantities | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 10.1609479193171 [square foot (conversion based)]
    NetVolume = 0.0260054560117453 [cubic foot (conversion based)]
  Qto_BuildingElementProxyQuantities | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 4.67859257859349 [square foot (conversion based)]
    NetVolume = 0.0119621361118389 [cubic foot (conversion based)]
  Qto_BuildingElementProxyQuantities | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 6.32860826990589 [square foot (conversion based)]
    NetVolume = 0.0161832162121665 [cubic foot (conversion based)]
  Qto_BuildingElementProxyQuantities | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 16.7602252961511 [square foot (conversion based)]
    NetVolume = 0.042909562122448 [cubic foot (conversion based)]
  Qto_BuildingElementProxyQuantities: 71 more contents on 79 objects not shown
  Pset_OpeningElementCommon | properties | on 24 objects (24 IFCOPENINGELEMENT)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Ground Rod" (IFCIDENTIFIER)
  Qto_OpeningElementBaseQuantities | quantities | on 8 objects (8 IFCOPENINGELEMENT)
    Depth = 0.635416666666666 [foot (conversion based)]
    Height = 0.635416666666515 [foot (conversion based)]
    Width = 1.30208333333333 [foot (conversion based)]
  Qto_OpeningElementBaseQuantities | quantities | on 6 objects (6 IFCOPENINGELEMENT)
    Depth = 0.635416666666666 [foot (conversion based)]
    Height = 0.96875 [foot (conversion based)]
    Width = 1.30208333333333 [foot (conversion based)]
  Qto_OpeningElementBaseQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    Depth = 0.635416666666664 [foot (conversion based)]
    Height = 0.635416666666515 [foot (conversion based)]
    Width = 1.30208333333333 [foot (conversion based)]
  Qto_OpeningElementBaseQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    Depth = 0.635416666666668 [foot (conversion based)]
    Height = 0.635416666666515 [foot (conversion based)]
    Width = 1.30208333333333 [foot (conversion based)]
  Qto_OpeningElementBaseQuantities | quantities | on 2 objects (2 IFCOPENINGELEMENT)
    Depth = 0.333333333561437 [foot (conversion based)]
    Height = 0.635416666666515 [foot (conversion based)]
    Width = 1.30208333333333 [foot (conversion based)]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 0.166666666666666 [foot (conversion based)]
    Height = 0.166666666666667 [foot (conversion based)]
    Width = 0.166666666666742 [foot (conversion based)]
  EPset_Status | properties | on 86 objects (52 IFCWALL, 34 IFCWINDOW)
    Status in {"EXISTING"} (IFCLABEL)
  EPset_Status | properties | on 2 objects (2 IFCWINDOW)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Door-Single-Panel:30" x 80":154643 | predefined | on 26 type objects
  Door-Single-Panel:30" x 80":154643:1 | predefined | on 26 type objects
  Pset_DoorCommon | properties | on 26 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 2.1946486495 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "_Type Name_" (IFCIDENTIFIER)
  Door-Single-Panel:30" x 84":154723 | predefined | on 5 type objects
  Door-Single-Panel:30" x 84":154723:1 | predefined | on 5 type objects
  Pset_ElementShading | properties | on 2 type objects
    Roughness = 1. (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_ProductRequirements | properties | on 2 type objects
    Category = "Walls" (IFCLABEL)
  Door-Single-Panel:36" x 84":154924 | predefined | on 2 type objects
  Door-Single-Panel:36" x 84":154924:1 | predefined | on 2 type objects
  Qto_DoorBaseQuantities | quantities | on 2 type objects
    Height = 6.6667 [foot (conversion based)]
    Width = 3. [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 type object
    Height = 6.6667 [foot (conversion based)]
    Width = 5. [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 type object
    Height = 6.6667 [foot (conversion based)]
    Width = 8. [foot (conversion based)]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 1 type object
    Depth = 2. (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Height = 2.70833333333333 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Width = 2. (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 1 type object
    Depth = 2.5 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Height = 6. (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Width = 4. (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_BuildingElementProxyProvisionForVoid | properties | on 1 type object
    Depth = 2.21354166666667 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Height = 3.08333333333333 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Width = 2.97916666666667 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_ManufacturerTypeInformation | properties | on 12 type objects
    ArticleNumber = "???" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 2 type objects
    Manufacturer = "Andersen Corporation" (IFCLABEL)
  Door-Gliding-Andersen-A_Series-Double:_Type Name_:2741442 | predefined | on 4 type objects
  BBIM_Roof | properties | on 1 type object
    Data = "{"roof_type": "HIP/GABLE ROOF", "generation_method": "ANGLE", "roof_thickness": 0.020833333081558464, "rafter_edge_angle": 1.5707963705062866, "angle": 0.6435028910636902, "percentage": 75.00028228759766, "path_data": {"edges": [[0, 1], [1, 2], [2, 3], [5, 0], [3, 4], [4, 5]], "verts": [[-17.666671752929688, -15.775275230407715, 0.0], [-17.66666603088379, 1.8160111904144287, 0.0], [0.0, 1.779841661453247, 0.0], [-1.5644263839931227e-06, -15.775287628173828, 0.0], [-4.045342445373535, -19.82063865661621, 0.0], [-13.62129020690918, -19.820634841918945, 0.0]], "gable_roof_angles": [0.0, 1.5707963705062866, 0.0, 0.0, 0.0, 0.0], "gable_roof_separate_verts": [0, 1, 0, 0, 0, 0]}}" (IFCTEXT)
  BBIM_Roof | properties | on 1 type object
    Data = "{"roof_type": "HIP/GABLE ROOF", "generation_method": "ANGLE", "roof_thickness": 0.8333333599285816, "rafter_edge_angle": 1.5707963705062866, "angle": 0.6435028910636902, "percentage": 75.00028228759766, "path_data": {"edges": [[0, 1], [1, 2], [2, 3], [3, 4], [4, 5], [5, 0]], "verts": [[-0.08918540924787521, -9.413394927978516, 0.0], [9.486763000488281, -9.413394927978516, 0.0], [13.532103538513184, -5.368052959442139, 0.0], [13.532105445861816, 12.18708324432373, 0.0], [-4.13455867767334, 12.223249435424805, 0.0], [-4.134566783905029, -5.3680291175842285, 0.0]], "gable_roof_angles": [0.0, 0.0, 0.0, 1.5707963705062866, 0.0, 0.0], "gable_roof_separate_verts": [0, 0, 0, 1, 0, 0]}}" (IFCTEXT)

Other addresses and roles
  postal address: "103 E SILVER SPRING DR, WHITEFISH BAY, WI 53217", "<Default>"
  postal address: "**ADDRESS OF PROJECT**", "<Default>"