IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "C:\Users\BHA\Desktop\exporter_old.ifc"
Time stamp: "2020-08-04T14:44:19"
Author: "Bernd Hahnebach"
Organization: "Flückiger + Bosshard AG, JägerPartner AG"
Organization: "Räffelstrasse 32, 8045 Zürich"
Preprocessor: "EDMsix Version 2.0100.09 Sep 7 2016"
Originating system: "Allplan 2020.1 18.06.2020 - 11:26:58"
Application: "Allplan" version "2020.1" identifier "Allplan" by Organization "Flückiger + Bosshard AG, JägerPartner AG"

People and organizations
  Person "Bernd" "Hahnebach" of Organization "Flückiger + Bosshard AG, JägerPartner AG"
  Owner history of Person "Bernd" "Hahnebach" of Organization "Flückiger + Bosshard AG, JägerPartner AG" | application "Allplan" version "2020.1" identifier "Allplan" by Organization "Flückiger + Bosshard AG, JägerPartner AG" | change ADDED | created 1596544991 (2020-08-04T12:43:11Z)

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "MA_BHA_Ablage_Probleme_BSP"
  IFCSITE "Default Site" | latitude 8° 0′ 0″ | longitude 46° 0′ 0″ | elevation above sea level 0.
    IFCBUILDING "Default Building" | postal address: "Zürich", "Schweiz"
      IFCBUILDINGSTOREY "Default Storey" | elevation 0.
        contains 2 elements
          2 x IFCWALLSTANDARDCASE | names: "Mehrschichten-Wand" | material: layers ("Backstein" 0.15, "Daemmung" 0.12, "Ortbeton" 0.2); layers ("Fertigelement Beton" 0.06, "Ortbeton" 0.17, "Daemmung" 0.08, "Fertigelement Beton" 0.05) | property sets: Pset_WallCommon, AllplanAttributes

Property sets
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    LoadBearing = TRUE (IFCBOOLEAN)
  AllplanAttributes | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Allright_Bauteil_ID = "0033HWa0000000011" (IFCDESCRIPTIVEMEASURE)
    Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE)
    Einheit = "St" (IFCDESCRIPTIVEMEASURE)
    Gewerk = "Betonarbeiten" (IFCDESCRIPTIVEMEASURE)
    IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE)
    Material = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--11" (IFCDESCRIPTIVEMEASURE)
    Object Layer Attributes #1: Allright_Bauteil_ID = "0033Wa 0000000014" (IFCDESCRIPTIVEMEASURE); Umbaukategorie = "Neubau" (IFCLABEL); Einheit = "m²" (IFCDESCRIPTIVEMEASURE); Gewerk = "Mauerarbeiten" (IFCDESCRIPTIVEMEASURE); Objektname = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Material = "Backstein" (IFCDESCRIPTIVEMEASURE); statisch_tragend = TRUE (IFCBOOLEAN); Außenbauteil = FALSE (IFCBOOLEAN); NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--14" (IFCDESCRIPTIVEMEASURE); IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE); Trittschallpegeldifferenz OHNE Bezugsdeckenverfahren = "keine" (IFCDESCRIPTIVEMEASURE); Fugenöffnung = "Gleichz.m.Rohbau_vollfugig" (IFCDESCRIPTIVEMEASURE)
    Object Layer Attributes #2: Allright_Bauteil_ID = "0033Wa 0000000013" (IFCDESCRIPTIVEMEASURE); Umbaukategorie = "Neubau" (IFCLABEL); Einheit = "m²" (IFCDESCRIPTIVEMEASURE); Gewerk = "Betonarbeiten" (IFCDESCRIPTIVEMEASURE); Objektname = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Material = "Daemmung" (IFCDESCRIPTIVEMEASURE); statisch_tragend = FALSE (IFCBOOLEAN); Außenbauteil = FALSE (IFCBOOLEAN); NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--13" (IFCDESCRIPTIVEMEASURE); IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE)
    Object Layer Attributes #3: Allright_Bauteil_ID = "0033Wa 0000000012" (IFCDESCRIPTIVEMEASURE); Umbaukategorie = "Neubau" (IFCLABEL); Einheit = "m²" (IFCDESCRIPTIVEMEASURE); Gewerk = "Betonarbeiten" (IFCDESCRIPTIVEMEASURE); Objektname = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Material = "Ortbeton" (IFCDESCRIPTIVEMEASURE); statisch_tragend = TRUE (IFCBOOLEAN); Außenbauteil = FALSE (IFCBOOLEAN); NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--12" (IFCDESCRIPTIVEMEASURE); IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE)
    Objektname = "Mehrsch-Wand" (IFCDESCRIPTIVEMEASURE)
    Umbaukategorie = "Neubau" (IFCLABEL)
  AllplanAttributes | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Allright_Bauteil_ID = "0033HWa0000000022" (IFCDESCRIPTIVEMEASURE)
    Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE)
    Einheit = "St" (IFCDESCRIPTIVEMEASURE)
    IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE)
    Material = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE)
    NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--22" (IFCDESCRIPTIVEMEASURE)
    Object Layer Attributes #1: Allright_Bauteil_ID = "0033Wa 0000000026" (IFCDESCRIPTIVEMEASURE); Umbaukategorie = "Neubau" (IFCLABEL); Einheit = "St" (IFCDESCRIPTIVEMEASURE); Gewerk = "Betonarbeiten" (IFCDESCRIPTIVEMEASURE); Objektname = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Material = "Fertigelement Beton" (IFCDESCRIPTIVEMEASURE); statisch_tragend = TRUE (IFCBOOLEAN); Außenbauteil = FALSE (IFCBOOLEAN); NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--26" (IFCDESCRIPTIVEMEASURE); IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE)
    Object Layer Attributes #2: Allright_Bauteil_ID = "0033Wa 0000000025" (IFCDESCRIPTIVEMEASURE); Umbaukategorie = "Neubau" (IFCLABEL); Einheit = "m³" (IFCDESCRIPTIVEMEASURE); Gewerk = "Betonarbeiten" (IFCDESCRIPTIVEMEASURE); Objektname = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Material = "Ortbeton" (IFCDESCRIPTIVEMEASURE); statisch_tragend = TRUE (IFCBOOLEAN); Außenbauteil = FALSE (IFCBOOLEAN); NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--25" (IFCDESCRIPTIVEMEASURE); IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE)
    Object Layer Attributes #3: Allright_Bauteil_ID = "0033Wa 0000000024" (IFCDESCRIPTIVEMEASURE); Umbaukategorie = "Neubau" (IFCLABEL); Einheit = "St" (IFCDESCRIPTIVEMEASURE); Gewerk = "Betonarbeiten" (IFCDESCRIPTIVEMEASURE); Objektname = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Material = "Daemmung" (IFCDESCRIPTIVEMEASURE); statisch_tragend = TRUE (IFCBOOLEAN); Außenbauteil = FALSE (IFCBOOLEAN); NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--24" (IFCDESCRIPTIVEMEASURE); IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE)
    Object Layer Attributes #4: Allright_Bauteil_ID = "0033Wa 0000000023" (IFCDESCRIPTIVEMEASURE); Umbaukategorie = "Neubau" (IFCLABEL); Einheit = "m²" (IFCDESCRIPTIVEMEASURE); Objektname = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Bezeichnung = "Mehrschichten-Wand" (IFCDESCRIPTIVEMEASURE); Material = "Fertigelement Beton" (IFCDESCRIPTIVEMEASURE); statisch_tragend = TRUE (IFCBOOLEAN); Außenbauteil = FALSE (IFCBOOLEAN); NOI_UUID = "2c3f7016-d5f2-4b9b-9ea7-6de7b5e546cf--23" (IFCDESCRIPTIVEMEASURE); IFC-Objekttyp = "IfcWall" (IFCDESCRIPTIVEMEASURE)
    Objektname = "Mehrsch-Wand" (IFCDESCRIPTIVEMEASURE)
    Umbaukategorie = "Neubau" (IFCLABEL)