IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "beam_me_up.ifc"
Time stamp: "2022-07-10T13:45:29+02:00"
Preprocessor: "IfcOpenShell v0.7.0-1b1fd1e6"
Originating system: "BlenderBIM 0.0.220516"
Authorization: "Nobody"

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 13 elements
          6 x IFCBEAM | type IFCBEAMTYPE "beam_type" | names: "Beam" | material: profiles ("beton") | property sets: EPset_Parametric
          1 x IFCSLAB | BASESLAB | names: "Vert"
          6 x IFCWALL | type IFCWALLTYPE "wall" | names: "Wall" | material: layers "brick" ("brick" 0.100000001490116) | property sets: EPset_Parametric, Qto_WallBaseQuantities

Types
  IFCBEAMTYPE "beam_type" | BEAM | 6 occurrences | material: profiles ("beton")
  IFCWALLTYPE "wall" | ELEMENTEDWALL | 6 occurrences | material: layers "brick" ("brick" 0.100000001490116)

Property sets
  EPset_Parametric | properties | on 6 objects (6 IFCBEAM)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 6 objects (6 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.38 [SQUARE_METRE]
    GrossSideArea = 11.1 [SQUARE_METRE]
    GrossVolume = 1.14 [CUBIC_METRE]
    Height = 3. [METRE]
    Length = 3.9 [METRE]
    NetFootprintArea = 0.38 [SQUARE_METRE]
    NetSideArea = 11.1 [SQUARE_METRE]
    NetVolume = 1.14 [CUBIC_METRE]
    Width = 0.1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.15 [SQUARE_METRE]
    GrossSideArea = 4.2 [SQUARE_METRE]
    GrossVolume = 0.45 [CUBIC_METRE]
    Height = 3. [METRE]
    Length = 1.6 [METRE]
    NetFootprintArea = 0.15 [SQUARE_METRE]
    NetSideArea = 4.2 [SQUARE_METRE]
    NetVolume = 0.45 [CUBIC_METRE]
    Width = 0.1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.13 [SQUARE_METRE]
    GrossSideArea = 3.9 [SQUARE_METRE]
    GrossVolume = 0.39 [CUBIC_METRE]
    Height = 3. [METRE]
    Length = 1.4 [METRE]
    NetFootprintArea = 0.13 [SQUARE_METRE]
    NetSideArea = 3.9 [SQUARE_METRE]
    NetVolume = 0.39 [CUBIC_METRE]
    Width = 0.1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.2 [SQUARE_METRE]
    GrossSideArea = 6. [SQUARE_METRE]
    GrossVolume = 0.6 [CUBIC_METRE]
    Height = 3. [METRE]
    Length = 2.1 [METRE]
    NetFootprintArea = 0.2 [SQUARE_METRE]
    NetSideArea = 6. [SQUARE_METRE]
    NetVolume = 0.6 [CUBIC_METRE]
    Width = 0.1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.25 [SQUARE_METRE]
    GrossSideArea = 7.2 [SQUARE_METRE]
    GrossVolume = 0.75 [CUBIC_METRE]
    Height = 3. [METRE]
    Length = 2.6 [METRE]
    NetFootprintArea = 0.25 [SQUARE_METRE]
    NetSideArea = 7.2 [SQUARE_METRE]
    NetVolume = 0.75 [CUBIC_METRE]
    Width = 0.1 [METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.35 [SQUARE_METRE]
    GrossSideArea = 10.2 [SQUARE_METRE]
    GrossVolume = 1.05 [CUBIC_METRE]
    Height = 3. [METRE]
    Length = 3.6 [METRE]
    NetFootprintArea = 0.35 [SQUARE_METRE]
    NetSideArea = 10.2 [SQUARE_METRE]
    NetVolume = 1.05 [CUBIC_METRE]
    Width = 0.1 [METRE]