IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition[DesignTransferView]"
File name: "Simple 1 bed rev Today-IFC4X3.ifc"
Time stamp: "2025-03-12T07:44:26+02:00"
Preprocessor: "IfcOpenShell 0.8.2-alpha250308"
Originating system: "Bonsai 0.8.2-alpha250308-47d11da"
Authorization: "Nobody"
Application: "Bonsai" version "0.8.1-alpha250203-c5185aa" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241028-4c3bb54" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha250130-af29f26" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241028-4c3bb54" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241122-71637f1" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241122-71637f1" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241127-25eecde" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

People and organizations
  110 x Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT)
  139 x Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change MODIFIED | created 1736770853 (2025-01-13T12:20:53Z) | last modified 1736770946 (2025-01-13T12:22:26Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  2 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha241028-4c3bb54" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change MODIFIED | created 1730209151 (2024-10-29T13:39:11Z) | last modified 1736347652 (2025-01-08T14:47:32Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  7 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha241028-4c3bb54" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1730209151 (2024-10-29T13:39:11Z) | last modified 1730209151 (2024-10-29T13:39:11Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha241028-4c3bb54" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha241028-4c3bb54" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change MODIFIED | created 1730209151 (2024-10-29T13:39:11Z) | last modified 1736361122 (2025-01-08T18:32:02Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  3 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1736347778 (2025-01-08T14:49:38Z) | last modified 1736347778 (2025-01-08T14:49:38Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1736349744 (2025-01-08T15:22:24Z) | last modified 1736349744 (2025-01-08T15:22:24Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha250106-8313c05" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  122 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha241122-71637f1" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1732539344 (2024-11-25T12:55:44Z) | last modified 1732539344 (2024-11-25T12:55:44Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha241122-71637f1" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha241028-4c3bb54" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change MODIFIED | created 1730209151 (2024-10-29T13:39:11Z) | last modified 1733484031 (2024-12-06T11:20:31Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha241127-25eecde" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

Units
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: degree (conversion based)
  CURRENCY: ZAR

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "Simple 1Bed House"
      IFCBUILDINGSTOREY "Outside"
        contains 43 elements
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Small Kitchen Bench" | names: "Furniture"
          2 x IFCWALL | type IFCWALLTYPE "110mm non-load bearing" | names: "Wall" | material: layers "brick" ("FNP-Red" 110.) | property sets: EPset_Parametric, Qto_WallBaseQuantities
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "50mm-PVC-90B" | names: "50mm-uPVC-90B"
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "15MM-CU-45" | names: "15mm-CU-45"
          2 x IFCBEAM | type IFCBEAMTYPE "Timber 38x114" | names: "Beam" | material: profiles "timber-material" ("Timber pine") | property sets: EPset_Parametric
          6 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "15mm-CU-T" | names: "15mm-CU-T"
          5 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "15mm-CU-90B" | names: "15mm-CU-90B"
          4 x IFCFURNITURE | type IFCFURNITURETYPE "BIC 600x564x2000" | names: "Furniture" | material: "Red Sligna"
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | names: "SanitaryTerminal"
          12 x IFCBEAM | type IFCBEAMTYPE "Single Lintol 1.4m" | names: "Lintol-single-1.4m" | property sets: Qto_BeamBaseQuantities
          2 x IFCELEMENTASSEMBLY | names: "Hot Water", "Default_Name" | parts: 13 IFCPIPEFITTING
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "Solar DB 150x200x100" | names: "ElectricDistributionBoard"
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "110mm-uPVC-Ptrap-UG" | names: "110-uPVC-Y-UG"
          2 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "15mm-CU-Male-Str" | names: "PipeFitting" | material: "Copper"
          1 x IFCELECTRICFLOWSTORAGEDEVICE | type IFCELECTRICFLOWSTORAGEDEVICETYPE "Battery 5kWh Lithiom" | names: "ElectricFlowStorageDevice" | material: "White PVA"
        IFCBUILDINGSTOREY "Garadge"
          contains 4 elements
            4 x IFCBEAM | BEAM | names: "Steel-100x100.003", "Steel-100x100.001" | property sets: EPset_Parametric, Qto_BeamBaseQuantities
        IFCBUILDINGSTOREY "Balcony"
          contains 7 elements
            1 x IFCSLAB | type IFCSLABTYPE "85mm surface bed" | names: "Slab" | material: layers "concrete" ("25 MPa wooden float" 85.) | property sets: EPset_Parametric, Qto_SlabBaseQuantities
            2 x IFCWALL | type IFCWALLTYPE "220mm load bearing" | names: "Wall" | material: layers "brick" ("FNP-Red" 220.) | property sets: EPset_Parametric, Qto_WallBaseQuantities
            4 x IFCBEAM | type IFCBEAMTYPE "Timber 38x114" | BEAM | names: "Timber-38x114x2000", "Timber-38x114x2000.001", "Timber-38x114x2000.003" (+1 more) | material: profiles "timber-material" ("Timber pine") | property sets: EPset_Parametric, Qto_BeamBaseQuantities
        IFCSPACE "Space0"
        IFCBUILDINGSTOREY "Garden"
          contains 15 elements
            1 x IFCTANK | type IFCTANKTYPE "5000ltJoJo tank" | names: "5000lt jojo tank"
            4 x IFCWALL | type IFCWALLTYPE "220mm foundation" | names: "Wall" | material: layers "brick" ("NFX-Clay" 220.) | property sets: EPset_Parametric, Qto_WallBaseQuantities
            4 x IFCSLAB | type IFCSLABTYPE "85mm surface bed" | names: "Concrete apron 850x85" | material: layers "concrete" ("25 MPa wooden float" 85.) | property sets: EPset_Parametric, Qto_SlabBaseQuantities
            1 x IFCTANK | type IFCTANKTYPE "11kg LPG Gas" | names: "11kg-LPG" | material: "Steel hot rolled"
            1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "110mm-UG-PVC-90B" | BEND | names: "110-dia-uPVC.001" | material: profiles ("uPVC") | property sets: Qto_PipeSegmentBaseQuantities, EPset_Parametric
            4 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "110 dia uPVC" | names: "110-dia-uPVC-UG" | material: profiles ("uPVC") | property sets: EPset_Parametric, Qto_PipeSegmentBaseQuantities, BBIM_Boolean
      IFCBUILDINGSTOREY "Building"
        contains 4 elements
          1 x IFCWALL | type IFCWALLTYPE "110mm non-load bearing" | names: "110mm NPF" | material: layers "brick" ("FNP-Red" 110.) | property sets: EPset_Parametric, Qto_WallBaseQuantities
          2 x IFCCOVERING | type IFCCOVERINGTYPE "25mm plaster" | names: "25mm plaster" | material: layers ("25 MPa wooden float" 25.) | property sets: EPset_Parametric, Qto_CoveringBaseQuantities
          1 x IFCELEMENTASSEMBLY | names: "Default_Name" | parts: 1 IFCCOVERING
        IFCBUILDINGSTOREY "Ground floor"
          contains 82 elements
            38 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "15mm Copper" | names: "15mm-CU-Cold", "15mm-cu-Cold", "15mm-cu-Hot.020" (+6 more) | material: profiles ("Copper") | property sets: EPset_Parametric, Qto_PipeSegmentBaseQuantities
            3 x IFCCOVERING | type IFCCOVERINGTYPE "25mm plaster" | names: "25mm plaster" | material: layers ("25 MPa wooden float" 25.) | property sets: EPset_Parametric, Qto_CoveringBaseQuantities
            6 x IFCOUTLET | type IFCOUTLETTYPE "4x4 Double Plug" | POWEROUTLET | names: "Double Plug.002", "Double Plug.001", "Double Plug.003" (+3 more) | material: "uPVC"
            4 x IFCWALL | type IFCWALLTYPE "220mm load bearing" | names: "220mm NPF external" | material: layers "brick" ("FNP-Red" 220.) | property sets: EPset_Parametric, Qto_WallBaseQuantities
            3 x IFCDOOR | type IFCDOORTYPE "Internal door LH" | names: "Intelnal door Swing Left", "Door"
            1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Single basin" | names: "Single Basin"
            1 x IFCSLAB | type IFCSLABTYPE "85mm surface bed" | names: "85mm concrete slab" | material: layers "concrete" ("25 MPa wooden float" 85.) | property sets: Qto_SlabBaseQuantities, EPset_Parametric
            5 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "Light Switch 2x4 single" | names: "2x4 LigthSwitch"
            1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Sink" | names: "Sink"
            2 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "50 dia PVC" | names: "50diaPVC-pipe" | material: profiles ("uPVC") | property sets: Qto_PipeSegmentBaseQuantities, EPset_Parametric
            1 x IFCWINDOW | type IFCWINDOWTYPE "PT126 600x1200" | names: "Window"
            1 x IFCWINDOW | type IFCWINDOWTYPE "SD 2421 XO" | DOUBLE_PANEL_VERTICAL | names: "SD 2421" | property sets: Qto_WindowBaseQuantities
            1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Shower 90x90" | names: "Shower"
            1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Neufert Dishwasher" | names: "15kg WM"
            1 x IFCCOVERING | type IFCCOVERINGTYPE "2 Coat PVA Paint" | names: "2Coat PVA Paint" | material: layers ("White PVA" 2.) | property sets: EPset_Parametric, Qto_CoveringBaseQuantities
            1 x IFCWINDOW | type IFCWINDOWTYPE "PTT186 600X1800" | names: "PTT186" | property sets: Qto_WindowBaseQuantities
            1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "Solar DC Isolator" | names: "DC Isolator"
            1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "4 plate ST" | names: "200lt fridge"
            2 x IFCWALL | type IFCWALLTYPE "110mm non-load bearing" | names: "110mm NPF" | material: layers "brick" ("FNP-Red" 110.) | property sets: Qto_WallBaseQuantities, EPset_Parametric
            2 x IFCELECTRICFLOWSTORAGEDEVICE | type IFCELECTRICFLOWSTORAGEDEVICETYPE "Battery 5kWh Lithiom" | names: "5KWH Battry" | material: "White PVA"
            1 x IFCFURNITURE | type IFCFURNITURETYPE "3 seater" | names: "3 seater couch"
            1 x IFCFURNITURE | type IFCFURNITURETYPE "King Size" | names: "King Size bed and side table"
            1 x IFCCOVERING | type IFCCOVERINGTYPE "DPC-250micron" | names: "DPM 250mic" | material: layers ("DPM-Green Plastic" 1.) | property sets: Qto_CoveringBaseQuantities, EPset_Parametric
            1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Generic Large Fridge Zone" | names: "200lt fridge"
            1 x IFCELEMENTASSEMBLY | names: "Bathroomwall"
            1 x IFCWINDOW | type IFCWINDOWTYPE "PTT1815 1500x1800" | names: "PTT1815" | property sets: Qto_WindowBaseQuantities
        IFCBUILDINGSTOREY "Roof"
        IFCBUILDINGSTOREY "Foundation"
          contains 23 elements
            8 x IFCWALL | type IFCWALLTYPE "220mm foundation" | names: "Wall", "220mm Foundation" | material: layers "brick" ("NFX-Clay" 220.) | property sets: EPset_Parametric, Qto_WallBaseQuantities, EPset_Status
            14 x IFCFOOTING | type IFCFOOTINGTYPE "Foundation 600x280" | names: "Footing", "600x280 Concrete foundation" | material: layers "concrete" ("25 MPa wooden float" 200.) | property sets: EPset_Parametric, Qto_FootingBaseQuantities, Pset_ConcreteElementGeneral
            1 x IFCSLAB | type IFCSLABTYPE "85mm surface bed" | names: "Slab" | material: layers "concrete" ("25 MPa wooden float" 85.) | property sets: Qto_SlabBaseQuantities, EPset_Parametric
IFCWORKPLAN "Plan"
  IFCWORKSCHEDULE "Plan" | ACTUAL

Types
  IFCFURNITURETYPE "Neufert Small Kitchen Bench" | 1 occurrence
  IFCWALLTYPE "110mm non-load bearing" | SOLIDWALL | 5 occurrences | material: layers "brick" ("FNP-Red" 110.) | property sets: EPset_Parametric
  IFCPIPEFITTINGTYPE "50mm-PVC-90B" | BEND | 1 occurrence
  IFCPIPEFITTINGTYPE "15MM-CU-45" | BEND | 2 occurrences
  IFCBEAMTYPE "Timber 38x114" | BEAM | 6 occurrences | material: profiles "timber-material" ("Timber pine")
  IFCPIPEFITTINGTYPE "15mm-CU-T" | BEND | 6 occurrences
  IFCPIPEFITTINGTYPE "15mm-CU-90B" | BEND | 5 occurrences
  IFCFURNITURETYPE "BIC 600x564x2000" | SHELF | 4 occurrences | material: "Red Sligna"
  IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | 1 occurrence
  IFCBEAMTYPE "Single Lintol 1.4m" | LINTEL | 12 occurrences
  IFCELECTRICDISTRIBUTIONBOARDTYPE "Solar DB 150x200x100" | SWITCHBOARD | 1 occurrence
  IFCPIPEFITTINGTYPE "110mm-uPVC-Ptrap-UG" | BEND | 1 occurrence
  IFCPIPEFITTINGTYPE "15mm-CU-Male-Str" | CONNECTOR | 2 occurrences | material: "Copper"
  IFCELECTRICFLOWSTORAGEDEVICETYPE "Battery 5kWh Lithiom" | BATTERY | 3 occurrences | material: "White PVA"
  IFCSLABTYPE "85mm surface bed" | BASESLAB | 7 occurrences | material: layers "concrete" ("25 MPa wooden float" 85.) | property sets: EPset_Parametric
  IFCWALLTYPE "220mm load bearing" | SOLIDWALL | 6 occurrences | material: layers "brick" ("FNP-Red" 220.) | property sets: EPset_Parametric, Pset_WallCommon
  IFCTANKTYPE "5000ltJoJo tank" | STORAGE | 1 occurrence
  IFCWALLTYPE "220mm foundation" | ELEMENTEDWALL | 12 occurrences | material: layers "brick" ("NFX-Clay" 220.) | property sets: EPset_Parametric, Pset_WallCommon
  IFCTANKTYPE "11kg LPG Gas" | STORAGE | 1 occurrence | material: "Steel hot rolled"
  IFCPIPEFITTINGTYPE "110mm-UG-PVC-90B" | BEND | 1 occurrence
  IFCPIPESEGMENTTYPE "110 dia uPVC" | RIGIDSEGMENT | 4 occurrences | material: profiles ("uPVC")
  IFCCOVERINGTYPE "25mm plaster" | CLADDING | 5 occurrences | material: layers ("25 MPa wooden float" 25.) | property sets: EPset_Parametric
  IFCPIPESEGMENTTYPE "15mm Copper" | RIGIDSEGMENT | 38 occurrences | material: profiles ("Copper")
  IFCOUTLETTYPE "4x4 Double Plug" | POWEROUTLET | 6 occurrences | material: "uPVC"
  IFCDOORTYPE "Internal door LH" | DOOR | SINGLE_SWING_LEFT | 3 occurrences | property sets: BBIM_Door | description "RDF4"
  IFCSANITARYTERMINALTYPE "Single basin" | WASHHANDBASIN | 1 occurrence
  IFCSWITCHINGDEVICETYPE "Light Switch 2x4 single" | SWITCHDISCONNECTOR | 5 occurrences
  IFCSANITARYTERMINALTYPE "Sink" | SINK | 1 occurrence
  IFCPIPESEGMENTTYPE "50 dia PVC" | RIGIDSEGMENT | 2 occurrences | material: profiles ("uPVC")
  IFCWINDOWTYPE "PT126 600x1200" | WINDOW | DOUBLE_PANEL_VERTICAL | 1 occurrence | property sets: BBIM_Window
  IFCWINDOWTYPE "SD 2421 XO" | WINDOW | DOUBLE_PANEL_VERTICAL | 1 occurrence | property sets: BBIM_Window
  IFCSANITARYTERMINALTYPE "Neufert Shower 90x90" | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "Neufert Dishwasher" | 1 occurrence
  IFCCOVERINGTYPE "2 Coat PVA Paint" | CLADDING | 1 occurrence | material: layers ("White PVA" 2.) | property sets: EPset_Parametric
  IFCWINDOWTYPE "PTT186 600X1800" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCELECTRICDISTRIBUTIONBOARDTYPE "Solar DC Isolator" | DISTRIBUTIONBOARD | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "4 plate ST" | ELECTRICCOOKER | 1 occurrence
  IFCFURNITURETYPE "3 seater" | SOFA | 1 occurrence
  IFCFURNITURETYPE "King Size" | BED | 1 occurrence
  IFCCOVERINGTYPE "DPC-250micron" | MEMBRANE | 1 occurrence | material: layers ("DPM-Green Plastic" 1.) | property sets: EPset_Parametric
  IFCELECTRICAPPLIANCETYPE "Generic Large Fridge Zone" | 1 occurrence
  IFCWINDOWTYPE "PTT1815 1500x1800" | WINDOW | TRIPLE_PANEL_LEFT | 1 occurrence | property sets: BBIM_Window
  IFCFOOTINGTYPE "Foundation 600x280" | STRIP_FOOTING | 14 occurrences | material: layers "concrete" ("25 MPa wooden float" 200.) | property sets: EPset_Parametric

Property sets
  EPset_Parametric | properties | on 55 objects (44 IFCPIPESEGMENT, 10 IFCBEAM, 1 IFCPIPEFITTING)
    Engine = "Bonsai.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 30 objects (23 IFCWALL, 7 IFCCOVERING)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 22 objects (14 IFCFOOTING, 7 IFCSLAB, 1 IFCCOVERING)
    Engine = "Bonsai.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 5 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  EPset_Parametric | properties | on 3 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  Qto_PipeSegmentBaseQuantities | quantities | on 3 objects (3 IFCPIPESEGMENT)
  Qto_PipeSegmentBaseQuantities | quantities | on 3 objects (3 IFCPIPESEGMENT)
    Length = 87.1143043517514 [MILLI METRE]
    NetCrossSectionArea = 7.46664875350689E-05 [SQUARE_METRE]
    OuterSurfaceArea = 0.0464977314695716 [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 2 objects (2 IFCPIPESEGMENT)
    Length = 300.939914420357 [MILLI METRE]
    NetCrossSectionArea = 7.46664875350689E-05 [SQUARE_METRE]
    OuterSurfaceArea = 0.23972699418664 [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 2 objects (2 IFCPIPESEGMENT)
    Length = 109.137771694757 [MILLI METRE]
    NetCrossSectionArea = 7.46664875350689E-05 [SQUARE_METRE]
    OuterSurfaceArea = 0.0365069014951587 [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 2 objects (2 IFCPIPESEGMENT)
    Length = 250. [MILLI METRE]
    NetCrossSectionArea = 7.46664875350689E-05 [SQUARE_METRE]
    OuterSurfaceArea = 0.0374573422595859 [SQUARE_METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 1 object (1 IFCPIPESEGMENT)
    Length = 167.819977456977 [MILLI METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 1 object (1 IFCPIPEFITTING)
    Length = 752.118304973238 [MILLI METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 1 object (1 IFCPIPESEGMENT)
    Length = 885.862937359611 [MILLI METRE]
  Qto_PipeSegmentBaseQuantities: 30 more contents on 30 objects not shown
  Qto_TaskBaseQuantities | quantities | on 3 objects (3 IFCTASK)
    StandardWork = 1.
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 4.56518796997873 [SQUARE_METRE]
    NetArea = 4.56518796997873 [SQUARE_METRE]
    Width = 25. [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 6.40254679904698 [SQUARE_METRE]
    NetArea = 6.40254679904698 [SQUARE_METRE]
    Width = 25. [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 4.57000844958027 [SQUARE_METRE]
    NetArea = 4.57000844958027 [SQUARE_METRE]
    Width = 25. [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 9.9488043799747 [SQUARE_METRE]
    NetArea = 9.9488043799747 [SQUARE_METRE]
    Width = 2. [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 6.46037811138281 [SQUARE_METRE]
    NetArea = 6.46037811138281 [SQUARE_METRE]
    Width = 2. [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 6.43875127136221 [SQUARE_METRE]
    NetArea = 6.43875127136221 [SQUARE_METRE]
    Width = 2. [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 6.40979027672317 [SQUARE_METRE]
    NetArea = 6.40979027672317 [SQUARE_METRE]
    Width = 25. [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 45.2466840285581 [SQUARE_METRE]
    NetArea = 45.2466840285581 [SQUARE_METRE]
    Width = 1. [MILLI METRE]
  Qto_BeamBaseQuantities | quantities | on 12 objects (12 IFCBEAM)
    GrossSurfaceArea = 0.534499593200601 [SQUARE_METRE]
    GrossVolume = 0.0115499921264617 [CUBIC_METRE]
    Length = 1399.99865722656 [MILLI METRE]
    NetSurfaceArea = 0.534499593200601 [SQUARE_METRE]
    NetVolume = 0.0115499921264617 [CUBIC_METRE]
    OuterSurfaceArea = 0.226499803161621 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 2 objects (2 IFCBEAM)
    GrossSurfaceArea = 0.630325531063479 [SQUARE_METRE]
    GrossVolume = 0.00885867681765458 [CUBIC_METRE]
    Length = 2044.93924691934 [MILLI METRE]
    NetSurfaceArea = 0.630325531063479 [SQUARE_METRE]
    NetVolume = 0.00885867681765458 [CUBIC_METRE]
    OuterSurfaceArea = 0.621661531063479 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 2 objects (2 IFCBEAM)
    GrossSurfaceArea = 0.630325460177021 [SQUARE_METRE]
    GrossVolume = 0.00885867580752255 [CUBIC_METRE]
    Length = 2044.9390137402 [MILLI METRE]
    NetSurfaceArea = 0.630325460177021 [SQUARE_METRE]
    NetVolume = 0.00885867580752255 [CUBIC_METRE]
    OuterSurfaceArea = 0.621661460177021 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    GrossSurfaceArea = 2.38809701343321 [SQUARE_METRE]
    GrossVolume = 0.00374561039259701 [CUBIC_METRE]
    Length = 3231.27597833267 [MILLI METRE]
    NetSurfaceArea = 2.38809701343321 [SQUARE_METRE]
    NetVolume = 0.00374561039259701 [CUBIC_METRE]
    OuterSurfaceArea = 2.03626868369499 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    GrossSurfaceArea = 2.38809601878747 [SQUARE_METRE]
    GrossVolume = 0.00374560883099588 [CUBIC_METRE]
    Length = 3231.27463675095 [MILLI METRE]
    NetSurfaceArea = 2.38809601878747 [SQUARE_METRE]
    NetVolume = 0.00374560883099588 [CUBIC_METRE]
    OuterSurfaceArea = 2.03626783474405 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    GrossSurfaceArea = 1.80249479415724 [SQUARE_METRE]
    GrossVolume = 0.00282621061040208 [CUBIC_METRE]
    Length = 2441.41362249511 [MILLI METRE]
    NetSurfaceArea = 1.80249479415724 [SQUARE_METRE]
    NetVolume = 0.00282621061040208 [CUBIC_METRE]
    OuterSurfaceArea = 1.53644494656 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    GrossSurfaceArea = 1.7556284327442 [SQUARE_METRE]
    GrossVolume = 0.00275263007901533 [CUBIC_METRE]
    Length = 2378.20010755804 [MILLI METRE]
    NetSurfaceArea = 1.7556284327442 [SQUARE_METRE]
    NetVolume = 0.00275263007901533 [CUBIC_METRE]
    OuterSurfaceArea = 1.49644352727501 [SQUARE_METRE]
  Qto_FootingBaseQuantities | quantities | on 6 objects (6 IFCFOOTING)
    Height = 170.000001788139 [MILLI METRE]
    Length = 420.001035813916 [MILLI METRE]
    NetVolume = 0.0142800353678772 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 2 objects (2 IFCFOOTING)
    Height = 200. [MILLI METRE]
    Length = 2329.8984375 [MILLI METRE]
    NetVolume = 0.288908401690006 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 2 objects (2 IFCFOOTING)
    Height = 200. [MILLI METRE]
    Length = 1064.40869140625 [MILLI METRE]
    NetVolume = 0.131987127626354 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 200. [MILLI METRE]
    Length = 8309.45318603516 [MILLI METRE]
    NetVolume = 1.11347011125793 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 200. [MILLI METRE]
    Length = 5384.35174560547 [MILLI METRE]
    NetVolume = 0.721504653846852 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 200. [MILLI METRE]
    Length = 8284.45410919189 [MILLI METRE]
    NetVolume = 1.110120212135 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 200. [MILLI METRE]
    Length = 5384.34936523438 [MILLI METRE]
    NetVolume = 0.721504334876454 [CUBIC_METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossSideArea = 2.30399985290316 [SQUARE_METRE]
    GrossVolume = 0.506879967638695 [CUBIC_METRE]
    Height = 1800.00007152557 [MILLI METRE]
    Length = 1279.99986741691 [MILLI METRE]
    NetSideArea = 2.30399985290316 [SQUARE_METRE]
    NetVolume = 0.506879967638695 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossSideArea = 0.272000123641046 [SQUARE_METRE]
    GrossVolume = 0.05984002720103 [CUBIC_METRE]
    Height = 800.000011920929 [MILLI METRE]
    Length = 340.00014948491 [MILLI METRE]
    NetSideArea = 0.272000123641046 [SQUARE_METRE]
    NetVolume = 0.05984002720103 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 14.9302502714345 [SQUARE_METRE]
    GrossVolume = 3.28465505971558 [CUBIC_METRE]
    Height = 2550.00019073486 [MILLI METRE]
    Length = 5854.99966850271 [MILLI METRE]
    NetSideArea = 14.9302502714345 [SQUARE_METRE]
    NetVolume = 3.28465505971558 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 9.80048476811418 [SQUARE_METRE]
    GrossVolume = 1.07805332449256 [CUBIC_METRE]
    Height = 2550.00019073486 [MILLI METRE]
    Length = 3843.32707257166 [MILLI METRE]
    NetSideArea = 9.80048476811418 [SQUARE_METRE]
    NetVolume = 1.07805332449256 [CUBIC_METRE]
    Width = 110. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 13.2545433517087 [SQUARE_METRE]
    GrossVolume = 2.91599953737591 [CUBIC_METRE]
    Height = 2550.00019073486 [MILLI METRE]
    Length = 5197.85974913553 [MILLI METRE]
    NetSideArea = 13.2545433517087 [SQUARE_METRE]
    NetVolume = 2.91599953737591 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 20.102491259267 [SQUARE_METRE]
    GrossVolume = 4.42254807703875 [CUBIC_METRE]
    Height = 2550.00019073486 [MILLI METRE]
    Length = 7883.32931593777 [MILLI METRE]
    NetSideArea = 20.102491259267 [SQUARE_METRE]
    NetVolume = 4.42254807703875 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 0.550062860775772 [SQUARE_METRE]
    GrossVolume = 0.12101382937067 [CUBIC_METRE]
    Height = 340.000003576279 [MILLI METRE]
    Length = 1617.83192644104 [MILLI METRE]
    NetSideArea = 0.550062860775772 [SQUARE_METRE]
    NetVolume = 0.12101382937067 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 0.640699043241439 [SQUARE_METRE]
    GrossVolume = 0.140953789513117 [CUBIC_METRE]
    Height = 340.000003576279 [MILLI METRE]
    Length = 1884.40893088902 [MILLI METRE]
    NetSideArea = 0.640699043241439 [SQUARE_METRE]
    NetVolume = 0.140953789513117 [CUBIC_METRE]
    Width = 220. [MILLI METRE]
  Qto_WallBaseQuantities: 13 more contents on 13 objects not shown
  BBIM_Boolean | properties | on 1 object (1 IFCPIPESEGMENT)
    Data = "[180687]" (IFCTEXT)
  Qto_WindowBaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Area = 1.35999992904663 [SQUARE_METRE]
    Height = 600. [MILLI METRE]
    Width = 1799.99987792969 [MILLI METRE]
  Qto_WindowBaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Area = 3.13624976177216 [SQUARE_METRE]
    Height = 1500. [MILLI METRE]
    Width = 1800. [MILLI METRE]
  Qto_WindowBaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Area = 5.55450043792728 [SQUARE_METRE]
    Height = 2090. [MILLI METRE]
    Width = 2400. [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 6.39781702118526 [SQUARE_METRE]
    GrossVolume = 0.543814446800747 [CUBIC_METRE]
    Length = 7526.84945678711 [MILLI METRE]
    NetArea = 6.39781702118526 [SQUARE_METRE]
    NetVolume = 0.543814446800747 [CUBIC_METRE]
    Perimeter = 16753.6911239781 [MILLI METRE]
    Width = 850.000015258789 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 6.39781618453003 [SQUARE_METRE]
    GrossVolume = 0.543814375685053 [CUBIC_METRE]
    Length = 7526.84799194336 [MILLI METRE]
    NetArea = 6.39781618453003 [SQUARE_METRE]
    NetVolume = 0.543814375685053 [CUBIC_METRE]
    Perimeter = 16753.6883163608 [MILLI METRE]
    Width = 850. [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 2.69728989894016 [SQUARE_METRE]
    GrossVolume = 0.229269641409914 [CUBIC_METRE]
    Length = 2314.77584838868 [MILLI METRE]
    NetArea = 2.69728989894016 [SQUARE_METRE]
    NetVolume = 0.229269641409914 [CUBIC_METRE]
    Perimeter = 6569.39808507487 [MILLI METRE]
    Width = 2323.15783691406 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 46.5459137650408 [SQUARE_METRE]
    GrossVolume = 3.95640267002847 [CUBIC_METRE]
    Length = 7674.32836914063 [MILLI METRE]
    NetArea = 46.5459137650408 [SQUARE_METRE]
    NetVolume = 3.95640267002847 [CUBIC_METRE]
    Perimeter = 27476.6719853264 [MILLI METRE]
    Width = 6074.99884033203 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 13.078429955983 [SQUARE_METRE]
    GrossVolume = 1.11166654625856 [CUBIC_METRE]
    Length = 3448.66381835938 [MILLI METRE]
    NetArea = 13.078429955983 [SQUARE_METRE]
    NetVolume = 1.11166654625856 [CUBIC_METRE]
    Perimeter = 14481.963684082 [MILLI METRE]
    Width = 3792.31802368164 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 6.62336210619151 [SQUARE_METRE]
    GrossVolume = 0.562985779026279 [CUBIC_METRE]
    Length = 7792.19554138184 [MILLI METRE]
    NetArea = 6.62336210619151 [SQUARE_METRE]
    NetVolume = 0.562985779026279 [CUBIC_METRE]
    Perimeter = 17284.3835449375 [MILLI METRE]
    Width = 849.999923706055 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 6.61439692110964 [SQUARE_METRE]
    GrossVolume = 0.562223738294319 [CUBIC_METRE]
    Length = 7781.64819335938 [MILLI METRE]
    NetArea = 6.61439692110964 [SQUARE_METRE]
    NetVolume = 0.562223738294319 [CUBIC_METRE]
    Perimeter = 17263.2888641514 [MILLI METRE]
    Width = 849.999931335449 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 2 objects (2 IFCOPENINGELEMENT)
    Area = 2.5644 [SQUARE_METRE]
    Depth = 2137. [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Volume = 2.43617514792481 [CUBIC_METRE]
    Width = 949.998107910156 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 2.70000040283204 [SQUARE_METRE]
    Depth = 1500.00012207031 [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Volume = 3.24000048339845 [CUBIC_METRE]
    Width = 1800.00012207031 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 5.01600058593749 [SQUARE_METRE]
    Depth = 2090.00024414062 [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Volume = 6.01920070312498 [CUBIC_METRE]
    Width = 2400. [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 1.06499996376042 [SQUARE_METRE]
    Depth = 599.999984741211 [MILLI METRE]
    Height = 500.000473022461 [MILLI METRE]
    Volume = 0.532499957504274 [CUBIC_METRE]
    Width = 1774.99998474121 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 2.00425840802555 [SQUARE_METRE]
    Depth = 2109.74681091309 [MILLI METRE]
    Height = 949.999496459961 [MILLI METRE]
    Volume = 1.00212915813889 [CUBIC_METRE]
    Width = 500.000274658203 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 2.61435078916718 [SQUARE_METRE]
    Depth = 2100.00024414062 [MILLI METRE]
    Height = 499.999816894531 [MILLI METRE]
    Volume = 1.30717491588166 [CUBIC_METRE]
    Width = 1244.92880249023 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 1.94522699616661 [SQUARE_METRE]
    Depth = 2100.00024414062 [MILLI METRE]
    Height = 926.298461914062 [MILLI METRE]
    Volume = 0.97261326062884 [CUBIC_METRE]
    Width = 499.999877929688 [MILLI METRE]
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCFOOTING)
    ConstructionToleranceClass = "10mm" (IFCLABEL)
    StrengthClass = "20Mpa" (IFCLABEL)
  EPset_Status | properties | on 1 object (1 IFCWALL)
    Status in {"NEW"} (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1:50" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/50" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1:20" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/20" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  Pset_WallCommon | properties | on 2 type objects
    AcousticRating (no value)
    Combustible (no value)
    Compartmentation (no value)
    ExtendToStructure (no value)
    FireRating (no value)
    IsExternal (no value)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference (no value)
    SurfaceSpreadOfFlame (no value)
    ThermalTransmittance (no value)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2100.0001430511475, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 115.00000208616257, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 110.00000685453415, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 600.0000238418579, "overall_width": 1200.0000476837158, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 600.0000238418579}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 2090.0001525878906, "overall_width": 2400.0000953674316, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 1200.0000476837158}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_VERTICAL", "overall_height": 600.0000238418579, "overall_width": 1800.0000715255737, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 400.0000059604645, "second_mullion_offset": 1400.0000953674316}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_LEFT", "overall_height": 1500.0001192092896, "overall_width": 1800.0000715255737, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 800.000011920929, "transom_thickness": 50.00000074505806, "first_transom_offset": 449.99998807907104}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)