IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "Martl_haus.ifc"
Time stamp: "2025-12-02T20:13:06+01:00"
Preprocessor: "IfcOpenShell 0.8.4-alpha251117"
Originating system: "Bonsai 0.8.4-alpha251117-487a4f3"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 17 elements
          8 x IFCWALL | type IFCWALLTYPE "Innenwand 16cm" | names: "Wall" | material: layers "Innenwand 16cm" ("Innenputz" 20.0000019073486, "Ziegel" 120.000007629395, "Innenputz" 20.0000019073486) | property sets: EPset_Parametric
          8 x IFCWALL | type IFCWALLTYPE "AussenWand 50cm" | names: "Wall" | material: layers "Wand Aussen" ("Innenputz" 20.0000019073486, "Ziegel" 250., "Wärmedämmung" 200., "Aussenputz" 30.0000019073486) | property sets: EPset_Parametric
          1 x IFCSLAB | type IFCSLABTYPE "FB Aufbau" | names: "Slab" | material: layers "Boden" ("Beton" 200.) | property sets: EPset_Parametric

Types
  IFCWALLTYPE "Innenwand 16cm" | STANDARD | 8 occurrences | material: layers "Innenwand 16cm" ("Innenputz" 20.0000019073486, "Ziegel" 120.000007629395, "Innenputz" 20.0000019073486) | property sets: EPset_Parametric
  IFCWALLTYPE "AussenWand 50cm" | SOLIDWALL | 8 occurrences | material: layers "Wand Aussen" ("Innenputz" 20.0000019073486, "Ziegel" 250., "Wärmedämmung" 200., "Aussenputz" 30.0000019073486) | property sets: EPset_Parametric
  IFCSLABTYPE "FB Aufbau" | FLOOR | 1 occurrence | material: layers "Boden" ("Beton" 200.) | property sets: EPset_Parametric

Property sets
  EPset_Parametric | properties | on 16 objects (16 IFCWALL)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 1 object (1 IFCSLAB)
    Engine = "Bonsai.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS3" (IFCLABEL)