IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "bonsai-wall-test.ifc"
Time stamp: "2026-03-19T18:59:24+01:00"
Preprocessor: "IfcOpenShell 0.8.4"
Originating system: "Bonsai 0.8.4"
Authorization: "Nobody"

Units
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 3 elements
          3 x IFCWALL | type IFCWALLTYPE "Brick wall" | names: "Wall" | material: layers "Brick Wall Layer Set" ("Stucco" 0.0199999995529652, "Brick" 0.300000011920929, "Insulation" 0.25, "Stucco" 0.0199999995529652) | property sets: EPset_Parametric

Types
  IFCWALLTYPE "Brick wall" | SOLIDWALL | 3 occurrences | material: layers "Brick Wall Layer Set" ("Stucco" 0.0199999995529652, "Brick" 0.300000011920929, "Insulation" 0.25, "Stucco" 0.0199999995529652) | property sets: EPset_Parametric

Property sets
  EPset_Parametric | properties | on 3 objects (3 IFCWALL)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS2" (IFCLABEL)