IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement [Architecture]"
File name: "0001"
Time stamp: "2021-01-28T16:57:10"
Author: "Hans Hendriks"
Author: "hhs@deBIMspecialist.nl"
Organization: "deBIMspecialist"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190412_1200(x64) - Exporter 20.2.1.0 - Alternate UI 20.2.1.0"
Authorization: "NBvT"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "Hans" "Hendriks" (telecom address: e-mail "hhs@deBIMspecialist.nl") of Organization "deBIMspecialist" description "deBIMspecialist advies"
  Owner history of Person "Hans" "Hendriks" (telecom address: e-mail "hhs@deBIMspecialist.nl") of Organization "deBIMspecialist" description "deBIMspecialist advies" | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1611849409 (2021-01-28T15:56:49Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Voorbeeldkozijn" | phase "Versie 1"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING "Voorbeeld Gebouw Kozijn" | long name "Voorbeeld Gebouw Kozijn" | postal address: "Nijverdal", "Netherlands" ("Voorbeeld kozijn")
      IFCBUILDINGSTOREY "00 begane grond" | long name "00 begane grond" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCELEMENTASSEMBLY | object type "Doors Assembly:Merk A" | USERDEFINED | names: "Doors Assembly:Merk A:410652" | parts: 6 IFCMEMBER, 2 IFCWINDOW, 1 IFCDOOR, 1 IFCFLOWTERMINAL, 1 IFCPLATE | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, CPset_31

Property sets
  Pset_ProductRequirements | properties | on 10 objects (6 IFCMEMBER, 2 IFCWINDOW, 1 IFCFLOWTERMINAL, 1 IFCPLATE)
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Category = "Assemblies" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "00 begane grond" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 7 objects (6 IFCMEMBER, 1 IFCDOOR)
    FireRating = "30" (IFCLABEL)
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Merk A" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (6 IFCMEMBER, 2 IFCWINDOW, 1 IFCDOOR, 1 IFCELEMENTASSEMBLY)
    Reference = "Merk A" (IFCIDENTIFIER)
  CPset_31 | properties | on 2 objects (2 IFCMEMBER)
    Kleurbinnenzijde = "RAL9001" (IFCTEXT)
    Kleurbuitenzijde = "RAL9012" (IFCTEXT)
    Onderdeel = "Stijl" (IFCTEXT)
  CPset_31 | properties | on 1 object (1 IFCMEMBER)
    Kleurbinnenzijde = "RAL9001" (IFCTEXT)
    Kleurbuitenzijde = "RAL9012" (IFCTEXT)
    Onderdeel = "Tussenstijl" (IFCTEXT)
  CPset_31 | properties | on 1 object (1 IFCMEMBER)
    Kleurbinnenzijde = "RAL9001" (IFCTEXT)
    Kleurbuitenzijde = "RAL9012" (IFCTEXT)
    Onderdeel = "Bovendorpel" (IFCTEXT)
  CPset_31 | properties | on 1 object (1 IFCMEMBER)
    Onderdeel = "Onderdorpelsysteem" (IFCTEXT)
  CPset_31 | properties | on 1 object (1 IFCMEMBER)
    Kleurbinnenzijde = "RAL9001" (IFCTEXT)
    Kleurbuitenzijde = "RAL9012" (IFCTEXT)
    Onderdeel = "Tussendorpel" (IFCTEXT)
  CPset_31 | properties | on 1 object (1 IFCDOOR)
    Draairichting = "DIN Links" (IFCTEXT)
    Kleurbinnenzijde = "RAL9001" (IFCTEXT)
    Kleurbuitenzijde = "RAL9012" (IFCTEXT)
    Onderdeel = "Deur met glas" (IFCTEXT)
  CPset_31 | properties | on 1 object (1 IFCWINDOW)
    Draairichting = "Draai-Rechts Kiep" (IFCTEXT)
    Kleurbinnenzijde = "RAL9001" (IFCTEXT)
    Kleurbuitenzijde = "RAL9012" (IFCTEXT)
    Onderdeel = "Raam" (IFCTEXT)
  CPset_31 | properties | on 1 object (1 IFCPLATE)
    Kleurbinnenzijde = "RAL9001" (IFCTEXT)
    Kleurbuitenzijde = "RAL9012" (IFCTEXT)
    Onderdeel = "Paneel" (IFCTEXT)
  CPset_31: 3 more contents on 3 objects not shown
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "30" (IFCLABEL)
    FireExit = TRUE (IFCBOOLEAN)
    FireRating = "30" (IFCLABEL)
    GlazingAreaFraction = 0.41 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Merk A" (IFCIDENTIFIER)
    SecurityRating = "WK1" (IFCLABEL)
    SelfClosing = TRUE (IFCBOOLEAN)
    SmokeStop = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 1.35 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCWINDOW)
    Manufacturer = "n.t.b." (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "30" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Merk A" (IFCIDENTIFIER)
    SecurityRating = "WK1" (IFCLABEL)
    SmokeStop = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 1.45 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "30" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Merk A" (IFCIDENTIFIER)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_PlateCommon | properties | on 1 object (1 IFCPLATE)
    AcousticRating = "30" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Merk A" (IFCIDENTIFIER)
    ThermalTransmittance = 1.3 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "Merk A" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "00 begane grond" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)