IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
File name: "Teste2-C.ifc"
Time stamp: "2025-02-06T11:22:02"
Author: "guiol"
Organization: "None"
Preprocessor: "26.1.0"
Originating system: "SAP2000"
Authorization: "None"
Application: "SAP2000" version "26.1.0" identifier "SAP2000" by Organization "Computers & Structures, Inc." (roles: MANUFACTURER)

People and organizations
  Person "Nameless" id "guiol" of Organization "None" (roles: STRUCTURALENGINEER)
  Owner history of Person "Nameless" id "guiol" of Organization "None" (roles: STRUCTURALENGINEER) | application "SAP2000" version "26.1.0" identifier "SAP2000" by Organization "Computers & Structures, Inc." (roles: MANUFACTURER) | change NOCHANGE | created 1738840922 (2025-02-06T11:22:02Z) | last modified 1738840922 (2025-02-06T11:22:02Z)
  Owner history of Person "Nameless" id "guiol" of Organization "None" (roles: STRUCTURALENGINEER) | application "SAP2000" version "26.1.0" identifier "SAP2000" by Organization "Computers & Structures, Inc." (roles: MANUFACTURER) | change MODIFIED | created 1738840922 (2025-02-06T11:22:02Z) | last modified 1738840922 (2025-02-06T11:22:02Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SECTIONMODULUSUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  MASSUNIT: KILOMUG (conversion based)
  MASSDENSITYUNIT: derived
  FORCEUNIT: TON FORCE (conversion based)
  TORQUEUNIT: derived
  PRESSUREUNIT: TONPERSQMETER (conversion based)
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  LINEARMOMENTUNIT: derived
  SHEARMODULUSUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALEXPANSIONCOEFFICIENTUNIT: derived

Spatial structure
IFCPROJECT "2506-SESI-PALCO-AND04-R0.sdb"
  IFCSITE "Site"
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "BASE LEVEL" | elevation 7.8501000E+000
        contains 72 elements
          4 x IFCCOLUMN | names: "1653", "1655", "2036" (+1 more) | material: profiles ("SAE 1020")
          68 x IFCBEAM | names: "1629", "1630", "1631" (+65 more) | material: profiles ("SAE 1020")
      IFCBUILDINGSTOREY "LEVEL 2" | elevation 9.4245000E+000
        contains 60 elements
          60 x IFCBEAM | names: "1493", "1498", "1" (+57 more) | material: profiles ("SAE 1020")
      IFCBUILDINGSTOREY "LEVEL 3" | elevation 9.5470000E+000
        contains 22 elements
          22 x IFCBEAM | names: "13", "18", "19" (+19 more) | material: profiles ("SAE 1020")
      IFCBUILDINGSTOREY "LEVEL 4" | elevation 9.6640000E+000
        contains 58 elements
          58 x IFCBEAM | names: "25", "30", "31" (+55 more) | material: profiles ("SAE 1020")
      IFCBUILDINGSTOREY "LEVEL 5" | elevation 9.8069000E+000
        contains 40 elements
          40 x IFCBEAM | names: "37", "42", "43" (+37 more) | material: profiles ("SAE 1020")
      IFCBUILDINGSTOREY "TOP LEVEL" | elevation 9.9498000E+000
        contains 68 elements
          68 x IFCBEAM | names: "60", "65", "180" (+65 more) | material: profiles ("SAE 1020")