IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "3.ifc"
Time stamp: "2024-02-23T16:52:53+01:00"
Preprocessor: "IfcOpenShell v0.7.0-6c9e130ca"
Originating system: "BlenderBIM 0.0.240218-c1cd228"
Authorization: "Nobody"

Units
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 4 elements
          1 x IFCWALL | type IFCWALLTYPE "TYPEX" | names: "Wall" | material: layers ("Green" 0.1) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "Cube-Green" | names: "Window-Green"
          1 x IFCWINDOW | type IFCWINDOWTYPE "Cube-Blue" | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "Param" | names: "Window" | material: constituents ("Lining": "Green", "Framing": "Blue", "Glazing": "Blue")

Types
  IFCWALLTYPE "TYPEX" | SOLIDWALL | 1 occurrence | material: layers ("Green" 0.1) | property sets: EPset_Parametric
  IFCWINDOWTYPE "Cube-Green" | 1 occurrence
  IFCWINDOWTYPE "Cube-Blue" | 1 occurrence
  IFCWINDOWTYPE "Param" | SINGLE_PANEL | 1 occurrence | material: constituents ("Lining": "Green", "Framing": "Blue", "Glazing": "Blue") | property sets: BBIM_Window

Property sets
  EPset_Parametric | properties | on 1 object (1 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS2" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 0.8999999761581421, "overall_width": 0.6000000238418579, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)