IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "sporenkap.ifc"
Time stamp: "2022-10-22T11:01:39+02:00"
Preprocessor: "IfcOpenShell v0.7.0-fa6bbf2d"
Originating system: "BlenderBIM 0.0.221020"
Authorization: "Nobody"

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  LENGTHUNIT: MILLI METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 14 elements
          10 x IFCBEAM | type IFCBEAMTYPE "ligger_75x175mm" | names: "Beam" | material: profiles ("vuren") | property sets: EPset_Parametric
          4 x IFCCOVERING | type IFCCOVERINGTYPE "underlayment_2440x1220x22mm" | names: "Covering" | material: profiles ("underlayment") | property sets: EPset_Parametric

Types
  IFCBEAMTYPE "ligger_75x175mm" | BEAM | 10 occurrences | material: profiles ("vuren")
  IFCCOVERINGTYPE "underlayment_2440x1220x22mm" | CLADDING | 4 occurrences | material: profiles ("underlayment")

Property sets
  EPset_Parametric | properties | on 14 objects (10 IFCBEAM, 4 IFCCOVERING)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)