IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "completo2.ifc"
Time stamp: "2026-02-05T18:06:13-03:00"
Author: "Eng. Cleber Feitosa"
Author: "cleber@feitosaengenharia.com"
Organization: "Feitosa Engenharia LTDA"
Preprocessor: "IfcOpenShell 0.8.4"
Originating system: "Bonsai 0.8.4"
Authorization: "Nobody"

Units
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  CURRENCY: BRL
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 921 elements
          15 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Interruptor Simples com Tomada" | names: "JunctionBox"
          95 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "Caixa Ortogonal" | names: "LightFixture"
          131 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite leve 1.1 2"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
          168 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite leve 3/4"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
          123 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite leve 1"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
          47 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Caixa de passagem espelho cego" | names: "JunctionBox" | property sets: Pset_ElectricalDeviceCommon
          25 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Reucao de eletrocalha" | names: "CableCarrierFitting"
          127 x IFCOUTLET | type IFCOUTLETTYPE "Tomada Simples" | names: "OutletAlta.035", "OutletMedia.037", "Outlet" (+101 more)
          15 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Interruptor Paralelo com Tomada" | names: "JunctionBox"
          10 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Derivação de eletrocalha" | names: "CableCarrierFitting"
          13 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Curva 90 3/4"" | names: "CableCarrierFitting"
          12 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Caixa de passagem subterrânea" | names: "JunctionBox"
          23 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite rigido subterraneo 3/4"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
          13 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite rigido subterraneo 3"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
          42 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Eletrocalha 75x150" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
          10 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "Caixa Ortogonal Subterranea" | names: "LightFixture"
          1 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "Interruptor Duplo" | names: "SwitchingDevice"
          10 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite aço 3/4"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
          2 x IFCOUTLET | type IFCOUTLETTYPE "Tomada Dupla" | names: "Outlet"
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "QDGB" | names: "ElectricDistributionBoard"
          10 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Caixa Arandela" | names: "JunctionBox"
          5 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite rigido subterraneo 1.1 2"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Qto_CableCarrierSegmentBaseQuantities, Condutores
          4 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Curva 90 3"" | names: "CableCarrierFitting"
          2 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite leve 2"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "QD3" | names: "ElectricDistributionBoard"
          2 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "Cobre Nu 50mm" | names: "CableSegment" | material: "Cobre Nu" | property sets: EPset_Parametric, Qto_CableSegmentBaseQuantities
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "QD5" | names: "ElectricDistributionBoard"
          2 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Caixa de passagem motor" | names: "JunctionBox"
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "QD2" | names: "ElectricDistributionBoard"
          2 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "Interruptor Paralelo" | names: "SwitchingDevice"
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "QD6" | names: "ElectricDistributionBoard"
          2 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Caixa Projetor" | names: "JunctionBox"
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "QD4" | names: "ElectricDistributionBoard"
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "QM1" | names: "ElectricDistributionBoard"
          1 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Interruptor Duplo com Tomada" | names: "JunctionBox"
          1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "QD1" | names: "ElectricDistributionBoard"
          1 x IFCSWITCHINGDEVICE | type IFCSWITCHINGDEVICETYPE "Interruptor Simples" | names: "SwitchingDevice"
        IFCSPACE "SPDA"
          contains 120 elements
            64 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "Cobre Nu 35mm" | names: "CableSegment" | material: "Cobre Nu" | property sets: EPset_Parametric, Pset_CableSegmentTypeCommon, Qto_CableSegmentBaseQuantities
            20 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "Cobre Nu 50mm" | names: "CableSegment" | material: "Cobre Nu" | property sets: EPset_Parametric, Pset_CableSegmentTypeCommon, Qto_CableSegmentBaseQuantities
            11 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Caixa de vista de aterramento com haste" | names: "JunctionBox"
            1 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "Mastro 3 x 2"" | names: "CableSegment" | property sets: Qto_CableSegmentBaseQuantities
            12 x IFCCABLESEGMENT | type IFCCABLESEGMENTTYPE "Aco galvanizado 10mm" | names: "CableSegment" | material: "Aco Galvanizado" | property sets: Qto_CableSegmentBaseQuantities
            7 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Abracadeira guia reforcada 2"" | names: "CableCarrierFitting"
            1 x IFCMEMBER | type IFCMEMBERTYPE "Franklin" | names: "Member" | property sets: Qto_MemberBaseQuantities
            1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "BEP" | names: "ElectricDistributionBoard"
            2 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite rigido subterraneo 1.1 2"" | names: "CableCarrierSegment" | material: "Cobre Nu" | property sets: EPset_Parametric, Qto_CableCarrierSegmentBaseQuantities
            1 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite leve 2"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Qto_CableCarrierSegmentBaseQuantities
        IFCSPACE "Dados"
          contains 136 elements
            21 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Derivacao horizontal de eletrocalha para eletroduto 1"" | names: "CableCarrierFitting"
            8 x IFCOUTLET | type IFCOUTLETTYPE "Saida TV" | names: "Outlet"
            49 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite leve 3/4"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Qto_CableCarrierSegmentBaseQuantities, Condutores
            18 x IFCOUTLET | type IFCOUTLETTYPE "Saida RJ45" | names: "Outlet"
            13 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Eletrocalha 100x100" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Condutores, Qto_CableCarrierSegmentBaseQuantities
            9 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite leve 1"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Qto_CableCarrierSegmentBaseQuantities, Condutores
            5 x IFCCABLECARRIERSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Conduite rigido aço galvanizado 1"" | names: "CableCarrierSegment" | material: profiles ("Unknown") | property sets: EPset_Parametric, Qto_CableCarrierSegmentBaseQuantities
            4 x IFCJUNCTIONBOX | type IFCJUNCTIONBOXTYPE "Caixa de passagem subterrânea para dados" | names: "JunctionBox"
            5 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Derivacao horizontal de eletrocalha para eletroduto 3/4"" | names: "CableCarrierFitting"
            2 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Curva de eletrocalha 100x100" | names: "CableCarrierFitting"
            1 x IFCCABLECARRIERFITTING | type IFCCABLECARRIERFITTINGTYPE "Curva 90 1"" | names: "CableCarrierFitting"
            1 x IFCELECTRICDISTRIBUTIONBOARD | type IFCELECTRICDISTRIBUTIONBOARDTYPE "Rack 5U 19"" | names: "ElectricDistributionBoard"

Types
  IFCJUNCTIONBOXTYPE "Interruptor Simples com Tomada" | DATA | 15 occurrences
  IFCLIGHTFIXTURETYPE "Caixa Ortogonal" | POINTSOURCE | 95 occurrences
  IFCCABLECARRIERSEGMENTTYPE "Conduite leve 1.1 2"" | CONDUITSEGMENT | 131 occurrences | material: profiles ("Unknown")
  IFCCABLECARRIERSEGMENTTYPE "Conduite leve 3/4"" | CONDUITSEGMENT | 217 occurrences | material: profiles ("Unknown")
  IFCCABLECARRIERSEGMENTTYPE "Conduite leve 1"" | CONDUITSEGMENT | 132 occurrences | material: profiles ("Unknown")
  IFCJUNCTIONBOXTYPE "Caixa de passagem espelho cego" | DATA | 47 occurrences
  IFCCABLECARRIERFITTINGTYPE "Reucao de eletrocalha" | REDUCER | 25 occurrences
  IFCOUTLETTYPE "Tomada Simples" | AUDIOVISUALOUTLET | 127 occurrences
  IFCJUNCTIONBOXTYPE "Interruptor Paralelo com Tomada" | DATA | 15 occurrences
  IFCCABLECARRIERFITTINGTYPE "Derivação de eletrocalha" | CROSS | 10 occurrences
  IFCCABLECARRIERFITTINGTYPE "Curva 90 3/4"" | BEND | 13 occurrences | property sets: BBIM_Fitting
  IFCJUNCTIONBOXTYPE "Caixa de passagem subterrânea" | DATA | 12 occurrences
  IFCCABLECARRIERSEGMENTTYPE "Conduite rigido subterraneo 3/4"" | CONDUITSEGMENT | 23 occurrences | material: profiles ("Unknown")
  IFCCABLECARRIERSEGMENTTYPE "Conduite rigido subterraneo 3"" | CONDUITSEGMENT | 13 occurrences | material: profiles ("Unknown")
  IFCCABLECARRIERSEGMENTTYPE "Eletrocalha 75x150" | CABLETRAYSEGMENT | 42 occurrences | material: profiles ("Unknown")
  IFCLIGHTFIXTURETYPE "Caixa Ortogonal Subterranea" | POINTSOURCE | 10 occurrences
  IFCSWITCHINGDEVICETYPE "Interruptor Duplo" | TOGGLESWITCH | 1 occurrence
  IFCCABLECARRIERSEGMENTTYPE "Conduite aço 3/4"" | CONDUITSEGMENT | 10 occurrences | material: profiles ("Unknown")
  IFCOUTLETTYPE "Tomada Dupla" | POWEROUTLET | 2 occurrences
  IFCELECTRICDISTRIBUTIONBOARDTYPE "QDGB" | DISTRIBUTIONBOARD | 1 occurrence
  IFCJUNCTIONBOXTYPE "Caixa Arandela" | DATA | 10 occurrences
  IFCCABLECARRIERSEGMENTTYPE "Conduite rigido subterraneo 1.1 2"" | CONDUITSEGMENT | 7 occurrences | material: profiles ("Unknown")
  IFCCABLECARRIERFITTINGTYPE "Curva 90 3"" | BEND | 4 occurrences | property sets: BBIM_Fitting
  IFCCABLECARRIERSEGMENTTYPE "Conduite leve 2"" | CONDUITSEGMENT | 3 occurrences | material: profiles ("Unknown")
  IFCELECTRICDISTRIBUTIONBOARDTYPE "QD3" | DISTRIBUTIONBOARD | 1 occurrence
  IFCCABLESEGMENTTYPE "Cobre Nu 50mm" | CONDUCTORSEGMENT | 22 occurrences | material: profiles ("Unknown")
  IFCELECTRICDISTRIBUTIONBOARDTYPE "QD5" | DISTRIBUTIONBOARD | 1 occurrence
  IFCJUNCTIONBOXTYPE "Caixa de passagem motor" | DATA | 2 occurrences
  IFCELECTRICDISTRIBUTIONBOARDTYPE "QD2" | DISTRIBUTIONBOARD | 1 occurrence
  IFCSWITCHINGDEVICETYPE "Interruptor Paralelo" | TOGGLESWITCH | 2 occurrences
  IFCELECTRICDISTRIBUTIONBOARDTYPE "QD6" | DISTRIBUTIONBOARD | 1 occurrence
  IFCJUNCTIONBOXTYPE "Caixa Projetor" | DATA | 2 occurrences
  IFCELECTRICDISTRIBUTIONBOARDTYPE "QD4" | DISTRIBUTIONBOARD | 1 occurrence
  IFCELECTRICDISTRIBUTIONBOARDTYPE "QM1" | DISTRIBUTIONBOARD | 1 occurrence
  IFCJUNCTIONBOXTYPE "Interruptor Duplo com Tomada" | DATA | 1 occurrence
  IFCELECTRICDISTRIBUTIONBOARDTYPE "QD1" | DISTRIBUTIONBOARD | 1 occurrence
  IFCSWITCHINGDEVICETYPE "Interruptor Simples" | TOGGLESWITCH | 1 occurrence
  IFCCABLESEGMENTTYPE "Cobre Nu 35mm" | CONDUCTORSEGMENT | 64 occurrences | material: profiles ("Unknown")
  IFCJUNCTIONBOXTYPE "Caixa de vista de aterramento com haste" | DATA | 11 occurrences
  IFCCABLESEGMENTTYPE "Mastro 3 x 2"" | CONDUCTORSEGMENT | 1 occurrence
  IFCCABLESEGMENTTYPE "Aco galvanizado 10mm" | CONDUCTORSEGMENT | 12 occurrences
  IFCCABLECARRIERFITTINGTYPE "Abracadeira guia reforcada 2"" | element type "Holder" | USERDEFINED | 7 occurrences
  IFCMEMBERTYPE "Franklin" | element type "Franklin" | USERDEFINED | 1 occurrence
  IFCELECTRICDISTRIBUTIONBOARDTYPE "BEP" | element type "BEP" | USERDEFINED | 1 occurrence
  IFCCABLECARRIERFITTINGTYPE "Derivacao horizontal de eletrocalha para eletroduto 1"" | REDUCER | 21 occurrences
  IFCOUTLETTYPE "Saida TV" | DATAOUTLET | 8 occurrences
  IFCOUTLETTYPE "Saida RJ45" | DATAOUTLET | 18 occurrences
  IFCCABLECARRIERSEGMENTTYPE "Eletrocalha 100x100" | CABLETRAYSEGMENT | 13 occurrences | material: profiles ("Unknown")
  IFCCABLECARRIERSEGMENTTYPE "Conduite rigido aço galvanizado 1"" | CONDUITSEGMENT | 5 occurrences | material: profiles ("Unknown")
  IFCJUNCTIONBOXTYPE "Caixa de passagem subterrânea para dados" | DATA | 4 occurrences
  IFCCABLECARRIERFITTINGTYPE "Derivacao horizontal de eletrocalha para eletroduto 3/4"" | REDUCER | 5 occurrences
  IFCCABLECARRIERFITTINGTYPE "Curva de eletrocalha 100x100" | BEND | 2 occurrences
  IFCCABLECARRIERFITTINGTYPE "Curva 90 1"" | BEND | 1 occurrence | property sets: BBIM_Fitting
  IFCELECTRICDISTRIBUTIONBOARDTYPE "Rack 5U 19"" | element type "DATA" | USERDEFINED | 1 occurrence

Property sets
  EPset_Parametric | properties | on 682 objects (596 IFCCABLECARRIERSEGMENT, 86 IFCCABLESEGMENT)
    Engine = "Bonsai.DumbProfile" (IFCLABEL)
  Condutores | properties | on 37 objects (37 IFCCABLECARRIERSEGMENT)
    StringProperty = "1 x CSU-4P" (IFCLABEL)
  Condutores | properties | on 19 objects (19 IFCCABLECARRIERSEGMENT)
    StringProperty = "3 QD3 - neutro, retorno ac - 2,5" (IFCLABEL)
  Condutores | properties | on 16 objects (16 IFCCABLECARRIERSEGMENT)
    StringProperty = "1 x COAXIAL" (IFCLABEL)
  Condutores | properties | on 15 objects (15 IFCCABLECARRIERSEGMENT)
    StringProperty = "3 QD1 - neutro, fase, terra - 2,5" (IFCLABEL)
  Condutores | properties | on 14 objects (14 IFCCABLECARRIERSEGMENT)
    StringProperty = "6 QD1 - neutro, fase, terra - 2,5" (IFCLABEL)
  Condutores | properties | on 12 objects (12 IFCCABLECARRIERSEGMENT)
    StringProperty = "5 QD3 - neutro, fase, terra - 2,5" (IFCLABEL)
  Condutores | properties | on 9 objects (9 IFCCABLECARRIERSEGMENT)
    StringProperty = "5 QD2 - neutro, fase, terra - 2,5" (IFCLABEL)
  Condutores | properties | on 8 objects (8 IFCCABLECARRIERSEGMENT)
    StringProperty = "8 QD3 - neutro, fase, terra - 2,5" (IFCLABEL)
  Condutores: 267 more contents on 456 objects not shown
  Qto_CableCarrierSegmentBaseQuantities | quantities | on 10 objects (10 IFCCABLECARRIERSEGMENT)
    Length = 2.07020286413715 [METRE]
  Qto_CableCarrierSegmentBaseQuantities | quantities | on 9 objects (9 IFCCABLECARRIERSEGMENT)
    Length = 2.07115265695208 [METRE]
  Qto_CableCarrierSegmentBaseQuantities | quantities | on 9 objects (9 IFCCABLECARRIERSEGMENT)
    Length = 0.971188306923395 [METRE]
  Qto_CableCarrierSegmentBaseQuantities | quantities | on 9 objects (9 IFCCABLECARRIERSEGMENT)
    Length = 0.971152771363023 [METRE]
  Qto_CableCarrierSegmentBaseQuantities | quantities | on 6 objects (6 IFCCABLECARRIERSEGMENT)
    Length = 0.970238219288186 [METRE]
  Qto_CableCarrierSegmentBaseQuantities | quantities | on 6 objects (6 IFCCABLECARRIERSEGMENT)
    Length = 0.970202679646632 [METRE]
  Qto_CableCarrierSegmentBaseQuantities | quantities | on 6 objects (6 IFCCABLECARRIERSEGMENT)
    Length = 2.62572886929168 [METRE]
  Qto_CableCarrierSegmentBaseQuantities | quantities | on 5 objects (5 IFCCABLECARRIERSEGMENT)
    Length = 2.03813261262887 [METRE]
  Qto_CableCarrierSegmentBaseQuantities: 507 more contents on 534 objects not shown
  Pset_CableSegmentTypeCommon | properties | on 54 objects (54 IFCCABLESEGMENT)
    Reference = "Teto" (IFCIDENTIFIER)
  Pset_CableSegmentTypeCommon | properties | on 27 objects (27 IFCCABLESEGMENT)
    Reference = "Solo" (IFCIDENTIFIER)
  Qto_CableSegmentBaseQuantities | quantities | on 13 objects (13 IFCCABLESEGMENT)
  Qto_CableSegmentBaseQuantities | quantities | on 4 objects (4 IFCCABLESEGMENT)
    Length = 1. [METRE]
  Qto_CableSegmentBaseQuantities | quantities | on 4 objects (4 IFCCABLESEGMENT)
    Length = 2.25 [METRE]
  Qto_CableSegmentBaseQuantities | quantities | on 3 objects (3 IFCCABLESEGMENT)
    Length = 1.40000009877341 [METRE]
  Qto_CableSegmentBaseQuantities | quantities | on 3 objects (3 IFCCABLESEGMENT)
    Length = 0.349999907612788 [METRE]
  Qto_CableSegmentBaseQuantities | quantities | on 3 objects (3 IFCCABLESEGMENT)
    Length = 0.950000770468148 [METRE]
  Qto_CableSegmentBaseQuantities | quantities | on 3 objects (3 IFCCABLESEGMENT)
    Length = 0.349998470711773 [METRE]
  Qto_CableSegmentBaseQuantities | quantities | on 2 objects (2 IFCCABLESEGMENT)
    Length = 1.5 [METRE]
  Qto_CableSegmentBaseQuantities: 62 more contents on 64 objects not shown
  Qto_MemberBaseQuantities | quantities | on 1 object (1 IFCMEMBER)
    GrossSurfaceArea = 0.210667329129574 [SQUARE_METRE]
    GrossVolume = 0.00280930090671649 [CUBIC_METRE]
    Length = 0.317450016736984 [METRE]
    NetSurfaceArea = 0.210667329129574 [SQUARE_METRE]
    NetVolume = 0.00280930090671649 [CUBIC_METRE]
    OuterSurfaceArea = 0.0470482258797469 [SQUARE_METRE]
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCJUNCTIONBOX)
  Qto_TaskBaseQuantities | quantities | on 4 objects (4 IFCTASK)
    StandardWork = 1.
  Qto_TaskBaseQuantities | quantities | on 1 object (1 IFCTASK)
    StandardWork = 2.
  Qto_TaskBaseQuantities | quantities | on 1 object (1 IFCTASK)
    StandardWork = 5.
  Qto_TaskBaseQuantities | quantities | on 1 object (1 IFCTASK)
    StandardWork = 7.
  Qto_TaskBaseQuantities | quantities | on 1 object (1 IFCTASK)
    StandardWork = 17.
  BBIM_Fitting | properties | on 3 type objects
    Data = "{"start_length": 0.10000000149011612, "end_length": 0.10000000149011612, "radius": 0.20000000298023224, "angle": 89.99999749552184, "lateral_axis": 0, "lateral_sign": 1.0, "z_axis_sign": -1, "main_profile_dimension": 0.0199999995529652}" (IFCTEXT)