IFC building model
Schema: "IFC4"
Description: "12d Model generated IFC file."
File name: "IFC22062021.ifc"
Application: "12d Model" version "14.0C2j" identifier "12d Model" by Organization "12d Solutions Pty Ltd." description "12d Solutions Pty Ltd."

People and organizations
  Person "Shilpa" of Organization "12d Solutions Pty Ltd." description "12d Solutions Pty Ltd."
  Owner history of Person "Shilpa" of Organization "12d Solutions Pty Ltd." description "12d Solutions Pty Ltd." | application "12d Model" version "14.0C2j" identifier "12d Model" by Organization "12d Solutions Pty Ltd." description "12d Solutions Pty Ltd." | change ADDED | created 1624327097 (2021-06-22T01:58:17Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "PUP Delivery" | description "No description set"
  IFCSITE "Default Site" | description "Description of Default Site"
    IFCBUILDING "PUP Water Link" | description "Description of PUP Water Link"
      contains 104 elements
        104 x IFCELEMENTASSEMBLY | object type "Super" | names: "PUP Water Lnk" | parts: 448 IFCFLOWSEGMENT | property sets: 12d Model
    IFCBUILDING "DR GEN" | description "Description of DR GEN"
      contains 2 elements
        2 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "DR IL", "DR NDF" | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "DR MH" | description "Description of DR MH"
      contains 64 elements
        58 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "DR MH" | descriptions: "test" | property sets: 12d Model
        6 x IFCBUILDINGELEMENTPROXY | object type "3D Tri-mesh" | USERDEFINED | names: "DR MH MOD" | descriptions: "12d Trimesh" | property sets: 12d Model
    IFCBUILDING "DR PIPE" | description "Description of DR PIPE"
      contains 31 elements
        30 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "DR DPO", "DR P" | descriptions: "test" | property sets: 12d Model
        1 x IFCBUILDINGELEMENTPROXY | object type "3D Tri-mesh" | USERDEFINED | names: "DR P MOD" | descriptions: "12d Trimesh" | property sets: 12d Model
    IFCBUILDING "DR PIT" | description "Description of DR PIT"
      contains 155 elements
        155 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "DR GT", "DR MHC", "DR MHS" | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "PUP Drge Junction" | description "Description of PUP Drge Junction"
      contains 161 elements
        161 x IFCBUILDINGELEMENTPROXY | object type "3D Tri-mesh" | USERDEFINED | names: "PUP Drge Jnct" | descriptions: "12d Trimesh" | property sets: 12d Model
    IFCBUILDING "PUP Drge Link" | description "Description of PUP Drge Link"
      contains 302 elements
        302 x IFCELEMENTASSEMBLY | object type "Super" | names: "PUP Drge Lnk" | parts: 342 IFCFLOWSEGMENT | property sets: 12d Model
    IFCBUILDING "PUP Drge Link Lateral" | description "Description of PUP Drge Link Lateral"
      contains 28 elements
        28 x IFCELEMENTASSEMBLY | object type "Super" | names: "PUP Drge Lnk" | parts: 30 IFCFLOWSEGMENT | property sets: 12d Model
    IFCBUILDING "PUP Drge Link Mesh" | description "Description of PUP Drge Link Mesh"
      contains 3 elements
        3 x IFCBUILDINGELEMENTPROXY | object type "3D Tri-mesh" | USERDEFINED | names: "PUP Drge Lnk" | descriptions: "12d Trimesh" | property sets: 12d Model
    IFCBUILDING "PUP Sewer Junction" | description "Description of PUP Sewer Junction"
      contains 23 elements
        23 x IFCBUILDINGELEMENTPROXY | object type "3D Tri-mesh" | USERDEFINED | names: "PUP Sewer Jnct" | descriptions: "12d Trimesh" | property sets: 12d Model
    IFCBUILDING "PUP Sewer Link" | description "Description of PUP Sewer Link"
      contains 50 elements
        50 x IFCELEMENTASSEMBLY | object type "Super" | names: "PUP Sewer Lnk" | parts: 59 IFCFLOWSEGMENT | property sets: 12d Model
    IFCBUILDING "PUP Sewer Link Lateral" | description "Description of PUP Sewer Link Lateral"
      contains 29 elements
        29 x IFCELEMENTASSEMBLY | object type "Super" | names: "PUP Sewer Lnk" | parts: 39 IFCFLOWSEGMENT | property sets: 12d Model
    IFCBUILDING "PUP Sewer RM Link" | description "Description of PUP Sewer RM Link"
      contains 3 elements
        3 x IFCELEMENTASSEMBLY | object type "Super" | names: "PUP Sewer RM Lnk" | parts: 45 IFCFLOWSEGMENT | property sets: 12d Model
    IFCBUILDING "PUP Unknown Link" | description "Description of PUP Unknown Link"
      contains 1 element
        1 x IFCELEMENTASSEMBLY | object type "Super" | names: "PUP Unknown Lnk" | parts: 1 IFCFLOWSEGMENT | property sets: 12d Model
    IFCBUILDING "PUP Water Junction" | description "Description of PUP Water Junction"
      contains 153 elements
        153 x IFCBUILDINGELEMENTPROXY | object type "3D Tri-mesh" | USERDEFINED | names: "PUP Water Jnct" | descriptions: "12d Trimesh" | property sets: 12d Model
    IFCBUILDING "SEW GEN" | description "Description of SEW GEN"
      contains 1 element
        1 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "SE NDF" | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "SEW PIPE" | description "Description of SEW PIPE"
      contains 1 element
        1 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "SE P" | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "SEW PIT" | description "Description of SEW PIT"
      contains 32 elements
        32 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "SE MH", "SE IO", "SE MHS" | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "SEW STRUCTURE" | description "Description of SEW STRUCTURE"
      contains 1 element
        1 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "SE STR" | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "US GEN" | description "Description of US GEN"
      contains 15 elements
        15 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "US NDF" | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "US PIT" | description "Description of US PIT"
      contains 317 elements
        317 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "US MHS", "US PITS", "US MH" (+12 more) | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "WS GEN" | description "Description of WS GEN"
      contains 10 elements
        10 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "WS NDF" | descriptions: "test" | property sets: 12d Model
    IFCBUILDING "WS PIPE" | description "Description of WS PIPE"
      contains 7 elements
        3 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "WS P" | descriptions: "test" | property sets: 12d Model
        4 x IFCBUILDINGELEMENTPROXY | object type "3D Tri-mesh" | USERDEFINED | names: "WS P MOD" | descriptions: "12d Trimesh" | property sets: 12d Model
    IFCBUILDING "WS PIT" | description "Description of WS PIT"
      contains 227 elements
        227 x IFCBUILDINGELEMENTPROXY | object type "Super" | USERDEFINED | names: "WS V", "WS MT", "WS FH" (+18 more) | descriptions: "test" | property sets: 12d Model

Property sets
  12d Model | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    IfcGlobalId = "2B5Klb02n0wu8989etEQxY" (IFCLABEL)
    Survey: Depth = 8.1E-1 (IFCREAL); Diameter = 1.E-1 (IFCREAL); Position = "OBVERT" (IFCLABEL); SUI_QL = "B" (IFCLABEL); Material = "STEEL" (IFCLABEL); Depth Class = "ACTUAL" (IFCLABEL); Dia Class = "ACTUAL" (IFCLABEL)
    string_no = "31" (IFCLABEL)
  12d Model | properties | on 1 object (1 IFCFLOWSEGMENT)
    Geometry: Justification = "Obvert" (IFCLABEL); Start x = 51931.177 (IFCREAL); Start y = 158115.545 (IFCREAL); Start z = 3.403 (IFCREAL); End x = 51923.207 (IFCREAL); End y = 158110.611 (IFCREAL); End z = 3.656 (IFCREAL)
    Label: PipeSize = "Ø100" (IFCLABEL)
    PUP: ID = "SBCP-L181120-00011025" (IFCLABEL); Owner = "BCC" (IFCLABEL); Description = "PIPE" (IFCLABEL); Creator = "B+B" (IFCLABEL); Creation Date = "20181126" (IFCLABEL); Creation Source = "SURVEY" (IFCLABEL); AS 4588 Quality = "B" (IFCLABEL); Comment = "nc" (IFCLABEL); Material = "STEEL" (IFCLABEL)
  12d Model | properties | on 1 object (1 IFCFLOWSEGMENT)
    Geometry: Justification = "Obvert" (IFCLABEL); Start x = 51923.207 (IFCREAL); Start y = 158110.611 (IFCREAL); Start z = 3.656 (IFCREAL); End x = 51921.346 (IFCREAL); End y = 158109.538 (IFCREAL); End z = 3.7 (IFCREAL)
    Label: PipeSize = "Ø100" (IFCLABEL)
    PUP: ID = "SBCP-L181120-00011026" (IFCLABEL); Owner = "BCC" (IFCLABEL); Description = "PIPE" (IFCLABEL); Creator = "B+B" (IFCLABEL); Creation Date = "20181126" (IFCLABEL); Creation Source = "SURVEY" (IFCLABEL); AS 4588 Quality = "B" (IFCLABEL); Comment = "nc" (IFCLABEL); Material = "STEEL" (IFCLABEL)
  12d Model | properties | on 1 object (1 IFCFLOWSEGMENT)
    Geometry: Justification = "Obvert" (IFCLABEL); Start x = 51921.346 (IFCREAL); Start y = 158109.538 (IFCREAL); Start z = 3.7 (IFCREAL); End x = 51916.727 (IFCREAL); End y = 158106.739 (IFCREAL); End z = 3.583 (IFCREAL)
    Label: PipeSize = "Ø100" (IFCLABEL)
    PUP: ID = "SBCP-L181120-00011027" (IFCLABEL); Owner = "BCC" (IFCLABEL); Description = "PIPE" (IFCLABEL); Creator = "B+B" (IFCLABEL); Creation Date = "20181126" (IFCLABEL); Creation Source = "SURVEY" (IFCLABEL); AS 4588 Quality = "B" (IFCLABEL); Comment = "nc" (IFCLABEL); Material = "STEEL" (IFCLABEL)
  12d Model | properties | on 1 object (1 IFCFLOWSEGMENT)
    Geometry: Justification = "Obvert" (IFCLABEL); Start x = 51916.727 (IFCREAL); Start y = 158106.739 (IFCREAL); Start z = 3.583 (IFCREAL); End x = 51913.308 (IFCREAL); End y = 158104.683 (IFCREAL); End z = 3.62 (IFCREAL)
    Label: PipeSize = "Ø100" (IFCLABEL)
    PUP: ID = "SBCP-L181120-00011028" (IFCLABEL); Owner = "BCC" (IFCLABEL); Description = "PIPE" (IFCLABEL); Creator = "B+B" (IFCLABEL); Creation Date = "20181126" (IFCLABEL); Creation Source = "SURVEY" (IFCLABEL); AS 4588 Quality = "B" (IFCLABEL); Comment = "nc" (IFCLABEL); Material = "STEEL" (IFCLABEL)
  12d Model | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    IfcGlobalId = "3dNKegJwD5aQmtkLb1qggo" (IFCLABEL)
    Survey: Depth = 6.E-1 (IFCREAL); Diameter = 1.E-1 (IFCREAL); Position = "OBVERT" (IFCLABEL); SUI_QL = "C" (IFCLABEL); Material = "NOT ASCERTAINED" (IFCLABEL); Depth Class = "ASSUMED" (IFCLABEL); Dia Class = "ASSUMED" (IFCLABEL)
    string_no = "50" (IFCLABEL)
  12d Model | properties | on 1 object (1 IFCFLOWSEGMENT)
    Geometry: Justification = "Obvert" (IFCLABEL); Start x = 51811.118 (IFCREAL); Start y = 158274.878 (IFCREAL); Start z = 4.036 (IFCREAL); End x = 51799.833 (IFCREAL); End y = 158293.379 (IFCREAL); End z = 3.823 (IFCREAL)
    Label: PipeSize = "Ø100" (IFCLABEL)
    PUP: ID = "SBCP-L181120-00011116" (IFCLABEL); Owner = "BCC" (IFCLABEL); Description = "PIPE" (IFCLABEL); Creator = "B+B" (IFCLABEL); Creation Date = "20181126" (IFCLABEL); Creation Source = "SURVEY" (IFCLABEL); AS 4588 Quality = "C" (IFCLABEL); Comment = "nc" (IFCLABEL); Material = "NOT ASCERTAINED" (IFCLABEL)
  12d Model | properties | on 1 object (1 IFCFLOWSEGMENT)
    Geometry: Justification = "Obvert" (IFCLABEL); Start x = 51799.833 (IFCREAL); Start y = 158293.379 (IFCREAL); Start z = 3.823 (IFCREAL); End x = 51799.272 (IFCREAL); End y = 158294.271 (IFCREAL); End z = 3.8 (IFCREAL)
    Label: PipeSize = "Ø100" (IFCLABEL)
    PUP: ID = "SBCP-L181120-00011117" (IFCLABEL); Owner = "BCC" (IFCLABEL); Description = "PIPE" (IFCLABEL); Creator = "B+B" (IFCLABEL); Creation Date = "20181126" (IFCLABEL); Creation Source = "SURVEY" (IFCLABEL); AS 4588 Quality = "C" (IFCLABEL); Comment = "nc" (IFCLABEL); Material = "NOT ASCERTAINED" (IFCLABEL)
  12d Model: 2676 more contents on 2676 objects not shown