IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2025-11-06T11:14:31"
Preprocessor: "IfcOpenShell 0.8.0"
Originating system: "IfcOpenShell 0.8.0"

Units
  LENGTHUNIT: foot (conversion based)

Spatial structure
IFCPROJECT "Superelevation Example"
  IFCSITE "Site"
    IFCROAD "Road1"
      IFCROADPART "RoadPart1" | LONGITUDINAL
        contains 1 element
          1 x IFCPAVEMENT | names: "Pavement"
  IFCALIGNMENT "A-Line"

Property sets
  Pset_Stationing | properties | on 3 objects (3 IFCREFERENT)
    Station = 500. (IFCLENGTHMEASURE) [foot (conversion based)]
  Pset_Stationing | properties | on 1 object (1 IFCREFERENT)
    Station = 6262.913775 (IFCLENGTHMEASURE) [foot (conversion based)]
  Pset_Stationing | properties | on 1 object (1 IFCREFERENT)
    Station = 5500. (IFCLENGTHMEASURE) [foot (conversion based)]
  Pset_Stationing | properties | on 1 object (1 IFCREFERENT)
    Station = 2456.785654 (IFCLENGTHMEASURE) [foot (conversion based)]
  Pset_Stationing | properties | on 1 object (1 IFCREFERENT)
    Station = 4376.008321 (IFCLENGTHMEASURE) [foot (conversion based)]
  Pset_Superelevation | properties | on 2 objects (2 IFCREFERENT)
    Side = "BOTH" (IFCLABEL)
    Superelevation = -0.02 (IFCRATIOMEASURE)
    TransitionSuperelevation = "Linear" (IFCLABEL)
  Pset_Superelevation | properties | on 2 objects (2 IFCREFERENT)
    Side = "RIGHT" (IFCLABEL)
    Superelevation = 0.02 (IFCRATIOMEASURE)
    TransitionSuperelevation = "Linear" (IFCLABEL)
  Pset_Superelevation | properties | on 2 objects (2 IFCREFERENT)
    Side = "LEFT" (IFCLABEL)
    Superelevation = -0.06 (IFCRATIOMEASURE)
    TransitionSuperelevation = "Linear" (IFCLABEL)
  Pset_Superelevation | properties | on 2 objects (2 IFCREFERENT)
    Side = "RIGHT" (IFCLABEL)
    Superelevation = 0.06 (IFCRATIOMEASURE)
    TransitionSuperelevation = "Linear" (IFCLABEL)