IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition[DesignTransferView]"
File name: "HFCC_TDRev5.ifc"
Time stamp: "2025-05-27T20:50:51+02:00"
Preprocessor: "IfcOpenShell 0.8.3-alpha250527"
Originating system: "Bonsai 0.8.3-alpha250527-72ef055"
Authorization: "Nobody"
Application: "Bonsai" version "0.7.11-alpha240820-736b50c" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241114-229e2da" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241114-229e2da" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
Application: "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

People and organizations
  118 x Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT)
  123 x Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  3 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.7.11-alpha240820-736b50c" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1724669985 (2024-08-26T10:59:45Z) | last modified 1724669985 (2024-08-26T10:59:45Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.7.11-alpha240820-736b50c" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  3 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change MODIFIED | created 1730547654 (2024-11-02T11:40:54Z) | last modified 1730547955 (2024-11-02T11:45:55Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  2 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change MODIFIED | created 1730547972 (2024-11-02T11:46:12Z) | last modified 1731919258 (2024-11-18T08:40:58Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.1-alpha241114-229e2da" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.1-alpha241031-06a6c2d" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change MODIFIED | created 1730547972 (2024-11-02T11:46:12Z) | last modified 1743623950 (2025-04-02T19:59:10Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.2-alpha250328-f08f9ad" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  3 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.7.11-alpha240820-736b50c" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1724250771 (2024-08-21T14:32:51Z) | last modified 1724250771 (2024-08-21T14:32:51Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.7.11-alpha240820-736b50c" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  3 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.2-alpha250226-2d0bd97" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1740680757 (2025-02-27T18:25:57Z) | last modified 1740680757 (2025-02-27T18:25:57Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.2-alpha250226-2d0bd97" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  3 x Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.2-alpha250223-973c9e2" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1740424389 (2025-02-24T19:13:09Z) | last modified 1740424389 (2025-02-24T19:13:09Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.2-alpha250223-973c9e2" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  Owner history of Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) | application "Bonsai" version "0.8.2-alpha250328-f08f9ad" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1743189645 (2025-03-28T19:20:45Z) | last modified 1743189645 (2025-03-28T19:20:45Z) by Person "Hari" "name test 240517" id "identification test 242517" (roles: SUPPLIER; postal address OFFICE; telecom address OFFICE: e-mail "roel.defloo@gmail.com") of Organization "Orginastion 250517" id "APTR" (roles: ARCHITECT) with "Bonsai" version "0.8.2-alpha250328-f08f9ad" identifier "Bonsai" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "HFCC"
  IFCSITE "My Site"
    IFCBUILDING "Todler_Dorm"
      IFCBUILDINGSTOREY "Foundation"
        contains 84 elements
          10 x IFCREINFORCINGMESH | type IFCREINFORCINGMESHTYPE "WeldMesh Ref395" | names: "ReinforcingMesh" | material: "Hot_rolled"
          7 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "110mm_uPVC_6000_AG" | names: "PipeSegment" | material: "DPM-Green Plastic" | property sets: Qto_PipeSegmentBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "Lintel Single 1.8m" | names: "Beam"
          30 x IFCSLAB | type IFCSLABTYPE "ConcreteApron800wide" | names: "Apron800wide" | material: layers ("25 MPa wooden float" 85.) | property sets: EPset_Parametric, Qto_SlabBaseQuantities
          5 x IFCSLAB | type IFCSLABTYPE "85mm surface bed" | names: "85mm-20MPA reinforced" | material: layers "concrete" ("25 MPa wooden float" 85.) | property sets: Qto_SlabBaseQuantities, EPset_Parametric
          1 x IFCRAMPFLIGHT | type IFCRAMPFLIGHTTYPE "Entrance_ramp1:12" | names: "RampFlight"
          6 x IFCWALL | type IFCWALLTYPE "220mm_Plinth" | STANDARD | names: "Wall", "220mm_Plinth_Wall" | material: layers ("NFX-Clay" 220.000015258789) | property sets: EPset_Parametric, Qto_WallBaseQuantities
          8 x IFCFOOTING | type IFCFOOTINGTYPE "600x230_Foundation" | names: "600x230x20MPa" | material: layers ("Undercoat_PVA" 600.) | property sets: EPset_Parametric, Qto_FootingBaseQuantities
          3 x IFCCOVERING | type IFCCOVERINGTYPE "60mmPaving" | names: "Covering" | material: layers ("Undercoat_PVA" 60.0000038146973) | property sets: EPset_Parametric, Qto_CoveringBaseQuantities
          4 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "110mm_uPVC_UG" | names: "PipeSegment", "110mm_uPVC_UG" | material: profiles ("DPM-Green Plastic") | property sets: EPset_Parametric, Qto_PipeSegmentBaseQuantities, EPset_Status
          1 x IFCCOVERING | type IFCCOVERINGTYPE "DPC-250micron" | names: "250micronDPM" | material: layers ("DPM-Green Plastic" 1.) | property sets: EPset_Parametric, Qto_CoveringBaseQuantities
          3 x IFCGEOGRAPHICELEMENT | type IFCGEOGRAPHICELEMENTTYPE "Backfill_90%_MOD" | names: "GeographicElement" | material: layers ("Undercoat_PVA" 100.) | property sets: EPset_Parametric
          4 x IFCWALL | type IFCWALLTYPE "220mm_Plinth" | names: "Wall", "220mm_Plinth_wall" | material: layers ("NFX-Clay" 220.000015258789) | property sets: EPset_Parametric, Qto_WallBaseQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Screed_25mm" | names: "25mmScreed" | material: layers ("Undercoat_PVA" 25.) | property sets: EPset_Parametric, Qto_CoveringBaseQuantities
        IFCSPACE "Services"
      IFCBUILDINGSTOREY "Ground_Floor"
        contains 81 elements
          13 x IFCWALL | type IFCWALLTYPE "Internal110" | names: "Wall" | material: layers "Internal_plaster_painted_wall" ("Undercoat_PVA" 2., "Undercoat_PVA" 1., "25 MPa wooden float" 15.0000009536743, "NFX-Clay" 110.000007629395, "25 MPa wooden float" 15.0000009536743, "Undercoat_PVA" 1., "Undercoat_PVA" 2.) | property sets: EPset_Parametric, Qto_WallBaseQuantities
          8 x IFCWINDOW | type IFCWINDOWTYPE "DoublePT69" | names: "PTT189", "Window", "DoublePT69" | property sets: Qto_WindowBaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "Lintel Single 1.2m" | names: "Lintel_Single_1.2m" | property sets: Qto_BeamBaseQuantities
          7 x IFCWINDOW | type IFCWINDOWTYPE "ALU_PT69" | names: "PT69" | property sets: Qto_WindowBaseQuantities
          12 x IFCBEAM | type IFCBEAMTYPE "Lintel Single 1.8m" | names: "Lintel_single_1.8m" | property sets: Qto_BeamBaseQuantities
          4 x IFCWINDOW | type IFCWINDOWTYPE "ALU_PT159" | names: "Window" | property sets: Qto_WindowBaseQuantities
          10 x IFCBEAM | type IFCBEAMTYPE "Lintel Single 2.7m" | names: "Single_lintel_2.7m" | property sets: Qto_BeamBaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "Lintel Single 2.1m" | names: "Single_Lintel_2.1m" | property sets: Qto_BeamBaseQuantities
          6 x IFCWALL | type IFCWALLTYPE "220mm_External" | names: "Wall" | material: layers ("Clay_Brick_Red" 220.000015258789) | property sets: EPset_Parametric, Qto_WallBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "Lintel Single 1.5m" | names: "Lintel_Single_1.5m" | property sets: Qto_BeamBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "D3" | names: "Door"
          6 x IFCBEAM | type IFCBEAMTYPE "Lintel Single 0.9m" | names: "Single_Lintel_0.9m" | property sets: Qto_BeamBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "D3" | SINGLE_SWING_LEFT | names: "Door"
          1 x IFCDOOR | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "Double_Alm_Door" | property sets: BBIM_Door
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Tiling" | names: "Tiling" | material: layers ("25 MPa wooden float" 8.) | property sets: EPset_Parametric, Qto_CoveringBaseQuantities, My_Qto
        IFCSPACE "Girls_Ablution"
        IFCSPACE "Boy_ablution"
        IFCSPACE "Entertainment"
        IFCSPACE "Hall"
        IFCSPACE "Kitchen"
        IFCSPACE "Wardroab"
        IFCSPACE "Entrance"
          contains 24 elements
            2 x IFCFURNITURE | type IFCFURNITURETYPE "Nappy-Changing-Station" | names: "Furniture"
            20 x IFCFURNITURE | type IFCFURNITURETYPE "Todle-Bed 1660x990" | names: "Furniture"
            2 x IFCFURNITURE | type IFCFURNITURETYPE "3/4-Bed 1880x107" | names: "Furniture"
      IFCBUILDINGSTOREY "Roof"
        contains 151 elements
          8 x IFCBEAM | type IFCBEAMTYPE "Timber_50x76x6600" | names: "Timber_50x76x6600" | material: "RawSawnPine" | property sets: Qto_BeamBaseQuantities
          41 x IFCBEAM | type IFCBEAMTYPE "Timber_50x78x3600" | names: "Timber_50x76x3600", "Timber_50x76x2035", "Timber_50x76x2470" | material: "RawSawnPine" | property sets: Qto_BeamBaseQuantities
          39 x IFCCOVERING | type IFCCOVERINGTYPE "Corrigated_762x17.5" | names: "Covering", "Corrigate_762x17.5x8320", "Corrigate_762x17.5x4600" | material: profiles ("Hot_rolled") | property sets: EPset_Parametric, Qto_CoveringBaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "220mm_External" | names: "Wall" | material: layers ("Clay_Brick_Red" 220.000015258789) | property sets: EPset_Parametric, Qto_WallBaseQuantities
          61 x IFCMEMBERTYPE | type IFCMEMBERTYPE "Timber_38x114x4600.056" | MEMBER | names: "Timber_38x114x4600" | property sets: Qto_BeamBaseQuantities
      IFCBUILDINGSTOREY "External"
        contains 12 elements
          6 x IFCWALL | type IFCWALLTYPE "220mm_External" | names: "Wall", "Rock_Wall" | descriptions: "Using_natuaral_rock" | material: layers ("Clay_Brick_Red" 220.000015258789) | property sets: EPset_Parametric, EPset_Status, Qto_WallBaseQuantities
          3 x IFCWALL | type IFCWALLTYPE "220mm_Plinth" | names: "Wall" | material: layers ("NFX-Clay" 220.000015258789) | property sets: EPset_Parametric, EPset_Status, Qto_WallBaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "85mm surface bed" | names: "Connection" | material: layers "concrete" ("25 MPa wooden float" 85.) | property sets: EPset_Parametric, Qto_SlabBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "D3" | names: "Door" | property sets: EPset_Status
          1 x IFCGEOGRAPHICELEMENT | TERRAIN | names: "NGL" | material: "Ceiling Board"
        IFCSPACE "Walk_Way"
        IFCSPACE "Courtyard"
      IFCBUILDINGSTOREY "TempWorks"
        contains 12 elements
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Weldmesh1.8m30mroll" | names: "FenceWeldMesh1.8m" | material: profiles ("Undercoat_PVA") | property sets: EPset_Parametric, EPset_Status, Qto_BuildingElementProxyQuantities
          7 x IFCWALL | type IFCWALLTYPE "Shutterply_Painted" | names: "Shutterply2200x1220x18" | material: "RawSawnPine" | property sets: Qto_WallBaseQuantities
          1 x IFCMEMBER | type IFCMEMBERTYPE "Timber_38x114x4600" | names: "Member"
IFCWORKPLAN "1stDraft" | PLANNED
  IFCWORKSCHEDULE "Test" | ACTUAL

Types
  IFCREINFORCINGMESHTYPE "WeldMesh Ref395" | 10 occurrences | material: "Hot_rolled"
  IFCPIPESEGMENTTYPE "110mm_uPVC_6000_AG" | RIGIDSEGMENT | 7 occurrences | material: "DPM-Green Plastic"
  IFCBEAMTYPE "Lintel Single 1.8m" | LINTEL | 13 occurrences
  IFCSLABTYPE "ConcreteApron800wide" | SIDEWALK | 30 occurrences | material: layers ("25 MPa wooden float" 85.) | property sets: EPset_Parametric
  IFCSLABTYPE "85mm surface bed" | BASESLAB | 6 occurrences | material: layers "concrete" ("25 MPa wooden float" 85.) | property sets: EPset_Parametric
  IFCRAMPFLIGHTTYPE "Entrance_ramp1:12" | STRAIGHT | 1 occurrence
  IFCWALLTYPE "220mm_Plinth" | STANDARD | 13 occurrences | material: layers ("NFX-Clay" 220.000015258789) | property sets: EPset_Parametric
  IFCFOOTINGTYPE "600x230_Foundation" | STRIP_FOOTING | 8 occurrences | material: layers ("Undercoat_PVA" 600.) | property sets: EPset_Parametric
  IFCCOVERINGTYPE "60mmPaving" | 3 occurrences | material: layers ("Undercoat_PVA" 60.0000038146973) | property sets: EPset_Parametric
  IFCPIPESEGMENTTYPE "110mm_uPVC_UG" | RIGIDSEGMENT | 4 occurrences | material: profiles ("DPM-Green Plastic")
  IFCCOVERINGTYPE "DPC-250micron" | MEMBRANE | 1 occurrence | material: layers ("DPM-Green Plastic" 1.) | property sets: EPset_Parametric
  IFCGEOGRAPHICELEMENTTYPE "Backfill_90%_MOD" | element type "Backfill_to_90%_MOD_AASMTD" | USERDEFINED | 3 occurrences | material: layers ("Undercoat_PVA" 100.) | property sets: EPset_Parametric
  IFCCOVERINGTYPE "Screed_25mm" | FLOORING | 1 occurrence | material: layers ("Undercoat_PVA" 25.) | property sets: EPset_Parametric
  IFCWALLTYPE "Internal110" | STANDARD | 13 occurrences | material: layers "Internal_plaster_painted_wall" ("Undercoat_PVA" 2., "Undercoat_PVA" 1., "25 MPa wooden float" 15.0000009536743, "NFX-Clay" 110.000007629395, "25 MPa wooden float" 15.0000009536743, "Undercoat_PVA" 1., "Undercoat_PVA" 2.) | property sets: EPset_Parametric
  IFCWINDOWTYPE "DoublePT69" | WINDOW | DOUBLE_PANEL_HORIZONTAL | 8 occurrences | property sets: BBIM_Window
  IFCBEAMTYPE "Lintel Single 1.2m" | LINTEL | 5 occurrences
  IFCWINDOWTYPE "ALU_PT69" | WINDOW | DOUBLE_PANEL_HORIZONTAL | 7 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "ALU_PT159" | WINDOW | TRIPLE_PANEL_RIGHT | 4 occurrences | property sets: BBIM_Window
  IFCBEAMTYPE "Lintel Single 2.7m" | LINTEL | 10 occurrences
  IFCBEAMTYPE "Lintel Single 2.1m" | LINTEL | 4 occurrences
  IFCWALLTYPE "220mm_External" | STANDARD | 14 occurrences | material: layers ("Clay_Brick_Red" 220.000015258789) | property sets: EPset_Parametric
  IFCBEAMTYPE "Lintel Single 1.5m" | LINTEL | 2 occurrences
  IFCDOORTYPE "D3" | DOOR | SINGLE_SWING_LEFT | 3 occurrences | property sets: BBIM_Door
  IFCBEAMTYPE "Lintel Single 0.9m" | LINTEL | 6 occurrences
  IFCCOVERINGTYPE "Tiling" | FLOORING | 1 occurrence | material: layers ("25 MPa wooden float" 8.) | property sets: EPset_Parametric
  IFCFURNITURETYPE "Nappy-Changing-Station" | element type "Nappy-Changing-Station" | FACTORY | USERDEFINED | 2 occurrences
  IFCFURNITURETYPE "Todle-Bed 1660x990" | FACTORY | BED | 20 occurrences
  IFCFURNITURETYPE "3/4-Bed 1880x107" | FACTORY | BED | 2 occurrences
  IFCBEAMTYPE "Timber_50x76x6600" | BEAM | 8 occurrences | material: "RawSawnPine"
  IFCBEAMTYPE "Timber_50x78x3600" | BEAM | 41 occurrences | material: "RawSawnPine"
  IFCCOVERINGTYPE "Corrigated_762x17.5" | ROOFING | 39 occurrences | material: profiles ("Hot_rolled")
  IFCMEMBERTYPE "Timber_38x114x4600.056" | MEMBER | 61 occurrences | description "Raw_Sawn_pine"
  IFCBUILDINGELEMENTPROXYTYPE "Weldmesh1.8m30mroll" | 4 occurrences | material: profiles ("Undercoat_PVA")
  IFCWALLTYPE "Shutterply_Painted" | PARTITIONING | 7 occurrences | material: "RawSawnPine" | property sets: EPset_Status
  IFCMEMBERTYPE "Timber_38x114x4600" | MEMBER | 1 occurrence

Property sets
  EPset_Parametric | properties | on 48 objects (40 IFCWALL, 8 IFCFOOTING)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 47 objects (39 IFCCOVERING, 4 IFCBUILDINGELEMENTPROXY, 4 IFCPIPESEGMENT)
    Engine = "Bonsai.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 45 objects (36 IFCSLAB, 6 IFCCOVERING, 3 IFCGEOGRAPHICELEMENT)
    Engine = "Bonsai.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 7 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  EPset_Parametric | properties | on 4 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  BBIM_Door | properties | on 1 object (1 IFCDOOR)
    Data = "{"door_type": "DOUBLE_DOOR_SINGLE_SWING", "overall_height": 2100.0001430511475, "overall_width": 1500.0001192092896, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 100.00000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2100.0001430511475, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 100.00000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  Qto_WallBaseQuantities | quantities | on 7 objects (7 IFCWALL)
    GrossSideArea = 2.68400007015467 [SQUARE_METRE]
    GrossVolume = 0.0483120991698541 [CUBIC_METRE]
    Height = 2200.00003278256 [MILLI METRE]
    Length = 1220.00001370907 [MILLI METRE]
    NetSideArea = 2.68400007015467 [SQUARE_METRE]
    NetVolume = 0.0483120991698541 [CUBIC_METRE]
    Width = 18.000036478043 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossSideArea = 7.00060036611635 [SQUARE_METRE]
    GrossVolume = 1.00808651146088 [CUBIC_METRE]
    Height = 2465.00015258789 [MILLI METRE]
    Length = 2839.99997272485 [MILLI METRE]
    NetSideArea = 7.00060036611635 [SQUARE_METRE]
    NetVolume = 1.00808651146088 [CUBIC_METRE]
    Width = 144.000009536743 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossSideArea = 2.24314985406733 [SQUARE_METRE]
    GrossVolume = 0.323013592355237 [CUBIC_METRE]
    Height = 2465.00015258789 [MILLI METRE]
    Length = 909.999884467492 [MILLI METRE]
    NetSideArea = 2.24314985406733 [SQUARE_METRE]
    NetVolume = 0.323013592355237 [CUBIC_METRE]
    Width = 144.000009536743 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossSideArea = 3.70799841742588 [SQUARE_METRE]
    GrossVolume = 0.815759715163787 [CUBIC_METRE]
    Height = 600.000023841858 [MILLI METRE]
    Length = 6179.99721908616 [MILLI METRE]
    NetSideArea = 3.70799841742588 [SQUARE_METRE]
    NetVolume = 0.815759715163787 [CUBIC_METRE]
    Width = 220.000015258789 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossSideArea = 10.2000004053116 [SQUARE_METRE]
    GrossVolume = 2.24400024480821 [CUBIC_METRE]
    Height = 1200.00004768372 [MILLI METRE]
    Length = 8500. [MILLI METRE]
    NetSideArea = 10.2000004053116 [SQUARE_METRE]
    NetVolume = 2.24400024480821 [CUBIC_METRE]
    Width = 220.000015258789 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 4.43700248325204 [SQUARE_METRE]
    GrossVolume = 0.647802422946282 [CUBIC_METRE]
    Height = 2465.00015258789 [MILLI METRE]
    Length = 1800.00099643927 [MILLI METRE]
    NetSideArea = 2.78461609272448 [SQUARE_METRE]
    NetVolume = 0.406553994170871 [CUBIC_METRE]
    Width = 146.000009536744 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 1.70400101757051 [SQUARE_METRE]
    GrossVolume = 0.374880247674045 [CUBIC_METRE]
    Height = 600.000023841858 [MILLI METRE]
    Length = 2840.00162593491 [MILLI METRE]
    NetSideArea = 1.70400101757051 [SQUARE_METRE]
    NetVolume = 0.374880247674045 [CUBIC_METRE]
    Width = 220.000015258789 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 9.36360110893253 [SQUARE_METRE]
    GrossVolume = 2.05999238684237 [CUBIC_METRE]
    Height = 3004.56080667291 [MILLI METRE]
    Length = 3060.00018119812 [MILLI METRE]
    NetSideArea = 7.01842872137437 [SQUARE_METRE]
    NetVolume = 1.54405442022855 [CUBIC_METRE]
    Width = 220.000015258806 [MILLI METRE]
  Qto_WallBaseQuantities: 29 more contents on 29 objects not shown
  Qto_BeamBaseQuantities | quantities | on 48 objects (48 IFCMEMBERTYPE)
    GrossSurfaceArea = 1.4070641461792 [SQUARE_METRE]
    GrossVolume = 0.0199272133361795 [CUBIC_METRE]
    Length = 4600. [MILLI METRE]
    NetSurfaceArea = 1.4070641461792 [SQUARE_METRE]
    NetVolume = 0.0199272133361795 [CUBIC_METRE]
    OuterSurfaceArea = 1.05746386541748 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 28 objects (28 IFCBEAM)
    GrossSurfaceArea = 0.914799629815574 [SQUARE_METRE]
    GrossVolume = 0.0136799877056377 [CUBIC_METRE]
    Length = 3599.99998509884 [MILLI METRE]
    NetSurfaceArea = 0.914799629815574 [SQUARE_METRE]
    NetVolume = 0.0136799877056377 [CUBIC_METRE]
    OuterSurfaceArea = 0.554799881072999 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 12 objects (12 IFCBEAM)
    GrossSurfaceArea = 0.682499527282619 [SQUARE_METRE]
    GrossVolume = 0.0148499910278284 [CUBIC_METRE]
    Length = 1799.99841308594 [MILLI METRE]
    NetSurfaceArea = 0.682499527282619 [SQUARE_METRE]
    NetVolume = 0.0148499910278284 [CUBIC_METRE]
    OuterSurfaceArea = 0.286499766540528 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 10 objects (10 IFCBEAM)
    GrossSurfaceArea = 1.01550027918817 [SQUARE_METRE]
    GrossVolume = 0.0222750102102764 [CUBIC_METRE]
    Length = 2700.00004768372 [MILLI METRE]
    NetSurfaceArea = 1.01550027918817 [SQUARE_METRE]
    NetVolume = 0.0222750102102764 [CUBIC_METRE]
    OuterSurfaceArea = 0.421500030517579 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 9 objects (9 IFCBEAM)
    GrossSurfaceArea = 0.914799629815574 [SQUARE_METRE]
    GrossVolume = 0.0136799877056377 [CUBIC_METRE]
    Length = 2470.17345428467 [MILLI METRE]
    NetSurfaceArea = 0.630083456917121 [SQUARE_METRE]
    NetVolume = 0.00938665072924414 [CUBIC_METRE]
    OuterSurfaceArea = 0.383066282868815 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 8 objects (8 IFCBEAM)
    GrossSurfaceArea = 1.67079955192044 [SQUARE_METRE]
    GrossVolume = 0.0250799856947448 [CUBIC_METRE]
    Length = 6600. [MILLI METRE]
    NetSurfaceArea = 1.67079955192044 [SQUARE_METRE]
    NetVolume = 0.0250799856947448 [CUBIC_METRE]
    OuterSurfaceArea = 1.01079979896976 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 7 objects (7 IFCMEMBERTYPE)
    GrossSurfaceArea = 1.4070641461792 [SQUARE_METRE]
    GrossVolume = 0.0199272133361795 [CUBIC_METRE]
    Length = 3990.74411656036 [MILLI METRE]
    NetSurfaceArea = 1.21886177324402 [SQUARE_METRE]
    NetVolume = 0.0172443756948296 [CUBIC_METRE]
    OuterSurfaceArea = 0.911929994793029 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 6 objects (6 IFCBEAM)
    GrossSurfaceArea = 0.349499396362252 [SQUARE_METRE]
    GrossVolume = 0.00742498645019384 [CUBIC_METRE]
    Length = 899.998291015625 [MILLI METRE]
    NetSurfaceArea = 0.349499396362252 [SQUARE_METRE]
    NetVolume = 0.00742498645019384 [CUBIC_METRE]
    OuterSurfaceArea = 0.151499717407279 [SQUARE_METRE]
  Qto_BeamBaseQuantities: 7 more contents on 19 objects not shown
  Qto_CoveringBaseQuantities | quantities | on 18 objects (18 IFCCOVERING)
    GrossArea = 3.65759990234971 [SQUARE_METRE]
    NetArea = 3.65759990234971 [SQUARE_METRE]
    Width = 17.5 [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 5 objects (5 IFCCOVERING)
    GrossArea = 6.40079980387232 [SQUARE_METRE]
    NetArea = 6.40079980387232 [SQUARE_METRE]
    Width = 17.5 [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 5 objects (5 IFCCOVERING)
    GrossArea = 6.40079980220903 [SQUARE_METRE]
    NetArea = 6.40079980220903 [SQUARE_METRE]
    Width = 17.5 [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 3 objects (3 IFCCOVERING)
    GrossArea = 6.40079980303803 [SQUARE_METRE]
    NetArea = 6.40079980303803 [SQUARE_METRE]
    Width = 17.5 [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 3 objects (3 IFCCOVERING)
    GrossArea = 3.505200315882 [SQUARE_METRE]
    NetArea = 3.505200315882 [SQUARE_METRE]
    Width = 17.5 [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 2 objects (2 IFCCOVERING)
    GrossArea = 6.40079980345518 [SQUARE_METRE]
    NetArea = 6.40079980345518 [SQUARE_METRE]
    Width = 17.5 [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 2 objects (2 IFCCOVERING)
    GrossArea = 6.40079980340237 [SQUARE_METRE]
    NetArea = 6.40079980340237 [SQUARE_METRE]
    Width = 17.5 [MILLI METRE]
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 155.842114010713 [SQUARE_METRE]
    NetArea = 155.842114010713 [SQUARE_METRE]
    Width = 1. [MILLI METRE]
  Qto_CoveringBaseQuantities: 6 more contents on 6 objects not shown
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 230.000004172325 [MILLI METRE]
    Length = 11910.4859970816 [MILLI METRE]
    NetVolume = 1.643580277539 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 230.000004172325 [MILLI METRE]
    Length = 14425.9278168741 [MILLI METRE]
    NetVolume = 1.99077806052824 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 230.000004172325 [MILLI METRE]
    Length = 3046.32678449626 [MILLI METRE]
    NetVolume = 0.420393089572453 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 230.000004172325 [MILLI METRE]
    Length = 1915.89925403171 [MILLI METRE]
    NetVolume = 0.264394085237083 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 230.000004172325 [MILLI METRE]
    Length = 12000.2034623207 [MILLI METRE]
    NetVolume = 1.65602809122596 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 230.000004172325 [MILLI METRE]
    Length = 11651.8287412749 [MILLI METRE]
    NetVolume = 1.60795238115087 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 230.000004172325 [MILLI METRE]
    Length = 3499.51491824952 [MILLI METRE]
    NetVolume = 0.482933066989913 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    Height = 230.000004172325 [MILLI METRE]
    Length = 11642.21301613 [MILLI METRE]
    NetVolume = 1.6066254110568 [CUBIC_METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 9 objects (9 IFCOPENINGELEMENT)
    Area = 0.636881286621095 [SQUARE_METRE]
    Depth = 500. [MILLI METRE]
    Height = 499.999938964844 [MILLI METRE]
    Volume = 0.318440604438399 [CUBIC_METRE]
    Width = 1273.76257324219 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 7 objects (7 IFCOPENINGELEMENT)
    Area = 1.08 [SQUARE_METRE]
    Depth = 900. [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Volume = 0.648 [CUBIC_METRE]
    Width = 600. [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    Area = 27.8604467773438 [SQUARE_METRE]
    Depth = 2500.00011534491 [MILLI METRE]
    Height = 11144.1787368131 [MILLI METRE]
    Volume = 13.9302182872717 [CUBIC_METRE]
    Width = 499.999816894531 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    Area = 1.8 [SQUARE_METRE]
    Depth = 899.999938964844 [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Volume = 1.61999989013672 [CUBIC_METRE]
    Width = 1500. [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    Area = 2.84772019042969 [SQUARE_METRE]
    Depth = 899.999976577092 [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Volume = 2.56294783131428 [CUBIC_METRE]
    Width = 2373.1001586914 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 3 objects (3 IFCOPENINGELEMENT)
    Area = 2.760531923918 [SQUARE_METRE]
    Depth = 500. [MILLI METRE]
    Height = 3500.33557128906 [MILLI METRE]
    Volume = 1.30577082727917 [CUBIC_METRE]
    Width = 3950.46142578124 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 2 objects (2 IFCOPENINGELEMENT)
    Area = 1.65238639052748 [SQUARE_METRE]
    Depth = 2100.00024414062 [MILLI METRE]
    Height = 786.850570678711 [MILLI METRE]
    Volume = 0.826193094410078 [CUBIC_METRE]
    Width = 499.999938964844 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 2 objects (2 IFCOPENINGELEMENT)
    Area = 2.52000029296874 [SQUARE_METRE]
    Depth = 2100.00024414062 [MILLI METRE]
    Height = 1200. [MILLI METRE]
    Volume = 2.26800026367187 [CUBIC_METRE]
    Width = 900. [MILLI METRE]
  Qto_OpeningElementBaseQuantities: 14 more contents on 15 objects not shown
  Qto_SlabBaseQuantities | quantities | on 23 objects (23 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 1.03999974670005 [SQUARE_METRE]
    GrossVolume = 0.0883999784695046 [CUBIC_METRE]
    Length = 1299.99987792969 [MILLI METRE]
    NetArea = 1.03999974670005 [SQUARE_METRE]
    NetVolume = 0.0883999784695046 [CUBIC_METRE]
    Perimeter = 4199.99951640753 [MILLI METRE]
    Width = 800.000004688759 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 48.0239889697232 [SQUARE_METRE]
    GrossVolume = 4.08203906242647 [CUBIC_METRE]
    Length = 5800.001953125 [MILLI METRE]
    NetArea = 48.0239889697232 [SQUARE_METRE]
    NetVolume = 4.08203906242647 [CUBIC_METRE]
    Perimeter = 28159.9953613284 [MILLI METRE]
    Width = 8279.99682617188 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 1.03999992370199 [SQUARE_METRE]
    GrossVolume = 0.0883999935146691 [CUBIC_METRE]
    Length = 1300. [MILLI METRE]
    NetArea = 1.03999992370199 [SQUARE_METRE]
    NetVolume = 0.0883999935146691 [CUBIC_METRE]
    Perimeter = 4199.99988261846 [MILLI METRE]
    Width = 800.000065723915 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 1.14198804559681 [SQUARE_METRE]
    GrossVolume = 0.0970689838757285 [CUBIC_METRE]
    Length = 1427.48516845703 [MILLI METRE]
    NetArea = 1.14198804559681 [SQUARE_METRE]
    NetVolume = 0.0970689838757285 [CUBIC_METRE]
    Perimeter = 4454.97021198273 [MILLI METRE]
    Width = 800.000058174126 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 0.877357885977135 [SQUARE_METRE]
    GrossVolume = 0.0745754203080565 [CUBIC_METRE]
    Length = 1096.69753265381 [MILLI METRE]
    NetArea = 0.877357885977135 [SQUARE_METRE]
    NetVolume = 0.0745754203080565 [CUBIC_METRE]
    Perimeter = 3793.39480972956 [MILLI METRE]
    Width = 799.999934736334 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 1.03999991879463 [SQUARE_METRE]
    GrossVolume = 0.0883999930975433 [CUBIC_METRE]
    Length = 1300. [MILLI METRE]
    NetArea = 1.03999991879463 [SQUARE_METRE]
    NetVolume = 0.0883999930975433 [CUBIC_METRE]
    Perimeter = 4199.99987506867 [MILLI METRE]
    Width = 800.000058174126 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 1.13599867925788 [SQUARE_METRE]
    GrossVolume = 0.09655988773692 [CUBIC_METRE]
    Length = 1419.99865722656 [MILLI METRE]
    NetArea = 1.13599867925788 [SQUARE_METRE]
    NetVolume = 0.09655988773692 [CUBIC_METRE]
    Perimeter = 4439.99696723679 [MILLI METRE]
    Width = 799.999896924288 [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 85. [MILLI METRE]
    GrossArea = 0.898147051820011 [SQUARE_METRE]
    GrossVolume = 0.0763424994047009 [CUBIC_METRE]
    Length = 1122.68405151368 [MILLI METRE]
    NetArea = 0.898147051820011 [SQUARE_METRE]
    NetVolume = 0.0763424994047009 [CUBIC_METRE]
    Perimeter = 3845.36776563786 [MILLI METRE]
    Width = 800.000065723915 [MILLI METRE]
  Qto_SlabBaseQuantities: 6 more contents on 6 objects not shown
  Qto_WindowBaseQuantities | quantities | on 8 objects (8 IFCWINDOW)
    Area = 1.33500002264977 [SQUARE_METRE]
    Height = 899.999976158142 [MILLI METRE]
    Width = 1200.00004768372 [MILLI METRE]
  Qto_WindowBaseQuantities | quantities | on 7 objects (7 IFCWINDOW)
    Area = 0.705000010579824 [SQUARE_METRE]
    Height = 899.999976158142 [MILLI METRE]
    Width = 600.000023841858 [MILLI METRE]
  Qto_WindowBaseQuantities | quantities | on 4 objects (4 IFCWINDOW)
    Area = 1.64625008519739 [SQUARE_METRE]
    Height = 899.999976158142 [MILLI METRE]
    Width = 1500.00011920929 [MILLI METRE]
  EPset_Status | properties | on 9 objects (6 IFCWALL, 2 IFCPIPESEGMENT, 1 IFCDOOR)
    Status in {"EXISTING"} (IFCLABEL)
  EPset_Status | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Status in {"TEMPORARY"} (IFCLABEL)
  EPset_Status | properties | on 1 object (1 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Qto_PipeSegmentBaseQuantities | quantities | on 7 objects (7 IFCPIPESEGMENT)
  Qto_PipeSegmentBaseQuantities | quantities | on 2 objects (2 IFCPIPESEGMENT)
    Length = 1999.99961871068 [MILLI METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 1 object (1 IFCPIPESEGMENT)
    Length = 10460.0001877444 [MILLI METRE]
  Qto_PipeSegmentBaseQuantities | quantities | on 1 object (1 IFCPIPESEGMENT)
    Length = 9999.99942779539 [MILLI METRE]
  EPset_Productivity | properties | on 1 object (1 IFCLABORRESOURCE)
    BaseQuantityConsumed = "h" (IFCDURATION)
    BaseQuantityProducedName = "Basin" (IFCLABEL)
    BaseQuantityProducedValue = 1.02999997138977 (IFCREAL)
  My_Qto | quantities | on 1 object (1 IFCCOVERING)
    MyDimension = 288.442693574024 [MILLI METRE]
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1:100" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/100" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  Qto_BuildingElementProxyQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 37.0250117888208 [SQUARE_METRE]
    NetVolume = 0.0369767289946663 [CUBIC_METRE]
  Qto_BuildingElementProxyQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 81.797306407243 [SQUARE_METRE]
    NetVolume = 0.0816993315440636 [CUBIC_METRE]
  Qto_BuildingElementProxyQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 10.8191992370412 [SQUARE_METRE]
    NetVolume = 0.010800000083819 [CUBIC_METRE]
  Qto_BuildingElementProxyQuantities | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    NetSurfaceArea = 21.6311984732747 [SQUARE_METRE]
    NetVolume = 0.021600000167638 [CUBIC_METRE]
  Qto_TaskBaseQuantities | quantities | on 15 objects (15 IFCTASK)
    StandardWork = 1.
  Qto_TaskBaseQuantities | quantities | on 3 objects (3 IFCTASK)
    StandardWork = 2.
  Qto_TaskBaseQuantities | quantities | on 2 objects (2 IFCTASK)
    StandardWork = 3.
  Qto_TaskBaseQuantities | quantities | on 1 object (1 IFCTASK)
    StandardWork = 366.
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_HORIZONTAL", "overall_height": 899.9999761581421, "overall_width": 1200.0000476837158, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 50.00000074505806, "first_transom_offset": 449.99998807907104}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_HORIZONTAL", "overall_height": 899.9999761581421, "overall_width": 600.0000238418579, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 50.00000074505806, "first_transom_offset": 300.00001192092896}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_RIGHT", "overall_height": 899.9999761581421, "overall_width": 1500.0001192092896, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 600.0000238418579, "transom_thickness": 50.00000074505806, "first_transom_offset": 300.00001192092896}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)