IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "test_tovendor.ifc"
Time stamp: "2023-03-31T09:27:13+02:00"
Preprocessor: "IfcOpenShell v0.7.0-476ab506d"
Originating system: "BlenderBIM 0.0.230331"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 4 elements
          2 x IFCWALL | type IFCWALLTYPE "WAL300" | names: "Wall" | material: layers ("Unknown" 0.3) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "WT01" | TRIPLE_PANEL_BOTTOM | names: "Window" | property sets: BBIM_Window
          1 x IFCDOOR | type IFCDOORTYPE "DT01" | SINGLE_SWING_LEFT | names: "Door" | property sets: BBIM_Door

Types
  IFCWALLTYPE "WAL300" | 2 occurrences | material: layers ("Unknown" 0.3)
  IFCWINDOWTYPE "WT01" | 1 occurrence
  IFCDOORTYPE "DT01" | 1 occurrence

Property sets
  EPset_Parametric | properties | on 2 objects (2 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  BBIM_Window | properties | on 1 object (1 IFCWINDOW)
    Data = "{"window_type": "TRIPLE_PANEL_BOTTOM", "overall_height": 1.5299999713897705, "overall_width": 1.4100000858306885, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "mullion_thickness": 0.05000000074505806, "first_mullion_offset": 0.30000001192092896, "transom_thickness": 0.05000000074505806, "first_transom_offset": 0.44999998807907104}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Door | properties | on 1 object (1 IFCDOOR)
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2.0, "overall_width": 1.4700000286102295, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.0, "casing_thickness": 0.07500000298023224, "casing_depth": 0.004999999888241291, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)