IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "window.ifc"
Time stamp: "2022-12-25T09:39:09+01:00"
Preprocessor: "IfcOpenShell v0.7.0-cdde5366"
Originating system: "BlenderBIM 0.0.221105"
Authorization: "Nobody"

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  LENGTHUNIT: MILLI METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 5 elements
          3 x IFCWINDOW | type IFCWINDOWTYPE "kozijn_1000x1000mm" | names: "kozijn_1000x1000mm"
          2 x IFCWALL | type IFCWALLTYPE "concrete_exterior_wall_200mm" | names: "concrete_exterior_wall_200mm" | material: layers "concrete" ("concrete" 200.) | property sets: EPset_Parametric

Types
  IFCWINDOWTYPE "kozijn_1000x1000mm" | WINDOW | 3 occurrences
  IFCWALLTYPE "concrete_exterior_wall_200mm" | 2 occurrences | material: layers "concrete" ("concrete" 200.) | property sets: Pset_WallCommon

Property sets
  EPset_Parametric | properties | on 2 objects (2 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  Pset_WallCommon | properties | on 1 type object
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)