IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "3bd hous240120.ifc"
Time stamp: "2024-01-26T13:18:49+02:00"
Preprocessor: "IfcOpenShell v0.7.0-6c9e130ca"
Originating system: "BlenderBIM 0.0.240119-5f4dfcf"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDINGSTOREY "My Storey"
      contains 84 elements
        19 x IFCWALL | type IFCWALLTYPE "110mm non-load bearing" | names: "Wall" | material: layers ("Unknown" 38.) | property sets: EPset_Parametric
        1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Double Basin" | names: "Double Basin"
        6 x IFCWALL | type IFCWALLTYPE "220mm load bearing" | names: "Wall" | material: layers ("Unknown" 220.) | property sets: EPset_Parametric
        2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Toilet" | names: "SanitaryTerminal"
        2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Shower" | names: "SanitaryTerminal"
        1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Single basin" | SINK | names: "Single Basin"
        1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Sink" | names: "SanitaryTerminal"
        2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Cistern" | names: "SanitaryTerminal"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "3 seater" | names: "Furniture"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "2 seater" | names: "Furniture"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "6 diner" | names: "Furniture"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "1 seat" | names: "Furniture"
        1 x IFCFURNITURE | type IFCFURNITURETYPE "King Size" | names: "Furniture"
        10 x IFCPLATE | type IFCPLATETYPE "18mm x600x1000 board" | names: "Plate" | material: layers ("Unknown" 18.) | property sets: EPset_Parametric
        1 x IFCSLAB | type IFCSLABTYPE "mezz" | names: "Slab" | material: layers ("Unknown" 95.) | property sets: EPset_Parametric
        3 x IFCFURNITURE | type IFCFURNITURETYPE "King Size.NHB" | names: "Furniture"
        2 x IFCDOOR | type IFCDOORTYPE "Internal door LH" | names: "Door"
        1 x IFCDOOR | type IFCDOORTYPE "Internal door RH" | names: "Door"
        1 x IFCSLAB | type IFCSLABTYPE "85mm floor slab" | names: "Slab" | material: layers ("Unknown" 85.) | property sets: EPset_Parametric
        3 x IFCWINDOW | type IFCWINDOWTYPE "1800x2100" | DOUBLE_PANEL_VERTICAL | names: "Window"
        6 x IFCWINDOW | type IFCWINDOWTYPE "600x1500" | names: "Window"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "200lt FF" | names: "ElectricAppliance"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "15kg WM" | names: "ElectricAppliance"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "13 plate DW" | names: "ElectricAppliance"
        2 x IFCWINDOW | type IFCWINDOWTYPE "1500x900" | WINDOW | TRIPLE_PANEL_HORIZONTAL | names: "Window"
        3 x IFCWINDOW | type IFCWINDOWTYPE "600x600" | WINDOW | names: "Window", "Window.012", "Window.014"
        1 x IFCWINDOW | type IFCWINDOWTYPE "600x1500" | DOUBLE_PANEL_VERTICAL | names: "Window"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "4 plate ST" | names: "ElectricAppliance"
        1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Micorwave" | names: "ElectricAppliance"
        1 x IFCDOOR | type IFCDOORTYPE "External door RD" | DOOR | names: "Door"
        5 x IFCBEAM | type IFCBEAMTYPE "Lintol 110x75" | names: "Beam" | material: profiles ("Unknown") | property sets: EPset_Parametric
        1 x IFCDOOR | type IFCDOORTYPE "External door RD" | names: "Door"

Types
  IFCWALLTYPE "110mm non-load bearing" | SOLIDWALL | 19 occurrences | material: layers ("Unknown" 38.) | property sets: EPset_Parametric
  IFCSANITARYTERMINALTYPE "Double Basin" | WASHHANDBASIN | 1 occurrence
  IFCWALLTYPE "220mm load bearing" | SOLIDWALL | 6 occurrences | material: layers ("Unknown" 220.) | property sets: EPset_Parametric
  IFCSANITARYTERMINALTYPE "Toilet" | TOILETPAN | 2 occurrences
  IFCSANITARYTERMINALTYPE "Shower" | SHOWER | 2 occurrences
  IFCSANITARYTERMINALTYPE "Single basin" | WASHHANDBASIN | 1 occurrence
  IFCSANITARYTERMINALTYPE "Sink" | SINK | 1 occurrence
  IFCSANITARYTERMINALTYPE "Cistern" | CISTERN | 2 occurrences
  IFCFURNITURETYPE "3 seater" | SOFA | 1 occurrence
  IFCFURNITURETYPE "2 seater" | SOFA | 1 occurrence
  IFCFURNITURETYPE "6 diner" | TABLE | 1 occurrence | description "1x1.6m tabke with 1m movement space"
  IFCFURNITURETYPE "1 seat" | SOFA | 1 occurrence
  IFCFURNITURETYPE "King Size" | BED | 1 occurrence
  IFCPLATETYPE "18mm x600x1000 board" | SHEET | 10 occurrences | material: layers ("Unknown" 18.) | property sets: EPset_Parametric
  IFCSLABTYPE "mezz" | FLOOR | 1 occurrence | material: layers ("Unknown" 95.) | property sets: EPset_Parametric
  IFCFURNITURETYPE "King Size.NHB" | BED | 3 occurrences
  IFCDOORTYPE "Internal door LH" | DOOR | SINGLE_SWING_LEFT | 2 occurrences | property sets: BBIM_Door | description "RDF4"
  IFCDOORTYPE "Internal door RH" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | property sets: BBIM_Door | description "RDF4"
  IFCSLABTYPE "85mm floor slab" | FLOOR | 1 occurrence | material: layers ("Unknown" 85.) | property sets: EPset_Parametric
  IFCWINDOWTYPE "1800x2100" | WINDOW | DOUBLE_PANEL_HORIZONTAL | 3 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "600x1500" | WINDOW | DOUBLE_PANEL_VERTICAL | 7 occurrences | property sets: BBIM_Window
  IFCELECTRICAPPLIANCETYPE "200lt FF" | FRIDGE_FREEZER | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "15kg WM" | WASHINGMACHINE | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "13 plate DW" | DISHWASHER | 1 occurrence
  IFCWINDOWTYPE "1500x900" | WINDOW | TRIPLE_PANEL_VERTICAL | 2 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "600x600" | WINDOW | SINGLE_PANEL | 3 occurrences | property sets: BBIM_Window
  IFCELECTRICAPPLIANCETYPE "4 plate ST" | ELECTRICCOOKER | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "Micorwave" | KITCHENMACHINE | 1 occurrence
  IFCDOORTYPE "External door RD" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | property sets: BBIM_Door
  IFCBEAMTYPE "Lintol 110x75" | LINTEL | 5 occurrences | material: profiles ("Unknown")

Property sets
  EPset_Parametric | properties | on 25 objects (25 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 12 objects (10 IFCPLATE, 2 IFCSLAB)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 6 objects (6 IFCBEAM)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 3 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2100.0001430511475, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 115.00000208616257, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 110.00000685453415, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 2100.0001430511475, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 115.00000208616257, "lining_thickness": 50.00000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 110.00000685453415, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 2000.0, "overall_width": 899.9999761581421, "lining_properties": {"lining_depth": 50.00000074505806, "lining_thickness": 220.0000137090683, "lining_offset": 0.0, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 0.0, "casing_thickness": 75.00000298023224, "casing_depth": 4.999999888241291, "threshold_thickness": 25.00000037252903, "threshold_depth": 100.00000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 35.00000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 2100.0001430511475, "overall_width": 1800.0000715255737, "lining_properties": {"lining_depth": 250.0, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 900.0000357627869}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 600.0000238418579, "overall_width": 1500.0001192092896, "lining_properties": {"lining_depth": 250.0, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "mullion_thickness": 50.00000074505806, "first_mullion_offset": 600.0000238418579}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_HORIZONTAL", "overall_height": 1500.0001192092896, "overall_width": 900.0000357627869, "lining_properties": {"lining_depth": 250.0, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903, "transom_thickness": 50.00000074505806, "first_transom_offset": 300.00001192092896, "second_transom_offset": 600.0000238418579}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 600.0000238418579, "overall_width": 600.0000238418579, "lining_properties": {"lining_depth": 250.0, "lining_thickness": 50.00000074505806, "lining_offset": 50.00000074505806, "lining_to_panel_offset_x": 25.00000037252903, "lining_to_panel_offset_y": 25.00000037252903}, "panel_properties": {"frame_depth": [34.999996185302734, 34.999996185302734, 34.999996185302734], "frame_thickness": [34.999996185302734, 34.999996185302734, 34.999996185302734]}}" (IFCTEXT)