IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition[DesignTransferView]"
File name: "test.ifc"
Time stamp: "2025-06-21T14:30:16+05:30"
Preprocessor: "IfcOpenShell 0.8.3-alpha250613"
Originating system: "Bonsai 0.8.3-alpha250613-9b8357c"
Authorization: "Nobody"

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 3 elements
          1 x IFCWALL | type IFCWALLTYPE "Wall 250mm export" | names: "Wall" | material: layers "brick" ("Plaster" 0.00999999977648258, "Brick" 0.230000004172325, "Plaster" 0.00999999977648258) | property sets: EPset_Parametric, Qto_WallBaseQuantities
          1 x IFCDOOR | type IFCDOORTYPE "Door" | names: "Door" | property sets: Qto_DoorBaseQuantities
          1 x IFCEARTHWORKSFILL | BACKFILL | names: "Slab" | property sets: My_Qto

Types
  IFCWALLTYPE "Wall 250mm export" | SOLIDWALL | 1 occurrence | material: layers "brick" ("Plaster" 0.00999999977648258, "Brick" 0.230000004172325, "Plaster" 0.00999999977648258) | property sets: EPset_Parametric
  IFCDOORTYPE "Door" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: BBIM_Door

Property sets
  My_Qto | quantities | on 1 object (1 IFCEARTHWORKSFILL)
    NetVolume = 6.49431267191696 [CUBIC_METRE]
  EPset_Parametric | properties | on 1 object (1 IFCWALL)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS2" (IFCLABEL)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 8.55699119377146 [SQUARE_METRE]
    GrossVolume = 2.07206032533756 [CUBIC_METRE]
    Height = 2.15000009536743 [METRE]
    Length = 3.97999580601841 [METRE]
    NetSideArea = 6.54199132967006 [SQUARE_METRE]
    NetVolume = 1.56831035180575 [CUBIC_METRE]
    Width = 0.25000000372529 [METRE]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 2.65229996101698 [SQUARE_METRE]
    Height = 2.02500009536743 [METRE]
    Perimeter = 5.95000009983778 [METRE]
    Width = 2.02500009536743 [METRE]
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2.0, "overall_width": 0.8999999761581421, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.0, "casing_thickness": 0.07500000298023224, "casing_depth": 0.004999999888241291, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)