IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "residential_building_milimeters_IFC4.ifc"
Time stamp: "2023-05-03T16:34:13+02:00"
Preprocessor: "IfcOpenShell v0.7.0-476ab506d"
Originating system: "BlenderBIM 0.0.230304"
Authorization: "Nobody"

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  LENGTHUNIT: MILLI METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "-01_fundering"
        contains 8 elements
          8 x IFCBEAM | type IFCBEAMTYPE "funderingsbalk_400x500mm" | names: "Beam" | material: profiles ("beton") | property sets: EPset_Parametric
      IFCBUILDINGSTOREY "00_begane_grond"
        contains 66 elements
          6 x IFCWALL | type IFCWALLTYPE "isolatie_120mm" | names: "isolatie_120mm" | material: layers ("isolatie" 120.) | property sets: EPset_Parametric
          6 x IFCWALL | type IFCWALLTYPE "binnenspouwblad_120mm" | names: "isolatie_120mm", "binnenspouwblad_120mm" | material: layers ("kalkzandsteen" 120.) | property sets: EPset_Parametric
          3 x IFCWALL | type IFCWALLTYPE "buitenspouwblad_100mm" | names: "buitenspouwblad_100mm" | material: layers ("baksteen" 100.) | property sets: EPset_Parametric
          17 x IFCMEMBER | type IFCMEMBERTYPE "stijl_HSB_wand" | names: "stijl_HSB_wand" | material: profiles ("vuren", "vuren") | property sets: EPset_Parametric, BBIM_Array
          30 x IFCCOVERING | type IFCCOVERINGTYPE "rabatdelen" | names: "rabatdelen" | material: profiles ("rabatdeel") | property sets: EPset_Parametric, BBIM_Array
          1 x IFCSLAB | type IFCSLABTYPE "betonvloer_200mm" | names: "Slab" | material: layers ("beton" 200.) | property sets: EPset_Parametric
          1 x IFCWALL | type IFCWALLTYPE "kalkzandsteen_214mm" | names: "Wall" | material: layers ("kalkzandsteen" 214.) | property sets: EPset_Parametric
          2 x IFCWALL | names: "voorgevel_garage", "voorgevel_entree" | parts: 69 IFCCOVERING, 6 IFCMEMBER, 5 IFCWALL

Types
  IFCBEAMTYPE "funderingsbalk_400x500mm" | BEAM | 8 occurrences | material: profiles ("beton")
  IFCWALLTYPE "isolatie_120mm" | ELEMENTEDWALL | 6 occurrences | material: layers ("isolatie" 120.) | property sets: EPset_Parametric
  IFCWALLTYPE "binnenspouwblad_120mm" | SOLIDWALL | 6 occurrences | material: layers ("kalkzandsteen" 120.) | property sets: EPset_Parametric
  IFCWALLTYPE "buitenspouwblad_100mm" | SOLIDWALL | 3 occurrences | material: layers ("baksteen" 100.) | property sets: EPset_Parametric
  IFCMEMBERTYPE "stijl_HSB_wand" | MEMBER | 17 occurrences | material: profiles ("vuren", "vuren")
  IFCCOVERINGTYPE "rabatdelen" | CLADDING | 30 occurrences | material: profiles ("rabatdeel")
  IFCSLABTYPE "betonvloer_200mm" | BASESLAB | 1 occurrence | material: layers ("beton" 200.) | property sets: EPset_Parametric
  IFCWALLTYPE "kalkzandsteen_214mm" | ELEMENTEDWALL | 1 occurrence | material: layers ("kalkzandsteen" 214.) | property sets: EPset_Parametric

Property sets
  Reference Image | properties | on 1 object (1 IFCBUILDING)
    Position X = "9.802644729614258" (IFCLABEL)
    Position Y = "6.879758358001709" (IFCLABEL)
    Position Z = "0.0" (IFCLABEL)
    Rotation X = "0.0" (IFCLABEL)
    Rotation Y = "-0.0" (IFCLABEL)
    Rotation Z = "0.0" (IFCLABEL)
    Scale X = "3.872007369995117" (IFCLABEL)
    Scale Y = "3.872007369995117" (IFCLABEL)
    Scale Z = "3.872007369995117" (IFCLABEL)
    image A = "C:\Algemeen\07_ifcopenshell\00_ifc\02_ifc_library\15-2088_werktekeningen_uitvoering\00_floor_plan_ground_floor.png" (IFCLABEL)
  EPset_Parametric | properties | on 130 objects (99 IFCCOVERING, 23 IFCMEMBER, 8 IFCBEAM)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 21 objects (21 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 1 object (1 IFCSLAB)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 4 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  EPset_Parametric | properties | on 1 type object
    LayerSetDirection = "AXIS3" (IFCLABEL)
  BBIM_Array | properties | on 68 objects (68 IFCCOVERING)
    Data (no value)
    Parent = "01FL6BYUn7S8DDdO9WeyXx" (IFCLABEL)
  BBIM_Array | properties | on 29 objects (29 IFCCOVERING)
    Data (no value)
    Parent = "2hsVxcMB93WQ1tc1Sx$_u_" (IFCLABEL)
  BBIM_Array | properties | on 14 objects (14 IFCMEMBER)
    Data (no value)
    Parent = "1n_CjfRDPEHhIDSmON5bCL" (IFCLABEL)
  BBIM_Array | properties | on 6 objects (6 IFCMEMBER)
    Data (no value)
    Parent = "0xQuuGnNrAiAWEH5os6VQr" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCMEMBER)
    Data = "[{"children": ["3Eec4zDjD5IPpP1debYq_H", "1QoatBSEn5zeifXmchChhu", "19DIg2$7bBrBzw09YbTGi8", "14PhGGJDz6HRyETSgsyOLq", "2rxG9546D3GedEEVqIJFLu"], "count": 6, "x": 0.0, "y": 550.0, "z": 0.0, "use_local_space": true, "sync_children": false, "dimension_input_type": "Increment"}]" (IFCLABEL)
    Parent = "0xQuuGnNrAiAWEH5os6VQr" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCMEMBER)
    Data = "[{"children": ["1ex_vzppTBlxUA3E1KKfsk", "0N4cz6PY9EfBMuFFgQmYy_", "1d3s2iFZf5gQZesl$yLsop", "3xDZwXFKzERwlM4xYc69OD", "0E6mrA8Gb3FwvUpDlwoAAz", "1pbA_lkyHDzvhqVIOEiZvA", "0iQD_TmFvDkhm_o7smR6av", "3I2D5sQhn2kO7LUxVtavcR", "1VUyw9tQ5F4ehIOG8WqGMK", "0MlKH49hnBWPLKuuDuofGo", "2XXe$OqnT7vBYnfOvs2z7q", "2HGVfQVR1F6Ab4l9q2BJNB", "2v1K7xO9L39Au4XhoA9Q4B", "2ajdx2BFfD5f82qR57F8GV"], "count": 15, "x": 0.0, "y": 550.0, "z": 0.0, "use_local_space": true, "sync_children": false, "dimension_input_type": "Increment"}]" (IFCLABEL)
    Parent = "1n_CjfRDPEHhIDSmON5bCL" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCCOVERING)
    Data = "[{"children": ["0WM0Oxarn7zvKy6nrFQKY0", "2_YS3d1s1A9Qu_0HJVSeFj", "0TWwaPxZH4tOZKbsVqXk5x", "0_5n2103T3_OHUIfWgNjoe", "0JPae8$V9FZebFmdmKfuwc", "21g6ZG5Pn0hPqGq2a22M92", "36IY1ZmQrBJ9b2KnzrgzXr", "36pWZ7Cx98KeIzi5XRkzWZ", "2MLhpo$nnAgwffkrcUSANd", "3q5$JkqznCIhd1tjtcv1mv", "2TRgD1AOb7ExuOnZqiC$z7", "3cYC0IO4X61xBVvcVpNEzp", "1Nt083Nh94eOmWEODlBeRh", "0az9ejOxD3JRFKbh7mfsid", "0vP5DkS8j9A9XBsoNG72vy", "0ow5vlJB19Z8xdfBzUYYKa", "0zGcvroFHFRQysfFtEd7EY", "3T_r9YF1j1qgyfoUX7sRPX", "3o1gam1QXCvxL8SPe8PVFm", "0daLm6F0HBgOiW9KlMuNhr", "281HjS5mL8MeCOkGCiEKu4", "3bRsaf_Xj6_xcjK3lww1A2", "09Qo5sSSv8G9kxoZO1RteF", "12rShpVbf9F9xLZPBJbCdk", "14I1eE0Tr1OBSvJryl4raW", "3uoYAZ3oPCOfMdJmPIOBbi", "1Z2p3Tg0b0r8UNhdSQgP6H", "0o$RVq$_fDOOiVkJUQhhD3", "0IcnXOBDbCQxs_LyqAvu8a"], "count": 30, "x": 0.0, "y": 0.0, "z": -100.0, "use_local_space": false, "sync_children": false, "dimension_input_type": "Increment"}]" (IFCLABEL)
    Parent = "01FL6BYUn7S8DDdO9WeyXx" (IFCLABEL)
  BBIM_Array | properties | on 1 object (1 IFCCOVERING)
    Data = "[{"children": ["0vfVX3cTDDiPUhDQ6jGxgX", "3k3ncX9OnBYgoLOcCMKOSt", "0s3hKabSn8xgTA4ZHTYAlq", "1BbD6$8iXFTgTu4mnzFWck", "2NMk9Cmd53twfB1gOxsevY", "2ZQbLBvDH2awD0ODWdYdRZ", "3FzAPNKtv05viTVnMQDWRe", "1J9x2SHsrBcwLCPp8Oj0xr", "1sISAXAMb1EP5yDcsxk65m", "1pGqmcThr4MRK8GsAIgiC9", "2nIphNBuzAiwIKpE5sR$WX", "2X5bzScdX9uBHLF4wx2uOq", "06qgLfas5DTuvBJZ3cooUS", "0Xj5GdM8L8_QK7uE1QXwCB", "1PhdFvXbf7LgVbS8gOT03s", "3GXWiFCC5F3wIyMGqd7bDs", "3v0P3S3ib7CvcRJMFqqUuG", "1sVPyogsXCcPLiBnP0g6tx", "2BS43PNHHASgatWtBYGz1E", "3ULYCTQBX9fwuc4xe0eH4Q", "3XmGodPLL3D8HIuVPMlme8", "1BRSPDUhf2qgzc3qkFjcoK", "3q6MiD$r17jeUyeWHbo$GI", "2bH5sepM5Cr82SUdEo3IY9", "0q2zqQLhLF_Rmy0_igSKnb", "2UNa$AmpH8nBDKqfbftxlo", "2GgnUVS7jCk8rmX5jLIJr7", "3rVmjtWV57GgkVTfVueYPQ", "3qDl813WP0auJhOqoOdJxh"], "count": 30, "x": 0.0, "y": 0.0, "z": -100.0, "use_local_space": false, "sync_children": false, "dimension_input_type": "Increment"}]" (IFCLABEL)
    Parent = "2hsVxcMB93WQ1tc1Sx$_u_" (IFCLABEL)
  BBIM_reference_image_00_floor_plan_ground_floor.png | properties | on 1 object (1 IFCBUILDING)
    Image ID = "198eb8e1-3419-4784-8590-72a92747a3e2" (IFCLABEL)
    Image Path = "C:\Algemeen\07_ifcopenshell\00_ifc\02_ifc_library\15-2088_werktekeningen_uitvoering\00_floor_plan_ground_floor.png" (IFCLABEL)
    Position X = "9.831565856933594" (IFCLABEL)
    Position Y = "6.848126411437988" (IFCLABEL)
    Position Z = "6.411690264940262e-06" (IFCLABEL)
    Rotation X = "0.0" (IFCLABEL)
    Rotation Y = "-0.0" (IFCLABEL)
    Rotation Z = "0.0" (IFCLABEL)
    Scale X = "3.904116630554199" (IFCLABEL)
    Scale Y = "3.904116630554199" (IFCLABEL)
    Scale Z = "3.904116630554199" (IFCLABEL)